<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="45.3898" y2="0" width="0" layer="20"/>
<wire x1="45.3898" y1="0" x2="45.3898" y2="48.26" width="0" layer="20"/>
<wire x1="45.3898" y1="48.26" x2="0" y2="48.26" width="0" layer="20"/>
<wire x1="0" y1="48.26" x2="0" y2="0" width="0" layer="20"/>
<text>48x, 49x Breakout Board</text>
<text>RevC 11/2020</text>
<text>Juan C.</text>
</plain>
<libraries>
<library name="Analog Devices iSensors">
<packages>
<package name="A3-16PA-2SV(71)-TOP">
</package>
<package name="ADIS1648X">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="Analog Devices iSensors" package="A3-16PA-2SV(71)-TOP" value="A3-16PA-2SV(71)T">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="Analog Devices iSensors" package="ADIS1648X" value="ADIS1648X">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="11"/>
<contactref element="J1" pad="12"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="14"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="13"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="DIO4">
<contactref element="J1" pad="16"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="DIO3/TDO">
<contactref element="J1" pad="15"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="DIO2">
<contactref element="J1" pad="14"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="DIO1">
<contactref element="J1" pad="13"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="DIN">
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="DOUT">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="!CS">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="SCLK">
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="!RST">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="TDI">
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="!TRST">
<contactref element="U1" pad="20"/>
</signal>
<signal name="TCK">
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="TMS">
<contactref element="U1" pad="19"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="!EMU">
<contactref element="U1" pad="21"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
