(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 54)
    (no_connects 0)
    (area 70.757381 47.211 183.618 112.431)
    (thickness 1.6)
    (drawings 13)
    (tracks 125)
    (zones 0)
    (modules 34)
    (nets 57)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.006)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.106)
    (user_trace_width 1.27)
    (user_trace_width 1.778)
    (user_trace_width 2.54)
    (trace_clearance 0.006)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.006)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.027)
    (via_drill 0.017)
    (via_min_size 0.027)
    (via_min_drill 0.013)
    (user_via 0.41 0.03)
    (user_via 1 0.5)
    (uvia_size 0.03)
    (uvia_drill 0.02)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.27 0.97)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 3V3_2)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 RESET)
  (net 5 3V3)
  (net 6 AREF)
  (net 7 GND)
  (net 8 A0)
  (net 9 A1)
  (net 10 A2)
  (net 11 A3)
  (net 12 A4)
  (net 13 A5)
  (net 14 SCK)
  (net 15 MOSI)
  (net 16 MISO)
  (net 17 RX)
  (net 18 TX)
  (net 19 RSRV)
  (net 20 VBAT)
  (net 21 EN)
  (net 22 VUSB)
  (net 23 D0)
  (net 24 D1)
  (net 25 D2)
  (net 26 D3)
  (net 27 D4)
  (net 28 D5)
  (net 29 D6)
  (net 30 SCL)
  (net 31 SDA)
  (net 32 "Net-(J1-Pad3)")
  (net 33 "Net-(K1-Pad1)")
  (net 34 "Net-(K1-Pad3)")
  (net 35 "Net-(K1-Pad4)")
  (net 36 "Net-(K2-Pad1)")
  (net 37 "Net-(K2-Pad3)")
  (net 38 "Net-(K2-Pad4)")
  (net 39 "Net-(L1-Pad1)")
  (net 40 "Net-(L1-Pad2)")
  (net 41 "Net-(L2-Pad1)")
  (net 42 "Net-(L2-Pad2)")
  (net 43 "Net-(Q1-Pad2)")
  (net 44 "Net-(Q2-Pad2)")
  (net 45 RELAY_SIGNAL_1)
  (net 46 RELAY_SIGNAL_2)
  (net 47 ADDR_0)
  (net 48 ADDR_1)
  (net 49 ADDR_2)
  (net 50 "Net-(U1-Pad12)")
  (net 51 "Net-(U1-Pad13)")
  (net 52 "Net-(U1-Pad14)")
  (net 53 "Net-(U1-Pad15)")
  (net 54 "Net-(U1-Pad16)")
  (net 55 "Net-(U1-Pad8)")
  (net 56 "Net-(U1-Pad17)")
  (net_class Default "This is the default net class."
    (clearance 0.006)
    (trace_width 0.006)
    (via_dia 0.027)
    (via_drill 0.017)
    (uvia_dia 0.03)
    (uvia_drill 0.02)
    (add_net 3V3)
    (add_net 3V3_2)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net ADDR_0)
    (add_net ADDR_1)
    (add_net ADDR_2)
    (add_net AREF)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net EN)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(K1-Pad1)")
    (add_net "Net-(K1-Pad3)")
    (add_net "Net-(K1-Pad4)")
    (add_net "Net-(K2-Pad1)")
    (add_net "Net-(K2-Pad3)")
    (add_net "Net-(K2-Pad4)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(L2-Pad2)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad8)")
    (add_net RELAY_SIGNAL_1)
    (add_net RELAY_SIGNAL_2)
    (add_net RESET)
    (add_net RSRV)
    (add_net RX)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net TX)
    (add_net VBAT)
    (add_net VUSB)
  )
  (module Symbols:OSHW-Logo2_14.6x12mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 90.297 67.056)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A1F40D8)
    (at 76.581 62.738)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference PIN1 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A1F40F0)
    (at 76.581 108.458)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference PIN2 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A1F28BE)
    (at 168.783 108.458)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference PIN4 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 130.048 73.152)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 3.81 -2.41) (layer F.SilkS))
    (fp_text value D (at 3.81 2.41) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 3V3_2))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F3068)
    (at 153.1112 73.1012)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 3.81 -2.41) (layer F.SilkS))
    (fp_text value D (at 3.81 2.41) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 3V3_2))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x16_Pitch2.54mm (layer F.Cu) (tedit 5A235C04)
    (at 75.311 66.548)
    (descr "Through hole straight pin header, 1x16, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x16 2.54mm single row")
    (fp_text reference H1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x16 (at 0 40.43) (layer F.Fab) hide)
    (fp_text user %R (at 0 19.05 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 RESET))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 3V3))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 AREF))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND) (zone_connect 2))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 A0))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 A1))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 A2))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 A3))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 A4))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 A5))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 SCK))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 MOSI))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 MISO))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 RX))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 TX))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 RSRV))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x16_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5A1F410A)
    (at 95.631 76.708)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference H2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x12 (at 0 30.27) (layer F.Fab) hide)
    (fp_text user %R (at 0 13.97 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 VBAT))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 EN))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 VUSB))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D0))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 D1))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 D2))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 D3))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 D4))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 D5))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 D6))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 SCL))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 SDA))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:BARREL_JACK (layer F.Cu) (tedit 5A235C2E)
    (at 122.682 74.295 270)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference J1 (at -8.45 5.75 450) (layer F.SilkS))
    (fp_text value Jack-DC (at -6.2 -5.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 22 VUSB))
    (pad 2 thru_hole rect (at -6 0 270) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 7 GND) (zone_connect 2))
    (pad 3 thru_hole rect (at -3 4.7 270) (size 3.5 3.5) (drill 3) (layers *.Cu *.Mask)
      (net 32 "Net-(J1-Pad3)"))
  )
  (module Relays_THT:Relay_SPDT_OMRON-G5LE-1 (layer F.Cu) (tedit 5A1F321C)
    (at 133.858 79.375)
    (descr "Omron Relay SPDT, http://www.omron.com/ecb/products/pdf/en-g5le.pdf")
    (tags "Omron Relay SPDT")
    (fp_text reference K1 (at 0 -3.8) (layer F.SilkS))
    (fp_text value G5LE-14 (at 0 20.95) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(K1-Pad1)"))
    (pad 2 thru_hole oval (at -6 2) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 3V3_2))
    (pad 3 thru_hole oval (at -6 14.2) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 34 "Net-(K1-Pad3)"))
    (pad 4 thru_hole oval (at 6 14.2) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 35 "Net-(K1-Pad4)"))
    (pad 5 thru_hole oval (at 6 2) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Relays_THT.3dshapes/Relay_SPDT_OMRON-G5LE-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relays_THT:Relay_SPDT_OMRON-G5LE-1 (layer F.Cu) (tedit 5A1F2E77)
    (at 156.8958 79.375)
    (descr "Omron Relay SPDT, http://www.omron.com/ecb/products/pdf/en-g5le.pdf")
    (tags "Omron Relay SPDT")
    (fp_text reference K2 (at 0 -3.8) (layer F.SilkS))
    (fp_text value G5LE-14 (at 0 20.95) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.7) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 36 "Net-(K2-Pad1)"))
    (pad 2 thru_hole oval (at -6 2) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 3V3_2))
    (pad 3 thru_hole oval (at -6 14.2) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 "Net-(K2-Pad3)"))
    (pad 4 thru_hole oval (at 6 14.2) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 38 "Net-(K2-Pad4)"))
    (pad 5 thru_hole oval (at 6 2) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Relays_THT.3dshapes/Relay_SPDT_OMRON-G5LE-1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5A1F3136)
    (at 145.796 104.267 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference "Relay 1" (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 "Net-(L1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5A1F2E4C)
    (at 168.656 104.267 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference "Relay 2" (at 1.27 -2.96 90) (layer F.SilkS))
    (fp_text value "Relay 2" (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 "Net-(L2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 "Net-(L2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TSR_1-2433:TSR-1-2433 (layer F.Cu) (tedit 5A235C25)
    (at 108.966 66.294 90)
    (descr TSR-1-2433)
    (tags "Integrated Circuit")
    (fp_text reference P1 (at -0.50851 -1.60514 90) (layer F.SilkS))
    (fp_text value TSR_1-2433 (at -0.50851 -1.60514 90) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.28 1.28) (drill 0.78) (layers *.Cu *.Mask F.SilkS)
      (net 22 VUSB))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.28 1.28) (drill 0.78) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND) (zone_connect 2))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.28 1.28) (drill 0.78) (layers *.Cu *.Mask F.SilkS)
      (net 1 3V3_2))
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A235C57)
    (at 141.1732 70.5612 270)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56 270) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 43 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 5A235C48)
    (at 164.211 70.5612 270)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56 270) (layer F.SilkS))
    (fp_text value PN2222A (at 1.27 2.79 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -3.56 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 44 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F33B7)
    (at 130.048 63.627)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 1K (at 3.81 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 RELAY_SIGNAL_1))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A235C5E)
    (at 130.048 68.326)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(Q1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F320B)
    (at 145.1864 91.313 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 1K (at 3.81 2.31 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 3V3_2))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F344F)
    (at 153.035 63.627)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 1K (at 3.81 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 RELAY_SIGNAL_2))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(Q2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A235C4E)
    (at 153.035 68.326)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 -2.31) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND) (zone_connect 2))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F2F18)
    (at 167.9956 91.313 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 1K (at 3.81 2.31 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 3V3_2))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(L2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 5A1F320F)
    (at 145.161 88.773 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference S1 (at 1.78 0 270) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 450) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
  )
  (module Connectors:GS2 (layer F.Cu) (tedit 586134A1)
    (at 168.021 88.773 180)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference S2 (at 1.78 0 270) (layer F.SilkS))
    (fp_text value GS2 (at -1.8 0 270) (layer F.Fab))
    (pad 1 smd rect (at 0 -0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 0 0.64 180) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5A235CA6)
    (at 120.904 90.17)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference ADDR_0 (at 0.127 4.953 90) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 47 ADDR_0))
    (pad 3 smd rect (at 0 1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (zone_connect 2))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5A235CB1)
    (at 117.856 90.17)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference ADDR_1 (at 0 4.953 90) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 48 ADDR_1))
    (pad 3 smd rect (at 0 1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (zone_connect 2))
  )
  (module Connectors:GS3 (layer F.Cu) (tedit 5A235CB6)
    (at 114.808 90.17)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference ADDR_2 (at 0 4.953 90) (layer F.SilkS))
    (fp_text value GS3 (at 1.8 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 -1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 5 3V3))
    (pad 2 smd rect (at 0 0) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 49 ADDR_2))
    (pad 3 smd rect (at 0 1.27) (size 1.27 0.97) (layers F.Cu F.Paste F.Mask)
      (net 7 GND) (zone_connect 2))
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_MKDS1.5-3pol (layer F.Cu) (tedit 5A1F3230)
    (at 128.8542 105.918)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference T1 (at -3.556 4.318) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 -6.6) (layer F.Fab) hide)
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 35 "Net-(K1-Pad4)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 34 "Net-(K1-Pad3)"))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 "Net-(K1-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS1.5-3pol.wrl
      (at (xyz 0.1968 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_MKDS1.5-3pol (layer F.Cu) (tedit 5A1F3243)
    (at 151.892 105.918)
    (descr "3-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference T2 (at -3.556 4.318) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5 -6.6) (layer F.Fab) hide)
    (fp_text user %R (at 5 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 10 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 38 "Net-(K2-Pad4)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 "Net-(K2-Pad3)"))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 36 "Net-(K2-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS1.5-3pol.wrl
      (at (xyz 0.1968 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-18_W7.62mm (layer F.Cu) (tedit 5A235C1A)
    (at 103.124 88.9)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MCP23008 (at 3.81 22.65) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 10.16) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 SCL))
    (pad 10 thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 RELAY_SIGNAL_1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 SDA))
    (pad 11 thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 RELAY_SIGNAL_2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 ADDR_2))
    (pad 12 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(U1-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 ADDR_1))
    (pad 13 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(U1-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 ADDR_0))
    (pad 14 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(U1-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 3V3))
    (pad 15 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(U1-Pad15)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(U1-Pad16)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(U1-Pad8)"))
    (pad 17 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(U1-Pad17)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND) (zone_connect 2))
    (pad 18 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 3V3))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-18_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:1pin (layer F.Cu) (tedit 5A1F2873)
    (at 168.783 62.738)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference PIN3 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 3) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.556 3.556) (drill 2.54) (layers *.Cu *.Mask))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F3626)
    (at 90.805 94.488 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 2.31 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 SCL))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5A1F363C)
    (at 86.233 97.028 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 3.81 -2.31 270) (layer F.SilkS))
    (fp_text value 4.7K (at 3.81 2.31 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 3V3))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 SDA))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_14.6x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 90.297 67.056 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (dimension 50.8 (width 0.3) (layer Dwgs.User)
    (gr_text "50.800 mm" (at 177.118 85.598 270) (layer Dwgs.User))
    (feature1 (pts (xy 168.783 110.998) (xy 178.468 110.998)))
    (feature2 (pts (xy 168.783 60.198) (xy 178.468 60.198)))
    (crossbar (pts (xy 175.768 60.198) (xy 175.768 110.998)))
    (arrow1a (pts (xy 175.768 110.998) (xy 175.181579 109.871496)))
    (arrow1b (pts (xy 175.768 110.998) (xy 176.354421 109.871496)))
    (arrow2a (pts (xy 175.768 60.198) (xy 175.181579 61.324504)))
    (arrow2b (pts (xy 175.768 60.198) (xy 176.354421 61.324504)))
  )
  (gr_text "Dual I2C Relay Featherwing\nby: Brandon Allen" (at 79.502 86.487 90) (layer B.SilkS))
  (dimension 48.641 (width 0.3) (layer Dwgs.User)
    (gr_text "48.641 mm" (at 98.3615 53.514) (layer Dwgs.User))
    (feature1 (pts (xy 122.682 57.023) (xy 122.682 52.164)))
    (feature2 (pts (xy 74.041 57.023) (xy 74.041 52.164)))
    (crossbar (pts (xy 74.041 54.864) (xy 122.682 54.864)))
    (arrow1a (pts (xy 122.682 54.864) (xy 121.555496 55.450421)))
    (arrow1b (pts (xy 122.682 54.864) (xy 121.555496 54.277579)))
    (arrow2a (pts (xy 74.041 54.864) (xy 75.167504 55.450421)))
    (arrow2b (pts (xy 74.041 54.864) (xy 75.167504 54.277579)))
  )
  (gr_line (start 168.783 110.998) (end 76.581 110.998) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.581 60.198) (end 168.783 60.198) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 97.282 (width 0.3) (layer Dwgs.User)
    (gr_text "97.282 mm" (at 122.682 48.561) (layer Dwgs.User))
    (feature1 (pts (xy 171.323 63.5) (xy 171.323 47.211)))
    (feature2 (pts (xy 74.041 63.5) (xy 74.041 47.211)))
    (crossbar (pts (xy 74.041 49.911) (xy 171.323 49.911)))
    (arrow1a (pts (xy 171.323 49.911) (xy 170.196496 50.497421)))
    (arrow1b (pts (xy 171.323 49.911) (xy 170.196496 49.324579)))
    (arrow2a (pts (xy 74.041 49.911) (xy 75.167504 50.497421)))
    (arrow2b (pts (xy 74.041 49.911) (xy 75.167504 49.324579)))
  )
  (gr_line (start 171.323 108.458) (end 171.323 62.738) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 168.783 108.458) (end 171.323 108.458) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 168.783 62.738) (end 168.783 60.198) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.041 108.458) (end 74.041 62.738) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 76.581 108.458) (end 76.581 110.998) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 76.581 62.738) (end 74.041 62.738) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.323 76.454) (xy 125.222 76.454) (xy 125.222 110.998) (xy 74.041 110.998) (xy 74.041 60.198)
        (xy 171.323 60.198)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.323 76.454) (xy 125.222 76.454) (xy 125.222 110.998) (xy 74.041 110.998) (xy 74.041 60.198)
        (xy 171.323 60.198)
      )
    )
  )
)
