(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 45)
    (tracks 1001)
    (zones 0)
    (modules 45)
    (nets 60)
  )
  (page USLetter)
  (title_block
    (title "Empyrean Alpha/Beta")
    (date 2016-08-07)
    (rev A)
    (company Etherkit)
    (comment 4 "Creative Commons CC-BY-SA")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.16)
    (zone_clearance 0.16)
    (zone_45_only yes)
    (trace_min 0.18)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.2 0.2)
    (pad_drill 0.15)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 VIN)
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 +3.3V)
  (net 9 "Net-(C9-Pad2)")
  (net 10 "Net-(D1-Pad1)")
  (net 11 TX_LED)
  (net 12 "Net-(D2-Pad1)")
  (net 13 RX_LED)
  (net 14 "Net-(D3-Pad1)")
  (net 15 "Net-(D3-Pad2)")
  (net 16 "Net-(D4-Pad1)")
  (net 17 "Net-(F1-Pad1)")
  (net 18 DM)
  (net 19 DP)
  (net 20 "Net-(J1-Pad4)")
  (net 21 SWDIO)
  (net 22 SWDCLK)
  (net 23 "Net-(J2-Pad6)")
  (net 24 "Net-(J2-Pad7)")
  (net 25 "Net-(J2-Pad8)")
  (net 26 RESET)
  (net 27 SPI_MOSI)
  (net 28 SPI_MISO)
  (net 29 SPI_SCK)
  (net 30 SCL)
  (net 31 SDA)
  (net 32 AREF)
  (net 33 A0)
  (net 34 A1)
  (net 35 A2)
  (net 36 A3)
  (net 37 A4)
  (net 38 A5)
  (net 39 D0/UART_RX)
  (net 40 D1/UART_TX)
  (net 41 D13)
  (net 42 D12)
  (net 43 D11)
  (net 44 D10)
  (net 45 D9)
  (net 46 D8)
  (net 47 D7)
  (net 48 D6)
  (net 49 D5)
  (net 50 D4)
  (net 51 D3)
  (net 52 D2)
  (net 53 USB_HOST_EN)
  (net 54 "Net-(R11-Pad1)")
  (net 55 "Net-(U2-Pad22)")
  (net 56 "Net-(U2-Pad37)")
  (net 57 "Net-(U2-Pad38)")
  (net 58 "Net-(JP2-Pad2)")
  (net 59 VUSB)
  (net_class Default "This is the default net class."
    (clearance 0.16)
    (trace_width 0.2)
    (via_dia 0.4)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net AREF)
    (add_net D0/UART_RX)
    (add_net D1/UART_TX)
    (add_net D10)
    (add_net D11)
    (add_net D12)
    (add_net D13)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net D9)
    (add_net DM)
    (add_net DP)
    (add_net GND)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net RESET)
    (add_net RX_LED)
    (add_net SCL)
    (add_net SDA)
    (add_net SPI_MISO)
    (add_net SPI_MOSI)
    (add_net SPI_SCK)
    (add_net SWDCLK)
    (add_net SWDIO)
    (add_net TX_LED)
    (add_net USB_HOST_EN)
    (add_net VIN)
    (add_net VUSB)
  )
  (module EtherkitKicadLibrary:Harwin_M50-3500542 (layer F.Cu) (tedit 5C00334E)
    (at 134.15 105.05 180)
    (solder_mask_margin 0.12)
    (solder_paste_margin -0.12)
    (clearance 0.12)
    (fp_text reference J2 (at -3.65 -1.65 180) (layer F.SilkS))
    (fp_text value "Harwin M50-3500542" (at 0 -2.5 180) (layer F.Fab) hide)
    (pad 10 thru_hole circle (at 2.54 -0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 26 RESET))
    (pad 9 thru_hole circle (at 2.54 0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8 thru_hole circle (at 1.27 -0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J2-Pad8)"))
    (pad 7 thru_hole circle (at 1.27 0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J2-Pad7)"))
    (pad 6 thru_hole circle (at 0 -0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J2-Pad6)"))
    (pad 5 thru_hole circle (at 0 0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at -1.27 -0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 22 SWDCLK))
    (pad 3 thru_hole circle (at -1.27 0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 21 SWDIO))
    (pad 1 thru_hole circle (at -2.54 0.635 180) (size 1 1) (drill 0.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 +3.3V))
  )
  (module EtherkitKicadLibrary:PinHeader_1x03_P2.54mm_Vertical_Unkeyed (layer F.Cu) (tedit 5C0031D0)
    (at 131.61 101.55 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value SPI (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 SPI_SCK))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 SPI_MISO))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 SPI_MOSI))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:PinHeader_1x15_P2.54mm_Vertical_Unkeyed (layer F.Cu) (tedit 5C002988)
    (at 125.01 101.55)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value PinHeader_1x15_P2.54mm_Vertical_Unkeyed (at 0 37.89) (layer F.Fab) hide)
    (fp_text user %R (at 0 17.78 90) (layer F.Fab))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:PinHeader_1x15_P2.54mm_Vertical_Unkeyed (layer F.Cu) (tedit 5C002988)
    (at 143.37 101.55)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value PinHeader_1x15_P2.54mm_Vertical_Unkeyed (at 0 37.89) (layer F.Fab) hide)
    (fp_text user %R (at 0 17.78 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:PinHeader_1x15_P2.54mm_Vertical_Unkeyed (layer F.Cu) (tedit 5C002988)
    (at 141.8 101.55)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X15 (at 0 37.89) (layer F.Fab) hide)
    (fp_text user %R (at 0 17.78 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 +3.3V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 RESET))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 D13))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 D12))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 D11))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 D10))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 D9))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 D8))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 D7))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 D6))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 D5))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 D4))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 D3))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 D2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:PinHeader_1x15_P2.54mm_Vertical_Unkeyed (layer F.Cu) (tedit 5C002988)
    (at 126.55 101.55)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X15 (at 0 37.89) (layer F.Fab) hide)
    (fp_text user %R (at 0 17.78 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 SDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 VUSB))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 VIN))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 +3.3V))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 AREF))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 A0))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 A1))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 A2))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 A3))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 A4))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 A5))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 D0/UART_RX))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 D1/UART_TX))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A8DA6A)
    (at 139.65 143.15 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 1.95 0) (layer F.SilkS))
    (fp_text value 4.7n (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A8BF5C)
    (at 129.1 119.7 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 1.8 0) (layer F.SilkS))
    (fp_text value 10u (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A89F50)
    (at 129.85 132.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.05) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 VIN))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A8BAB8)
    (at 132.95 114.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -1.1 -1.2) (layer F.SilkS))
    (fp_text value 15 (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A8BAC2)
    (at 129.95 114.35 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -0.9 -1.2) (layer F.SilkS))
    (fp_text value 15 (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A89F37)
    (at 135.65 137 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -1.7 0) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A89FA1)
    (at 133.05 133.4)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.05) (layer F.SilkS))
    (fp_text value 10u (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A8C2E3)
    (at 135.45 116.6 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -1.9 -0.5 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A8C295)
    (at 138.55 119.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0 -1.15) (layer F.SilkS))
    (fp_text value 1u (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 57A8BE82)
    (at 129.85 130.45)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 0 -1.05) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58BB3901)
    (at 135.2 113.45 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -1.85 -0.25 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 RESET))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:Lite-On_LTST-C170 (layer F.Cu) (tedit 57A8BD9A)
    (at 129.35 108.6 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D1 (at 2.25 0 180) (layer F.SilkS))
    (fp_text value Red (at 0 -1.75 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at -1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 TX_LED))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:Lite-On_LTST-C170 (layer F.Cu) (tedit 57A8BDD6)
    (at 138.95 108.45 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 2.05 0 180) (layer F.SilkS))
    (fp_text value Yellow (at 0 -1.75 90) (layer F.Fab) hide)
    (pad 1 smd rect (at 1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at -1.05 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 RX_LED))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:Lite-On_LTST-C170 (layer F.Cu) (tedit 57A8C6CA)
    (at 138.95 112.45 270)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D3 (at -1.05 1.5) (layer F.SilkS))
    (fp_text value Blue (at 0 -1.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at 1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at -1.05 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:Lite-On_LTST-C170 (layer F.Cu) (tedit 57A8B898)
    (at 141.2 140.65 180)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D4 (at 1.3 1.3 180) (layer F.SilkS))
    (fp_text value Green (at 0 -1.75 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210 (layer F.Cu) (tedit 57A8A2A7)
    (at 127.45 140.9 180)
    (descr "Resistor SMD 1210, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference F1 (at -2.7 -1.3 180) (layer F.SilkS))
    (fp_text value "Bel 0ZCH0050FF2G" (at 0 2.7 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(F1-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 2.5) (layers F.Cu F.Paste F.Mask)
      (net 4 VIN))
    (model Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:FCI_10118194-0001LF (layer F.Cu) (tedit 57A8A2BA)
    (at 134.15 145.6)
    (solder_mask_margin 0.1)
    (clearance 0.1)
    (fp_text reference J1 (at -2.2 -0.7) (layer F.SilkS))
    (fp_text value "FCI 10118194-0001LF" (at 0 -5.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.3 -4.15) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 59 VUSB))
    (pad 2 smd rect (at -0.65 -4.15) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 18 DM))
    (pad 3 smd rect (at 0 -4.15) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 19 DP))
    (pad 4 smd rect (at 0.65 -4.15) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.3 -4.15) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.5 -4.15) (size 1.45 1.15) (drill oval 0.85 0.55) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 6 thru_hole oval (at -2.5 -4.15) (size 1.45 1.15) (drill oval 0.85 0.55) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 6 thru_hole oval (at 3.5 -1.45) (size 1.2 1.75) (drill oval 0.6 1.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 6 thru_hole oval (at -3.5 -1.45) (size 1.2 1.75) (drill oval 0.6 1.15) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8BF88)
    (at 129.25 116.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 0.05 -1.3) (layer F.SilkS))
    (fp_text value 10u (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8BD10)
    (at 129.6 104.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.65 0) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8DA62)
    (at 141.35 143.15 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.95 0) (layer F.SilkS))
    (fp_text value 1M (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8C670)
    (at 138.45 117.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.65 1.25) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 USB_HOST_EN))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad4)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8BD4A)
    (at 138.75 104.65 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.65 0) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8C70C)
    (at 138.7 115.2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -1.8 0.3) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8B8AF)
    (at 138.4 140.3 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 1.75 0.05) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(JP2-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58BB38D9)
    (at 132.8 112.7 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0.5 1.2 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 RESET))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8C4B2)
    (at 129.85 112.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 -1.2) (layer F.SilkS))
    (fp_text value 330 (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 RESET))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:Alps_SKQMASE010 (layer F.Cu) (tedit 58BB38E8)
    (at 134.15 109)
    (fp_text reference S1 (at -3.7 1.7) (layer F.SilkS))
    (fp_text value "Alps SKQMASE010" (at 0 -2.7) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.7 0) (size 1.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(R11-Pad1)"))
    (pad 2 smd rect (at 2.7 0) (size 1.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module EtherkitKicadLibrary:SOT23-5 (layer F.Cu) (tedit 57A89F5A)
    (at 133.25 136.6)
    (attr smd)
    (fp_text reference U1 (at 0 -1.35) (layer F.SilkS))
    (fp_text value LP2985 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.27) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 4 VIN))
    (pad 3 smd rect (at 0.9525 1.27) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 4 VIN))
    (pad 5 smd rect (at -0.9525 -1.27) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0 1.27) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.9525 -1.27) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8A28E)
    (at 135.4 139.55)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference VR1 (at 1.65 -0.05 90) (layer F.SilkS))
    (fp_text value CG0603MLC-05E (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 DP))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 57A8A296)
    (at 132.7 139.55 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference VR2 (at 1.55 0 270) (layer F.SilkS))
    (fp_text value CG0603MLC-05E (at 0 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 DM))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:ECS_ECS-.327-12.5-34B-TR (layer F.Cu) (tedit 57A8A1A8)
    (at 132.2 117.55 225)
    (fp_text reference X1 (at 2.687006 -0.282843 315) (layer F.SilkS))
    (fp_text value ECS-.327-12.5-34B-TR (at 0 -1.95 225) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.249999 0 225) (size 1.1 1.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.249999 0 225) (size 1.1 1.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
  )
  (module EtherkitKicadLibrary:TQFP-48_7x7mm_Pitch0.5mm (layer F.Cu) (tedit 57A8C8D1)
    (at 134.15 125 315)
    (descr "48 LEAD TQFP 7x7mm (see MICREL TQFP7x7-48LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U2 (at 3.818377 4.242641 315) (layer F.SilkS))
    (fp_text value ATSAMD21GxA (at 0 -6.05 315) (layer F.Fab) hide)
    (pad 1 smd rect (at -4.35 -2.75 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -4.35 -2.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 3 smd rect (at -4.35 -1.749999 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 33 A0))
    (pad 4 smd rect (at -4.35 -1.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 32 AREF))
    (pad 5 smd rect (at -4.35 -0.750001 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.35 -0.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 7 smd rect (at -4.35 0.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 34 A1))
    (pad 8 smd rect (at -4.35 0.750001 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 35 A2))
    (pad 9 smd rect (at -4.35 1.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 36 A3))
    (pad 10 smd rect (at -4.35 1.749999 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 37 A4))
    (pad 11 smd rect (at -4.35 2.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 46 D8))
    (pad 12 smd rect (at -4.35 2.75 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 45 D9))
    (pad 13 smd rect (at -2.75 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 D4))
    (pad 14 smd rect (at -2.25 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 51 D3))
    (pad 15 smd rect (at -1.749999 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 40 D1/UART_TX))
    (pad 16 smd rect (at -1.25 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 39 D0/UART_RX))
    (pad 17 smd rect (at -0.750001 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 18 smd rect (at -0.25 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 0.25 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 SPI_MOSI))
    (pad 20 smd rect (at 0.750001 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 29 SPI_SCK))
    (pad 21 smd rect (at 1.25 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 28 SPI_MISO))
    (pad 22 smd rect (at 1.749999 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U2-Pad22)"))
    (pad 23 smd rect (at 2.25 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 52 D2))
    (pad 24 smd rect (at 2.75 4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 D5))
    (pad 25 smd rect (at 4.35 2.75 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 43 D11))
    (pad 26 smd rect (at 4.35 2.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 41 D13))
    (pad 27 smd rect (at 4.35 1.749999 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 44 D10))
    (pad 28 smd rect (at 4.35 1.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 42 D12))
    (pad 29 smd rect (at 4.35 0.750001 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 48 D6))
    (pad 30 smd rect (at 4.35 0.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 47 D7))
    (pad 31 smd rect (at 4.35 -0.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 31 SDA))
    (pad 32 smd rect (at 4.35 -0.750001 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 30 SCL))
    (pad 33 smd rect (at 4.35 -1.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 DM))
    (pad 34 smd rect (at 4.35 -1.749999 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 DP))
    (pad 35 smd rect (at 4.35 -2.25 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 36 smd rect (at 4.35 -2.75 315) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 37 smd rect (at 2.75 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U2-Pad37)"))
    (pad 38 smd rect (at 2.25 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U2-Pad38)"))
    (pad 39 smd rect (at 1.749999 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 TX_LED))
    (pad 40 smd rect (at 1.25 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 RESET))
    (pad 41 smd rect (at 0.750001 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 USB_HOST_EN))
    (pad 42 smd rect (at 0.25 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 43 smd rect (at -0.25 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad2)"))
    (pad 44 smd rect (at -0.750001 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 45 smd rect (at -1.25 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 22 SWDCLK))
    (pad 46 smd rect (at -1.749999 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 21 SWDIO))
    (pad 47 smd rect (at -2.25 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 38 A5))
    (pad 48 smd rect (at -2.75 -4.35 45) (size 1.3 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 RX_LED))
    (model Housings_QFP.3dshapes/TQFP-48_7x7mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model /usr/share/kicad/modules/packages3d/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:OSHWLogo4mm (layer B.Cu) (tedit 0)
    (at 130.7 109.3 180)
    (fp_text reference G*** (at 0 -2.35966 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0 2.35966 180) (layer B.SilkS) hide)
  )
  (module EtherkitKicadLibrary:EtherkitLogoSmall (layer B.Cu) (tedit 0)
    (at 138.7 109.75 180)
    (fp_text reference Ref** (at 0 -3.25 180) (layer B.SilkS) hide)
    (fp_text value Val** (at 0 2.95 180) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58BB1D4D)
    (at 139.2 130 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 1.5) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 +3.3V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:SOT523 (layer F.Cu) (tedit 58BB38F9)
    (at 136.85 113.2)
    (descr SOT23)
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at -0.1 1.35) (layer F.SilkS))
    (fp_text value DMG1012T-7 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.5 -0.65) (size 0.4 0.51) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.5 -0.65) (size 0.4 0.51) (layers F.Cu F.Paste F.Mask)
      (net 41 D13))
    (pad 3 smd rect (at 0 0.65) (size 0.4 0.51) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:SOLDER_JUMPER_NC (layer F.Cu) (tedit 5BFF2FE3)
    (at 129.87 137.79 180)
    (fp_text reference JP1 (at 0 1.52 180) (layer F.SilkS))
    (fp_text value "VUSB Disable" (at -0.2 -0.15 180) (layer F.Fab) hide)
    (pad 2 smd trapezoid (at 0.7 0 180) (size 0.5 1.5) (rect_delta 0.5 0 ) (layers F.Cu F.Mask)
      (net 17 "Net-(F1-Pad1)") (zone_connect 2))
    (pad 1 smd trapezoid (at -0.7 0 180) (size 0.5 1.5) (rect_delta -0.5 0 ) (layers F.Cu F.Mask)
      (net 59 VUSB) (zone_connect 2))
    (pad 1 smd rect (at -0.32 0 180) (size 0.3 2) (layers F.Cu F.Mask)
      (net 59 VUSB) (zone_connect 2))
    (pad 2 smd rect (at 0.32 0 180) (size 0.3 2) (layers F.Cu F.Mask)
      (net 17 "Net-(F1-Pad1)"))
    (pad "" smd rect (at 0 0 180) (size 1 0.5) (layers F.Cu F.Mask))
  )
  (module EtherkitKicadLibrary:SOLDER_JUMPER_NC (layer B.Cu) (tedit 5BFF2B08)
    (at 140.7 141.2 180)
    (fp_text reference JP2 (at 0 -2.2 180) (layer B.SilkS))
    (fp_text value "Power LED Enable" (at 0 -1.95 180) (layer B.Fab) hide)
    (pad "" smd rect (at 0 0 180) (size 1 0.5) (layers B.Cu B.Mask))
    (pad 2 smd rect (at 0.32 0 180) (size 0.3 2) (layers B.Cu B.Mask)
      (net 58 "Net-(JP2-Pad2)"))
    (pad 1 smd rect (at -0.32 0 180) (size 0.3 2) (layers B.Cu B.Mask)
      (net 8 +3.3V) (zone_connect 2))
    (pad 1 smd trapezoid (at -0.7 0 180) (size 0.5 1.5) (rect_delta -0.5 0 ) (layers B.Cu B.Mask)
      (net 8 +3.3V) (zone_connect 2))
    (pad 2 smd trapezoid (at 0.7 0 180) (size 0.5 1.5) (rect_delta 0.5 0 ) (layers B.Cu B.Mask)
      (net 58 "Net-(JP2-Pad2)") (zone_connect 2))
  )
  (module EtherkitKicadLibrary:PinHeader_1x03_P2.54mm_Vertical_Unkeyed (layer F.Cu) (tedit 5C002B5A)
    (at 131.61 100 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value PinHeader_1x03_P2.54mm_Vertical_Unkeyed (at 0 7.41 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text MOSI (at 130.4 101.55 90) (layer F.SilkS))
  (gr_text MISO (at 132.9 101.6 90) (layer F.SilkS))
  (gr_text SCK (at 135.45 101.6 90) (layer F.SilkS))
  (gr_text "Creative Commons\nLicense\nCC BY-SA 4.0" (at 139.45 136.45) (layer B.SilkS))
  (gr_text 2019 (at 139.45 117.1) (layer B.SilkS))
  (gr_text etherkit.com (at 139.55 115.4) (layer B.SilkS))
  (gr_text "Empyrean α/β" (at 134.25 113.55) (layer B.SilkS))
  (gr_text β (at 126 143.7) (layer B.SilkS))
  (gr_text α (at 126.1 141.4) (layer B.SilkS))
  (gr_text "Beta 1" (at 127.2 139.9) (layer B.Cu))
  (gr_text PWR (at 142.2 139.35) (layer F.SilkS))
  (gr_text D2 (at 140.35 137 90) (layer F.SilkS))
  (gr_text D3 (at 140.35 134.55 90) (layer F.SilkS))
  (gr_text D4 (at 140.35 132.05 90) (layer F.SilkS))
  (gr_text D5 (at 140.35 129.5 90) (layer F.SilkS))
  (gr_text D6 (at 140.35 126.95 90) (layer F.SilkS))
  (gr_text D7 (at 140.35 124.45 90) (layer F.SilkS))
  (gr_text D8 (at 140.35 121.95 90) (layer F.SilkS))
  (gr_text D9 (at 140.35 119.3 90) (layer F.SilkS))
  (gr_text D10 (at 140.35 116.8 90) (layer F.SilkS))
  (gr_text D11 (at 140.35 114.25 90) (layer F.SilkS))
  (gr_text D12 (at 140.35 111.7 90) (layer F.SilkS))
  (gr_text D13 (at 140.35 109.15 90) (layer F.SilkS))
  (gr_text RST (at 140.35 106.6 90) (layer F.SilkS))
  (gr_text GND (at 140.35 104.05 90) (layer F.SilkS))
  (gr_text SCL (at 128 101.55 270) (layer F.SilkS))
  (gr_text SDA (at 128 104.15 270) (layer F.SilkS))
  (gr_text VUSB (at 128 106.65 270) (layer F.SilkS))
  (gr_text VIN (at 128 109.15 270) (layer F.SilkS))
  (gr_text 3.3V (at 128 111.75 270) (layer F.SilkS))
  (gr_text GND (at 128 114.4 270) (layer F.SilkS))
  (gr_text AREF (at 128 116.9 270) (layer F.SilkS))
  (gr_text A0 (at 128 119.4 270) (layer F.SilkS))
  (gr_text A1 (at 128 121.9 270) (layer F.SilkS))
  (gr_text A2 (at 128 124.55 270) (layer F.SilkS))
  (gr_text A3 (at 128 127.05 270) (layer F.SilkS))
  (gr_text A4 (at 128 129.55 270) (layer F.SilkS))
  (gr_text A5 (at 128 132.05 270) (layer F.SilkS))
  (gr_text D0 (at 128 134.5 270) (layer F.SilkS))
  (gr_text 3.3V (at 140.35 101.55 90) (layer F.SilkS))
  (gr_text D1 (at 128 137.05 270) (layer F.SilkS))
  (gr_line (start 125 145.6) (end 125 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.3 145.6) (end 125 145.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.3 100) (end 143.3 145.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 100) (end 143.3 100) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.18))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.18) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 130 145.6) (xy 130 143) (xy 130.5 143) (xy 130.5 141) (xy 137.8 141)
        (xy 137.8 143) (xy 138.3 143) (xy 138.3 145.6)
      )
    )
  )
  (zone (net 2) (net_name "Net-(C1-Pad2)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 130 145.6) (xy 130 143) (xy 130.5 143) (xy 130.5 141) (xy 137.8 141)
        (xy 137.8 143) (xy 138.3 143) (xy 138.3 145.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.16))
    (min_thickness 0.18)
    (fill yes (arc_segments 16) (thermal_gap 0.16) (thermal_bridge_width 0.22) (smoothing chamfer))
    (polygon
      (pts
        (xy 125 145.6) (xy 125 100) (xy 143.3 100) (xy 143.3 145.6) (xy 138.6 145.6)
        (xy 138.6 143) (xy 138.6 140.8) (xy 129.75 140.8) (xy 129.75 143) (xy 129.75 145.6)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.16))
    (min_thickness 0.18)
    (fill yes (arc_segments 32) (thermal_gap 0.16) (thermal_bridge_width 0.22) (smoothing chamfer))
    (polygon
      (pts
        (xy 125 145.6) (xy 125 100) (xy 143.3 100) (xy 143.3 145.6) (xy 138.6 145.6)
        (xy 138.6 143) (xy 138.6 140.8) (xy 129.75 140.8) (xy 129.75 143) (xy 129.75 145.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.18) (thermal_bridge_width 0.22))
    (polygon
      (pts
        (xy 127.3 140.9) (xy 127.3 142.25) (xy 128.65 142.25) (xy 128.65 140.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.18) (thermal_bridge_width 0.22))
    (polygon
      (pts
        (xy 127.3 143.05) (xy 127.3 144.4) (xy 128.65 144.4) (xy 128.65 143.05)
      )
    )
  )
)
