<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="12.7" y1="0" x2="12.7" y2="10.16" width="0.254" layer="20"/>
<wire x1="12.7" y1="10.16" x2="0" y2="10.16" width="0.254" layer="20"/>
<wire x1="0" y1="10.16" x2="0" y2="0" width="0.254" layer="20"/>
<wire x1="0" y1="0" x2="12.7" y2="0" width="0.254" layer="20"/>
<text>MSOP10</text>
<text>KD0GLS</text>
<text>2019</text>
</plain>
<libraries>
<library name="kd0gls">
<description>KD0GLS Amateur Radio Design Library</description>
<packages>
<package name="PIN_SQUARE">
</package>
<package name="PIN_ROUND">
</package>
<package name="MSOP10">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="1" library="kd0gls" package="PIN_SQUARE" value="PIN_SQUARE"/>
<element name="2" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="3" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="4" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="5" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="6" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="7" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="8" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="9" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="10" library="kd0gls" package="PIN_ROUND" value="PIN_ROUND"/>
<element name="U1" library="kd0gls" package="MSOP10" value="CS4344"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="1" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="2" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="3" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="4" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="5" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="6" pad="1"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="7" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="8" pad="1"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="9" pad="1"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="10" pad="1"/>
<contactref element="U1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
