(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6002)
    (drawings 7)
    (tracks 71)
    (zones 0)
    (modules 2)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.127)
    (segment_width 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (solder_mask_min_width 0.1)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 /1)
  (net 2 /0)
  (net 3 /3)
  (net 4 /2)
  (net 5 /5)
  (net 6 /4)
  (net 7 /7)
  (net 8 /6)
  (net 9 /9)
  (net 10 /8)
  (net 11 /Anode)
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /0)
    (add_net /1)
    (add_net /2)
    (add_net /3)
    (add_net /4)
    (add_net /5)
    (add_net /6)
    (add_net /7)
    (add_net /8)
    (add_net /9)
    (add_net /Anode)
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module mynixies:mynixies-SK-116-2 (layer F.Cu) (tedit 200000)
    (at 159.5 109)
    (attr virtual)
    (fp_text reference NX1 (at 0 -7.5) (layer F.SilkS) hide)
    (fp_text value "Tube Other Side" (at 0 -8) (layer B.SilkS))
    (pad P$12 thru_hole circle (at 4.32816 2.49936) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 10 /8))
    (pad P$11 thru_hole circle (at 2.49936 4.32816) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 7 /7))
    (pad P$10 thru_hole circle (at 0 4.99872) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 8 /6))
    (pad P$9 thru_hole circle (at -2.49936 4.32816) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 5 /5))
    (pad P$8 thru_hole circle (at -4.32816 2.49936) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 6 /4))
    (pad P$7 thru_hole circle (at -4.99872 0) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 3 /3))
    (pad P$6 thru_hole circle (at -4.32816 -2.49936) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 4 /2))
    (pad P$5 thru_hole circle (at -2.49936 -4.32816) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad P$4 thru_hole circle (at 0 -4.99872) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask))
    (pad P$3 thru_hole circle (at 2.49936 -4.32816) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 11 /Anode))
    (pad P$2 thru_hole circle (at 4.32816 -2.49936) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 2 /0))
    (pad P$1 thru_hole circle (at 4.99872 0) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Mask)
      (net 9 /9))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A42B)
    (at 153.15 121.77 270)
    (descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x06 2.54mm double row")
    (fp_text reference J1 (at -1.27 2.77 270) (layer B.SilkS) hide)
    (fp_text value "Socket This Side" (at -4.77 -6.35 180) (layer B.SilkS))
    (fp_text user %R (at -1.27 -6.35) (layer B.Fab))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /0))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /2))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /4))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /7))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /6))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /9))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /8))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Anode))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Anode))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Mill-Max 0665-0-15-15-30-27-10-0" (at 159.5 102.25) (layer B.SilkS))
  (gr_text XN-12/CD66 (at 159.5 101.75) (layer F.SilkS))
  (gr_circle (center 159.5 109) (end 162.854102 109) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 150 124) (end 150 100) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 169 124) (end 150 124) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 169 100) (end 169 124) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 150 100) (end 169 100) (layer Edge.Cuts) (width 0.127))
)
