(kicad_pcb (version 20171130) (host pcbnew "(5.1.2-1)-1")
  (general
    (thickness 1.6)
    (drawings 11)
    (tracks 42)
    (zones 0)
    (modules 7)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 SDA)
  (net 2 SCL)
  (net 3 VDD)
  (net 4 GND)
  (net 5 "Net-(JP1-Pad2)")
  (net 6 "Net-(TP1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(TP1-Pad1)")
    (add_net SCL)
    (add_net SDA)
    (add_net VDD)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5FE8CD1D)
    (at 126.365 69.215 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value "Pin Header" (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 SCL))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 SDA))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VDD))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer B.Cu) (tedit 5A0F774F)
    (at 126.619 61.214)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference INT (at 0 1.448) (layer B.SilkS))
    (fp_text value INT (at 0 -1.55) (layer B.Fab))
    (fp_text user %R (at 0 1.45) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (net 6 "Net-(TP1-Pad1)"))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 129.032 59.055 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.286 0 270) (layer F.SilkS))
    (fp_text value SDA_PU (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VDD))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 131.191 59.055 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.286 0 270) (layer F.SilkS))
    (fp_text value SCL_PU (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VDD))
    (pad 1 smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 133.477 61.087 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.413 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VDD))
    (pad 1 smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module siege:veml6030 (layer F.Cu) (tedit 5FE8C1F5)
    (at 130.175 62.58)
    (fp_text reference U1 (at 0 2.825) (layer F.SilkS) hide)
    (fp_text value VEML6030 (at 0 -2) (layer F.Fab))
    (pad 6 smd rect (at 0.85 -0.65) (size 0.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 VDD))
    (pad 5 smd rect (at 0.85 0) (size 0.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 SCL))
    (pad 4 smd rect (at 0.875 0.65) (size 0.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(JP1-Pad2)"))
    (pad 3 smd rect (at -0.875 0.65) (size 0.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(TP1-Pad1)"))
    (pad 2 smd rect (at -0.875 0) (size 0.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 SDA))
    (pad 1 smd rect (at -0.875 -0.65) (size 0.55 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_Pad1.0x1.5mm (layer B.Cu) (tedit 5C756B4C)
    (at 130.175 65.405)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.8) (layer B.SilkS) hide)
    (fp_text value ADDR_SET (at 0 -2 45) (layer B.Fab) hide)
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 5 "Net-(JP1-Pad2)"))
    (pad 3 smd rect (at 1.3 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 4 GND))
    (pad 1 smd rect (at -1.3 0) (size 1 1.5) (layers B.Cu B.Mask)
      (net 3 VDD))
  )
  (gr_text SCL (at 133.985 66.294 90) (layer F.SilkS))
  (gr_text SDA (at 131.445 66.294 90) (layer F.SilkS))
  (gr_text VDD (at 128.905 66.294 90) (layer F.SilkS))
  (gr_text GND (at 126.365 66.421 90) (layer F.SilkS))
  (gr_text VEML6030 (at 129.921 56.769) (layer B.SilkS))
  (gr_text 0x10 (at 133.858 65.405) (layer B.SilkS))
  (gr_text 0x48 (at 126.492 65.405) (layer B.SilkS))
  (gr_line (start 135.763 55.118) (end 124.587 55.118) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 135.763 70.993) (end 135.763 55.118) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.587 70.993) (end 135.763 70.993) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.587 70.993) (end 124.587 55.118) (layer Edge.Cuts) (width 0.05))
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 124.587 55.118) (xy 135.763 55.118) (xy 135.763 70.993) (xy 124.587 70.993)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 124.587 55.118) (xy 135.763 55.118) (xy 135.763 70.993) (xy 124.587 70.993)
      )
    )
  )
)
