(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 50)
    (no_connects 0)
    (area 120.5726 74.3 201.35 118.8834)
    (thickness 1.6002)
    (drawings 14)
    (tracks 163)
    (zones 0)
    (modules 29)
    (nets 20)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.508)
    (user_trace_width 0.254)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 1.27)
    (user_trace_width 2.032)
    (user_trace_width 2.54)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory cap_switch_gerber_rev_2/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 ICSPDAT)
  (net 3 ICSPCLK)
  (net 4 MCLR)
  (net 5 RELAY)
  (net 6 "Net-(D1-Pad1)")
  (net 7 +5V)
  (net 8 CAP_SEN)
  (net 9 "Net-(C4-Pad1)")
  (net 10 "Net-(D1-Pad2)")
  (net 11 "Net-(D3-Pad1)")
  (net 12 "Net-(D3-Pad2)")
  (net 13 "Net-(D7-Pad2)")
  (net 14 "Net-(BUTTON1-Pad1)")
  (net 15 "Net-(LIGHT1-Pad1)")
  (net 16 "Net-(REL1-Pad3)")
  (net 17 "Net-(REL1-Pad4)")
  (net 18 "Net-(D6-Pad3)")
  (net 19 "Net-(D8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +5V)
    (add_net CAP_SEN)
    (add_net GND)
    (add_net ICSPCLK)
    (add_net ICSPDAT)
    (add_net MCLR)
    (add_net "Net-(BUTTON1-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D6-Pad3)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(LIGHT1-Pad1)")
    (add_net "Net-(REL1-Pad3)")
    (add_net "Net-(REL1-Pad4)")
    (add_net RELAY)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58BDDDE5)
    (at 152.5 98 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.456 0.083 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Bottom) (tedit 58BC70AE)
    (at 149.09 102.28 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0.254 -1.778 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers Bottom B.Paste B.Mask)
      (net 9 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers Bottom B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer Bottom) (tedit 58BDE10C)
    (at 152.146 93.98 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D6 (at -3.7338 2.3876 90) (layer B.SilkS))
    (fp_text value SBAS116LT1G (at 0 -2.5 90) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers Bottom B.Paste B.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers Bottom B.Paste B.Mask))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers Bottom B.Paste B.Mask)
      (net 18 "Net-(D6-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes\SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer Bottom) (tedit 583F3954)
    (at 162.814 111.76)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D8 (at 0 2.5) (layer B.SilkS))
    (fp_text value SBAS116LT1G (at 0 -2.5) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers Bottom B.Paste B.Mask)
      (net 19 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers Bottom B.Paste B.Mask))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers Bottom B.Paste B.Mask)
      (net 7 +5V))
    (model TO_SOT_Packages_SMD.3dshapes\SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer Top) (tedit 58BC70FD)
    (at 141.47 92.882 180)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference P1 (at -0.762 -2.794 180) (layer F.SilkS))
    (fp_text value PROG (at 1.27 4.93 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 ICSPDAT))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 MCLR))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 ICSPCLK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer Top) (tedit 58BC7020)
    (at 126.484 115.996)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at -2.032 0) (layer F.SilkS))
    (fp_text value TBD (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(LIGHT1-Pad1)"))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer Top) (tedit 58BC7024)
    (at 126.484 112.948)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at -2.032 0) (layer F.SilkS))
    (fp_text value TBD (at 0.95 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(LIGHT1-Pad1)"))
    (pad 2 thru_hole oval (at 1.9 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer Top) (tedit 5874F706)
    (at 145.534 100.502 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 0.95 -1.86 270) (layer F.SilkS))
    (fp_text value TBD (at 0.95 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 2 thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(C4-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer Bottom) (tedit 58BDE111)
    (at 153.916 89.834 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.4116 -1.7838 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.7 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 4 MCLR))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers Bottom B.Paste B.Mask)
      (net 18 "Net-(D6-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical (layer Top) (tedit 5874F706)
    (at 145.534 105.074 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 0.95 -1.86 270) (layer F.SilkS))
    (fp_text value TBD (at 0.95 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(D7-Pad2)"))
    (pad 2 thru_hole oval (at 1.9 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 RELAY))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib:OJ-SH-105LM-000 (layer Top) (tedit 58972F91)
    (at 167.632 116.758 90)
    (fp_text reference REL1 (at 5.1308 -8.4916 90) (layer F.SilkS))
    (fp_text value OJ-SH-105LM-000 (at 8.255 -5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 1.25 -1.3 90) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 +5V))
    (pad 2 thru_hole rect (at 1.25 -8.9 90) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask)
      (net 19 "Net-(D8-Pad1)"))
    (pad 3 thru_hole rect (at 16.49 -8.9 90) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 "Net-(REL1-Pad3)"))
    (pad 4 thru_hole rect (at 13.95 -1.3 90) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 "Net-(REL1-Pad4)"))
    (model ../../../../../../Users/Michael/Desktop/Projects/Capacitive_Switch_2017-02-04/lib.pretty/ENG_CVM_CVM_1461404-1_C2.3d_stp/1461404-1.wrl
      (at (xyz 0.36 0.2 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 180 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3Lead_TabPin2 (layer Top) (tedit 58B9F0AF)
    (at 138.5 101)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value NCV8664 (at 0 4.5) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0) (size 2 3.8) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers Top F.Paste F.Mask)
      (net 7 +5V))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers Top F.Paste F.Mask)
      (net 14 "Net-(BUTTON1-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer Top) (tedit 0)
    (at 152.5 94 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U2 (at 0 -1.27 90) (layer F.SilkS))
    (fp_text value PIC12F1572 (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 2 ICSPDAT))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 3 ICSPCLK))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 8 CAP_SEN))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 4 MCLR))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 9 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 5 RELAY))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers Top F.Paste F.Mask)
      (net 7 +5V))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm_FlatTop (layer Bottom) (tedit 58BC70A7)
    (at 152.5 101 270)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 1.28 -2.94 270) (layer B.SilkS))
    (fp_text value LED_W (at 1.27 -2.96 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(C4-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm_FlatTop (layer Bottom) (tedit 5880A862)
    (at 152.5 109 90)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D7 (at 1.27 2.96 90) (layer B.SilkS))
    (fp_text value LED_R (at 1.27 -2.96 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer Top) (tedit 58BDE08C)
    (at 127.5 97.708 270)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference BUTTON1 (at 1.86 -2.3194 270) (layer F.SilkS))
    (fp_text value Conn_Lumberg (at 1.75 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(BUTTON1-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer Top) (tedit 58BC7170)
    (at 145.5 93)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference CAP_SENS1 (at 1.812 -3.166) (layer F.SilkS))
    (fp_text value Capacitive_Button (at 0 4.93) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 CAP_SEN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 ICSPCLK))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_D3.0mm_FlatTop (layer Bottom) (tedit 5880A862)
    (at 170.5 114)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm_FlatTop (layer Bottom) (tedit 5880A862)
    (at 170.5 92)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm_FlatTop (layer Bottom) (tedit 5880A862)
    (at 132.5 114)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm_FlatTop (layer Bottom) (tedit 5880A862)
    (at 132.5 92)
    (descr "LED, Round, FlatTop, diameter 3.0mm, 2 pins, http://www.kingbright.com/attachments/file/psearch/000/00/00/L-47XEC(Ver.9A).pdf")
    (tags "LED Round FlatTop diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 1.27 2.96) (layer B.SilkS))
    (fp_text value LED (at 1.27 -2.96) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED_D3.0mm_FlatTop.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer Top) (tedit 58BDE099)
    (at 127.5 105.328 270)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference LIGHT1 (at 1.4536 -2.3702 270) (layer F.SilkS))
    (fp_text value Conn_Lumberg (at 1.75 6 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(LIGHT1-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer Top) (tedit 58BDE0A8)
    (at 177.03 105.328 90)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference RELAY1 (at 1.8484 -2.1764 90) (layer F.SilkS))
    (fp_text value Conn_Lumberg (at 1.75 6 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(REL1-Pad3)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "Net-(REL1-Pad4)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_PT-3.5mm_2pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer Top) (tedit 58BC705B)
    (at 132.5 100 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.042 -0.08 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 14 "Net-(BUTTON1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer Top) (tedit 5862ED52)
    (at 178.5 92)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P2 (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.39) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer Top) (tedit 58BC69A3)
    (at 178.5 114)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (fp_text reference P3 (at 2.34 -3.592) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 3.85) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer Top) (tedit 58BC6998)
    (at 126.5 92)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (fp_text reference P4 (at 3.54 -2.42) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 3.85) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer Top) (tedit 58C3203B)
    (at 145.5 113 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at 3.006 -3.586 180) (layer F.SilkS))
    (fp_text value BSP75N (at 0 4.5 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers Top F.Paste F.Mask)
      (net 19 "Net-(D8-Pad1)"))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers Top F.Paste F.Mask)
      (net 5 RELAY))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-C_EIA-6032-28_Hand (layer Top) (tedit 57B6E980)
    (at 136.652 107.696 180)
    (descr "Tantalum capacitor, Case C, EIA 6032-28, 6.0x3.2x2.5mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at 0 -3.35 180) (layer F.SilkS))
    (fp_text value 22uF (at 0 3.35 180) (layer F.Fab))
    (pad 1 smd rect (at -3.125 0 180) (size 3.75 2.5) (layers Top F.Paste F.Mask)
      (net 7 +5V))
    (pad 2 smd rect (at 3.125 0 180) (size 3.75 2.5) (layers Top F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-C_EIA-6032-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MP 2017" (at 133.2 103.1 90) (layer B.SilkS))
  (gr_text BU+ (at 124.46 97.79 90) (layer B.SilkS))
  (gr_text LED+ (at 124.46 105.156 90) (layer B.SilkS))
  (gr_text GND (at 124.46 101.346 90) (layer B.SilkS))
  (gr_text GND (at 124.46 108.966 90) (layer B.SilkS))
  (dimension 26 (width 0.3) (layer Dwgs.User)
    (gr_text "26.000 mm" (at 139.5 83.65) (layer Dwgs.User))
    (feature1 (pts (xy 152.5 91) (xy 152.5 82.3)))
    (feature2 (pts (xy 126.5 91) (xy 126.5 82.3)))
    (crossbar (pts (xy 126.5 85) (xy 152.5 85)))
    (arrow1a (pts (xy 152.5 85) (xy 151.373496 85.586421)))
    (arrow1b (pts (xy 152.5 85) (xy 151.373496 84.413579)))
    (arrow2a (pts (xy 126.5 85) (xy 127.626504 85.586421)))
    (arrow2b (pts (xy 126.5 85) (xy 127.626504 84.413579)))
  )
  (dimension 22 (width 0.3) (layer Dwgs.User)
    (gr_text "22.000 mm" (at 189.85 103 90) (layer Dwgs.User))
    (feature1 (pts (xy 177.5 92) (xy 191.2 92)))
    (feature2 (pts (xy 177.5 114) (xy 191.2 114)))
    (crossbar (pts (xy 188.5 114) (xy 188.5 92)))
    (arrow1a (pts (xy 188.5 92) (xy 189.086421 93.126504)))
    (arrow1b (pts (xy 188.5 92) (xy 187.913579 93.126504)))
    (arrow2a (pts (xy 188.5 114) (xy 189.086421 112.873496)))
    (arrow2b (pts (xy 188.5 114) (xy 187.913579 112.873496)))
  )
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 194.85 103 90) (layer Dwgs.User))
    (feature1 (pts (xy 181.5 88) (xy 196.2 88)))
    (feature2 (pts (xy 181.5 118) (xy 196.2 118)))
    (crossbar (pts (xy 193.5 118) (xy 193.5 88)))
    (arrow1a (pts (xy 193.5 88) (xy 194.086421 89.126504)))
    (arrow1b (pts (xy 193.5 88) (xy 192.913579 89.126504)))
    (arrow2a (pts (xy 193.5 118) (xy 194.086421 116.873496)))
    (arrow2b (pts (xy 193.5 118) (xy 192.913579 116.873496)))
  )
  (dimension 52 (width 0.3) (layer Dwgs.User)
    (gr_text "52.000 mm" (at 152.5 79.65) (layer Dwgs.User))
    (feature1 (pts (xy 178.5 91) (xy 178.5 78.3)))
    (feature2 (pts (xy 126.5 91) (xy 126.5 78.3)))
    (crossbar (pts (xy 126.5 81) (xy 178.5 81)))
    (arrow1a (pts (xy 178.5 81) (xy 177.373496 81.586421)))
    (arrow1b (pts (xy 178.5 81) (xy 177.373496 80.413579)))
    (arrow2a (pts (xy 126.5 81) (xy 127.626504 81.586421)))
    (arrow2b (pts (xy 126.5 81) (xy 127.626504 80.413579)))
  )
  (dimension 60 (width 0.3) (layer Dwgs.User)
    (gr_text "60.000 mm" (at 152.5 75.65) (layer Dwgs.User))
    (feature1 (pts (xy 182.5 88) (xy 182.5 74.3)))
    (feature2 (pts (xy 122.5 88) (xy 122.5 74.3)))
    (crossbar (pts (xy 122.5 77) (xy 182.5 77)))
    (arrow1a (pts (xy 182.5 77) (xy 181.373496 77.586421)))
    (arrow1b (pts (xy 182.5 77) (xy 181.373496 76.413579)))
    (arrow2a (pts (xy 122.5 77) (xy 123.626504 77.586421)))
    (arrow2b (pts (xy 122.5 77) (xy 123.626504 76.413579)))
  )
  (gr_line (start 182.5 118) (end 122.5 118) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.5 88) (end 182.5 118) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.5 88) (end 182.5 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.5 118) (end 122.5 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 182 117.5) (xy 174.5 117.5) (xy 174.5 111.5) (xy 177 109) (xy 179.5 109)
        (xy 181 107.5) (xy 181 100) (xy 177 96) (xy 158.5 96) (xy 155.5 99)
        (xy 155.5 117.5) (xy 123 117.5) (xy 123 88.5) (xy 182 88.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.257 93.472) (xy 151.257 90.551) (xy 143.256 90.551) (xy 143.256 95.25) (xy 144.907 97.028)
        (xy 147.066 97.028) (xy 147.066 95.123) (xy 148.209 93.98) (xy 150.368 93.98) (xy 151.003 93.345)
        (xy 151.003 93.218)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 182 117.5) (xy 174.5 117.5) (xy 174.5 111.5) (xy 177 109) (xy 179.5 109)
        (xy 181 107.5) (xy 181 100) (xy 177 96) (xy 158.5 96) (xy 155.5 99)
        (xy 155.5 117.5) (xy 123 117.5) (xy 123 88.5) (xy 182 88.5)
      )
    )
  )
)
