<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<circle x="20" y="20" radius="3.7" width="0.001" layer="46"/>
<text>gChart</text>
<text>BLF</text>
<text>+</text>
<text>_</text>
<text>_</text>
<text>+</text>
<text>v2.0</text>
<text>60AA</text>
<text>Batt Check</text>
<wire x1="16" y1="12" x2="24" y2="12" width="0.001" layer="46"/>
<wire x1="28" y1="16" x2="28" y2="24" width="0.001" layer="46"/>
<wire x1="24" y1="28" x2="16" y2="28" width="0.001" layer="46"/>
<wire x1="12" y1="24" x2="12" y2="16" width="0.001" layer="46"/>
<wire x1="16" y1="28" x2="12" y2="24" width="0.001" layer="46" curve="36.869898"/>
<wire x1="28" y1="24" x2="24" y2="28" width="0.001" layer="46" curve="36.869898"/>
<wire x1="24" y1="12" x2="28" y2="16" width="0.001" layer="46" curve="36.869898"/>
<wire x1="12" y1="16" x2="16" y2="12" width="0.001" layer="46" curve="36.869898"/>
</plain>
<libraries>
<library name="Omten1288">
<packages>
<package name="OMTEN1288">
<description>Omten 1288 Switch</description>
</package>
</packages>
</library>
<library name="smd-ipc">
<description>&lt;b&gt;IPC Standard SMD Packages&lt;/b&gt;&lt;p&gt;
This is a package-only library, based on the Surface Mount Design and Land Pattern Standard developed by the 
Institute for Interconnecting and Packaging electronic Circuits (IPC).&lt;p&gt;
Source:&lt;p&gt;
IPC-SM-782&lt;br&gt;
Revision A, August 1993&lt;br&gt;
Includes Amendment 1, October 1996&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="R0805">
<description>&lt;b&gt;Chip RESISTOR, 0805 EIA (2012 Metric)&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ref-packages">
<description>&lt;b&gt;Reference Package&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="SOT23-6L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="SC70">
<description>&lt;b&gt;SC70-3 Reflow soldering&lt;/b&gt;&lt;p&gt;
Philips SC01_Mounting_1996.pdf&lt;p&gt;
ROHM : UMT3 ; EIAJ : SC-70</description>
</package>
</packages>
</library>
<library name="ref-packages-longpad">
<description>&lt;b&gt;Reference Package&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="E$1" library="Omten1288" package="OMTEN1288" value=""/>
<element name="IC" library="ref-packages" package="SOT23-6L" value="">
<attribute name="VALUE"/>
</element>
<element name="R" library="smd-ipc" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="ref-packages-longpad" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D4" library="ref-packages-longpad" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D2" library="ref-packages-longpad" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="D3" library="ref-packages-longpad" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C" library="smd-ipc" package="R0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PFET" library="ref-packages" package="SC70" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="POS">
<contactref element="PFET" pad="3"/>
<contactref element="C" pad="2"/>
<contactref element="R" pad="2"/>
</signal>
<signal name="L3">
<contactref element="D3" pad="C"/>
<contactref element="IC" pad="4"/>
</signal>
<signal name="L4">
<contactref element="D4" pad="C"/>
<contactref element="IC" pad="3"/>
</signal>
<signal name="LP">
<contactref element="D3" pad="A"/>
<contactref element="R" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="L1">
<contactref element="D1" pad="C"/>
<contactref element="IC" pad="6"/>
</signal>
<signal name="L2">
<contactref element="D2" pad="C"/>
<contactref element="IC" pad="5"/>
</signal>
<signal name="GND">
<contactref element="IC" pad="2"/>
<contactref element="PFET" pad="1"/>
<contactref element="C" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="IC" pad="1"/>
<contactref element="PFET" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
