(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 102)
    (zones 0)
    (modules 4)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.4064)
    (user_trace_width 0.4572)
    (user_trace_width 0.6096)
    (user_trace_width 0.8128)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.3048)
    (via_min_drill 0.254)
    (user_via 0.3048 0.254)
    (user_via 0.3556 0.3048)
    (user_via 0.4572 0.4064)
    (user_via 0.5588 0.508)
    (user_via 0.8636 0.8128)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.1524)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.254)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.15)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.254)
    (pad_size 1 0.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 /nTRST)
  (net 3 /TDI)
  (net 4 /SWDIO_TMS)
  (net 5 /SWCLK_TCLK)
  (net 6 /RTCK)
  (net 7 /SWO_TDO)
  (net 8 /RESET)
  (net 9 "Net-(J1-Pad17)")
  (net 10 /5V)
  (net 11 "Net-(J1-Pad2)")
  (net 12 GND)
  (net 13 /PWR_SEL)
  (net 14 /nTRST_SEL)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /5V)
    (add_net /PWR_SEL)
    (add_net /RESET)
    (add_net /RTCK)
    (add_net /SWCLK_TCLK)
    (add_net /SWDIO_TMS)
    (add_net /SWO_TDO)
    (add_net /TDI)
    (add_net /nTRST)
    (add_net /nTRST_SEL)
    (add_net GND)
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad2)")
    (add_net VCC)
  )
  (module Straddle:Straddle-10-Male (layer B.Cu) (tedit 5BACC972)
    (at 127 97.155 180)
    (attr smd)
    (fp_text reference J2 (at 8.001 0 180) (layer F.SilkS))
    (fp_text value Conn_02x05_Odd_Even (at 0 -17 180) (layer B.Fab))
    (pad 10 smd rect (at -5.08 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 8 /RESET))
    (pad 8 smd rect (at -2.54 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 3 /TDI))
    (pad 6 smd rect (at 0 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 7 /SWO_TDO))
    (pad 4 smd rect (at 2.54 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 5 /SWCLK_TCLK))
    (pad 2 smd rect (at 5.08 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 4 /SWDIO_TMS))
    (pad 9 smd rect (at -5.08 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 14 /nTRST_SEL))
    (pad 7 smd rect (at -2.54 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 6 /RTCK))
    (pad 5 smd rect (at 0 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 13 /PWR_SEL))
    (pad 3 smd rect (at 2.54 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 1 smd rect (at 5.08 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 1 VCC))
  )
  (module Straddle:Straddle-20-Female (layer F.Cu) (tedit 0)
    (at 127 76.2 180)
    (attr smd)
    (fp_text reference J1 (at -13.589 0 180) (layer F.SilkS))
    (fp_text value Conn_02x10_Odd_Even (at 0 17 180) (layer F.Fab))
    (pad 20 smd rect (at 11.43 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 18 smd rect (at 8.89 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 16 smd rect (at 6.35 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 14 smd rect (at 3.81 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 12 smd rect (at 1.27 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 10 smd rect (at -1.27 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 8 smd rect (at -3.81 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 6 smd rect (at -6.35 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 4 smd rect (at -8.89 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 12 GND))
    (pad 2 smd rect (at -11.43 0 180) (size 1.5 4) (layers B.Cu B.Mask)
      (net 11 "Net-(J1-Pad2)"))
    (pad 19 smd rect (at 11.43 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 10 /5V))
    (pad 17 smd rect (at 8.89 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 9 "Net-(J1-Pad17)"))
    (pad 15 smd rect (at 6.35 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 8 /RESET))
    (pad 13 smd rect (at 3.81 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 7 /SWO_TDO))
    (pad 11 smd rect (at 1.27 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 6 /RTCK))
    (pad 9 smd rect (at -1.27 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 5 /SWCLK_TCLK))
    (pad 7 smd rect (at -3.81 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 4 /SWDIO_TMS))
    (pad 5 smd rect (at -6.35 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 3 /TDI))
    (pad 3 smd rect (at -8.89 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 2 /nTRST))
    (pad 1 smd rect (at -11.43 0 180) (size 1.5 4) (layers F.Cu F.Mask)
      (net 1 VCC))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391ABA)
    (at 134.62 82.169 180)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference TRST (at 0 -2.413 180) (layer F.SilkS))
    (fp_text value SolderJumper_2_Bridged (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd custom (at 0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 14 /nTRST_SEL) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 2 /nTRST) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
        (gr_poly (pts
           (xy 0.9 -0.3) (xy 0.4 -0.3) (xy 0.4 0.3) (xy 0.9 0.3)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5BACC7BF)
    (at 118.11 81.28 180)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0.127 -2.54 180) (layer F.SilkS) hide)
    (fp_text value SolderJumper_3_Open (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 13 /PWR_SEL))
    (pad 3 smd custom (at 1.3 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 10 /5V) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -1.3 0 180) (size 1 0.5) (layers F.Cu F.Mask)
      (net 12 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
  )
  (gr_text J-Link (at 127 81.026) (layer F.SilkS))
  (gr_text TC2050 (at 127 92.456) (layer F.SilkS))
  (gr_text "+\n" (at 116.713 83.185) (layer F.SilkS))
  (gr_text - (at 119.126 83.185) (layer F.SilkS))
  (gr_line (start 112.141 82.804) (end 112.141 73.152) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 116.9035 90.424) (end 112.141 82.804) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 116.9035 99.4664) (end 116.9035 90.424) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.0965 99.4664) (end 116.9035 99.4664) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.0965 90.424) (end 137.0965 99.4664) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 141.859 82.804) (end 137.0965 90.424) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 141.859 73.152) (end 141.859 82.804) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 112.141 73.152) (end 141.859 73.152) (layer Edge.Cuts) (width 0.2))
  (zone (net 12) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.762) (thermal_bridge_width 0.762))
    (polygon
      (pts
        (xy 112.141 73.152) (xy 112.141 82.804) (xy 116.967 90.424) (xy 116.967 99.441) (xy 137.033 99.441)
        (xy 137.033 90.424) (xy 141.859 82.804) (xy 141.859 73.152)
      )
    )
  )
  (zone (net 12) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.141 73.152) (xy 112.141 82.804) (xy 116.967 90.424) (xy 116.967 99.441) (xy 137.033 99.441)
        (xy 137.033 90.424) (xy 141.859 82.804) (xy 141.859 73.152)
      )
    )
  )
)
