(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 51)
    (no_connects 17)
    (area 154.872999 87.372999 169.627001 102.127001)
    (thickness 1.6)
    (drawings 21)
    (tracks 324)
    (zones 0)
    (modules 10)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.155)
    (trace_clearance 0.155)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.155)
    (segment_width 0.254)
    (edge_width 0.254)
    (via_size 0.55)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.901 0.901)
    (pad_drill 0)
    (pad_to_mask_clearance 0.03)
    (aux_axis_origin 0 0)
    (grid_origin 155 87.5)
    (visible_elements FFFFFF9F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 +5V)
  (net 6 "Net-(U1-Pad13)")
  (net 7 "Net-(U1-Pad14)")
  (net 8 /D+)
  (net 9 /D-)
  (net 10 /C2D)
  (net 11 /C2CK)
  (net 12 /P0.3)
  (net 13 /P0.2)
  (net 14 /P0.1)
  (net 15 /P0.0)
  (net 16 /P0.7)
  (net 17 /P0.6)
  (net 18 /P0.5)
  (net 19 /P0.4)
  (net 20 "Net-(SW1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.155)
    (trace_width 0.155)
    (via_dia 0.55)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /C2CK)
    (add_net /C2D)
    (add_net /D+)
    (add_net /D-)
    (add_net /P0.0)
    (add_net /P0.1)
    (add_net /P0.2)
    (add_net /P0.3)
    (add_net /P0.4)
    (add_net /P0.5)
    (add_net /P0.6)
    (add_net /P0.7)
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(SW1-Pad1)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
  )
  (net_class gnd ""
    (clearance 0.155)
    (trace_width 0.2)
    (via_dia 0.55)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (module key_switch:Cherry_MX_Matias_No_Silk_Border (layer B.Cu) (tedit 59D21A45)
    (at 162.25 94.75)
    (tags switch)
    (fp_text reference SW1 (at 0 -6) (layer Cmts.User))
    (fp_text value SW_Push (at 1 -3.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at 2.5 3.683) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.81 2.54) (size 2.3 2.3) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 0 0) (size 4 4) (drill 4) (layers *.Cu *.Mask B.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask B.SilkS))
    (pad 1 thru_hole circle (at -2.54 5.08) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 20 "Net-(SW1-Pad1)"))
    (pad 1 thru_hole circle (at -2.5 4) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 20 "Net-(SW1-Pad1)"))
    (model cherry_mx1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59D222F7)
    (at 159 94.1)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 5.6 0 90) (layer Cmts.User))
    (fp_text value 0.1uF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer Cmts.User))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59D222FB)
    (at 158.6 93.1)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 1.7 0 90) (layer Cmts.User))
    (fp_text value 4.7uF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer Cmts.User))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59D22319)
    (at 160.2 92.3 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C3 (at -0.3 0.6 270) (layer Cmts.User))
    (fp_text value 0.1uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402_NoSilk (layer B.Cu) (tedit 59D222EE)
    (at 161.1 91.7 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 1.7 -0.7 360) (layer Cmts.User))
    (fp_text value 4.7uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module usb_connector:micro_usb_no_silk (layer B.Cu) (tedit 59BC86E6)
    (at 165.75 90.5)
    (fp_text reference J1 (at -3.9 -4.05) (layer Cmts.User))
    (fp_text value USB_OTG (at -0.07 -4.18) (layer B.Fab))
    (pad 6 smd rect (at -3.2 0.25) (size 1.3 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 3.2 0.25) (size 1.3 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad "" np_thru_hole circle (at -1.95 0.14) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
    (pad 6 smd rect (at -1.15 -2) (size 1.9 1.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 6 thru_hole circle (at -2.825 -2) (size 2 2) (drill 1.35) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 smd rect (at 1.3 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 8 /D+))
    (pad 2 smd rect (at -0.65 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 9 /D-))
    (pad 1 smd rect (at -1.3 1.05) (size 0.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 6 thru_hole circle (at 2.825 -2) (size 2 2) (drill 1.35) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 6 smd rect (at 1.15 -2) (size 1.9 1.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad "" np_thru_hole circle (at 1.95 0.14) (size 0.6 0.6) (drill 0.6) (layers *.Cu *.Mask))
  )
  (module qfn:QFN20_silabs (layer B.Cu) (tedit 59D2336D)
    (at 157.5 90.25 180)
    (fp_text reference U1 (at 0 3.2 180) (layer Cmts.User))
    (fp_text value EFM8UB1_QFN20 (at 0 -3.2 180) (layer B.Fab))
    (pad 16 smd rect (at 1.25 1.25 180) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /P0.6))
    (pad 11 smd rect (at 1.25 -1.25 180) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(SW1-Pad1)"))
    (pad 6 smd rect (at -1.25 -1.25 180) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 21 smd rect (at -0.45 -0.45 90) (size 0.901 0.901) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 0.45 -0.45 90) (size 0.901 0.901) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 21 smd rect (at 0.45 0.45 90) (size 0.901 0.901) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.55 0.75 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 /P0.0))
    (pad 3 smd rect (at -1.55 0.25 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -1.55 -0.25 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 /D+))
    (pad 5 smd rect (at -1.55 -0.75 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /D-))
    (pad 7 smd rect (at -0.75 -1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 8 smd rect (at -0.25 -1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 9 smd rect (at 0.25 -1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 /C2CK))
    (pad 10 smd rect (at 0.75 -1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 /C2D))
    (pad 12 smd rect (at 1.55 -0.75 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 13 smd rect (at 1.55 -0.25 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(U1-Pad13)"))
    (pad 14 smd rect (at 1.55 0.25 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 1.55 0.75 90) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 16 /P0.7))
    (pad 17 smd rect (at 0.75 1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 18 /P0.5))
    (pad 18 smd rect (at 0.25 1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 19 /P0.4))
    (pad 19 smd rect (at -0.25 1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 12 /P0.3))
    (pad 20 smd rect (at -0.75 1.55 180) (size 0.3 0.9) (layers B.Cu B.Paste B.Mask)
      (net 13 /P0.2))
    (pad 1 smd rect (at -1.25 1.25 180) (size 0.3 0.3) (layers B.Cu B.Paste B.Mask)
      (net 14 /P0.1))
    (pad 21 smd rect (at -0.45 0.45 90) (size 0.901 0.901) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Housings_DFN_QFN.3dshapes/UQFN-20-1EP_3x3mm_Pitch0.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module connectors:Pin_Header_Angled_1x04_Pitch1.27mm_no_silk_castellated (layer B.Cu) (tedit 59D21DD6)
    (at 168.25 100.65)
    (descr "Through hole angled pin header, 1x04, 1.27mm pitch, 4.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 1.27mm single row")
    (fp_text reference J3 (at 2.4325 1.635) (layer Cmts.User))
    (fp_text value Conn_01x04 (at 2.4325 -5.445) (layer B.Fab))
    (pad 1 thru_hole circle (at 1.27 0) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 /P0.3))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 12 /P0.3))
    (pad 2 thru_hole rect (at 0 -1.27) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 13 /P0.2))
    (pad 3 thru_hole rect (at 0 -2.54) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 14 /P0.1))
    (pad 4 thru_hole rect (at 0 -3.81) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 15 /P0.0))
    (pad 2 thru_hole circle (at 1.27 -1.27) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 /P0.2))
    (pad 3 thru_hole circle (at 1.27 -2.54) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 /P0.1))
    (pad 4 thru_hole circle (at 1.27 -3.81) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 15 /P0.0))
  )
  (module connectors:Pin_Header_Angled_1x04_Pitch1.27mm_no_silk_castellated (layer B.Cu) (tedit 59D21DD6)
    (at 161.75 100.65 270)
    (descr "Through hole angled pin header, 1x04, 1.27mm pitch, 4.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 1.27mm single row")
    (fp_text reference J4 (at 2.4325 1.635 270) (layer Cmts.User))
    (fp_text value Conn_01x04 (at 2.4325 -5.445 270) (layer B.Fab))
    (pad 1 thru_hole circle (at 1.27 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 /P0.7))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 16 /P0.7))
    (pad 2 thru_hole rect (at 0 -1.27 270) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 17 /P0.6))
    (pad 3 thru_hole rect (at 0 -2.54 270) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 18 /P0.5))
    (pad 4 thru_hole rect (at 0 -3.81 270) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 19 /P0.4))
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 /P0.6))
    (pad 3 thru_hole circle (at 1.27 -2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 /P0.5))
    (pad 4 thru_hole circle (at 1.27 -3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 19 /P0.4))
  )
  (module connectors:Pin_Header_Angled_1x04_Pitch1.27mm_no_silk_castellated (layer B.Cu) (tedit 59D21DD6)
    (at 156.225 96.85 180)
    (descr "Through hole angled pin header, 1x04, 1.27mm pitch, 4.0mm pin length, single row")
    (tags "Through hole angled pin header THT 1x04 1.27mm single row")
    (fp_text reference J2 (at 2.4325 1.635 180) (layer Cmts.User))
    (fp_text value Conn_01x04 (at 2.4325 -5.445 180) (layer B.Fab))
    (pad 1 thru_hole circle (at 1.27 0 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole rect (at 0 -1.27 180) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 10 /C2D))
    (pad 3 thru_hole rect (at 0 -2.54 180) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 11 /C2CK))
    (pad 4 thru_hole rect (at 0 -3.81 180) (size 1.7 1) (drill 0.65 (offset 0.4 0)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 /C2D))
    (pad 3 thru_hole circle (at 1.27 -2.54 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 /C2CK))
    (pad 4 thru_hole circle (at 1.27 -3.81 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (gr_text 2 (at 167.15 99.35) (layer B.SilkS))
  (gr_text 5V (at 157.575 96.85) (layer B.SilkS))
  (gr_text D (at 157.375 98.125) (layer B.SilkS))
  (gr_text K (at 157.4 99.4) (layer B.SilkS))
  (gr_text G (at 157.475 100.65) (layer B.SilkS))
  (gr_text "7\n" (at 161.75 99.45) (layer B.SilkS))
  (gr_text "6\n" (at 163 99.45) (layer B.SilkS))
  (gr_text 3 (at 167.2 100.65) (layer B.SilkS))
  (gr_text 0 (at 168.7 95.6) (layer B.SilkS))
  (gr_line (start 155 102) (end 155 87.5) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 169.5 102) (end 155 102) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 169.5 87.5) (end 169.5 102) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 155 87.5) (end 169.5 87.5) (angle 90) (layer Edge.Cuts) (width 0.254))
)
