(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 51)
    (no_connects 0)
    (area 154.942199 73.742776 201.292801 110.421133)
    (thickness 1.6)
    (drawings 21)
    (tracks 157)
    (zones 0)
    (modules 29)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1778)
    (user_trace_width 0.1778)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (trace_clearance 0.1778)
    (zone_clearance 0.1778)
    (zone_45_only yes)
    (trace_min 0.1778)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.3048)
    (via_min_size 0.508)
    (via_min_drill 0.3048)
    (user_via 0.6858 0.3302)
    (user_via 0.8636 0.508)
    (user_via 1.1176 0.762)
    (user_via 1.3716 1.016)
    (uvia_size 0.508)
    (uvia_drill 0.3048)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.3048)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.508 0.508)
    (mod_text_width 0.0635)
    (pad_size 8.6 8.6)
    (pad_drill 4.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 139.065 111.125)
    (visible_elements 7FFEDF7F)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +5V)
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(P1-Pad2)")
  (net 6 "Net-(P1-Pad4)")
  (net 7 DI)
  (net 8 "Net-(P2-Pad4)")
  (net 9 DO)
  (net 10 "Net-(P3-Pad1)")
  (net 11 "Net-(P4-Pad1)")
  (net 12 "Net-(P5-Pad1)")
  (net 13 "Net-(P6-Pad1)")
  (net 14 "Net-(P7-Pad1)")
  (net 15 "Net-(P8-Pad1)")
  (net 16 CLK)
  (net 17 "#SS")
  (net 18 "Net-(R5-Pad2)")
  (net 19 "Net-(R6-Pad2)")
  (net 20 "Net-(R7-Pad2)")
  (net 21 "Net-(R8-Pad2)")
  (net 22 "Net-(R9-Pad2)")
  (net 23 "Net-(R10-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.508)
    (via_drill 0.3048)
    (uvia_dia 0.508)
    (uvia_drill 0.3048)
    (add_net "#SS")
    (add_net +5V)
    (add_net CLK)
    (add_net DI)
    (add_net DO)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59127C64)
    (at 176.53 90.17 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.016 90) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59127C54)
    (at 173.99 92.075 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59127C07)
    (at 175.26 83.185 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 1.905 0.635 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59127C4F)
    (at 172.085 92.075 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -2.159 0 180) (layer F.SilkS))
    (fp_text value 47uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 59127C37)
    (at 170.18 90.17 90)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.016 270) (layer F.SilkS))
    (fp_text value red (at 0 1.35 90) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.8 0 270) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module PJS-icons:metroid (layer F.Cu) (tedit 59128195)
    (at 185.1025 81.5975 315)
    (fp_text reference icon1 (at -6.286179 -3.14309 315) (layer F.SilkS) hide)
    (fp_text value Metroid (at 0 -2.54 315) (layer F.SilkS) hide)
    (pad "" smd circle (at -0.635 0 315) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0.635 0 315) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
    (pad "" smd circle (at 0 -0.635 315) (size 0.635 0.635) (layers F.Cu F.Paste F.Mask))
  )
  (module PJS-pth-parts:OST_on-shore_OSTTE050104 (layer F.Cu) (tedit 59127C68)
    (at 163.195 81.28 270)
    (fp_text reference P1 (at -1.778 -2.921 270) (layer F.SilkS))
    (fp_text value OSTTE050104 (at 2 3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 7 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 10.5 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at 14 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 DO))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59127C21)
    (at 170.815 85.725 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P2 (at 2.159 -1.397 180) (layer F.SilkS))
    (fp_text value program (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 DO))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 59127C87)
    (at 180.975 103.505 90)
    (fp_text reference P3 (at -1.778 0.127 180) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.905 3.175 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 10 "Net-(P3-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 59127C82)
    (at 179.07 100.965 90)
    (fp_text reference P4 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.905 3.175 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 11 "Net-(P4-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 59127CA9)
    (at 188.595 103.505 90)
    (fp_text reference P5 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.905 3.175 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 12 "Net-(P5-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 59127CA2)
    (at 186.69 100.965 90)
    (fp_text reference P6 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.905 3.175 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 13 "Net-(P6-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 59127C8B)
    (at 184.785 103.505 90)
    (fp_text reference P7 (at -1.778 0.127 180) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.905 3.175 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 "Net-(P7-Pad1)"))
  )
  (module Wire_Pads:SolderWirePad_single_1mmDrill (layer F.Cu) (tedit 59127C92)
    (at 182.88 100.965 90)
    (fp_text reference P8 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.905 3.175 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 15 "Net-(P8-Pad1)"))
  )
  (module PJS-pth-parts:OST_on-shore_OSTTE050104 (layer B.Cu) (tedit 59127C78)
    (at 193.04 81.28 270)
    (fp_text reference P9 (at -1.651 2.921 270) (layer B.SilkS))
    (fp_text value OSTTE050104 (at 2 -3 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 3.5 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 CLK))
    (pad 3 thru_hole circle (at 7 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at 10.5 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 "#SS"))
    (pad 5 thru_hole circle (at 14 0 270) (size 2 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 DI))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127C57)
    (at 176.53 93.98 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.143 90) (layer F.SilkS))
    (fp_text value no_pop (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127C2B)
    (at 167.64 86.36 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.651 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127C4B)
    (at 170.18 93.345 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.143 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127C47)
    (at 167.64 90.805 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.651 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 59127CDB)
    (at 182.245 92.075 90)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -0.254 5.08 270) (layer F.SilkS))
    (fp_text value PIC16F15324 (at 0 5.375 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R6-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R5-Pad2)"))
    (pad 4 smd rect (at -2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at -2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R10-Pad2)"))
    (pad 6 smd rect (at -2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R9-Pad2)"))
    (pad 7 smd rect (at -2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R8-Pad2)"))
    (pad 8 smd rect (at 2.7 3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R7-Pad2)"))
    (pad 9 smd rect (at 2.7 2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "#SS"))
    (pad 10 smd rect (at 2.7 1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 CLK))
    (pad 11 smd rect (at 2.7 0 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 DI))
    (pad 12 smd rect (at 2.7 -1.27 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 DO))
    (pad 13 smd rect (at 2.7 -2.54 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P2-Pad4)"))
    (pad 14 smd rect (at 2.7 -3.81 90) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 59127CF4)
    (at 175.26 80.645)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U2 (at -1.905 0 90) (layer F.SilkS))
    (fp_text value NL27WZ17 (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at -0.95 0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad4)"))
    (pad 5 smd rect (at 0.95 0) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -0.95 0) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.95 0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "#SS"))
    (pad 6 smd rect (at 0.95 -0.65) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 CLK))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127CC8)
    (at 180.975 97.79 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 1.651 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127CCE)
    (at 179.07 97.79 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.651 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127CB1)
    (at 188.595 97.79 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 1.651 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127CB8)
    (at 186.69 97.79 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 1.651 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(P6-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127CBC)
    (at 184.785 97.79 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 1.651 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P7-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59127CC0)
    (at 182.88 97.79 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 1.651 0 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P8-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 59127CE9)
    (at 170.18 100.965)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (fp_text reference P10 (at 0.889 7.62) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 5.3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59128481)
    (at 188.595 89.535 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 1.651 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 DI))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "20AWG \nwire max\n<---" (at 193.04 100.33) (layer F.SilkS))
  (gr_text "Climbing \nwall \nsensor V2" (at 162.687 101.727 270) (layer F.SilkS))
  (gr_text "PJS 9MAY2017\nMIT licence" (at 182.245 95.885) (layer B.SilkS))
  (gr_text "To master" (at 165.481 88.265 270) (layer B.SilkS))
  (gr_text "To slave" (at 190.881 88.265 90) (layer B.SilkS))
  (gr_text DO (at 160.655 95.25 270) (layer B.SilkS))
  (gr_text SS# (at 195.58 91.948 90) (layer B.SilkS))
  (gr_text GND (at 195.707 88.265 90) (layer B.SilkS))
  (gr_text "CLK\n" (at 195.707 84.709 90) (layer B.SilkS))
  (gr_text DI (at 195.58 95.25 90) (layer B.SilkS))
  (gr_text SS# (at 160.528 91.821 270) (layer B.SilkS))
  (gr_text GND (at 160.528 88.265 270) (layer B.SilkS))
  (gr_text "CLK\n" (at 160.528 84.709 270) (layer B.SilkS))
  (gr_text 5V (at 195.834 81.153 90) (layer B.SilkS))
  (gr_text 5V (at 160.528 81.28 270) (layer B.SilkS))
  (gr_line (start 159.385 106.045) (end 159.385 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.85 106.045) (end 159.385 106.045) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.85 105.41) (end 196.85 106.045) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.385 105.41) (end 159.385 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 196.85 78.74) (end 196.85 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.385 78.74) (end 196.85 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 3) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.1778)
    (fill yes (arc_segments 16) (thermal_gap 0.1778) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.85 83.185) (xy 177.8 83.185) (xy 177.8 83.82) (xy 176.53 83.82) (xy 176.53 83.185)
        (xy 175.26 81.915) (xy 170.18 81.915) (xy 168.91 83.185) (xy 159.385 83.185) (xy 159.385 78.74)
        (xy 196.85 78.74)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.1778)
    (fill yes (arc_segments 16) (thermal_gap 0.1778) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.85 106.045) (xy 159.385 106.045) (xy 159.385 78.74) (xy 196.85 78.74)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads (clearance 0.1778))
    (min_thickness 0.1778)
    (fill yes (arc_segments 16) (thermal_gap 0.1778) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.85 106.045) (xy 159.385 106.045) (xy 159.385 78.74) (xy 196.85 78.74)
      )
    )
  )
)
