(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 47)
    (no_connects 0)
    (area 73.924999 30.924999 108.275001 68.075001)
    (thickness 1.6)
    (drawings 26)
    (tracks 254)
    (zones 0)
    (modules 21)
    (nets 13)
  )
  (page A)
  (title_block
    (title "CAN Inerconnect Board")
    (date 2018-07-10)
    (rev 1.0)
    (company XZERES)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFF7BBF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(R4-Pad1)")
  (net 4 /RXD1)
  (net 5 /TXD2)
  (net 6 /TXD1)
  (net 7 /RXD2)
  (net 8 /CANH1)
  (net 9 /CANL1)
  (net 10 /CANH2)
  (net 11 /CANL2)
  (net 12 "Net-(R3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CANH1)
    (add_net /CANH2)
    (add_net /CANL1)
    (add_net /CANL2)
    (add_net /RXD1)
    (add_net /RXD2)
    (add_net /TXD1)
    (add_net /TXD2)
    (add_net GND)
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net VCC)
  )
  (module Arduino:SOIC-14 (layer F.Cu) (tedit 5A7CF048)
    (at 83 49 270)
    (fp_text reference U1 (at -5.5 1.5 360) (layer F.SilkS))
    (fp_text value MCP25612FD (at 0 0 270) (layer F.Fab) hide)
    (pad 4 smd rect (at 0 2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 4 /RXD1))
    (pad 3 smd rect (at -1.27 2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -2.54 2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.81 2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /TXD1))
    (pad 5 smd rect (at 1.27 2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /TXD2))
    (pad 6 smd rect (at 2.54 2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 7 smd rect (at 3.81 2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 8 smd rect (at 3.81 -2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /RXD2))
    (pad 9 smd rect (at 2.54 -2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /CANL2))
    (pad 10 smd rect (at 1.27 -2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /CANH2))
    (pad 11 smd rect (at 0 -2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R4-Pad1)"))
    (pad 12 smd rect (at -1.27 -2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /CANL1))
    (pad 13 smd rect (at -2.54 -2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /CANH1))
    (pad 14 smd rect (at -3.81 -2.7 270) (size 0.6 1.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad1)"))
  )
  (module Arduino:TP-SMD (layer F.Cu) (tedit 5B451AD2)
    (at 82.042 66.548)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference J3 (at 0 0) (layer F.Fab) hide)
    (fp_text value TXD1 (at -0.052 -2.78 90) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 6 /TXD1))
  )
  (module Arduino:TP-SMD (layer F.Cu) (tedit 5B451AF1)
    (at 84.582 66.548)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference J4 (at 0 0) (layer F.Fab) hide)
    (fp_text value RXD1 (at -0.052 -3.034 90) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 4 /RXD1))
  )
  (module Arduino:TP-SMD (layer F.Cu) (tedit 5B451B18)
    (at 87.122 66.548)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference J5 (at 0 0) (layer F.Fab) hide)
    (fp_text value RXD2 (at -0.052 -3.034 90) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 7 /RXD2))
  )
  (module Arduino:TP-SMD (layer F.Cu) (tedit 5B4516A1)
    (at 89.408 33.02)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference J1 (at 0 0) (layer F.Fab) hide)
    (fp_text value GND (at 0 1.778) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 1 GND))
  )
  (module Arduino:TP-SMD (layer F.Cu) (tedit 5B451B26)
    (at 89.662 66.548)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference J8 (at 0 0) (layer F.Fab) hide)
    (fp_text value TXD2 (at -0.052 -3.034 90) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 5 /TXD2))
  )
  (module Arduino:C_0603_Hand (layer F.Cu) (tedit 5B4503F3)
    (at 77 47 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:C_0603_Hand (layer F.Cu) (tedit 5B4503F1)
    (at 77 52 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm_SMD_Pin1Right (layer F.Cu) (tedit 5B45076C)
    (at 85.904 58.152 90)
    (descr "surface-mounted straight pin header, 1x04, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x04 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference J2 (at 0 -6.14 90) (layer F.SilkS))
    (fp_text value Conn_01x04 (at -0.048 0.096 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at -1.655 -1.27 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /RXD1))
    (pad 4 smd rect (at -1.655 3.81 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /TXD2))
    (pad 1 smd rect (at 1.655 -3.81 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /TXD1))
    (pad 3 smd rect (at 1.655 1.27 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /RXD2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm_SMD_Pin1Right (layer F.Cu) (tedit 5B45022D)
    (at 86.868 39.116 90)
    (descr "surface-mounted straight pin header, 1x03, 2.54mm pitch, single row, style 2 (pin 1 right)")
    (tags "Surface mounted pin header SMD 1x03 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference J9 (at 0 -4.87 90) (layer F.SilkS))
    (fp_text value Conn_01x03 (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at -1.655 0 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.655 -2.54 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at 1.655 2.54 90) (size 2.51 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:TP-SMD (layer F.Cu) (tedit 5B45169D)
    (at 84.328 33.02 90)
    (descr "Mesurement Point, Round, SMD Pad, DM 3mm,")
    (tags "Mesurement Point Round SMD Pad 3mm")
    (attr virtual)
    (fp_text reference J10 (at 0 0 90) (layer F.Fab) hide)
    (fp_text value VCC (at -1.778 0 180) (layer F.SilkS))
    (pad 1 smd circle (at 0 0 90) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 2 VCC))
  )
  (module Arduino:R_0603_Hand (layer F.Cu) (tedit 5B44FEFB)
    (at 91 47.5 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 3 0 180) (layer F.SilkS))
    (fp_text value 120Ω (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 /CANL1))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /CANH1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:R_0603_Hand (layer F.Cu) (tedit 5B4506A1)
    (at 91 52.5)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -3 0) (layer F.SilkS))
    (fp_text value 120Ω (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /CANL2))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 /CANH2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:R_0603_Hand (layer F.Cu) (tedit 5B44FEF7)
    (at 91 45)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3 0) (layer F.SilkS))
    (fp_text value 0Ω (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:R_0603_Hand (layer F.Cu) (tedit 5B44FF05)
    (at 91 50)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -3 0) (layer F.SilkS))
    (fp_text value 0Ω (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:6-pin_hdr (layer F.Cu) (tedit 5B460CAB)
    (at 102 40 270)
    (fp_text reference J6 (at -7 2.6 360) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 -2 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -5 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -3 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 8 /CANH1))
    (pad 3 thru_hole circle (at -1 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 9 /CANL1))
    (pad 4 thru_hole circle (at 1 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 3 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 10 /CANH2))
    (pad 6 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 11 /CANL2))
  )
  (module Arduino:6-pin_hdr (layer F.Cu) (tedit 5B46104B)
    (at 102 58 270)
    (fp_text reference J7 (at -7 2.5 360) (layer F.SilkS))
    (fp_text value Conn_01x06_Male (at 0 -2 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -5 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -3 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 8 /CANH1))
    (pad 3 thru_hole circle (at -1 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 9 /CANL1))
    (pad 4 thru_hole circle (at 1 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 3 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 10 /CANH2))
    (pad 6 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.85) (layers *.Cu *.Mask)
      (net 11 /CANL2))
  )
  (module Arduino:R_0603_Hand (layer B.Cu) (tedit 5B460C07)
    (at 83 45)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -3.2 0) (layer B.SilkS))
    (fp_text value 0Ω (at 0 0) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 /TXD1))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 /CANH1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:R_0603_Hand (layer B.Cu) (tedit 5B460C09)
    (at 83 47.7)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -3.2 0.1) (layer B.SilkS))
    (fp_text value 0Ω (at 0 -0.1) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 /RXD1))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 /CANL1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:R_0603_Hand (layer B.Cu) (tedit 5B460C0D)
    (at 83 50.1)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -3.2 0.1) (layer B.SilkS))
    (fp_text value 0Ω (at 0 0.1) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 5 /TXD2))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 /CANH2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Arduino:R_0603_Hand (layer B.Cu) (tedit 5B460C10)
    (at 82.9 52.6)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -3.1 0) (layer B.SilkS))
    (fp_text value 0Ω (at 0.1 0) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 /RXD2))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 11 /CANL2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 98.5 53) (layer F.SilkS))
  (gr_text FCANH (at 97.5 55) (layer F.SilkS))
  (gr_text FCANL (at 97.5 57) (layer F.SilkS))
  (gr_text GND (at 98.5 59) (layer F.SilkS))
  (gr_text CANH (at 98 61) (layer F.SilkS))
  (gr_text CANL (at 98 63) (layer F.SilkS))
  (gr_text CANL (at 98 45) (layer F.SilkS))
  (gr_text CANH (at 98 43) (layer F.SilkS))
  (gr_text GND (at 98.5 41) (layer F.SilkS))
  (gr_text FCANL (at 97.5 39) (layer F.SilkS))
  (gr_text FCANH (at 97.5 37) (layer F.SilkS))
  (gr_text GND (at 98.5 35) (layer F.SilkS))
  (gr_text RX2<->CANL (at 90.4 52.6) (layer B.SilkS))
  (gr_text TX2<->CANH (at 90.4 50.2) (layer B.SilkS))
  (gr_text RX1<->FCANL (at 90.8 47.8) (layer B.SilkS))
  (gr_text TX1<->FCANH (at 90.8 45) (layer B.SilkS))
  (gr_line (start 74 32) (end 74 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75 68) (end 74 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106 68) (end 75 68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 67) (end 106 68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 32) (end 107 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75 31) (end 74 32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 77 31) (end 75 31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79 31) (end 77 31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106 31) (end 79 31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 32) (end 106 31) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86 39) (xy 85 40) (xy 85 41) (xy 83 43) (xy 79 43)
        (xy 77 45) (xy 77 46) (xy 78 47) (xy 78 51) (xy 79 52)
        (xy 79 57) (xy 74 57) (xy 74 32) (xy 75 31) (xy 86 31)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106 31) (xy 75 31) (xy 74 32) (xy 74 67) (xy 75 68)
        (xy 106 68) (xy 107 67) (xy 107 32)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 107 32) (xy 107 67) (xy 106 68) (xy 75 68) (xy 74 67)
        (xy 74 58) (xy 80 58) (xy 80 44) (xy 83 44) (xy 87 40)
        (xy 87 31) (xy 106 31)
      )
    )
  )
)
