(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-rc2-dev-655-ge0ca5bab1)")
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 138)
    (zones 0)
    (modules 2)
    (nets 19)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.4)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.778 1.778)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad34)")
  (net 3 Side_Select)
  (net 4 Read_Data)
  (net 5 Write_Protect)
  (net 6 Track_00)
  (net 7 Write_Gate)
  (net 8 Write_Data)
  (net 9 Step)
  (net 10 Step_Direction)
  (net 11 Motor_On)
  (net 12 "Net-(J1-Pad14)")
  (net 13 DS_B)
  (net 14 DS_A)
  (net 15 Index)
  (net 16 "Net-(J1-Pad6)")
  (net 17 "Net-(J1-Pad4)")
  (net 18 "Net-(J1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net DS_A)
    (add_net DS_B)
    (add_net GND)
    (add_net Index)
    (add_net Motor_On)
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net Read_Data)
    (add_net Side_Select)
    (add_net Step)
    (add_net Step_Direction)
    (add_net Track_00)
    (add_net Write_Data)
    (add_net Write_Gate)
    (add_net Write_Protect)
  )
  (module Connectors_Multicomp:Multicomp_MC9A22-3434_2x17x2.54mm_Angled (layer Top) (tedit 56C61E6B)
    (at 128.1761 98.2345)
    (descr http://www.farnell.com/cad/360651.pdf)
    (tags "connector multicomp MC9A MC9A22")
    (fp_text reference J1 (at -3 -15) (layer F.SilkS))
    (fp_text value Conn_02x17_Odd_Even (at 20.32 -5.5) (layer F.Fab))
    (pad 34 thru_hole circle (at 40.64 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad34)"))
    (pad 33 thru_hole circle (at 40.64 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 32 thru_hole circle (at 38.1 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 Side_Select))
    (pad 31 thru_hole circle (at 38.1 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 30 thru_hole circle (at 35.56 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 Read_Data))
    (pad 29 thru_hole circle (at 35.56 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 28 thru_hole circle (at 33.02 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 Write_Protect))
    (pad 27 thru_hole circle (at 33.02 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole circle (at 30.48 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 Track_00))
    (pad 25 thru_hole circle (at 30.48 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole circle (at 27.94 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 Write_Gate))
    (pad 23 thru_hole circle (at 27.94 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 22 thru_hole circle (at 25.4 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 Write_Data))
    (pad 21 thru_hole circle (at 25.4 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 20 thru_hole circle (at 22.86 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 Step))
    (pad 19 thru_hole circle (at 22.86 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 18 thru_hole circle (at 20.32 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 Step_Direction))
    (pad 17 thru_hole circle (at 20.32 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole circle (at 17.78 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 Motor_On))
    (pad 15 thru_hole circle (at 17.78 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole circle (at 15.24 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad14)"))
    (pad 13 thru_hole circle (at 15.24 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at 12.7 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 DS_B))
    (pad 11 thru_hole circle (at 12.7 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 10.16 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 DS_A))
    (pad 9 thru_hole circle (at 10.16 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at 7.62 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 Index))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 5.08 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad6)"))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad4)"))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module AtarianComputing:Atari_ST_Floppy (layer Top) (tedit 5B421645)
    (at 148.5011 107.061)
    (fp_text reference U1 (at -0.005 -9.60374) (layer F.SilkS) hide)
    (fp_text value Atari_ST_Floppy (at 0 10.668) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 5.08) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 Read_Data))
    (pad 3 thru_hole circle (at -2.286 4.572) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -4.191 3.048) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 DS_A))
    (pad 7 thru_hole circle (at -4.953 0.762) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole circle (at -4.826 -1.524) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 Step_Direction))
    (pad 11 thru_hole circle (at -3.429 -4.445) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 Write_Data))
    (pad 13 thru_hole circle (at -2.032 -1.016) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 Track_00))
    (pad 14 thru_hole circle (at 0 1.016) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 Write_Protect))
    (pad 12 thru_hole circle (at 2.028335 -1.019142) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 Write_Gate))
    (pad 2 thru_hole circle (at 2.282335 4.568858) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 Side_Select))
    (pad 8 thru_hole circle (at 4.822335 -1.527142) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 Motor_On))
    (pad 4 thru_hole circle (at 4.187335 3.044858) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 Index))
    (pad 6 thru_hole circle (at 4.949335 0.758858) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 DS_B))
    (pad 10 thru_hole circle (at 3.425335 -4.448142) (size 1.778 1.778) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 Step))
  )
  (gr_text "Atari ST Floppy Adapter" (at 148.5011 100.465) (layer F.SilkS))
  (gr_text PIN34 (at 171.958 95.758) (layer F.SilkS))
  (gr_text PIN33 (at 171.958 98.1605) (layer F.SilkS))
  (gr_text PIN2 (at 125.222 95.758) (layer F.SilkS))
  (gr_text PIN1 (at 125.222 98.1605) (layer F.SilkS))
  (gr_text Ø1.2mm (at 148.5011 104.14) (layer F.SilkS))
  (gr_line (start 154 115) (end 157 112) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157 104.5) (end 157 112) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 157 104.5) (end 160 101.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 101.5) (end 160 101.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 101.5) (end 174.5 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.5 100) (end 124 101.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137 101.5) (end 140 104.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 104.5) (end 140 112) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137 101.5) (end 124 101.5) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 140 112) (end 143 115) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 115) (end 143 115) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.5 84.201) (end 174.5 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.5 84.201) (end 174.5 84.201) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122.5 84.201) (end 122.5 100) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer Top) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.1105 83.8835) (xy 174.6885 84.0105) (xy 174.6885 100.203) (xy 172.847 102.0445) (xy 160.0835 102.108)
        (xy 157.4165 104.9655) (xy 157.48 112.7125) (xy 153.6065 116.3955) (xy 143.0655 116.078) (xy 139.1285 112.4585)
        (xy 139.192 105.156) (xy 136.5885 102.108) (xy 123.825 102.108) (xy 121.9835 99.8855) (xy 121.9835 84.0105)
      )
    )
  )
  (zone (net 0) (net_name "") (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.4))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.555 84.201) (xy 174.498 84.328) (xy 174.498 99.949) (xy 172.974 101.473) (xy 160.02 101.6)
        (xy 156.972 104.394) (xy 156.972 111.887) (xy 154.051 114.935) (xy 143.002 115.062) (xy 140.081 112.014)
        (xy 140.081 104.648) (xy 137.16 101.727) (xy 124.079 101.473) (xy 122.555 99.949)
      )
    )
  )
)
