(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 75)
    (no_connects 0)
    (area 148.514999 55.804999 242.010001 87.705001)
    (thickness 1.6)
    (drawings 29)
    (tracks 223)
    (zones 0)
    (modules 33)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 1.1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFE6F7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U1-Pad12)")
  (net 3 "Net-(D10-Pad1)")
  (net 4 "Net-(D11-Pad1)")
  (net 5 /lin_common/12V_UNPROTECTED)
  (net 6 /lin_common/A0)
  (net 7 /lin_common/A1)
  (net 8 /lin_common/A2)
  (net 9 /lin_common/A3)
  (net 10 /Sheet584DA639/+12V)
  (net 11 /Sheet584DA639/+5V)
  (net 12 /Sheet584DA639/LBUS)
  (net 13 /Sheet584D6B96/CHAN_B)
  (net 14 /Sheet584D6B96/CHAN_A)
  (net 15 /Sheet584D7AB5/CHAN_B)
  (net 16 /Sheet584D7AB5/CHAN_A)
  (net 17 /Sheet584D8209/CHAN_B)
  (net 18 /Sheet584D8209/CHAN_A)
  (net 19 /Sheet584D84B8/CHAN_B)
  (net 20 /Sheet584D84B8/CHAN_A)
  (net 21 "Net-(D12-Pad1)")
  (net 22 "Net-(D14-Pad1)")
  (net 23 "Net-(D13-Pad1)")
  (net 24 "Net-(D16-Pad1)")
  (net 25 "Net-(D15-Pad1)")
  (net 26 "Net-(D18-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.508)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Sheet584D6B96/CHAN_A)
    (add_net /Sheet584D6B96/CHAN_B)
    (add_net /Sheet584D7AB5/CHAN_A)
    (add_net /Sheet584D7AB5/CHAN_B)
    (add_net /Sheet584D8209/CHAN_A)
    (add_net /Sheet584D8209/CHAN_B)
    (add_net /Sheet584D84B8/CHAN_A)
    (add_net /Sheet584D84B8/CHAN_B)
    (add_net /Sheet584DA639/+12V)
    (add_net /Sheet584DA639/+5V)
    (add_net /Sheet584DA639/LBUS)
    (add_net /lin_common/12V_UNPROTECTED)
    (add_net /lin_common/A0)
    (add_net /lin_common/A1)
    (add_net /lin_common/A2)
    (add_net /lin_common/A3)
    (add_net GND)
    (add_net "Net-(D10-Pad1)")
    (add_net "Net-(D11-Pad1)")
    (add_net "Net-(D12-Pad1)")
    (add_net "Net-(D13-Pad1)")
    (add_net "Net-(D14-Pad1)")
    (add_net "Net-(D15-Pad1)")
    (add_net "Net-(D16-Pad1)")
    (add_net "Net-(D18-Pad1)")
    (add_net "Net-(U1-Pad12)")
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 541A9C39)
    (at 200.66 79.375 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 0 3.175 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.7 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /Sheet584DA639/+12V))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 189.865 79.375 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.83 0 270) (layer F.SilkS))
    (fp_text value 1uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 /Sheet584DA639/+5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 222.885 64.77)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 13 /Sheet584D6B96/CHAN_B))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 233.045 64.77)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D4 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 14 /Sheet584D6B96/CHAN_A))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 182.245 64.77)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D5 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 15 /Sheet584D7AB5/CHAN_B))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 192.405 64.77)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D6 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 16 /Sheet584D7AB5/CHAN_A))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 202.565 64.77)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D7 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 17 /Sheet584D8209/CHAN_B))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 212.725 64.77)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D8 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 18 /Sheet584D8209/CHAN_A))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 161.925 64.77)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D9 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 19 /Sheet584D84B8/CHAN_B))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 172.085 64.77)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D10 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.635 0) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 20 /Sheet584D84B8/CHAN_A))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-20_5.3x7.2mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 194.945 70.485)
    (descr "20-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at -5.715 0) (layer F.SilkS))
    (fp_text value PIC16F1829LIN (at 0 4.75) (layer F.Fab))
    (pad 1 smd rect (at -3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 /Sheet584DA639/+5V))
    (pad 2 smd rect (at -3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 16 /Sheet584D7AB5/CHAN_A))
    (pad 3 smd rect (at -3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 /Sheet584D7AB5/CHAN_B))
    (pad 4 smd rect (at -3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 /lin_common/A2))
    (pad 5 smd rect (at -3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 9 /lin_common/A3))
    (pad 6 smd rect (at -3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /Sheet584D84B8/CHAN_A))
    (pad 7 smd rect (at -3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 19 /Sheet584D84B8/CHAN_B))
    (pad 8 smd rect (at -3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 12 /Sheet584DA639/LBUS))
    (pad 10 smd rect (at -3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 11 /Sheet584DA639/+5V))
    (pad 11 smd rect (at 3.6 2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 10 /Sheet584DA639/+12V))
    (pad 12 smd rect (at 3.6 2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 3.6 1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad12)"))
    (pad 14 smd rect (at 3.6 0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 /Sheet584D6B96/CHAN_A))
    (pad 15 smd rect (at 3.6 0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 13 /Sheet584D6B96/CHAN_B))
    (pad 16 smd rect (at 3.6 -0.325) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 /Sheet584D8209/CHAN_A))
    (pad 17 smd rect (at 3.6 -0.975) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 17 /Sheet584D8209/CHAN_B))
    (pad 18 smd rect (at 3.6 -1.625) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 /lin_common/A0))
    (pad 19 smd rect (at 3.6 -2.275) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 /lin_common/A1))
    (pad 20 smd rect (at 3.6 -2.925) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_SSOP.3dshapes/SSOP-20_5.3x7.2mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 187.325 79.375 270)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /Sheet584DA639/LBUS))
    (pad 2 smd rect (at 1.25 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5753A53E)
    (at 203.835 79.375 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 -2 270) (layer F.SilkS))
    (fp_text value 1N4148W-7-F (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 10 /Sheet584DA639/+12V))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 5 /lin_common/12V_UNPROTECTED))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock (layer F.Cu) (tedit 5794C14F)
    (at 162.055 71.125)
    (descr "Sabre™ Right Angle Header, 43160-XX03, http://www.molex.com/pdm_docs/sd/431601102_sd.pdf")
    (tags "connector molex sabre 43160")
    (fp_text reference P1 (at -5 0) (layer F.SilkS))
    (fp_text value MOLEX-0431603103 (at 7.49 17.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 5 /lin_common/12V_UNPROTECTED))
    (pad 1 thru_hole rect (at 0 -3.18) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 5 /lin_common/12V_UNPROTECTED))
    (pad 2 thru_hole circle (at 7.49 0) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 12 /Sheet584DA639/LBUS))
    (pad 2 thru_hole circle (at 7.49 -3.18) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 12 /Sheet584DA639/LBUS))
    (pad 3 thru_hole circle (at 14.98 0) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 14.98 -3.18) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -4.75 13.13) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 19.73 13.13) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (model /home/cpriscal/Projets/lin_modules/common/3d/Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock (layer F.Cu) (tedit 5794C14F)
    (at 212.855 71.125)
    (descr "Sabre™ Right Angle Header, 43160-XX03, http://www.molex.com/pdm_docs/sd/431601102_sd.pdf")
    (tags "connector molex sabre 43160")
    (fp_text reference P2 (at -5 0) (layer F.SilkS))
    (fp_text value MOLEX-0431603103 (at 7.49 17.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 5 /lin_common/12V_UNPROTECTED))
    (pad 1 thru_hole rect (at 0 -3.18) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 5 /lin_common/12V_UNPROTECTED))
    (pad 2 thru_hole circle (at 7.49 0) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 12 /Sheet584DA639/LBUS))
    (pad 2 thru_hole circle (at 7.49 -3.18) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 12 /Sheet584DA639/LBUS))
    (pad 3 thru_hole circle (at 14.98 0) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 14.98 -3.18) (size 3 3) (drill 1.78) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad "" thru_hole circle (at -4.75 13.13) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 19.73 13.13) (size 4 4) (drill 3) (layers *.Cu *.Mask))
    (model /home/cpriscal/Projets/lin_modules/common/3d/Molex_Sabre_43160-XX03_03x7.49mm_Angled_BoardLock.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier4 (layer F.Cu) (tedit 0)
    (at 225.425 59.69 180)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference P3 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value TE-282836-4 (at 0 5.08 180) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 21 "Net-(D12-Pad1)"))
    (pad 1 thru_hole rect (at -7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 4 "Net-(D11-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 GND))
    (model /home/cpriscal/Projets/lin_modules/common/3d/te-282836-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier4 (layer F.Cu) (tedit 0)
    (at 205.105 59.69 180)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference P5 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value TE-282836-4 (at 0 5.08 180) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 24 "Net-(D16-Pad1)"))
    (pad 1 thru_hole rect (at -7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 25 "Net-(D15-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 GND))
    (model /home/cpriscal/Projets/lin_modules/common/3d/te-282836-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Copal_CHS-04TB (layer F.Cu) (tedit 584490CC)
    (at 194.945 79.375 270)
    (descr "8-Lead Plastic Small Outline (SM) - Medium, 5.28 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference S1 (at 0 -4.191 270) (layer F.SilkS))
    (fp_text value DIP_SWITCH_4 (at 0 4.318 270) (layer F.Fab))
    (fp_text user N (at 2.032 -1.143 270) (layer F.Fab))
    (fp_text user O (at 2.032 -2.413 270) (layer F.Fab))
    (fp_text user 1 (at -1.905 -1.905 270) (layer F.Fab))
    (fp_text user 2 (at -1.905 -0.635 270) (layer F.Fab))
    (fp_text user 3 (at -1.905 0.635 270) (layer F.Fab))
    (fp_text user 4 (at -1.905 1.905 270) (layer F.Fab))
    (pad 1 smd rect (at -3.65 -1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /lin_common/A0))
    (pad 3 smd rect (at -3.65 -0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /lin_common/A1))
    (pad 5 smd rect (at -3.65 0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 /lin_common/A2))
    (pad 7 smd rect (at -3.65 1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /lin_common/A3))
    (pad 8 smd rect (at 3.65 1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.65 0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 3.65 -0.635 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 3.65 -1.905 270) (size 1.7 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/cpriscal/Projets/lin_modules/common/3d/copal-chs-04tb.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier4 (layer F.Cu) (tedit 0)
    (at 184.785 59.69 180)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference P4 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value TE-282836-4 (at 0 5.08 180) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 22 "Net-(D14-Pad1)"))
    (pad 1 thru_hole rect (at -7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 23 "Net-(D13-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 GND))
    (model /home/cpriscal/Projets/lin_modules/common/3d/te-282836-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier4 (layer F.Cu) (tedit 0)
    (at 164.465 59.69 180)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference P6 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value TE-282836-4 (at 0 5.08 180) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 26 "Net-(D18-Pad1)"))
    (pad 1 thru_hole rect (at -7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 3 "Net-(D10-Pad1)"))
    (pad 4 thru_hole circle (at 7.62 0 180) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask)
      (net 1 GND))
    (model /home/cpriscal/Projets/lin_modules/common/3d/te-282836-4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x05 (layer B.Cu) (tedit 0)
    (at 189.865 85.725 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 5.1 270) (layer B.SilkS))
    (fp_text value CONN_01X05 (at 0 3.1 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 /lin_common/A2))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /Sheet584DA639/+5V))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 /lin_common/A1))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 /lin_common/A0))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x05.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 227.965 64.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D11 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D11-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 217.805 64.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D12 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D12-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 187.325 64.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D13 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D13-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 177.165 64.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D14 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D14-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 207.645 64.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D15 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D15-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 197.485 64.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D16 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D16-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 167.005 64.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D17 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_SMD:SOD-323_HandSoldering (layer F.Cu) (tedit 57A875DC)
    (at 156.845 64.77 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D18 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value RSB36V (at 0.1 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(D18-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 584DEFD1)
    (at 151.765 84.455)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 584DF049)
    (at 151.765 59.69)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 584DF061)
    (at 238.76 59.69)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_Pad_Via (layer F.Cu) (tedit 584DF064)
    (at 238.76 84.455)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_Pad_Via (at 0 3.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.166726 1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.65 0) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -1.65) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.166726 -1.166726) (size 0.6 0.6) (drill 0.4) (layers *.Cu *.Mask))
  )
  (gr_text 12V (at 212.725 74.295) (layer B.SilkS))
  (gr_text LIN (at 220.345 74.295) (layer B.SilkS))
  (gr_text GND (at 227.965 74.295) (layer B.SilkS))
  (gr_text GND (at 177.165 74.295) (layer B.SilkS))
  (gr_text LIN (at 169.545 74.295) (layer B.SilkS))
  (gr_text 12V (at 161.925 74.295) (layer B.SilkS))
  (gr_text 7 (at 159.385 64.77) (layer B.SilkS))
  (gr_text 6 (at 169.545 64.77) (layer B.SilkS))
  (gr_text 5 (at 179.705 64.77) (layer B.SilkS))
  (gr_text 4 (at 189.865 64.77) (layer B.SilkS))
  (gr_text 3 (at 200.025 64.77) (layer B.SilkS))
  (gr_text 2 (at 210.185 64.77) (layer B.SilkS))
  (gr_text 1 (at 220.345 64.77) (layer B.SilkS))
  (gr_text 0 (at 230.505 64.77) (layer B.SilkS))
  (gr_line (start 148.59 87.63) (end 148.59 55.88) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 241.935 87.63) (end 148.59 87.63) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 241.935 55.88) (end 241.935 87.63) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.59 55.88) (end 241.935 55.88) (layer Edge.Cuts) (width 0.15))
  (gr_text "8 inputs LIN module\nrev 2    Dec 2016\nCedric Priscal" (at 194.945 73.66) (layer B.SilkS))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.59 55.88) (xy 241.935 55.88) (xy 241.935 87.63) (xy 148.59 87.63)
      )
    )
  )
)
