(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 67.31 99.06)
    (grid_origin 87.757 92.4052)
    (pcbplotparams
      (layerselection 0x0001000_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+3V3")
  (net 3 "+5V")
  (net 4 "+3.3VA")
  (net 5 "Net-(D1-K)")
  (net 6 "Net-(D2-A)")
  (net 7 "Net-(D3-A)")
  (net 8 "/EN")
  (net 9 "RTS")
  (net 10 "DTR")
  (net 11 "/IO0")
  (net 12 "Net-(D4-A)")
  (net 13 "/eTX")
  (net 14 "unconnected-(J1-ID-Pad4)")
  (net 15 "/LINKLED")
  (net 16 "/ACTLED")
  (net 17 "/eRX")
  (net 18 "unconnected-(J2-NC-Pad7)")
  (net 19 "/TX+")
  (net 20 "/TX-")
  (net 21 "/RX+")
  (net 22 "/nRST")
  (net 23 "Net-(U3-RXD)")
  (net 24 "/SLED")
  (net 25 "/RXD1")
  (net 26 "/MDIO")
  (net 27 "Net-(U5-RXER{slash}PHYAD0)")
  (net 28 "/CRS_DV")
  (net 29 "/RXD0")
  (net 30 "Net-(U5-RXD1{slash}MODE1)")
  (net 31 "/TXD0")
  (net 32 "/TXEN")
  (net 33 "/TXD1")
  (net 34 "/MDC")
  (net 35 "/XTAL")
  (net 36 "/RBIAS")
  (net 37 "GND1")
  (net 38 "/VDDCR")
  (net 39 "Net-(U5-CRS_DV{slash}MODE2)")
  (net 40 "Net-(U5-RXD0{slash}MODE0)")
  (net 41 "/+3V3_LAN")
  (net 42 "/PHY_POWER")
  (net 43 "/PHY_CLK")
  (net 44 "unconnected-(U2-SENSOR_VP-Pad4)")
  (net 45 "Net-(J2-Pad12)")
  (net 46 "/RX-")
  (net 47 "unconnected-(U2-SENSOR_VN-Pad5)")
  (net 48 "unconnected-(U2-IO14-Pad13)")
  (net 49 "unconnected-(U2-IO13-Pad16)")
  (net 50 "unconnected-(U2-SHD{slash}SD2-Pad17)")
  (net 51 "unconnected-(U2-SWP{slash}SD3-Pad18)")
  (net 52 "unconnected-(U2-SCS{slash}CMD-Pad19)")
  (net 53 "unconnected-(U2-SCK{slash}CLK-Pad20)")
  (net 54 "unconnected-(U2-SDO{slash}SD0-Pad21)")
  (net 55 "unconnected-(U2-SDI{slash}SD1-Pad22)")
  (net 56 "unconnected-(U2-IO15-Pad23)")
  (net 57 "unconnected-(U2-IO4-Pad26)")
  (net 58 "unconnected-(U2-IO16-Pad27)")
  (net 59 "unconnected-(U2-IO5-Pad29)")
  (net 60 "unconnected-(U2-NC-Pad32)")
  (net 61 "Net-(U3-UD+)")
  (net 62 "Net-(U3-UD-)")
  (net 63 "unconnected-(U3-NC-Pad7)")
  (net 64 "unconnected-(U3-NC-Pad8)")
  (net 65 "unconnected-(U3-~{CTS}-Pad9)")
  (net 66 "unconnected-(U3-~{DSR}-Pad10)")
  (net 67 "unconnected-(U3-~{RI}-Pad11)")
  (net 68 "unconnected-(U3-~{DCD}-Pad12)")
  (net 69 "unconnected-(U3-R232-Pad15)")
  (net 70 "unconnected-(U5-XTAL2-Pad4)")
  (net 71 "unconnected-(U5-INT{slash}REFCLKO-Pad14)")
  (net 72 "/VBUS")
  (net 73 "/DM")
  (net 74 "/DP")
  (net 75 "/IO32")
  (net 76 "/IO33")
  (net 77 "/IO34")
  (net 78 "/IO35")
  (net 79 "Net-(J2-Pad10)")
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 135.1788 65.4936 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at -2.273 -0.0635 180) (layer "F.SilkS"))
    (fp_text value "100n" (at -6.8196 0.3048 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 132.3848 65.5196 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at 2.1144 -0.2278 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 7.2012 0 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/EN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 80.0608 74.61 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C3" (at -2.479 0.0635 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 15.5042 -0.4826 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 90.5256 73.9292 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C5" (at -2.3012 0.0254 180) (layer "F.SilkS"))
    (fp_text value "22u" (at -15.1282 0.0254 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 88.3666 73.9242 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C6" (at -2.1946 0.0381 180) (layer "F.SilkS"))
    (fp_text value "22u" (at -0.1118 15.5448 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "F.Cu")
    (at 76.327 64.0842 180)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D1" (at 0 1.5494) (layer "F.SilkS"))
    (fp_text value "B5817W" (at -6.6602 -0.2032 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.02 1.529 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.25 0 180) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.25 0 180) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/VBUS") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Castellated" (layer "F.Cu")
    (at 69.2785 77.733 90)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D2" (at 2.295 -0.0127 180) (layer "F.SilkS"))
    (fp_text value "RED" (at 0.0598 -5.6515 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8125 0 90) (size 1.225 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8125 0 90) (size 1.225 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Castellated" (layer "F.Cu")
    (at 68.961 63.11 -90)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.38 90) (layer "F.SilkS"))
    (fp_text value "GREEN" (at 0 1.38 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8125 0 270) (size 1.225 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8125 0 270) (size 1.225 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (at 80.3402 64.0842 180)
    (descr "Fuse SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resettable fuse, polymeric positive temperature coefficient")
    (property "ki_keywords" "resettable fuse PTC PPTC polyfuse polyswitch")
    (attr smd)
    (fp_text reference "F1" (at 0 1.5494) (layer "F.SilkS"))
    (fp_text value "750mA" (at -2.1168 3.729 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173904348)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173904348)
      (net 5 "Net-(D1-K)") (pintype "passive"))
    (model "${KISYS3DMOD}/Fuse.3dshapes/Fuse_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CPB:USB_Micro-B_CNC_C10418" (layer "F.Cu")
    (at 73.66 70.104 90)
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB Micro Type B connector")
    (property "ki_keywords" "connector USB micro")
    (attr through_hole)
    (fp_text reference "J1" (at 4.1288 -1.283 180) (layer "F.SilkS"))
    (fp_text value "USB_B_Micro" (at 0 -7.25 90) (layer "F.Fab"))
    (pad "1" smd rect (at 1.3 -0.8 90) (size 0.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/VBUS") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" smd rect (at 0.65 -0.8 90) (size 0.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/DM") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" smd rect (at 0 -0.8 90) (size 0.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/DP") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" smd rect (at -0.65 -0.8 90) (size 0.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "unconnected-(J1-ID-Pad4)") (pinfunction "ID") (pintype "passive+no_connect"))
    (pad "5" smd rect (at -1.3 -0.8 90) (size 0.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "6" thru_hole oval (at -3.625 -4 90) (size 2 3) (drill oval 1) (layers "*.Cu" "*.Mask")
      (net 37 "GND1") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.425 -1.32 90) (size 1 2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 37 "GND1") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at -1.7 -5.55 90) (size 1.4 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "GND1") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect (at 1.7 -5.55 90) (size 1.4 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "GND1") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.425 -1.32 90) (size 1 2) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 37 "GND1") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval (at 3.625 -4 90) (size 2 3) (drill oval 1) (layers "*.Cu" "*.Mask")
      (net 37 "GND1") (pinfunction "Shield") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6_Handsoldering" (layer "F.Cu")
    (at 105.604 71.3636)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.1A Ic, 50V Vce, Dual NPN Input Resistor Transistors, SOT-363")
    (property "ki_keywords" "Dual NPN Transistor")
    (attr smd)
    (fp_text reference "Q1" (at 0.1235 2.2075) (layer "F.SilkS"))
    (fp_text value "UMH3N" (at 1.076 -14.112 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "RTS") (pinfunction "E1") (pintype "passive"))
    (pad "2" smd rect (at -1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "DTR") (pinfunction "B1") (pintype "input"))
    (pad "3" smd rect (at -1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/IO0") (pinfunction "C2") (pintype "passive"))
    (pad "4" smd rect (at 1.33 0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "DTR") (pinfunction "E2") (pintype "passive"))
    (pad "5" smd rect (at 1.33 0) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "RTS") (pinfunction "B2") (pintype "input"))
    (pad "6" smd rect (at 1.33 -0.65) (size 1.5 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/EN") (pinfunction "C1") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 112.0902 70.0024)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R1" (at -0.0005 1.524) (layer "F.SilkS"))
    (fp_text value "10K" (at -4.94 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/EN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 102.553 67.31 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R2" (at -0.004 -1.4952) (layer "F.SilkS"))
    (fp_text value "470R" (at -0.5466 -15.0114) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/eTX") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U3-RXD)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 72.072 77.6224)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 1.397) (layer "F.SilkS"))
    (fp_text value "1K5" (at -7.8618 0.1524) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(D2-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 72.1492 62.8396)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R7" (at 0.0122 1.4732 180) (layer "F.SilkS"))
    (fp_text value "1K5" (at 0.1524 -2.7178 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(D3-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/SLED") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 92.456 94.1832)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R17" (at -2.899 0.022) (layer "F.SilkS"))
    (fp_text value "1K5" (at 0.301 8.222) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(J2-Pad10)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/LINKLED") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 92.4565 95.7707 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R18" (at 2.921 -0.0127) (layer "F.SilkS"))
    (fp_text value "1K5" (at -0.4505 -8.1345) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/ACTLED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J2-Pad12)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 93.218 66.929 -90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "USB serial converter, UART, SOIC-16")
    (property "ki_keywords" "USB UART Serial Converter Interface")
    (attr smd)
    (fp_text reference "U3" (at -4.572 3.429) (layer "F.SilkS"))
    (fp_text value "CH340C" (at -8.7884 0.1016) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 -3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/eRX") (pinfunction "TXD") (pintype "output"))
    (pad "3" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(U3-RXD)") (pinfunction "RXD") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pinfunction "V3") (pintype "passive"))
    (pad "5" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(U3-UD+)") (pinfunction "UD+") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(U3-UD-)") (pinfunction "UD-") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.475 3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "unconnected-(U3-NC-Pad7)") (pinfunction "NC") (pintype "no_connect"))
    (pad "8" smd roundrect (at -2.475 4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "unconnected-(U3-NC-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (pad "9" smd roundrect (at 2.475 4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "unconnected-(U3-~{CTS}-Pad9)") (pinfunction "~{CTS}") (pintype "input+no_connect"))
    (pad "10" smd roundrect (at 2.475 3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "unconnected-(U3-~{DSR}-Pad10)") (pinfunction "~{DSR}") (pintype "input+no_connect"))
    (pad "11" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "unconnected-(U3-~{RI}-Pad11)") (pinfunction "~{RI}") (pintype "input+no_connect"))
    (pad "12" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "unconnected-(U3-~{DCD}-Pad12)") (pinfunction "~{DCD}") (pintype "input+no_connect"))
    (pad "13" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "DTR") (pinfunction "~{DTR}") (pintype "output"))
    (pad "14" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "RTS") (pinfunction "~{RTS}") (pintype "output"))
    (pad "15" smd roundrect (at 2.475 -3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "unconnected-(U3-R232-Pad15)") (pinfunction "R232") (pintype "input+no_connect"))
    (pad "16" smd roundrect (at 2.475 -4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 106.3498 95.3262 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C11" (at -2.908 0 90) (layer "F.SilkS"))
    (fp_text value "1u1R" (at 5.8804 -0.3302 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/VDDCR") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 99.8474 95.3138 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C12" (at -2.8451 0.0254 90) (layer "F.SilkS"))
    (fp_text value "10n" (at 5.4226 -0.2032 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 108.0008 95.3262 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C13" (at -2.908 0 -90) (layer "F.SilkS"))
    (fp_text value "470p" (at 5.8042 -0.254 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/VDDCR") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 110.1852 89.2302)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R6" (at 2.4135 0.0635) (layer "F.SilkS"))
    (fp_text value "10R" (at 28.4094 0.381) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U5-RXER{slash}PHYAD0)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/+3V3_LAN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 102.1334 79.5396 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R8" (at 2.45568 0.02032 270) (layer "F.SilkS"))
    (fp_text value "10K" (at 6.1723 0.0254 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/+3V3_LAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/nRST") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 110.1974 92.6846)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R9" (at 2.4135 0.0635) (layer "F.SilkS"))
    (fp_text value "10R" (at 28.4602 0.2286) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U5-RXD1{slash}MODE1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/RXD1") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 110.2106 83.693)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R10" (at 2.921 -0.381) (layer "F.SilkS"))
    (fp_text value "1K5" (at -28.3078 -0.2032) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/+3V3_LAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/MDIO") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 110.1852 85.8012 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R11" (at -2.9215 0) (layer "F.SilkS"))
    (fp_text value "10R" (at -28.4094 -0.2794) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/CRS_DV") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(U5-CRS_DV{slash}MODE2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 110.1974 91.1606)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R14" (at 2.9215 0.0635) (layer "F.SilkS"))
    (fp_text value "10R" (at 28.4602 0.0762) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(U5-RXD0{slash}MODE0)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/RXD0") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 123.825 93.4842 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R15" (at -2.79908 -0.02032 90) (layer "F.SilkS"))
    (fp_text value "33R" (at -5.4488 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/XTAL") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/PHY_CLK") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 92.4306 91.9988 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R16" (at 2.9591 -0.0889 180) (layer "F.SilkS"))
    (fp_text value "49R9" (at 27.2928 -0.0762 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/RX+") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 92.456 89.027 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R22" (at 2.8575 -0.5207 180) (layer "F.SilkS"))
    (fp_text value "49R9" (at 27.4452 0.0508 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/RX-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (layer "F.Cu")
    (at 102.3874 88.0618 90)
    (descr "QFN, 24 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=278), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "LAN8720 Ethernet PHY with RMII interface, QFN-24")
    (property "ki_keywords" "ETH PHY RMII")
    (attr smd)
    (fp_text reference "U5" (at 3.0566 0.0254) (layer "F.SilkS"))
    (fp_text value "LAN8720A" (at 12.2682 0.0254) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "" smd roundrect (at -0.65 -0.65 90) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.2380942857))
    (pad "" smd roundrect (at -0.65 0.65 90) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.2380942857))
    (pad "" smd roundrect (at 0.65 -0.65 90) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.2380942857))
    (pad "" smd roundrect (at 0.65 0.65 90) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.2380942857))
    (pad "1" smd roundrect (at -1.9375 -1.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pinfunction "VDD2A") (pintype "power_in"))
    (pad "2" smd roundrect (at -1.9375 -0.75 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/LINKLED") (pinfunction "LED2/nINTSEL") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.9375 -0.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "/ACTLED") (pinfunction "LED1/REGOFF") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -1.9375 0.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "unconnected-(U5-XTAL2-Pad4)") (pinfunction "XTAL2") (pintype "passive+no_connect"))
    (pad "5" smd roundrect (at -1.9375 0.75 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/XTAL") (pinfunction "XTAL1/CLKIN") (pintype "passive"))
    (pad "6" smd roundrect (at -1.9375 1.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/VDDCR") (pinfunction "VDDCR") (pintype "power_in"))
    (pad "7" smd roundrect (at -1.25 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "Net-(U5-RXD1{slash}MODE1)") (pinfunction "RXD1/MODE1") (pintype "output"))
    (pad "8" smd roundrect (at -0.75 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(U5-RXD0{slash}MODE0)") (pinfunction "RXD0/MODE0") (pintype "output"))
    (pad "9" smd roundrect (at -0.25 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/+3V3_LAN") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "10" smd roundrect (at 0.25 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U5-RXER{slash}PHYAD0)") (pinfunction "RXER/PHYAD0") (pintype "output"))
    (pad "11" smd roundrect (at 0.75 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "Net-(U5-CRS_DV{slash}MODE2)") (pinfunction "CRS_DV/MODE2") (pintype "output"))
    (pad "12" smd roundrect (at 1.25 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/MDIO") (pinfunction "MDIO") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 1.9375 1.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/MDC") (pinfunction "MDC") (pintype "input"))
    (pad "14" smd roundrect (at 1.9375 0.75 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "unconnected-(U5-INT{slash}REFCLKO-Pad14)") (pinfunction "INT/REFCLKO") (pintype "output+no_connect"))
    (pad "15" smd roundrect (at 1.9375 0.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/nRST") (pinfunction "RST") (pintype "input"))
    (pad "16" smd roundrect (at 1.9375 -0.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/TXEN") (pinfunction "TXEN") (pintype "input"))
    (pad "17" smd roundrect (at 1.9375 -0.75 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/TXD0") (pinfunction "TXD0") (pintype "input"))
    (pad "18" smd roundrect (at 1.9375 -1.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/TXD1") (pinfunction "TXD1") (pintype "input"))
    (pad "19" smd roundrect (at 1.25 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pinfunction "VDD1A") (pintype "power_in"))
    (pad "20" smd roundrect (at 0.75 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/TX-") (pinfunction "TXN") (pintype "output"))
    (pad "21" smd roundrect (at 0.25 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/TX+") (pinfunction "TXP") (pintype "output"))
    (pad "22" smd roundrect (at -0.25 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/RX-") (pinfunction "RXN") (pintype "output"))
    (pad "23" smd roundrect (at -0.75 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/RX+") (pinfunction "RXP") (pintype "output"))
    (pad "24" smd roundrect (at -1.25 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/RBIAS") (pinfunction "RBIAS") (pintype "input"))
    (pad "25" smd rect (at 0 0 90) (size 2.6 2.6) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CPB:RJ45_Hanrun_HR911105A_Oval" (layer "F.Cu")
    (at 82.042 83.82 -90)
    (descr "http://www.kosmodrom.com.ua/pdf/HR911105A.pdf")
    (tags "RJ45 Magjack")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RJ connector, 8P8C (8 positions 8 connected), two LEDs, RJ45, Shielded")
    (property "ki_keywords" "8P8C RJ female connector led")
    (attr through_hole)
    (fp_text reference "J2" (at 13.3985 -3.556) (layer "F.SilkS"))
    (fp_text value "HR911105A" (at 4.44 19.935 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.44 6.36 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -1.275 6.36 270) (size 3.25 3.25) (drill 3.25) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 10.155 6.36 270) (size 3.25 3.25) (drill 3.25) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 1.5 2.5) (drill 0.9 (offset 0 0.5)) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.167)
      (net 19 "/TX+") (pinfunction "TD+") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.26 -2.54 270) (size 1.5 2.5) (drill 0.9 (offset 0 -0.5)) (layers "*.Cu" "*.Mask")
      (net 20 "/TX-") (pinfunction "TD-") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 0 270) (size 1.5 2.5) (drill 0.9 (offset 0 0.5)) (layers "*.Cu" "*.Mask")
      (net 21 "/RX+") (pinfunction "RD+") (pintype "passive"))
    (pad "4" thru_hole oval (at 3.8 -2.54 270) (size 1.5 2.5) (drill 0.9 (offset 0 -0.5)) (layers "*.Cu" "*.Mask")
      (net 4 "+3.3VA") (pinfunction "TC") (pintype "passive"))
    (pad "5" thru_hole oval (at 5.08 0 270) (size 1.5 2.5) (drill 0.9 (offset 0 0.5)) (layers "*.Cu" "*.Mask")
      (net 4 "+3.3VA") (pinfunction "RC") (pintype "passive"))
    (pad "6" thru_hole oval (at 6.34 -2.54 270) (size 1.5 2.5) (drill 0.9 (offset 0 -0.5)) (layers "*.Cu" "*.Mask")
      (net 46 "/RX-") (pinfunction "RD-") (pintype "passive"))
    (pad "7" thru_hole oval (at 7.62 0 270) (size 1.5 2.5) (drill 0.9 (offset 0 0.5)) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(J2-NC-Pad7)") (pinfunction "NC") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval (at 8.88 -2.54 270) (size 1.5 2.5) (drill 0.9 (offset 0 -0.5)) (layers "*.Cu" "*.Mask")
      (net 37 "GND1") (pinfunction "GND") (pintype "passive"))
    (pad "9" thru_hole oval (at -2.185 11.26 270) (size 1.8 2.5) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 4 "+3.3VA") (pintype "passive"))
    (pad "10" thru_hole oval (at 0.355 11.26 270) (size 1.8 2.5) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(J2-Pad10)") (pintype "passive"))
    (pad "11" thru_hole oval (at 8.525 11.26 270) (size 1.8 2.5) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 37 "GND1") (pintype "passive"))
    (pad "12" thru_hole oval (at 11.065 11.26 270) (size 1.8 2.5) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(J2-Pad12)") (pintype "passive"))
    (pad "SH" thru_hole oval (at -3.305 3.31 270) (size 2.5 3) (drill 1.63 (offset 0 -0.25)) (layers "*.Cu" "*.Mask")
      (net 37 "GND1") (pintype "passive"))
    (pad "SH" thru_hole oval (at 12.185 3.31 270) (size 2.5 3) (drill 1.63 (offset 0 -0.25)) (layers "*.Cu" "*.Mask")
      (net 37 "GND1") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_RJ.3dshapes/RJ45_Hanrun_HR911105A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 92.456 84.709 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R20" (at 2.8575 -0.07112 180) (layer "F.SilkS"))
    (fp_text value "49R9" (at 27.3436 -0.0254 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/TX-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 103.9368 79.5404 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C9" (at -2.90352 -0.22352 -90) (layer "F.SilkS"))
    (fp_text value "100n" (at 6.5787 0 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/nRST") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 83.0326 69.6468 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C7" (at -2.4892 0) (layer "F.SilkS"))
    (fp_text value "100n" (at 14.1856 0.2032) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-6_Handsoldering" (layer "F.Cu")
    (at 83.947 66.929)
    (descr "6-pin SOT-23 package, Handsoldering")
    (tags "SOT-23-6 Handsoldering")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6")
    (property "ki_keywords" "usb ethernet video")
    (attr smd)
    (fp_text reference "U6" (at 1.397 -2.54) (layer "F.SilkS"))
    (fp_text value "USBLC6-2SC6" (at -0.3556 -8.4582) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/DM") (pinfunction "I/O1") (pintype "passive"))
    (pad "2" smd rect (at -1.35 0) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "3" smd rect (at -1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/DP") (pinfunction "I/O2") (pintype "passive"))
    (pad "4" smd rect (at 1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(U3-UD+)") (pinfunction "I/O2") (pintype "passive"))
    (pad "5" smd rect (at 1.35 0) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VBUS") (pintype "passive"))
    (pad "6" smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(U3-UD-)") (pinfunction "I/O1") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 101.5746 74.549 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R4" (at -2.0574 0 180) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/PHY_POWER") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 98.6536 74.93 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at -0.0889 2.3368) (layer "F.SilkS"))
    (fp_text value "HT7233" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd rect (at -1.1 0 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "3" smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "/PHY_POWER") (pinfunction "CE") (pintype "input"))
    (pad "4" smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "/+3V3_LAN") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 73.978 75.946)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.43) (layer "F.SilkS"))
    (fp_text value "0R" (at -7.8872 -0.1016) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 92.456 87.4522 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R21" (at 2.794 0.1905 180) (layer "F.SilkS"))
    (fp_text value "49R9" (at 27.242 0.3302 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/TX+") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CPB:ESP32-WROOM-32U-HandSoldering" (layer "F.Cu")
    (at 128.3208 79.9846 -90)
    (descr "Single 2.4 GHz Wi-Fi and Bluetooth combo chip with U.FL connector, https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32d_esp32-wroom-32u_datasheet_en.pdf")
    (tags "Single 2.4 GHz Wi-Fi and Bluetooth combo  chip")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "RF Module, ESP32-D0WD SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, external antenna, SMD")
    (property "ki_keywords" "RF Radio BT ESP ESP32 Espressif external U.FL antenna")
    (clearance 0.6)
    (attr smd)
    (fp_text reference "U2" (at 8.001 11.176) (layer "F.SilkS"))
    (fp_text value "ESP32-WROOM-32U" (at -0.0508 -11.3284 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -8.5 -8.255 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -8.5 -6.985 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" smd roundrect (at -8.5 -5.715 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/EN") (pinfunction "EN") (pintype "input"))
    (pad "4" smd roundrect (at -8.5 -4.445 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "unconnected-(U2-SENSOR_VP-Pad4)") (pinfunction "SENSOR_VP") (pintype "input+no_connect"))
    (pad "5" smd roundrect (at -8.5 -3.175 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "unconnected-(U2-SENSOR_VN-Pad5)") (pinfunction "SENSOR_VN") (pintype "input+no_connect"))
    (pad "6" smd roundrect (at -8.5 -1.905 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/IO34") (pinfunction "IO34") (pintype "input"))
    (pad "7" smd roundrect (at -8.5 -0.635 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "/IO35") (pinfunction "IO35") (pintype "input"))
    (pad "8" smd roundrect (at -8.5 0.635 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "/IO32") (pinfunction "IO32") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -8.5 1.905 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/IO33") (pinfunction "IO33") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -8.5 3.175 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/RXD0") (pinfunction "IO25") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -8.5 4.445 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "/RXD1") (pinfunction "IO26") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -8.5 5.715 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/CRS_DV") (pinfunction "IO27") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -8.5 6.985 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "unconnected-(U2-IO14-Pad13)") (pinfunction "IO14") (pintype "bidirectional+no_connect"))
    (pad "14" smd roundrect (at -8.5 8.255 270) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/PHY_POWER") (pinfunction "IO12") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -5.715 9.255 180) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "16" smd roundrect (at -4.445 9.255) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "unconnected-(U2-IO13-Pad16)") (pinfunction "IO13") (pintype "bidirectional+no_connect"))
    (pad "17" smd roundrect (at -3.175 9.255) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "unconnected-(U2-SHD{slash}SD2-Pad17)") (pinfunction "SHD/SD2") (pintype "bidirectional+no_connect"))
    (pad "18" smd roundrect (at -1.905 9.255) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "unconnected-(U2-SWP{slash}SD3-Pad18)") (pinfunction "SWP/SD3") (pintype "bidirectional+no_connect"))
    (pad "19" smd roundrect (at -0.635 9.255) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "unconnected-(U2-SCS{slash}CMD-Pad19)") (pinfunction "SCS/CMD") (pintype "bidirectional+no_connect"))
    (pad "20" smd roundrect (at 0.635 9.255) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "unconnected-(U2-SCK{slash}CLK-Pad20)") (pinfunction "SCK/CLK") (pintype "bidirectional+no_connect"))
    (pad "21" smd roundrect (at 1.905 9.255) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "unconnected-(U2-SDO{slash}SD0-Pad21)") (pinfunction "SDO/SD0") (pintype "bidirectional+no_connect"))
    (pad "22" smd roundrect (at 3.175 9.255) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "unconnected-(U2-SDI{slash}SD1-Pad22)") (pinfunction "SDI/SD1") (pintype "bidirectional+no_connect"))
    (pad "23" smd roundrect (at 4.445 9.255) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "unconnected-(U2-IO15-Pad23)") (pinfunction "IO15") (pintype "bidirectional+no_connect"))
    (pad "24" smd roundrect (at 5.715 9.255) (size 2.5 0.9) (drill (offset -0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "/SLED") (pinfunction "IO2") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 8.5 8.255 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/IO0") (pinfunction "IO0") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 8.5 6.985 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "unconnected-(U2-IO4-Pad26)") (pinfunction "IO4") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 8.5 5.715 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "unconnected-(U2-IO16-Pad27)") (pinfunction "IO16") (pintype "bidirectional+no_connect"))
    (pad "28" smd roundrect (at 8.5 4.445 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/PHY_CLK") (pinfunction "IO17") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 8.5 3.175 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "unconnected-(U2-IO5-Pad29)") (pinfunction "IO5") (pintype "bidirectional+no_connect"))
    (pad "30" smd roundrect (at 8.5 1.905 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/MDIO") (pinfunction "IO18") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 8.5 0.635 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/TXD0") (pinfunction "IO19") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 8.5 -0.635 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "unconnected-(U2-NC-Pad32)") (pinfunction "NC") (pintype "no_connect"))
    (pad "33" smd roundrect (at 8.5 -1.905 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/TXEN") (pinfunction "IO21") (pintype "bidirectional"))
    (pad "34" smd roundrect (at 8.5 -3.175 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "/eRX") (pinfunction "RXD0/IO3") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 8.5 -4.445 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/eTX") (pinfunction "TXD0/IO1") (pintype "bidirectional"))
    (pad "36" smd roundrect (at 8.5 -5.715 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/TXD1") (pinfunction "IO22") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 8.5 -6.985 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/MDC") (pinfunction "IO23") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 8.5 -8.255 270) (size 2.5 0.9) (drill (offset 0.5 0)) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "39" smd rect (at -1 -0.755 270) (size 5 5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/RF_Module.3dshapes/ESP32-WROOM-32U.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 99.441 69.202 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C4" (at 2.0952 0 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 11.0614 0.1778 270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 93.53072 80.54848)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C14" (at 0.57628 1.44272 180) (layer "F.SilkS"))
    (fp_text value "22n" (at -16.5484 0.0762 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (at 93.53804 77.20584 180)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Ferrite bead, small symbol")
    (property "ki_keywords" "L ferrite bead inductor filter")
    (attr smd)
    (fp_text reference "FB1" (at 0.06604 1.31064 180) (layer "F.SilkS"))
    (fp_text value "30R" (at -3.04302 -0.00508 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/+3V3_LAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pintype "passive"))
    (model "${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 104.7242 95.3262 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C15" (at -2.959 0 -90) (layer "F.SilkS"))
    (fp_text value "10n" (at 6.1723 -0.0254 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/VDDCR") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Castellated" (layer "F.Cu")
    (at 85.93328 78.85176)
    (descr "LED SMD 0603 (1608 Metric), castellated end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED castellated")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode, small symbol")
    (property "ki_keywords" "LED diode light-emitting-diode")
    (attr smd)
    (fp_text reference "D4" (at -2.81178 0.02794) (layer "F.SilkS"))
    (fp_text value "RED" (at -28.6258 0.0762) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8125 0) (size 1.225 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8125 0) (size 1.225 0.85) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric_Castellated.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 110.173 87.4014)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R13" (at 2.9078 0.0508) (layer "F.SilkS"))
    (fp_text value "1K5" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/+3V3_LAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/CRS_DV") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 89.22004 78.8416)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R5" (at -0.08128 -1.33096) (layer "F.SilkS"))
    (fp_text value "1K5" (at -27.7114 -0.0508) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D4-A)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/+3V3_LAN") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 93.53012 78.87208)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C17" (at -1.83612 0.00762 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (at 98.1964 95.3008 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small symbol")
    (property "ki_keywords" "R resistor")
    (attr smd)
    (fp_text reference "R19" (at 2.921 0 90) (layer "F.SilkS"))
    (fp_text value "12K1" (at -6.0706 0.2794 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/RBIAS") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 90.932 82.2452)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C16" (at -2.921 0.0635) (layer "F.SilkS"))
    (fp_text value "22n" (at -16.4976 0.1778) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3VA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (at 84.2772 73.8886)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -0.0127 -2.3114) (layer "F.SilkS"))
    (fp_text value "HT7233" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd rect (at -1.1 0) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "3" smd rect (at -1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "+5V") (pinfunction "CE") (pintype "input"))
    (pad "4" smd rect (at 1.1 0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "5" smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "+3V3") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (at 97.536 80.9498 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C10" (at -0.1013 -1.4859 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 4.8898 0.0762 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/+3V3_LAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 97.8068 78.9686 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C8" (at -2.3962 0.02032 180) (layer "F.SilkS"))
    (fp_text value "22u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/+3V3_LAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_PicoBlade_53047-0410_1x04_P1.25mm_Vertical" (layer "F.Cu")
    (at 126.832 66.5052 180)
    (descr "Molex PicoBlade Connector System, 53047-0410, 4 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J4" (at -2.875 0.1) (layer "F.SilkS"))
    (fp_text value "GPIO" (at 1.88 2.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.88 -1.35) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 0.8 1.3) (drill 0.5) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 75 "/IO32") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.25 0 180) (size 0.8 1.3) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 76 "/IO33") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.5 0 180) (size 0.8 1.3) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 2 "+3V3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 3.75 0 180) (size 0.8 1.3) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_PicoBlade_53047-0410_1x04_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_PicoBlade_53047-0410_1x04_P1.25mm_Vertical" (layer "F.Cu")
    (at 76.807 71.9052 90)
    (descr "Molex PicoBlade Connector System, 53047-0410, 4 Pins per row (http://www.molex.com/pdm_docs/sd/530470610_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade side entry")
    (property "Sheetfile" "ESP32-Ethgate.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J3" (at -2.5 -0.25 180) (layer "F.SilkS"))
    (fp_text value "USB" (at 5.9668 -0.0736 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.88 -1.35 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 0.8 1.3) (drill 0.5) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.25 0 90) (size 0.8 1.3) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 74 "/DP") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.5 0 90) (size 0.8 1.3) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 73 "/DM") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 3.75 0 90) (size 0.8 1.3) (drill 0.5) (layers "*.Cu" "*.Mask")
      (net 72 "/VBUS") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_PicoBlade_53047-0410_1x04_P1.25mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 138.557 60.96) (end 67.31 60.96)
    (layer "Edge.Cuts"))
  (gr_line (start 138.557 99.06) (end 138.557 60.96)
    (layer "Edge.Cuts"))
  (gr_line (start 67.31 99.06) (end 138.557 99.06)
    (layer "Edge.Cuts"))
  (gr_line (start 67.31 60.96) (end 67.31 99.06)
    (layer "Edge.Cuts"))
  (gr_text "ESP32-Ethgate v2.4\ncperiod 2022" (at 110.007 63.7052) (layer "F.SilkS"))
  (gr_text "D+" (at 78.0542 70.6628) (layer "F.SilkS"))
  (gr_text "GND" (at 124.557 65.0052 90) (layer "F.SilkS"))
  (gr_text "IO33" (at 125.757 65.0052 90) (layer "F.SilkS"))
  (gr_text "5V" (at 78.0542 68.1228) (layer "F.SilkS"))
  (gr_text "D-" (at 78.0542 69.3928) (layer "F.SilkS"))
  (gr_text "GND" (at 78.0542 71.9328) (layer "F.SilkS"))
  (gr_text "3V" (at 123.157 65.0052 90) (layer "F.SilkS"))
  (gr_text "IO32" (at 126.957 65.0052 90) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.6))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.6) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 139.827 100.0252)
        (xy 89.027 100.0252)
        (xy 88.9 77.994997)
        (xy 74.295 77.994997)
        (xy 74.295 59.3852)
        (xy 139.827 59.3852)
      )
    )
  )
  (zone (net 37) (net_name "GND1") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.6))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.6) (thermal_bridge_width 0.6) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 73.66 78.74)
        (xy 88.265 78.74)
        (xy 88.265 100.0252)
        (xy 66.167 100.0252)
        (xy 66.167 60.6552)
        (xy 73.66 60.96)
      )
    )
  )
  (zone (net 36) (net_name "/RBIAS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30173)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.3214 93.6758)
        (xy 98.0714 93.6758)
        (xy 97.7964 94.123406)
        (xy 98.1964 94.4768)
        (xy 98.5964 94.123406)
      )
    )
  )
  (zone (net 73) (net_name "/DM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30088)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 75.766707 69.254)
        (xy 75.766707 69.654)
        (xy 76.557 69.8052)
        (xy 76.808 69.4052)
        (xy 76.403927 69.035648)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30099)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.95572 79.62348)
        (xy 92.55572 79.62348)
        (xy 92.322847 80.212376)
        (xy 92.75572 80.54948)
        (xy 93.188593 80.212376)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30179)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 86.2322 73.1386)
        (xy 86.2322 72.7386)
        (xy 85.9072 72.6136)
        (xy 85.3762 72.9386)
        (xy 85.9072 73.2636)
      )
    )
  )
  (zone (net 8) (net_name "/EN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30140)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.189133 67.065921)
        (xy 132.584207 67.003347)
        (xy 132.835527 66.616397)
        (xy 132.384644 66.293613)
        (xy 131.935531 66.61858)
      )
    )
  )
  (zone (net 19) (net_name "/TX+") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30045)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 88.829204 86.4302)
        (xy 88.829204 86.1802)
        (xy 87.85961 85.754872)
        (xy 87.629 86.3092)
        (xy 87.85961 86.863528)
      )
    )
  )
  (zone (net 42) (net_name "/PHY_POWER") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30028)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.749196 67.9034)
        (xy 107.625589 67.522978)
        (xy 106.57739 67.924072)
        (xy 106.806049 68.478709)
        (xy 107.361328 68.70801)
      )
    )
  )
  (zone (net 72) (net_name "/VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30187)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 73.91 69.004)
        (xy 73.91 68.604)
        (xy 73.66 68.554)
        (xy 72.859 68.804)
        (xy 73.66 69.054)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30190)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 83.871982 73.149524)
        (xy 84.071974 72.803112)
        (xy 83.7072 72.638224)
        (xy 83.176334 72.938101)
        (xy 83.7072 73.2636)
      )
    )
  )
  (zone (net 22) (net_name "/nRST") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30126)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.699316 79.457293)
        (xy 102.876093 79.280516)
        (xy 102.6084 78.623914)
        (xy 102.132693 78.713893)
        (xy 101.967715 79.1146)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30090)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.9788 67.1686)
        (xy 135.3788 67.1686)
        (xy 135.6288 66.591486)
        (xy 135.1788 66.2676)
        (xy 134.7288 66.591486)
      )
    )
  )
  (zone (net 12) (net_name "Net-(D4-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30169)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.59504 78.7166)
        (xy 87.59504 78.9666)
        (xy 88.042647 79.2416)
        (xy 88.39604 78.8416)
        (xy 88.042647 78.4416)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30144)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.084295 81.139872)
        (xy 99.006257 80.74756)
        (xy 98.630062 80.497245)
        (xy 98.31002 80.949995)
        (xy 98.637758 81.397212)
      )
    )
  )
  (zone (net 38) (net_name "/VDDCR") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30092)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.4248 94.3512)
        (xy 105.4248 94.7512)
        (xy 106.013696 94.984073)
        (xy 106.3508 94.5512)
        (xy 106.013696 94.118327)
      )
    )
  )
  (zone (net 62) (net_name "Net-(U3-UD-)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30138)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 86.402 66.1892)
        (xy 86.402 65.7892)
        (xy 86.077 65.661189)
        (xy 85.296 65.979)
        (xy 86.077 66.304)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30113)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 91.023335 88.068621)
        (xy 91.306178 88.351464)
        (xy 91.808583 87.9272)
        (xy 91.631707 87.451493)
        (xy 91.231 87.339393)
      )
    )
  )
  (zone (net 12) (net_name "Net-(D4-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30108)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.78328 78.9666)
        (xy 87.78328 78.7166)
        (xy 87.2271 78.442936)
        (xy 86.74478 78.85176)
        (xy 87.2271 79.260584)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30091)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 91.85572 80.34848)
        (xy 91.85572 80.74848)
        (xy 92.432833 80.99848)
        (xy 92.75672 80.54848)
        (xy 92.432833 80.09848)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_track$") (hatch edge 0.5)
    (priority 30195)
    (attr (teardrop (type track_end)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.75896 86.5104)
        (xy 98.75896 86.2604)
        (xy 98.35896 86.1854)
        (xy 98.35796 86.3854)
        (xy 98.35896 86.5854)
      )
    )
  )
  (zone (net 43) (net_name "/PHY_CLK") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30167)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 124.0008 91.8592)
        (xy 123.7508 91.8592)
        (xy 123.447565 92.291728)
        (xy 123.825 92.6602)
        (xy 124.246991 92.326115)
      )
    )
  )
  (zone (net 73) (net_name "/DM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30157)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 81.492 65.7052)
        (xy 81.492 66.1052)
        (xy 81.817 66.252609)
        (xy 82.598 65.979)
        (xy 81.817 65.654)
      )
    )
  )
  (zone (net 42) (net_name "/PHY_POWER") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 120.239903 69.334379)
        (xy 119.843327 69.386593)
        (xy 119.632927 69.873496)
        (xy 120.06593 71.485591)
        (xy 120.497494 69.871732)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.1058 69.094338)
        (xy 135.5058 69.094338)
        (xy 135.733128 68.14921)
        (xy 135.1788 67.9186)
        (xy 134.624472 68.14921)
      )
    )
  )
  (zone (net 15) (net_name "/LINKLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30119)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 94.008632 93.594744)
        (xy 93.831855 93.417967)
        (xy 93.179387 93.7082)
        (xy 93.280293 94.183907)
        (xy 93.681 94.342197)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D3-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30161)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 69.753907 64.117958)
        (xy 69.691325 63.722886)
        (xy 69.380812 63.496421)
        (xy 68.960013 63.922656)
        (xy 69.381241 64.346423)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30115)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.9724 93.6388)
        (xy 99.7224 93.6388)
        (xy 99.3974 94.215913)
        (xy 99.8474 94.5398)
        (xy 100.2974 94.215913)
      )
    )
  )
  (zone (net 32) (net_name "/TXEN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30042)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 130.3508 90.8496)
        (xy 130.1008 90.8496)
        (xy 129.671472 91.81999)
        (xy 130.2258 92.0506)
        (xy 130.780128 91.81999)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30129)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.399372 66.074345)
        (xy 134.29582 66.460707)
        (xy 134.842696 66.701473)
        (xy 135.179765 66.268858)
        (xy 134.842696 65.835727)
      )
    )
  )
  (zone (net 42) (net_name "/PHY_POWER") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30132)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.6996 73.524)
        (xy 100.6996 73.924)
        (xy 101.223063 74.108776)
        (xy 101.5756 73.724)
        (xy 101.223063 73.339224)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30170)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.84504 78.9666)
        (xy 90.84504 78.7166)
        (xy 90.397433 78.4416)
        (xy 90.04404 78.8416)
        (xy 90.397433 79.2416)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30182)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 84.12535 74.980306)
        (xy 83.925356 74.633894)
        (xy 83.7072 74.5136)
        (xy 83.176334 74.839099)
        (xy 83.7072 75.144321)
      )
    )
  )
  (zone (net 31) (net_name "/TXD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30048)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.5124 82.929761)
        (xy 101.7624 82.929761)
        (xy 102.154328 81.96681)
        (xy 101.6 81.7362)
        (xy 101.045672 81.96681)
      )
    )
  )
  (zone (net 34) (net_name "/MDC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.1808 90.6846)
        (xy 135.4308 90.6846)
        (xy 135.738673 90.095704)
        (xy 135.3058 88.4836)
        (xy 134.872927 90.095704)
      )
    )
  )
  (zone (net 33) (net_name "/TXD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30044)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.968916 94.693061)
        (xy 129.792139 94.516284)
        (xy 128.80239 94.898872)
        (xy 129.031293 95.453907)
        (xy 129.586328 95.68281)
      )
    )
  )
  (zone (net 8) (net_name "/EN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 116.676209 68.4816)
        (xy 116.676209 68.8816)
        (xy 117.62639 69.337528)
        (xy 117.857 68.7832)
        (xy 117.62639 68.228872)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30160)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 110.388947 89.712428)
        (xy 110.535891 89.914682)
        (xy 111.113043 89.7052)
        (xy 111.011009 89.229613)
        (xy 110.6102 89.072054)
      )
    )
  )
  (zone (net 28) (net_name "/CRS_DV") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30175)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 111.844405 85.818788)
        (xy 111.748736 85.587819)
        (xy 111.315006 85.360313)
        (xy 111.009277 85.801582)
        (xy 111.392204 86.156885)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30147)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.8056 91.7988)
        (xy 90.8056 92.1988)
        (xy 91.253207 92.3988)
        (xy 91.6066 91.9988)
        (xy 91.253207 91.5988)
      )
    )
  )
  (zone (net 26) (net_name "/MDIO") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30142)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 111.630054 84.273231)
        (xy 111.806831 84.096454)
        (xy 111.4356 83.488004)
        (xy 111.034893 83.692293)
        (xy 111.010855 84.168)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30097)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.95512 77.94708)
        (xy 92.55512 77.94708)
        (xy 92.322247 78.535976)
        (xy 92.75512 78.87308)
        (xy 93.187993 78.535976)
      )
    )
  )
  (zone (net 25) (net_name "/RXD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30047)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.3274 79.528548)
        (xy 114.5774 79.528548)
        (xy 115.032128 78.56321)
        (xy 114.4778 78.3326)
        (xy 113.923472 78.56321)
      )
    )
  )
  (zone (net 73) (net_name "/DM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30186)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 73.91 69.654)
        (xy 73.91 69.254)
        (xy 73.66 69.204)
        (xy 72.859 69.454)
        (xy 73.66 69.704)
      )
    )
  )
  (zone (net 31) (net_name "/TXD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.5608 90.6846)
        (xy 127.8108 90.6846)
        (xy 128.118673 90.095704)
        (xy 127.6858 88.4836)
        (xy 127.252927 90.095704)
      )
    )
  )
  (zone (net 21) (net_name "/RX+") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30158)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.341373 91.104008)
        (xy 93.099893 91.168712)
        (xy 92.870824 91.647263)
        (xy 93.255858 91.999765)
        (xy 93.640376 91.647263)
      )
    )
  )
  (zone (net 42) (net_name "/PHY_POWER") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30150)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.6086 73.987)
        (xy 100.6086 73.587)
        (xy 99.716414 73.655)
        (xy 99.7526 73.98)
        (xy 100.2836 74.193434)
      )
    )
  )
  (zone (net 10) (net_name "DTR") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30192)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.254014 71.500054)
        (xy 103.427059 71.680483)
        (xy 104.295867 71.5636)
        (xy 104.274721 71.362908)
        (xy 103.524 71.33978)
      )
    )
  )
  (zone (net 8) (net_name "/EN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30114)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.613541 66.078218)
        (xy 131.333607 66.363938)
        (xy 132.034893 66.71825)
        (xy 132.385514 66.295299)
        (xy 132.048696 65.861727)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30063)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 116.0038 70.897973)
        (xy 116.2538 70.897973)
        (xy 116.883264 70.223464)
        (xy 116.459 69.7982)
        (xy 115.859 69.7992)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30029)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.127773 65.5542)
        (xy 106.127773 65.1542)
        (xy 105.453264 64.599736)
        (xy 105.028 65.024)
        (xy 105.029 65.624)
      )
    )
  )
  (zone (net 38) (net_name "/VDDCR") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30096)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.2748 94.7512)
        (xy 107.2748 94.3512)
        (xy 106.685904 94.118327)
        (xy 106.3488 94.5512)
        (xy 106.685904 94.984073)
      )
    )
  )
  (zone (net 29) (net_name "/RXD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30040)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.2708 72.8156)
        (xy 125.0208 72.8156)
        (xy 124.591472 73.78599)
        (xy 125.1458 74.0166)
        (xy 125.700128 73.78599)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30086)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 84.481299 78.004144)
        (xy 84.299692 78.360539)
        (xy 84.50828 78.866647)
        (xy 85.12167 78.852214)
        (xy 85.286425 78.42676)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30069)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 89.3006 72.7742)
        (xy 89.3006 73.1742)
        (xy 89.954929 73.46017)
        (xy 90.5266 72.9792)
        (xy 89.954929 72.49823)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30112)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 94.525458 76.311185)
        (xy 94.125622 76.299751)
        (xy 93.904691 76.865878)
        (xy 94.325512 77.206839)
        (xy 94.746389 76.865878)
      )
    )
  )
  (zone (net 45) (net_name "Net-(J2-Pad12)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30168)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.8315 95.633)
        (xy 90.8315 95.883)
        (xy 91.275356 96.165087)
        (xy 91.6325 95.7707)
        (xy 91.282844 95.365105)
      )
    )
  )
  (zone (net 8) (net_name "/EN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30146)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 110.4652 69.8024)
        (xy 110.4652 70.2024)
        (xy 110.912807 70.4024)
        (xy 111.2662 70.0024)
        (xy 110.912807 69.6024)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30032)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.860877 68.754079)
        (xy 104.14372 69.036922)
        (xy 105.0798 69.0784)
        (xy 105.080507 68.477693)
        (xy 104.655536 68.054136)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.8094 80.5656)
        (xy 101.8094 80.1656)
        (xy 100.83901 79.811272)
        (xy 100.6084 80.3656)
        (xy 100.83901 80.919928)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30078)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.490078 80.51628)
        (xy 99.772923 80.799119)
        (xy 100.37979 80.919928)
        (xy 100.610107 80.364893)
        (xy 100.185136 79.941336)
      )
    )
  )
  (zone (net 42) (net_name "/PHY_POWER") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30194)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.1466 73.924)
        (xy 102.1466 73.524)
        (xy 101.991021 73.382579)
        (xy 101.5736 73.724)
        (xy 101.991021 74.065421)
      )
    )
  )
  (zone (net 16) (net_name "/ACTLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30057)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.804867 93.007057)
        (xy 95.981643 93.183832)
        (xy 97.028 93.3862)
        (xy 97.028707 92.785493)
        (xy 96.603736 92.361936)
      )
    )
  )
  (zone (net 38) (net_name "/VDDCR") (layer "F.Cu") (name "$teardrop_track$") (hatch edge 0.5)
    (priority 30196)
    (attr (teardrop (type track_end)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.4748 94.1512)
        (xy 106.2248 94.1512)
        (xy 106.1498 94.5512)
        (xy 106.3498 94.5522)
        (xy 106.5498 94.5512)
      )
    )
  )
  (zone (net 17) (net_name "/eRX") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30081)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 131.695783 87.337179)
        (xy 131.295817 87.331983)
        (xy 131.062927 87.873496)
        (xy 131.495788 88.485599)
        (xy 131.928673 87.873496)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30185)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 73.91 71.604)
        (xy 73.91 71.204)
        (xy 73.66 71.154)
        (xy 72.859 71.404)
        (xy 73.66 71.654)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 116.945068 85.540424)
        (xy 116.8494 85.771394)
        (xy 117.431316 86.116851)
        (xy 119.066723 85.699982)
        (xy 117.454696 85.266727)
      )
    )
  )
  (zone (net 11) (net_name "/IO0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30200)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.16483 72.402142)
        (xy 104.406309 72.337433)
        (xy 104.480507 72.2136)
        (xy 104.273742 72.012635)
        (xy 104.080288 72.2136)
      )
    )
  )
  (zone (net 28) (net_name "/CRS_DV") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30152)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 110.8852 86.6762)
        (xy 111.1352 86.6762)
        (xy 111.394976 86.152737)
        (xy 111.0102 85.8002)
        (xy 110.625424 86.152737)
      )
    )
  )
  (zone (net 25) (net_name "/RXD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30041)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 124.0008 74.2126)
        (xy 123.7508 74.2126)
        (xy 123.321472 75.18299)
        (xy 123.8758 75.4136)
        (xy 124.430128 75.18299)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_track$") (hatch edge 0.5)
    (priority 30198)
    (attr (teardrop (type track_end)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.769271 76.0242)
        (xy 93.769271 76.2742)
        (xy 94.169271 76.3492)
        (xy 94.170271 76.1492)
        (xy 94.169271 75.9492)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30067)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.1416 72.7386)
        (xy 87.1416 73.1386)
        (xy 87.795929 73.45517)
        (xy 88.3676 72.9742)
        (xy 87.795929 72.49323)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30109)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.630181 94.892668)
        (xy 100.852407 94.56008)
        (xy 100.264193 94.166216)
        (xy 99.846569 94.538245)
        (xy 100.0974 94.9888)
      )
    )
  )
  (zone (net 17) (net_name "/eRX") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.299851 84.120706)
        (xy 133.582694 84.403549)
        (xy 134.51941 83.967928)
        (xy 134.290507 83.412893)
        (xy 133.735472 83.18399)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30116)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 89.850571 83.190341)
        (xy 90.236941 83.086819)
        (xy 90.541099 82.654299)
        (xy 90.156742 82.244235)
        (xy 89.724127 82.581304)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30121)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 109.828965 88.225742)
        (xy 110.005742 88.048965)
        (xy 109.748 87.264912)
        (xy 109.347293 87.400693)
        (xy 109.209636 87.8764)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D1-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30046)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 78.165201 63.8842)
        (xy 78.165201 64.2842)
        (xy 78.778827 64.6592)
        (xy 79.3162 64.0842)
        (xy 78.778827 63.5092)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30031)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.914496 84.798746)
        (xy 107.631653 84.515903)
        (xy 106.7308 84.5408)
        (xy 106.730093 85.141507)
        (xy 107.155064 85.565064)
      )
    )
  )
  (zone (net 75) (net_name "/IO32") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30034)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.4858 68.977761)
        (xy 127.8858 68.977761)
        (xy 127.707 67.9552)
        (xy 127.107 67.9542)
        (xy 126.682736 68.379464)
      )
    )
  )
  (zone (net 61) (net_name "Net-(U3-UD+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30135)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.328397 65.669408)
        (xy 92.714767 65.772933)
        (xy 92.838257 65.385606)
        (xy 92.583258 64.453035)
        (xy 92.283 65.279)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30033)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.603929 64.028313)
        (xy 115.321086 63.74547)
        (xy 114.637736 64.548936)
        (xy 115.061293 64.973907)
        (xy 115.662 64.9732)
      )
    )
  )
  (zone (net 26) (net_name "/MDIO") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.2908 90.6846)
        (xy 126.5408 90.6846)
        (xy 126.848673 90.095704)
        (xy 126.4158 88.4836)
        (xy 125.982927 90.095704)
      )
    )
  )
  (zone (net 74) (net_name "/DP") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30105)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 75.849356 70.432541)
        (xy 75.696274 70.802089)
        (xy 76.403927 71.024752)
        (xy 76.807923 70.655582)
        (xy 76.403927 70.285648)
      )
    )
  )
  (zone (net 75) (net_name "/IO32") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.8858 69.2846)
        (xy 127.4858 69.2846)
        (xy 127.252927 69.873496)
        (xy 127.6858 71.4856)
        (xy 128.118673 69.873496)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.5058 69.2846)
        (xy 135.1058 69.2846)
        (xy 134.872927 69.873496)
        (xy 135.3058 71.4856)
        (xy 135.738673 69.873496)
      )
    )
  )
  (zone (net 15) (net_name "/LINKLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30054)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 95.789626 91.494318)
        (xy 95.936568 91.696574)
        (xy 96.79839 91.943528)
        (xy 97.028809 91.388613)
        (xy 96.79839 90.834872)
      )
    )
  )
  (zone (net 38) (net_name "/VDDCR") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30143)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.471023 93.708341)
        (xy 106.224101 93.747449)
        (xy 105.940701 94.167101)
        (xy 106.349956 94.552187)
        (xy 106.799013 94.227136)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30075)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 82.425509 62.731504)
        (xy 82.376726 62.976697)
        (xy 82.821172 63.74231)
        (xy 83.37648 63.512895)
        (xy 83.3755 62.9127)
      )
    )
  )
  (zone (net 20) (net_name "/TX-") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30181)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.204161 85.426394)
        (xy 93.420667 85.551392)
        (xy 93.665776 85.060537)
        (xy 93.281499 84.708134)
        (xy 92.939579 85.125421)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.3788 66.7196)
        (xy 134.9788 66.7196)
        (xy 134.624472 67.68999)
        (xy 135.1788 67.9206)
        (xy 135.733128 67.68999)
      )
    )
  )
  (zone (net 26) (net_name "/MDIO") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30061)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.135038 93.065938)
        (xy 125.958261 92.889161)
        (xy 125.178736 93.616696)
        (xy 125.602293 94.041667)
        (xy 126.203 94.04096)
      )
    )
  )
  (zone (net 13) (net_name "/eTX") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30023)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.865317 66.526199)
        (xy 129.478947 66.629723)
        (xy 129.152672 67.52559)
        (xy 129.707258 67.756165)
        (xy 130.261328 67.52559)
      )
    )
  )
  (zone (net 38) (net_name "/VDDCR") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30094)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.6492 94.7512)
        (xy 105.6492 94.3512)
        (xy 105.060304 94.118327)
        (xy 104.7232 94.5512)
        (xy 105.060304 94.984073)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30124)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 73.670863 77.416)
        (xy 73.670863 77.016)
        (xy 72.940468 77.1474)
        (xy 72.896 77.6224)
        (xy 73.297 77.863761)
      )
    )
  )
  (zone (net 27) (net_name "Net-(U5-RXER{slash}PHYAD0)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30127)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.794284 88.487507)
        (xy 108.617507 88.664284)
        (xy 108.9602 89.395885)
        (xy 109.360907 89.230907)
        (xy 109.450885 88.7552)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30183)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 83.830664 72.546265)
        (xy 83.507056 72.311155)
        (xy 83.039258 72.6136)
        (xy 83.176613 72.939409)
        (xy 83.7072 72.857246)
      )
    )
  )
  (zone (net 23) (net_name "Net-(U3-RXD)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30148)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.928 67.11)
        (xy 100.928 67.51)
        (xy 101.375607 67.71)
        (xy 101.729 67.31)
        (xy 101.375607 66.91)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30103)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 91.118117 83.913274)
        (xy 90.835274 84.196117)
        (xy 91.231 84.874685)
        (xy 91.631707 84.709707)
        (xy 91.721685 84.234)
      )
    )
  )
  (zone (net 42) (net_name "/PHY_POWER") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.7716 73.587)
        (xy 101.7716 73.987)
        (xy 102.74199 74.341328)
        (xy 102.9726 73.787)
        (xy 102.74199 73.232672)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30035)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.225 80.177329)
        (xy 98.625 80.177329)
        (xy 99.080142 79.679011)
        (xy 98.7568 78.9676)
        (xy 98.2568 78.900274)
      )
    )
  )
  (zone (net 25) (net_name "/RXD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30085)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.7508 72.6846)
        (xy 124.0008 72.6846)
        (xy 124.308673 72.095704)
        (xy 123.8758 71.4836)
        (xy 123.442927 72.095704)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30172)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 73.7742 62.9646)
        (xy 73.7742 62.7146)
        (xy 73.326593 62.4396)
        (xy 72.9732 62.8396)
        (xy 73.326593 63.2396)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30151)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.758639 65.759247)
        (xy 94.139061 65.635641)
        (xy 94.153 65.279)
        (xy 93.852691 64.453049)
        (xy 93.625281 65.404007)
      )
    )
  )
  (zone (net 62) (net_name "Net-(U3-UD-)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30131)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 91.113 65.729)
        (xy 91.513 65.729)
        (xy 91.601582 65.336403)
        (xy 91.313 64.453)
        (xy 91.024418 65.336403)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30070)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 89.5916 73.1742)
        (xy 89.5916 72.7742)
        (xy 88.937271 72.49323)
        (xy 88.3656 72.9742)
        (xy 88.937271 73.45517)
      )
    )
  )
  (zone (net 25) (net_name "/RXD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30164)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 111.793631 92.370545)
        (xy 111.616854 92.193768)
        (xy 111.040884 92.2096)
        (xy 111.021693 92.685307)
        (xy 111.4224 92.913362)
      )
    )
  )
  (zone (net 13) (net_name "/eTX") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30080)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.965771 87.332177)
        (xy 132.565829 87.325443)
        (xy 132.332927 87.873496)
        (xy 132.765784 88.485599)
        (xy 133.198673 87.873496)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30037)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.243 82.41)
        (xy 89.843 82.41)
        (xy 89.697 83.5152)
        (xy 90.297 83.5162)
        (xy 90.721264 83.090936)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 91.060262 84.421105)
        (xy 91.343105 84.138262)
        (xy 90.851328 83.28559)
        (xy 90.296293 83.514493)
        (xy 90.06739 84.069528)
      )
    )
  )
  (zone (net 46) (net_name "/RX-") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30156)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.089 89.902)
        (xy 93.339 89.902)
        (xy 93.653838 89.396402)
        (xy 93.281 89.026)
        (xy 92.896224 89.378537)
      )
    )
  )
  (zone (net 74) (net_name "/DP") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30184)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 73.91 70.304)
        (xy 73.91 69.904)
        (xy 73.66 69.854)
        (xy 72.859 70.104)
        (xy 73.66 70.354)
      )
    )
  )
  (zone (net 29) (net_name "/RXD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30177)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 111.86741 91.112712)
        (xy 111.728515 90.904847)
        (xy 111.298937 90.700824)
        (xy 111.021569 91.161155)
        (xy 111.411115 91.492333)
      )
    )
  )
  (zone (net 22) (net_name "/nRST") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30125)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.9388 81.2154)
        (xy 104.1888 81.2154)
        (xy 104.394673 80.626504)
        (xy 103.9368 80.3144)
        (xy 103.537561 80.706087)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30106)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 109.015653 82.79941)
        (xy 108.73281 83.082253)
        (xy 108.9856 83.815807)
        (xy 109.386307 83.693707)
        (xy 109.546505 83.218)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30104)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.625 80.0248)
        (xy 98.225 80.0248)
        (xy 97.903841 80.575211)
        (xy 98.311 80.9508)
        (xy 98.743873 80.613696)
      )
    )
  )
  (zone (net 29) (net_name "/RXD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30083)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.0208 72.6846)
        (xy 125.2708 72.6846)
        (xy 125.578673 72.095704)
        (xy 125.1458 71.4836)
        (xy 124.712927 72.095704)
      )
    )
  )
  (zone (net 20) (net_name "/TX-") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30053)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 89.855912 85.7753)
        (xy 89.969408 85.552548)
        (xy 89.581328 84.68259)
        (xy 89.026109 84.911747)
        (xy 88.79739 85.466528)
      )
    )
  )
  (zone (net 76) (net_name "/IO33") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.615775 69.382788)
        (xy 126.215825 69.389026)
        (xy 125.982927 69.873496)
        (xy 126.415815 71.485599)
        (xy 126.848673 69.873496)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 91.553129 92.1988)
        (xy 91.553129 91.7988)
        (xy 90.3986 91.6274)
        (xy 90.3976 92.2274)
        (xy 90.62821 92.781728)
      )
    )
  )
  (zone (net 16) (net_name "/ACTLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30117)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.998758 95.166719)
        (xy 93.821981 94.989942)
        (xy 93.172522 95.2957)
        (xy 93.280793 95.771407)
        (xy 93.6815 95.925182)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30087)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 85.921381 78.267661)
        (xy 85.638538 77.984819)
        (xy 84.932647 78.42676)
        (xy 85.120073 78.852467)
        (xy 85.73328 78.809588)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.148401 81.497844)
        (xy 107.431244 81.215001)
        (xy 106.954928 80.33919)
        (xy 106.399893 80.568093)
        (xy 106.17099 81.123128)
      )
    )
  )
  (zone (net 29) (net_name "/RXD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30065)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.567269 77.651815)
        (xy 113.790021 77.765309)
        (xy 114.65661 77.414728)
        (xy 114.427453 76.859509)
        (xy 113.872672 76.63079)
      )
    )
  )
  (zone (net 46) (net_name "/RX-") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30060)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.335383 90.3752)
        (xy 90.335383 90.1252)
        (xy 89.705264 89.350936)
        (xy 89.28 89.7752)
        (xy 89.281 90.3752)
      )
    )
  )
  (zone (net 72) (net_name "/VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30110)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 74.861761 64.968902)
        (xy 75.256835 64.90633)
        (xy 75.566662 64.5842)
        (xy 75.076844 64.083213)
        (xy 74.577 64.5842)
      )
    )
  )
  (zone (net 32) (net_name "/TXEN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30072)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.948218 82.952969)
        (xy 103.198182 82.957209)
        (xy 103.627528 82.09381)
        (xy 103.073216 81.863201)
        (xy 102.518872 82.09381)
      )
    )
  )
  (zone (net 28) (net_name "/CRS_DV") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30084)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 122.4808 72.6846)
        (xy 122.7308 72.6846)
        (xy 123.038673 72.095704)
        (xy 122.6058 71.4836)
        (xy 122.172927 72.095704)
      )
    )
  )
  (zone (net 26) (net_name "/MDIO") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30137)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 110.437874 84.279162)
        (xy 110.584822 84.481414)
        (xy 111.176601 84.168)
        (xy 111.036409 83.692413)
        (xy 110.6356 83.558255)
      )
    )
  )
  (zone (net 28) (net_name "/CRS_DV") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30039)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 122.7308 72.4092)
        (xy 122.4808 72.4092)
        (xy 122.051472 73.37959)
        (xy 122.6058 73.6102)
        (xy 123.160128 73.37959)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30052)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.849943 72.423648)
        (xy 91.072171 72.756234)
        (xy 92.0242 72.9392)
        (xy 92.025031 72.338645)
        (xy 91.599936 71.914936)
      )
    )
  )
  (zone (net 43) (net_name "/PHY_CLK") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.7508 90.6846)
        (xy 124.0008 90.6846)
        (xy 124.308673 90.095704)
        (xy 123.8758 88.4836)
        (xy 123.442927 90.095704)
      )
    )
  )
  (zone (net 30) (net_name "Net-(U5-RXD1{slash}MODE1)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30188)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.701425 92.559619)
        (xy 108.697175 92.809581)
        (xy 109.020012 93.084608)
        (xy 109.373399 92.684617)
        (xy 109.020001 92.284608)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30055)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 112.272969 64.2132)
        (xy 112.272969 64.4632)
        (xy 113.411 64.6842)
        (xy 113.412 64.0842)
        (xy 112.986736 63.659936)
      )
    )
  )
  (zone (net 73) (net_name "/DM") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30122)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 77.938788 69.454547)
        (xy 77.661368 69.166385)
        (xy 77.210073 69.035648)
        (xy 76.80628 69.405893)
        (xy 77.220196 69.767987)
      )
    )
  )
  (zone (net 74) (net_name "/DP") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30101)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 77.857 70.8552)
        (xy 77.857 70.4552)
        (xy 77.210073 70.285648)
        (xy 76.806 70.6552)
        (xy 77.210073 71.024752)
      )
    )
  )
  (zone (net 34) (net_name "/MDC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30043)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 135.4308 90.8496)
        (xy 135.1808 90.8496)
        (xy 134.751472 91.81999)
        (xy 135.3058 92.0506)
        (xy 135.860128 91.81999)
      )
    )
  )
  (zone (net 35) (net_name "/XTAL") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30155)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 123.166408 94.792035)
        (xy 123.340592 94.971365)
        (xy 123.990908 94.7092)
        (xy 123.825717 94.308504)
        (xy 123.35 94.218865)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30038)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 91.67042 72.6916)
        (xy 91.67042 72.2916)
        (xy 90.422637 72.4792)
        (xy 90.5246 72.9792)
        (xy 91.2506 73.213643)
      )
    )
  )
  (zone (net 6) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30134)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 70.038071 77.205297)
        (xy 70.191149 76.835748)
        (xy 69.7035 76.543162)
        (xy 69.277577 76.920118)
        (xy 69.688199 77.39742)
      )
    )
  )
  (zone (net 22) (net_name "/nRST") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30089)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.239855 79.644278)
        (xy 103.063078 79.821055)
        (xy 103.4618 80.523427)
        (xy 103.937507 80.316107)
        (xy 104.085311 79.8654)
      )
    )
  )
  (zone (net 79) (net_name "Net-(J2-Pad10)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30058)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 70.971033 87.276138)
        (xy 71.151543 87.103177)
        (xy 71.357 86.0552)
        (xy 70.756309 86.054478)
        (xy 70.332736 86.479464)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30107)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.55512 78.11834)
        (xy 92.95512 78.11834)
        (xy 93.171389 77.545802)
        (xy 92.75054 77.20484)
        (xy 92.329691 77.545802)
      )
    )
  )
  (zone (net 33) (net_name "/TXD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30051)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.761704 82.911498)
        (xy 100.984456 82.798002)
        (xy 100.630328 81.76159)
        (xy 100.075547 81.990309)
        (xy 99.84639 82.545528)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 82.35093 65.059691)
        (xy 82.474537 64.67927)
        (xy 81.940199 63.796932)
        (xy 81.364249 64.083891)
        (xy 81.339975 64.784199)
      )
    )
  )
  (zone (net 9) (net_name "RTS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30193)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.333159 70.687907)
        (xy 103.428831 70.918875)
        (xy 104.281195 70.9136)
        (xy 104.274923 70.713218)
        (xy 103.524 70.58795)
      )
    )
  )
  (zone (net 28) (net_name "/CRS_DV") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30066)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.297212 75.78141)
        (xy 113.473988 75.958186)
        (xy 114.3762 75.9364)
        (xy 114.376907 75.335693)
        (xy 113.951936 74.912136)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30027)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.66746 71.02487)
        (xy 101.563936 70.6385)
        (xy 100.68661 70.311672)
        (xy 100.456035 70.866258)
        (xy 100.68661 71.420328)
      )
    )
  )
  (zone (net 21) (net_name "/RX+") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30059)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.197041 90.8752)
        (xy 90.197041 90.6252)
        (xy 89.154 90.6622)
        (xy 89.153 91.2622)
        (xy 89.578264 91.686464)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30118)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 70.1285 78.958)
        (xy 70.1285 78.558)
        (xy 69.7035 78.213825)
        (xy 69.2775 78.5455)
        (xy 69.653501 79.077439)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30064)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.928561 64.0822)
        (xy 100.928561 63.8322)
        (xy 99.822 63.662)
        (xy 99.821 64.262)
        (xy 100.246264 64.686264)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30133)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.2584 80.1656)
        (xy 101.2584 80.5656)
        (xy 101.781863 80.749376)
        (xy 102.1344 80.3646)
        (xy 101.781863 79.979824)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_track$") (hatch edge 0.5)
    (priority 30199)
    (attr (teardrop (type track_end)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.997627 94.293817)
        (xy 99.759864 94.371072)
        (xy 100.061579 94.680221)
        (xy 100.203309 94.539751)
        (xy 100.279537 94.354024)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30071)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.968405 89.755552)
        (xy 108.141923 89.575576)
        (xy 107.767728 88.72119)
        (xy 107.212681 88.950106)
        (xy 106.98379 89.505128)
      )
    )
  )
  (zone (net 16) (net_name "/ACTLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30049)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.2624 91.967857)
        (xy 102.0124 91.967857)
        (xy 101.452072 92.91219)
        (xy 102.0064 93.1428)
        (xy 102.560728 92.91219)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30191)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.066169 75.675914)
        (xy 98.866145 76.022308)
        (xy 99.2236 76.184619)
        (xy 99.754465 75.8805)
        (xy 99.2236 75.555)
      )
    )
  )
  (zone (net 76) (net_name "/IO33") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30025)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.150137 69.002296)
        (xy 126.530559 68.878691)
        (xy 126.161328 67.77559)
        (xy 125.606691 68.004249)
        (xy 125.37739 68.559528)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30130)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.354817 81.459822)
        (xy 89.962503 81.381796)
        (xy 89.724127 81.909096)
        (xy 90.156805 82.24618)
        (xy 90.589873 81.909096)
      )
    )
  )
  (zone (net 5) (net_name "Net-(D1-K)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30082)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 78.577 64.2842)
        (xy 78.577 63.8842)
        (xy 78.077 63.5842)
        (xy 77.576 64.0842)
        (xy 78.077 64.5842)
      )
    )
  )
  (zone (net 79) (net_name "Net-(J2-Pad10)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30176)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.773618 94.188481)
        (xy 90.912514 94.396344)
        (xy 91.33232 94.62818)
        (xy 91.631831 94.182645)
        (xy 91.246062 93.832475)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30159)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.058826 76.573838)
        (xy 98.345774 76.295162)
        (xy 98.0836 75.905422)
        (xy 97.552904 75.879283)
        (xy 97.433749 76.205)
      )
    )
  )
  (zone (net 45) (net_name "Net-(J2-Pad12)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30050)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 73.574024 92.964952)
        (xy 73.397247 92.788175)
        (xy 72.52739 93.250872)
        (xy 72.756293 93.805907)
        (xy 73.311328 94.03481)
      )
    )
  )
  (zone (net 42) (net_name "/PHY_POWER") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30141)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.6086 73.924)
        (xy 100.6086 73.524)
        (xy 99.705042 73.655)
        (xy 99.7526 73.98)
        (xy 100.2836 74.160419)
      )
    )
  )
  (zone (net 39) (net_name "Net-(U5-CRS_DV{slash}MODE2)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30174)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.540979 85.991568)
        (xy 108.665985 86.208068)
        (xy 109.1602 86.2762)
        (xy 109.361066 85.8007)
        (xy 108.9602 85.528924)
      )
    )
  )
  (zone (net 11) (net_name "/IO0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30120)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 119.1658 88.3596)
        (xy 119.1658 88.6096)
        (xy 119.6158 88.9346)
        (xy 120.0668 88.4846)
        (xy 119.6158 88.0346)
      )
    )
  )
  (zone (net 7) (net_name "Net-(D3-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30111)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 70.554967 63.326031)
        (xy 70.832941 63.613659)
        (xy 71.414902 63.3146)
        (xy 71.324919 62.838906)
        (xy 70.9242 62.673934)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30180)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 82.526531 75.179679)
        (xy 82.761643 75.503286)
        (xy 83.306452 75.1636)
        (xy 83.178009 74.838013)
        (xy 82.6472 74.891842)
      )
    )
  )
  (zone (net 8) (net_name "/EN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 118.845949 64.266094)
        (xy 118.563106 63.983251)
        (xy 117.62639 64.418872)
        (xy 117.855293 64.973907)
        (xy 118.410328 65.20281)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30068)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 81.2858 75.76)
        (xy 81.2858 75.36)
        (xy 80.631471 75.07903)
        (xy 80.0598 75.56)
        (xy 80.631471 76.04097)
      )
    )
  )
  (zone (net 17) (net_name "/eRX") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30026)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 130.778407 66.774414)
        (xy 130.397983 66.898014)
        (xy 130.763672 67.99681)
        (xy 131.318309 67.768151)
        (xy 131.54761 67.212872)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30128)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 110.444284 88.487507)
        (xy 110.267507 88.664284)
        (xy 110.6102 89.395885)
        (xy 111.010907 89.230907)
        (xy 111.100885 88.7552)
      )
    )
  )
  (zone (net 19) (net_name "/TX+") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30178)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 93.285355 86.563603)
        (xy 93.068847 86.688599)
        (xy 92.896224 87.100663)
        (xy 93.281499 87.453066)
        (xy 93.622421 87.035779)
      )
    )
  )
  (zone (net 3) (net_name "+5V") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30136)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 84.192 66.729)
        (xy 84.192 67.129)
        (xy 84.517 67.254)
        (xy 85.298 66.929)
        (xy 84.517 66.604)
      )
    )
  )
  (zone (net 6) (net_name "Net-(D2-A)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30162)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 70.65423 77.203988)
        (xy 70.371388 77.48683)
        (xy 70.847407 77.899449)
        (xy 71.247707 77.623107)
        (xy 71.047 77.1474)
      )
    )
  )
  (zone (net 72) (net_name "/VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30100)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 75.757 67.9552)
        (xy 75.757 68.3552)
        (xy 76.403927 68.524752)
        (xy 76.808 68.1552)
        (xy 76.403927 67.785648)
      )
    )
  )
  (zone (net 38) (net_name "/VDDCR") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30098)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.0758 94.3512)
        (xy 107.0758 94.7512)
        (xy 107.664696 94.984073)
        (xy 108.0018 94.5512)
        (xy 107.664696 94.118327)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30093)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.55572 79.79708)
        (xy 92.95572 79.79708)
        (xy 93.187993 79.208184)
        (xy 92.75512 78.87108)
        (xy 92.322247 79.208184)
      )
    )
  )
  (zone (net 26) (net_name "/MDIO") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30166)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 111.314989 83.604613)
        (xy 111.138213 83.781389)
        (xy 111.1854 84.2518)
        (xy 111.786107 84.252507)
        (xy 111.7854 83.6518)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30077)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.228627 88.1868)
        (xy 106.228627 88.4368)
        (xy 106.659072 89.18041)
        (xy 107.2144 88.9508)
        (xy 107.2134 88.3508)
      )
    )
  )
  (zone (net 17) (net_name "/eRX") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30102)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 96.630459 65.7983)
        (xy 96.9133 65.515459)
        (xy 96.693 64.409348)
        (xy 96.392293 64.453293)
        (xy 96.385446 65.429)
      )
    )
  )
  (zone (net 72) (net_name "/VBUS") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30165)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 76.947973 67.312396)
        (xy 76.578423 67.465468)
        (xy 76.38607 67.797579)
        (xy 76.807382 68.156123)
        (xy 77.186437 67.780946)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30073)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.956778 77.770255)
        (xy 98.556822 77.776107)
        (xy 98.27583 78.397929)
        (xy 98.756814 78.969599)
        (xy 99.23777 78.397929)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30030)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.9788 65.1542)
        (xy 113.9788 65.5542)
        (xy 115.062 65.5732)
        (xy 115.063 64.9732)
        (xy 114.637736 64.548936)
      )
    )
  )
  (zone (net 13) (net_name "/eTX") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30123)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.151863 67.1036)
        (xy 104.151863 66.7036)
        (xy 103.421468 66.835)
        (xy 103.377 67.31)
        (xy 103.778 67.551361)
      )
    )
  )
  (zone (net 38) (net_name "/VDDCR") (layer "F.Cu") (name "$teardrop_track$") (hatch edge 0.5)
    (priority 30197)
    (attr (teardrop (type track_end)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.4748 94.1512)
        (xy 106.2248 94.1512)
        (xy 106.1498 94.5512)
        (xy 106.3498 94.5522)
        (xy 106.5498 94.5512)
      )
    )
  )
  (zone (net 15) (net_name "/LINKLED") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30076)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.754846 91.041285)
        (xy 101.50965 90.992512)
        (xy 100.76079 91.444472)
        (xy 100.990205 91.99978)
        (xy 101.5904 91.9988)
      )
    )
  )
  (zone (net 13) (net_name "/eTX") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30056)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.680997 86.842179)
        (xy 133.050549 86.995247)
        (xy 133.75741 86.634928)
        (xy 133.528182 86.079677)
        (xy 132.973472 85.85099)
      )
    )
  )
  (zone (net 33) (net_name "/TXD1") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30036)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.614209 90.578132)
        (xy 133.830714 90.703133)
        (xy 134.23628 90.2346)
        (xy 134.0363 88.483734)
        (xy 133.5858 90.0096)
      )
    )
  )
  (zone (net 34) (net_name "/MDC") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30074)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.953757 83.361098)
        (xy 105.201617 83.393724)
        (xy 105.634128 82.55101)
        (xy 105.07993 82.320409)
        (xy 104.525472 82.55101)
      )
    )
  )
  (zone (net 61) (net_name "Net-(U3-UD+)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30139)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 86.402 68.0688)
        (xy 86.402 67.6688)
        (xy 86.077 67.554)
        (xy 85.296 67.879)
        (xy 86.077 68.19681)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.729546 69.906503)
        (xy 99.446703 70.189346)
        (xy 99.902672 71.09561)
        (xy 100.457707 70.866707)
        (xy 100.68661 70.311672)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30154)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.497151 83.672465)
        (xy 108.719387 84.005046)
        (xy 109.107695 84.151862)
        (xy 109.386431 83.692445)
        (xy 108.997419 83.358578)
      )
    )
  )
  (zone (net 8) (net_name "/EN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30149)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 111.608872 69.294302)
        (xy 111.321444 69.016122)
        (xy 110.957504 69.563443)
        (xy 111.264505 70.003118)
        (xy 111.6652 69.7274)
      )
    )
  )
  (zone (net 40) (net_name "Net-(U5-RXD0{slash}MODE0)") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30171)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 108.5724 91.0356)
        (xy 108.5724 91.2856)
        (xy 109.020007 91.5606)
        (xy 109.3734 91.1606)
        (xy 109.020007 90.7606)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30163)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.025921 84.037119)
        (xy 91.743076 83.75428)
        (xy 91.355084 84.2491)
        (xy 91.630293 84.709707)
        (xy 92.031 84.434)
      )
    )
  )
  (zone (net 28) (net_name "/CRS_DV") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30153)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 111.1352 86.5264)
        (xy 110.8852 86.5264)
        (xy 110.613224 87.049863)
        (xy 110.998 87.4024)
        (xy 111.382776 87.049863)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30024)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 91.593686 97.6344)
        (xy 91.593686 97.2344)
        (xy 90.65361 96.727672)
        (xy 90.423 97.282)
        (xy 90.65361 97.836328)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30079)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.047383 70.790026)
        (xy 100.330226 70.507183)
        (xy 99.916 69.798701)
        (xy 99.440293 69.976293)
        (xy 99.268656 70.427)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30145)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.7152 70.2532)
        (xy 113.7152 69.8532)
        (xy 113.282671 69.624965)
        (xy 112.9142 70.0024)
        (xy 113.248284 70.424391)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 113.735 69.8532)
        (xy 113.735 70.2532)
        (xy 114.70539 70.607528)
        (xy 114.936 70.0532)
        (xy 114.70539 69.498872)
      )
    )
  )
  (zone (net 32) (net_name "/TXEN") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 130.1008 90.6846)
        (xy 130.3508 90.6846)
        (xy 130.658673 90.095704)
        (xy 130.2258 88.4836)
        (xy 129.792927 90.095704)
      )
    )
  )
  (zone (net 31) (net_name "/TXD0") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30062)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.8108 93.115573)
        (xy 127.5608 93.115573)
        (xy 126.829736 93.758936)
        (xy 127.254 94.1842)
        (xy 127.854 94.1832)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30189)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.263 70.177)
        (xy 98.263 69.777)
        (xy 97.963 69.276478)
        (xy 97.662 69.404)
        (xy 97.963 70.105475)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "F.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30095)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.516 69.777)
        (xy 98.516 70.177)
        (xy 99.104896 70.409873)
        (xy 99.442 69.977)
        (xy 99.104896 69.544127)
      )
    )
  )
  (zone (net 0) (net_name "") (layers "F&B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.696693 81.0052)
        (xy 89.357 81.0052)
        (xy 96.2406 86.487)
        (xy 100.92944 86.8172)
        (xy 100.98024 90.45194)
        (xy 96.012 90.54846)
        (xy 91.157 95.0052)
        (xy 74.79961 95.044492)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.82))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.82) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 139.827 100.0252)
        (xy 88.9 100.0252)
        (xy 88.9 78.105)
        (xy 74.295 78.105)
        (xy 74.295 59.3852)
        (xy 139.827 59.3852)
      )
    )
  )
  (zone (net 37) (net_name "GND1") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.6))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.6) (thermal_bridge_width 0.6) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 73.66 78.74)
        (xy 88.265 78.74)
        (xy 88.265 100.0252)
        (xy 66.167 100.0252)
        (xy 66.167 60.6552)
        (xy 73.66 60.6552)
      )
    )
  )
  (zone (net 17) (net_name "/eRX") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30012)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 132.025106 68.757149)
        (xy 132.307949 68.474306)
        (xy 131.872328 67.53759)
        (xy 131.317293 67.766493)
        (xy 131.08839 68.321528)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30015)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.224 93.422348)
        (xy 90.624 93.422348)
        (xy 90.952928 92.45701)
        (xy 90.3986 92.2264)
        (xy 89.844272 92.45701)
      )
    )
  )
  (zone (net 46) (net_name "/RX-") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30054)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 88.219829 90.103057)
        (xy 88.219829 90.353057)
        (xy 89.281 90.3752)
        (xy 89.282 89.7752)
        (xy 88.856736 89.350936)
      )
    )
  )
  (zone (net 16) (net_name "/ACTLED") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30032)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.228 92.9112)
        (xy 98.228 92.6612)
        (xy 97.25761 92.231872)
        (xy 97.027 92.7862)
        (xy 97.25761 93.340528)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30016)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.624 91.032452)
        (xy 90.224 91.032452)
        (xy 89.844272 91.99779)
        (xy 90.3986 92.2284)
        (xy 90.952928 91.99779)
      )
    )
  )
  (zone (net 29) (net_name "/RXD0") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30057)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 124.007937 73.942522)
        (xy 124.085192 74.180284)
        (xy 124.91619 74.569928)
        (xy 125.146751 74.015291)
        (xy 124.91619 73.461272)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30046)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.30115 86.02972)
        (xy 107.647558 85.82972)
        (xy 107.285128 84.91119)
        (xy 106.7303 85.139934)
        (xy 106.50119 85.695128)
      )
    )
  )
  (zone (net 42) (net_name "/PHY_POWER") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30024)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 103.319196 72.706223)
        (xy 102.962797 72.524622)
        (xy 102.417272 73.55739)
        (xy 102.971146 73.787891)
        (xy 103.525928 73.55739)
      )
    )
  )
  (zone (net 20) (net_name "/TX-") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30066)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 88.522848 84.231272)
        (xy 88.346072 84.408048)
        (xy 88.427 84.9122)
        (xy 89.027707 84.912907)
        (xy 89.027 84.3122)
      )
    )
  )
  (zone (net 21) (net_name "/RX+") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30042)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.978466 91.2602)
        (xy 87.978466 91.5102)
        (xy 88.92439 91.816528)
        (xy 89.155 91.2622)
        (xy 88.92439 90.707872)
      )
    )
  )
  (zone (net 8) (net_name "/EN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30008)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 117.656 66.1732)
        (xy 118.056 66.1732)
        (xy 118.410328 65.20281)
        (xy 117.856 64.9722)
        (xy 117.301672 65.20281)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30036)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.622 64.137)
        (xy 98.622 64.387)
        (xy 99.59239 64.816328)
        (xy 99.823 64.262)
        (xy 99.59239 63.707672)
      )
    )
  )
  (zone (net 34) (net_name "/MDC") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30056)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.434766 92.689642)
        (xy 134.548258 92.912394)
        (xy 135.53541 92.603928)
        (xy 135.306691 92.049147)
        (xy 134.751472 91.81999)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30013)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 101.809201 80.5646)
        (xy 101.809201 80.1646)
        (xy 100.83901 79.811272)
        (xy 100.6084 80.3656)
        (xy 100.83901 80.919928)
      )
    )
  )
  (zone (net 26) (net_name "/MDIO") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30037)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 124.403 93.91596)
        (xy 124.403 94.16596)
        (xy 125.37339 94.595288)
        (xy 125.604 94.04096)
        (xy 125.37339 93.486632)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30017)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.210705 80.318)
        (xy 105.210705 80.718)
        (xy 106.17099 81.123128)
        (xy 106.4016 80.5688)
        (xy 106.17099 80.014472)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30055)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 116.2538 68.700427)
        (xy 116.0038 68.700427)
        (xy 115.859 69.7992)
        (xy 116.459 69.8002)
        (xy 116.883264 69.374936)
      )
    )
  )
  (zone (net 32) (net_name "/TXEN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30053)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 129.173747 92.4072)
        (xy 129.173747 92.6572)
        (xy 130.2258 92.6496)
        (xy 130.2268 92.0496)
        (xy 129.801536 91.625336)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30023)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.224 89.561686)
        (xy 90.624 89.561686)
        (xy 90.825928 88.62161)
        (xy 90.2716 88.391)
        (xy 89.717272 88.62161)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30018)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 105.229 67.288505)
        (xy 104.829 67.288505)
        (xy 104.525472 68.24879)
        (xy 105.0798 68.4794)
        (xy 105.634128 68.24879)
      )
    )
  )
  (zone (net 76) (net_name "/IO33") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30014)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.782 66.810173)
        (xy 125.382 66.810173)
        (xy 125.052672 67.77559)
        (xy 125.607 68.0062)
        (xy 126.161328 67.77559)
      )
    )
  )
  (zone (net 25) (net_name "/RXD1") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30063)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.387595 78.294407)
        (xy 115.625357 78.217153)
        (xy 114.70741 77.779272)
        (xy 114.477491 78.332649)
        (xy 114.902064 78.757864)
      )
    )
  )
  (zone (net 79) (net_name "Net-(J2-Pad10)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30002)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 70.632 85.975)
        (xy 70.882 85.975)
        (xy 71.672347 84.875573)
        (xy 70.782 84.174)
        (xy 69.872353 84.862678)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30022)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.262 68.878462)
        (xy 114.862 68.878462)
        (xy 114.380672 69.82359)
        (xy 114.935 70.0542)
        (xy 115.489328 69.82359)
      )
    )
  )
  (zone (net 41) (net_name "/+3V3_LAN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30031)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 107.9722 87.922107)
        (xy 107.5722 87.922107)
        (xy 106.789136 88.526536)
        (xy 107.2134 88.9518)
        (xy 107.8134 88.9508)
      )
    )
  )
  (zone (net 42) (net_name "/PHY_POWER") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30028)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.079834 69.329122)
        (xy 106.362677 69.611965)
        (xy 107.231264 68.902664)
        (xy 106.807707 68.477693)
        (xy 106.207 68.4784)
      )
    )
  )
  (zone (net 34) (net_name "/MDC") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30047)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 106.244434 82.6242)
        (xy 106.244434 82.3742)
        (xy 105.30941 81.767072)
        (xy 105.0788 82.3214)
        (xy 105.30941 82.875728)
      )
    )
  )
  (zone (net 26) (net_name "/MDIO") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30041)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 112.515087 85.209064)
        (xy 112.691864 85.032287)
        (xy 112.339728 84.02219)
        (xy 111.784693 84.251093)
        (xy 111.55579 84.806128)
      )
    )
  )
  (zone (net 15) (net_name "/LINKLED") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30060)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.976291 91.266162)
        (xy 99.971464 91.516114)
        (xy 100.436072 92.22841)
        (xy 100.991399 91.998819)
        (xy 100.9904 91.3988)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30050)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.549031 63.9552)
        (xy 114.549031 63.7052)
        (xy 113.411 63.4842)
        (xy 113.41 64.0842)
        (xy 113.835264 64.508464)
      )
    )
  )
  (zone (net 29) (net_name "/RXD0") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30038)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.363916 76.100261)
        (xy 115.187139 75.923484)
        (xy 114.19739 76.306072)
        (xy 114.426293 76.861107)
        (xy 114.981328 77.09001)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30019)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.1732 84.700043)
        (xy 90.5732 84.700043)
        (xy 90.851328 83.74481)
        (xy 90.297 83.5142)
        (xy 89.742672 83.74481)
      )
    )
  )
  (zone (net 76) (net_name "/IO33") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30064)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 125.382 67.5552)
        (xy 125.782 67.5552)
        (xy 125.951552 66.908273)
        (xy 125.582 66.5042)
        (xy 125.212448 66.908273)
      )
    )
  )
  (zone (net 32) (net_name "/TXEN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30049)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.068381 81.320199)
        (xy 104.019613 81.075003)
        (xy 102.84359 81.309872)
        (xy 103.07222 81.864395)
        (xy 103.627528 82.09381)
      )
    )
  )
  (zone (net 25) (net_name "/RXD1") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30039)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 122.938884 76.172739)
        (xy 123.115661 76.349516)
        (xy 124.10541 75.966928)
        (xy 123.876507 75.411893)
        (xy 123.321472 75.18299)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30025)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 99.318969 70.92)
        (xy 99.318969 71.32)
        (xy 100.457 71.466)
        (xy 100.458 70.866)
        (xy 100.032736 70.441736)
      )
    )
  )
  (zone (net 19) (net_name "/TX+") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30034)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 86.43 86.1842)
        (xy 86.43 86.4342)
        (xy 87.40039 86.863528)
        (xy 87.631 86.3092)
        (xy 87.40039 85.754872)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30009)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.624 96.082)
        (xy 90.224 96.082)
        (xy 89.869672 97.05239)
        (xy 90.424 97.283)
        (xy 90.978328 97.05239)
      )
    )
  )
  (zone (net 75) (net_name "/IO32") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30027)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.032 66.831201)
        (xy 126.632 66.831201)
        (xy 126.507 67.9552)
        (xy 127.107 67.9562)
        (xy 127.531264 67.530936)
      )
    )
  )
  (zone (net 46) (net_name "/RX-") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30005)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 85.074886 89.026832)
        (xy 85.068558 88.776914)
        (xy 84.05167 89.62967)
        (xy 84.581001 90.160025)
        (xy 85.671611 89.427824)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30010)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 104.829 66.224)
        (xy 105.229 66.224)
        (xy 105.583328 65.25361)
        (xy 105.029 65.023)
        (xy 104.474672 65.25361)
      )
    )
  )
  (zone (net 20) (net_name "/TX-") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30004)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 85.0404 83.741576)
        (xy 84.863624 83.5648)
        (xy 84.05167 84.54967)
        (xy 84.581293 85.080707)
        (xy 85.551126 84.33)
      )
    )
  )
  (zone (net 17) (net_name "/eRX") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30011)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.4898 82.2136)
        (xy 134.0898 82.2136)
        (xy 133.735472 83.18399)
        (xy 134.2898 83.4146)
        (xy 134.844128 83.18399)
      )
    )
  )
  (zone (net 31) (net_name "/TXD0") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30043)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.293935 94.816577)
        (xy 126.371186 95.054341)
        (xy 127.48361 94.737528)
        (xy 127.254951 94.182891)
        (xy 126.699672 93.95359)
      )
    )
  )
  (zone (net 13) (net_name "/eTX") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30030)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 133.3468 84.9974)
        (xy 132.9468 84.9974)
        (xy 132.9278 86.0806)
        (xy 133.5278 86.0816)
        (xy 133.952064 85.656336)
      )
    )
  )
  (zone (net 15) (net_name "/LINKLED") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30035)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 98.228 91.5142)
        (xy 98.228 91.2642)
        (xy 97.25761 90.834872)
        (xy 97.027 91.3892)
        (xy 97.25761 91.943528)
      )
    )
  )
  (zone (net 16) (net_name "/ACTLED") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30058)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.940507 93.019282)
        (xy 100.875815 93.260766)
        (xy 101.77679 93.696128)
        (xy 102.007365 93.142058)
        (xy 101.77679 92.587472)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30007)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 114.862 66.1732)
        (xy 115.262 66.1732)
        (xy 115.616328 65.20281)
        (xy 115.062 64.9722)
        (xy 114.507672 65.20281)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30062)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 124.774918 65.670123)
        (xy 124.492077 65.387281)
        (xy 124.085014 65.948397)
        (xy 124.331293 66.505907)
        (xy 124.732 66.56406)
      )
    )
  )
  (zone (net 31) (net_name "/TXD0") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30051)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 102.262297 82.703252)
        (xy 102.436303 82.523748)
        (xy 102.154328 81.50759)
        (xy 101.599282 81.736504)
        (xy 101.37039 82.291528)
      )
    )
  )
  (zone (net 33) (net_name "/TXD1") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30052)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 100.975541 82.686518)
        (xy 101.152318 82.509741)
        (xy 100.500264 81.566936)
        (xy 100.075293 81.990493)
        (xy 100.076 82.5912)
      )
    )
  )
  (zone (net 28) (net_name "/CRS_DV") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30061)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 121.594218 74.08006)
        (xy 121.599167 74.33001)
        (xy 122.6058 74.2092)
        (xy 122.606799 73.609181)
        (xy 122.051472 73.37959)
      )
    )
  )
  (zone (net 75) (net_name "/IO32") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30065)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 126.639977 67.599172)
        (xy 127.026339 67.49562)
        (xy 127.216776 67.031737)
        (xy 126.831742 66.504235)
        (xy 126.447224 67.031737)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30001)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 87.078937 87.8046)
        (xy 87.078937 87.4046)
        (xy 85.869013 86.92709)
        (xy 84.581 87.62)
        (xy 85.869013 88.31291)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30000)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 72.474569 82.705612)
        (xy 72.757412 82.422769)
        (xy 71.896703 81.190628)
        (xy 70.781293 81.634293)
        (xy 70.567633 82.535)
      )
    )
  )
  (zone (net 19) (net_name "/TX+") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30003)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 82.649741 85.188718)
        (xy 82.826518 85.011941)
        (xy 82.792 83.629805)
        (xy 82.041293 83.819293)
        (xy 81.595869 84.57)
      )
    )
  )
  (zone (net 8) (net_name "/EN") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30006)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 118.056 67.5832)
        (xy 117.656 67.5832)
        (xy 117.301672 68.55359)
        (xy 117.856 68.7842)
        (xy 118.410328 68.55359)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30026)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 89.204089 83.233001)
        (xy 89.08048 83.613422)
        (xy 90.06739 84.069528)
        (xy 90.297951 83.515509)
        (xy 90.06739 82.960872)
      )
    )
  )
  (zone (net 33) (net_name "/TXD1") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30044)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 127.859283 95.46536)
        (xy 127.859283 95.71536)
        (xy 128.80239 96.007528)
        (xy 129.033 95.4532)
        (xy 128.80239 94.898872)
      )
    )
  )
  (zone (net 13) (net_name "/eTX") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30029)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 130.131236 68.895279)
        (xy 130.414079 68.612436)
        (xy 130.307 67.7552)
        (xy 129.706293 67.754493)
        (xy 129.282736 68.179464)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30021)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 134.003643 67.71962)
        (xy 133.997999 68.11958)
        (xy 134.94919 68.473928)
        (xy 135.179799 67.919614)
        (xy 134.94919 67.365272)
      )
    )
  )
  (zone (net 79) (net_name "Net-(J2-Pad10)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30033)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 70.882 84.8552)
        (xy 70.632 84.8552)
        (xy 70.202672 85.82559)
        (xy 70.757 86.0562)
        (xy 71.311328 85.82559)
      )
    )
  )
  (zone (net 45) (net_name "Net-(J2-Pad12)") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30045)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 71.939975 94.645448)
        (xy 72.116752 94.822225)
        (xy 72.98661 94.359528)
        (xy 72.757707 93.804493)
        (xy 72.202672 93.57559)
      )
    )
  )
  (zone (net 28) (net_name "/CRS_DV") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30048)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 115.276406 74.629719)
        (xy 115.151408 74.413213)
        (xy 114.14659 74.782072)
        (xy 114.375334 75.336899)
        (xy 114.930528 75.56601)
      )
    )
  )
  (zone (net 2) (net_name "+3V3") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30059)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 92.853274 71.793248)
        (xy 92.60977 71.475908)
        (xy 91.79459 71.784872)
        (xy 92.023407 72.339808)
        (xy 92.578528 72.56881)
      )
    )
  )
  (zone (net 24) (net_name "/SLED") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30040)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 84.572974 63.625)
        (xy 84.572974 63.375)
        (xy 83.60511 62.958372)
        (xy 83.3745 63.5127)
        (xy 83.60511 64.067028)
      )
    )
  )
  (zone (net 4) (net_name "+3.3VA") (layer "B.Cu") (name "$teardrop_padvia$") (hatch edge 0.5)
    (priority 30020)
    (attr (teardrop (type padvia)))
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 90.5732 87.212209)
        (xy 90.1732 87.212209)
        (xy 89.717272 88.16239)
        (xy 90.2716 88.393)
        (xy 90.825928 88.16239)
      )
    )
  )
)
