(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 70)
    (no_connects 3)
    (area 42.73 109.515 378.480476 131.885)
    (thickness 1.6)
    (drawings 5)
    (tracks 343)
    (zones 0)
    (modules 26)
    (nets 25)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(CN1-Pad2)")
  (net 3 "Net-(CN1-Pad3)")
  (net 4 "Net-(CN2-Pad2)")
  (net 5 "Net-(CN2-Pad3)")
  (net 6 "Net-(CN6-Pad2)")
  (net 7 "Net-(CN6-Pad3)")
  (net 8 "Net-(CN10-Pad2)")
  (net 9 "Net-(CN10-Pad3)")
  (net 10 "Net-(CN11-Pad2)")
  (net 11 "Net-(CN11-Pad3)")
  (net 12 "Net-(CN15-Pad2)")
  (net 13 "Net-(CN15-Pad3)")
  (net 14 "Net-(CN19-Pad2)")
  (net 15 "Net-(CN19-Pad3)")
  (net 16 GND)
  (net 17 "Net-(CN4-Pad2)")
  (net 18 "Net-(CN4-Pad3)")
  (net 19 "Net-(CN8-Pad2)")
  (net 20 "Net-(CN8-Pad3)")
  (net 21 "Net-(CN13-Pad2)")
  (net 22 "Net-(CN13-Pad3)")
  (net 23 "Net-(CN17-Pad2)")
  (net 24 "Net-(CN17-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(CN1-Pad2)")
    (add_net "Net-(CN1-Pad3)")
    (add_net "Net-(CN10-Pad2)")
    (add_net "Net-(CN10-Pad3)")
    (add_net "Net-(CN11-Pad2)")
    (add_net "Net-(CN11-Pad3)")
    (add_net "Net-(CN13-Pad2)")
    (add_net "Net-(CN13-Pad3)")
    (add_net "Net-(CN15-Pad2)")
    (add_net "Net-(CN15-Pad3)")
    (add_net "Net-(CN17-Pad2)")
    (add_net "Net-(CN17-Pad3)")
    (add_net "Net-(CN19-Pad2)")
    (add_net "Net-(CN19-Pad3)")
    (add_net "Net-(CN2-Pad2)")
    (add_net "Net-(CN2-Pad3)")
    (add_net "Net-(CN4-Pad2)")
    (add_net "Net-(CN4-Pad3)")
    (add_net "Net-(CN6-Pad2)")
    (add_net "Net-(CN6-Pad3)")
    (add_net "Net-(CN8-Pad2)")
    (add_net "Net-(CN8-Pad3)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 2)
    (via_dia 1.7)
    (via_drill 0.8)
    (uvia_dia 1.7)
    (uvia_drill 1)
    (add_net +5V)
    (add_net GND)
  )
  (module plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 67.18 127 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN1 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(CN1-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(CN1-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 0)
    (at 84.1 121.5 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.5 -2.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 0)
    (at 156.4 121.4 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.5 -2.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 0)
    (at 223.1 121.4 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.5 -2.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2.5_P5 (layer F.Cu) (tedit 0)
    (at 289.7 121.5 180)
    (descr "Film Capacitor Length 7mm x Width 2.5mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C4 (at 2.5 -2.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 2.5 2.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at 5 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 57FCFE2C)
    (at 89 121.5 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(CN1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module plan44:plan44-STELVIO-2P-508 (layer F.Cu) (tedit 57FE31A0)
    (at 43.18 121.92)
    (attr virtual)
    (fp_text reference J1 (at 19.05 4.318 90) (layer F.SilkS))
    (fp_text value STELVIO-2P-508 (at 12.7 -11.43) (layer F.Fab))
    (pad 1 thru_hole rect (at 15.24 0) (size 2.54 2.54) (drill 1.19888) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 16 GND))
    (pad 2 thru_hole circle (at 10.16 0) (size 2.54 2.54) (drill 1.19888) (layers *.Cu F.Paste F.SilkS F.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 133.68 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN3 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CN2-Pad3)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CN2-Pad2)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
  )
  (module plan44:plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 100.48 126.9 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN2 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(CN2-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CN2-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 374.4 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN20 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(CN19-Pad3)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(CN19-Pad2)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 341.1 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN19 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(CN19-Pad2)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(CN19-Pad3)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 307.8 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN18 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(CN17-Pad3)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(CN17-Pad2)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 274.5 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN17 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(CN17-Pad2)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(CN17-Pad3)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 241.2 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN16 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(CN15-Pad3)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(CN15-Pad2)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 207.9 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN15 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(CN15-Pad2)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(CN15-Pad3)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 174.6 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN14 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(CN13-Pad3)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(CN13-Pad2)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 141.3 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN13 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(CN13-Pad2)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(CN13-Pad3)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 108.1 126.9 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN12 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(CN11-Pad3)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(CN11-Pad2)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
  )
  (module plan44:plan44-WS2813-CONN (layer B.Cu) (tedit 57FE3506)
    (at 74.8 127 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN11 (at 3.81 -3.81 360) (layer B.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 -3.81 360) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 -2.54 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(CN11-Pad2)"))
    (pad 3 smd oval (at 0 -5.08 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(CN11-Pad3)"))
    (pad 4 smd oval (at 0 -7.62 90) (size 3.81 1.9304) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 366.78 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN10 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(CN10-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(CN10-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 333.48 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN9 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CN8-Pad3)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(CN8-Pad2)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
  )
  (module plan44:plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 300.18 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN8 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(CN8-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(CN8-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 266.88 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN7 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CN6-Pad3)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CN6-Pad2)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
  )
  (module plan44:plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 233.58 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN6 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(CN6-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(CN6-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module plan44:plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 200.28 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN5 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-IN (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(CN4-Pad3)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(CN4-Pad2)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
  )
  (module plan44:plan44-WS2813-CONN (layer F.Cu) (tedit 57FE3506)
    (at 166.98 126.8 90)
    (descr WS2813-CONN)
    (tags WS2813-CONN)
    (attr virtual)
    (fp_text reference CN4 (at 3.81 3.81 180) (layer F.SilkS))
    (fp_text value WS2813-CONN-OUT (at -3.81 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 2 smd oval (at 0 2.54 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(CN4-Pad2)"))
    (pad 3 smd oval (at 0 5.08 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(CN4-Pad3)"))
    (pad 4 smd oval (at 0 7.62 90) (size 3.81 1.9304) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (gr_line (start 49.53 119.634) (end 49.53 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 377.19 119.634) (end 49.53 119.634) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 377.19 120.142) (end 377.19 119.634) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 377.19 129.54) (end 377.19 120.142) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 49.53 129.54) (end 377.19 129.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 16) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 376.682 129.032) (xy 50.038 129.032) (xy 50.038 120.142) (xy 376.682 120.142)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 376.682 129.032) (xy 50.038 129.032) (xy 50.038 120.142) (xy 376.682 120.142)
      )
    )
  )
)
