(kicad_pcb (version 4) (host pcbnew "(2015-09-06 BZR 6161, Git 6b3ff2d)-product")
  (general
    (links 5)
    (no_connects 0)
    (area 98.6 97.651 130.700001 129.069)
    (thickness 1.6)
    (drawings 8)
    (tracks 213)
    (zones 0)
    (modules 2)
    (nets 6)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.08 5.08)
    (pad_drill 2.54)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF77F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U1-Pad1)")
  (net 3 "Net-(U1-Pad3)")
  (net 4 "Net-(U1-Pad4)")
  (net 5 "Net-(U1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net GND)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad3)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 1)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
  )
  (module "Reference Parts:OX-2050-BEE-20744" (layer F.Cu) (tedit 5B7C791F)
    (at 116.5 112.8)
    (fp_text reference U16 (at -1.27 -13.97) (layer F.SilkS) hide)
    (fp_text value OX-2050-BEE-20744-100M00000 (at 0 15.24) (layer F.Fab) hide)
    (pad 5 thru_hole circle (at -9.525 9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad4)"))
    (pad 4 thru_hole circle (at 9.525 9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad5)"))
    (pad 3 thru_hole circle (at 9.525 -9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -9.525 -9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad3)"))
  )
  (module "Reference Parts:OX-2050-BEE-20744" (layer F.Cu) (tedit 5B7C78BC)
    (at 113.6 112.8)
    (fp_text reference U1 (at -1.27 -13.97) (layer F.SilkS) hide)
    (fp_text value OX-2050-BEE-20744-100M00000 (at 0 15.24) (layer F.Fab) hide)
    (pad 5 thru_hole circle (at -9.525 9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(U1-Pad5)"))
    (pad 4 thru_hole circle (at 9.525 9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(U1-Pad4)"))
    (pad 3 thru_hole circle (at 9.525 -9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at 0 -9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -9.525 -9.525) (size 1.905 1.905) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(U1-Pad1)"))
  )
  (gr_text OCXO (at 107.07 124.39) (layer F.SilkS))
  (gr_text PCB (at 104.16 119.86) (layer F.SilkS))
  (gr_text "NDR584 OCXO\nREV 2" (at 115.5 113.8) (layer B.SilkS))
  (gr_text FRONT (at 115.2 112.9) (layer F.SilkS))
  (gr_line (start 130 100) (end 130 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 100) (end 130 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 100) (end 100 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 126) (end 130 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.4 99.5) (xy 130.3 99.5) (xy 130.3 126.7) (xy 99 126.7) (xy 99 99.4)
        (xy 99.5 99.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99 99.3) (xy 130.6 99.3) (xy 130.6 126.9) (xy 98.8 126.9) (xy 98.8 99.2)
        (xy 99 99.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.7 99.4) (xy 130.7 126.8) (xy 98.8 126.8) (xy 98.8 99.4) (xy 130.7 99.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.8 99.2) (xy 99.1 99.2) (xy 98.8 99.35) (xy 98.8 99.2)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.7 99.4) (xy 98.8 99.35) (xy 98.8 99.4) (xy 98.7 99.4)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.8 99.3) (xy 130.3 99.3) (xy 130.3 126.9) (xy 98.6 126.9) (xy 98.6 99.2)
        (xy 99 99.2)
      )
    )
  )
)
