(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 75)
    (no_connects 0)
    (area 127 84.455 208.280001 160.745)
    (thickness 1.6)
    (drawings 40)
    (tracks 176)
    (zones 0)
    (modules 23)
    (nets 35)
  )
  (page USLetter)
  (title_block
    (title "Cable Tester")
    (date 2018-12-11)
    (rev 0.0)
    (company "Sigma Design")
    (comment 1 "K. Olsen")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.5)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 VCC)
  (net 6 "Net-(J1-Pad8)")
  (net 7 "Net-(J1-Pad10)")
  (net 8 "Net-(J1-Pad11)")
  (net 9 "Net-(J1-Pad12)")
  (net 10 "Net-(J1-Pad13)")
  (net 11 "Net-(J1-Pad14)")
  (net 12 "Net-(J1-Pad15)")
  (net 13 "Net-(J1-Pad16)")
  (net 14 "Net-(J1-Pad30)")
  (net 15 "Net-(D2-Pad2)")
  (net 16 "Net-(D3-Pad2)")
  (net 17 "Net-(D4-Pad2)")
  (net 18 /D8)
  (net 19 /D9)
  (net 20 /D10)
  (net 21 /D11)
  (net 22 /D12)
  (net 23 /D13)
  (net 24 "Net-(J1-Pad3)")
  (net 25 "Net-(J1-Pad9)")
  (net 26 "Net-(J1-Pad17)")
  (net 27 "Net-(J1-Pad18)")
  (net 28 "Net-(J1-Pad19)")
  (net 29 "Net-(J1-Pad20)")
  (net 30 "Net-(J1-Pad21)")
  (net 31 "Net-(J1-Pad22)")
  (net 32 "Net-(D5-Pad2)")
  (net 33 "Net-(D6-Pad2)")
  (net 34 "Net-(D7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D12)
    (add_net /D13)
    (add_net /D8)
    (add_net /D9)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5C1166FA)
    (at 181.61 144.78 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.03 270) (layer F.Fab))
    (fp_text user %R (at 0 6.35 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VCC))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5C1166DC)
    (at 199.39 144.78 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.03 270) (layer F.Fab))
    (fp_text user %R (at 0 6.35 360) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad14)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad13)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad10)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad9)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5C11669F)
    (at 160.02 101.6 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 20.11 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad30)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /D13))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /D12))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /D11))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /D10))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /D9))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /D8))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 5C11667C)
    (at 181.61 101.6 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X08 (at 0 20.11 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J1-Pad22)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad21)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad20)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad19)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad18)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad17)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad16)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad15)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5C11624E)
    (at 167.64 114.3)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /D8))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /D9))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /D10))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /D11))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /D12))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /D13))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5C116248)
    (at 193.04 114.3)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad14)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad13)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad10)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad9)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:arduino_header locked (layer F.Cu) (tedit 5C115A34)
    (at 169 123)
    (descr "Arduino Header")
    (tags Arduino)
    (fp_text reference J1 (at -13.044 28.384) (layer F.SilkS) hide)
    (fp_text value Arduino_Header (at -6.186 28.384) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -5.08 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -2.54 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 5.08 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 5 VCC))
    (pad 6 thru_hole oval (at 7.62 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 10.16 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole oval (at 12.7 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 17.78 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J1-Pad9)"))
    (pad 10 thru_hole oval (at 20.32 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 22.86 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad11)"))
    (pad 12 thru_hole oval (at 25.4 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 27.94 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 30.48 24.13) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 30.48 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 27.94 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at 25.4 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J1-Pad17)"))
    (pad 18 thru_hole oval (at 22.86 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J1-Pad18)"))
    (pad 19 thru_hole oval (at 20.32 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(J1-Pad19)"))
    (pad 20 thru_hole oval (at 17.78 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J1-Pad20)"))
    (pad 21 thru_hole oval (at 15.24 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(J1-Pad21)"))
    (pad 22 thru_hole oval (at 12.7 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(J1-Pad22)"))
    (pad 23 thru_hole oval (at 8.636 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D8))
    (pad 24 thru_hole oval (at 6.096 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D9))
    (pad 25 thru_hole oval (at 3.556 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D10))
    (pad 26 thru_hole oval (at 1.016 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D11))
    (pad 27 thru_hole oval (at -1.524 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 22 /D12))
    (pad 28 thru_hole oval (at -4.064 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 23 /D13))
    (pad 29 thru_hole oval (at -6.604 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 30 thru_hole oval (at -9.14146 -24.13) (size 1.524 2.1971) (drill 0.99822) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad30)"))
    (model walter/conn_misc/arduino_header.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 5C11B14D)
    (at 161.29 144.145 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 1.91 3.06 180) (layer F.SilkS) hide)
    (fp_text value PWR (at 1.27 -3.175 180) (layer F.SilkS))
    (fp_text user + (at 3.302 1.524 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 5C11B204)
    (at 167.64 134.62 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D7 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 5C11B1FD)
    (at 172.72 134.62 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D6 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(D6-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 5C11B1F6)
    (at 177.8 134.62 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D5 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 5C11B1F1)
    (at 182.88 134.62 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D4 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 5C11B1EA)
    (at 187.96 134.62 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myFootPrints:LED-3MM (layer F.Cu) (tedit 5C11B1E3)
    (at 193.04 134.62 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 1.91 3.06 90) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 -1.524 90) (layer F.Fab))
    (fp_text user + (at 3.302 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole rect (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5C11B987)
    (at 161.29 114.3)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J22 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /D8))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /D9))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /D10))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /D11))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /D12))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /D13))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5C11B98E)
    (at 199.39 114.3)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J33 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 15.03) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad14)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad13)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad10)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad9)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5C11B142)
    (at 161.925 140.97)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0 -1.905) (layer F.Fab))
    (fp_text value 1K (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 VCC))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5C11B1B2)
    (at 173.99 119.38 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R7 (at 0 -1.905 90) (layer F.Fab))
    (fp_text value 1K (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 34 "Net-(D7-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 31 "Net-(J1-Pad22)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5C11B1B8)
    (at 176.53 119.38 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R6 (at 0 -1.905 90) (layer F.Fab))
    (fp_text value 1K (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 33 "Net-(D6-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 30 "Net-(J1-Pad21)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5C11B1C2)
    (at 179.07 119.38 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R5 (at 0 -1.905 90) (layer F.Fab))
    (fp_text value 1K (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 32 "Net-(D5-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 29 "Net-(J1-Pad20)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5C11B1C8)
    (at 181.61 119.38 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R4 (at 0 -1.905 90) (layer F.Fab))
    (fp_text value 1K (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 28 "Net-(J1-Pad19)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5C11B1D0)
    (at 184.15 119.38 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R3 (at 0 -1.905 90) (layer F.Fab))
    (fp_text value 1K (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 27 "Net-(J1-Pad18)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module myFootPrints:Resistor_Horz (layer F.Cu) (tedit 5C11B1D8)
    (at 186.69 119.38 90)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at 0 -1.905 90) (layer F.Fab))
    (fp_text value 1K (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 3.175 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 26 "Net-(J1-Pad17)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 20.32 (width 0.3) (layer Dwgs.User)
    (gr_text "0.8000 in" (at 146.05 90.09) (layer Dwgs.User))
    (feature1 (pts (xy 135.89 95.25) (xy 135.89 88.74)))
    (feature2 (pts (xy 156.21 95.25) (xy 156.21 88.74)))
    (crossbar (pts (xy 156.21 91.44) (xy 135.89 91.44)))
    (arrow1a (pts (xy 135.89 91.44) (xy 137.016504 90.853579)))
    (arrow1b (pts (xy 135.89 91.44) (xy 137.016504 92.026421)))
    (arrow2a (pts (xy 156.21 91.44) (xy 155.083496 90.853579)))
    (arrow2b (pts (xy 156.21 91.44) (xy 155.083496 92.026421)))
  )
  (gr_text "Remove\nPower\nFirst!" (at 161.036 131.064) (layer F.SilkS))
  (gr_text "METER\nPOINTS" (at 161.29 111.252) (layer F.SilkS))
  (gr_text "1   2   3   4   5   6" (at 180.34 137.16) (layer F.SilkS))
  (gr_text "Molex SL:\nPCB Male Header 075430005\nFemale Housing 50579406\n" (at 200.66 106.68) (layer B.SilkS))
  (gr_text "Molex SL:\nPCB Male Header 075430005\nFemale Housing 50579406\n" (at 144.145 156.845) (layer Dwgs.User))
  (gr_text "Solid = Good\nBlink = Crossed\nOut  = No Cont." (at 170.434 111.252) (layer F.SilkS))
  (gr_line (start 160.02 96.52) (end 157.48 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.02 149.86) (end 157.48 149.86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.21 97.79) (end 156.21 148.59) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "RST\n3V3\n5V\nGND\nGND\nVin" (at 175.26 143.51 90) (layer F.SilkS))
  (gr_text "A0\nA1\nA2\nA3\nA4\nA5" (at 193.04 143.51 90) (layer F.SilkS))
  (gr_text "ARF\nGND\nD13\nD12\nD11\nD10\nD9\nD8" (at 168.91 102.87 90) (layer F.SilkS))
  (gr_text "D7\nD6\nD5\nD4\nD3\nD2\nD1\nD0" (at 190.5 102.87 90) (layer F.SilkS))
  (gr_text "1\n2\n3\n4\n5\n6" (at 201.93 120.65) (layer F.SilkS))
  (gr_text "1\n2\n3\n4\n5\n6" (at 158.75 120.65) (layer F.SilkS))
  (gr_text "Cable\nTester" (at 174.498 127.254) (layer F.SilkS))
  (gr_arc (start 157.48 97.79) (end 156.21 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 157.48 148.59) (end 157.48 149.86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Cable Tester\nVer 0.0\nDec 2018" (at 203.2 139.7) (layer B.SilkS))
  (gr_line (start 199.39 149.86) (end 160.02 149.86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.47 144.78) (end 201.93 147.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.47 111.76) (end 204.47 144.78) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 201.93 109.22) (end 204.47 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 201.93 99.06) (end 201.93 109.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.02 96.52) (end 199.39 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 199.39 99.06) (end 199.39 96.52) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 199.39 147.32) (end 201.93 147.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 205.74 149.86) (xy 129.54 149.86) (xy 129.54 88.9) (xy 205.74 88.9)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 208.28 150.495) (xy 127 150.495) (xy 127 84.455) (xy 208.28 84.455)
      )
    )
  )
)
