<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<hole x="11.15" y="29" drill="3.5"/>
<hole x="87.55" y="29" drill="3.5"/>
<hole x="11.15" y="61.15" drill="3.5"/>
<hole x="87.55" y="61.15" drill="3.5"/>
<hole x="97.79" y="9.2075" drill="1.3"/>
<hole x="82.55" y="6.6675" drill="1.3"/>
<text>REMOTE
SWITCH</text>
<text>GND
</text>
<text>S
</text>
<text>VCC
</text>
<text>PANEL
BUTTONS</text>
<text>K3NG ARDUINO ROTATOR
CONTROL BOARD V3
DESIGNED BY M0UPU</text>
<text>See http://blog.radioartisan.com
/yaesu-rotator-computer-serial-interface/
For latest code</text>
<text>See http://ava.upuaut.net
/rotator-computer-serial-interface/
For schematics &amp; PCB ordering info</text>
<text>PCB Made by www.hackvana.com</text>
<text>RESET</text>
<text>VCC</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>CCW</text>
<text>DOWN</text>
<text>UP</text>
<text>CW</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="0805">
</package>
<package name="0603-CAP">
</package>
<package name="LCD-16X2_NOHOLES">
</package>
<package name="1X02">
</package>
<package name="DUEMILANOVE_SHIELD">
</package>
<package name="1X03">
</package>
<package name="OSHW-LOGO-L">
</package>
<package name="LED-0603">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="TACTILE_SWITCH_TALL">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="Ava">
<packages>
<package name="TYCO_ELECTRONICS_POT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun" package="RJ45-8" value="RJ45-8PTH"/>
<element name="Q1" library="SparkFun" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="C9" library="SparkFun" package="0603-CAP" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="Q3" library="SparkFun" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="C11" library="SparkFun" package="0603-CAP" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="Q4" library="SparkFun" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="C12" library="SparkFun" package="0603-CAP" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="Q5" library="SparkFun" package="SOT23" value="">
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="C14" library="SparkFun" package="0603-CAP" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="U2" library="SparkFun" package="LCD-16X2_NOHOLES" value="LCD-16X2NOHOLES"/>
<element name="CCW" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UP" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DOWN" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CW" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun" package="DUEMILANOVE_SHIELD" value="ARDUINO_SHIELDLABEL"/>
<element name="U$2" library="Ava" package="TYCO_ELECTRONICS_POT" value="TYCO_ELECTRONICS_POT"/>
<element name="R3" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun" package="0603-CAP" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun" package="0603-CAP" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="REMOTESWITCH" library="SparkFun" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SparkFun" package="OSHW-LOGO-L" value=""/>
<element name="LED1" library="SparkFun" package="LED-0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="LED2" library="SparkFun" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="SparkFun" package="LED-0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="LED4" library="SparkFun" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="SparkFun" package="LED-0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="LED6" library="SparkFun" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="SparkFun" package="LED-0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun" package="0805" value="1k">
<attribute name="NAME"/>
</element>
<element name="LED8" library="SparkFun" package="LED3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun" package="TACTILE_SWITCH_TALL" value="RESET"/>
<element name="I2C" library="SparkFun" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="+5V">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="5V"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="REMOTESWITCH" pad="3"/>
<contactref element="I2C" pad="4"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="8"/>
<contactref element="Q1" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="CW" pad="2"/>
<contactref element="CCW" pad="2"/>
<contactref element="UP" pad="2"/>
<contactref element="DOWN" pad="2"/>
<contactref element="U1" pad="GND@2"/>
<contactref element="U1" pad="GND@1"/>
<contactref element="U1" pad="GND@0"/>
<contactref element="U$2" pad="P$3"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U2" pad="16"/>
<contactref element="REMOTESWITCH" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="K"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="K"/>
<contactref element="LED5" pad="C"/>
<contactref element="LED6" pad="K"/>
<contactref element="LED7" pad="C"/>
<contactref element="LED8" pad="K"/>
<contactref element="S1" pad="A2"/>
<contactref element="I2C" pad="3"/>
</signal>
<signal name="LCD_RS">
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="D12"/>
</signal>
<signal name="AZIMUTH_V">
<contactref element="U1" pad="A0"/>
<contactref element="R3" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="ELEVATION_V">
<contactref element="U1" pad="A1"/>
<contactref element="R4" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="ROTATE_CCW">
<contactref element="U$1" pad="4"/>
<contactref element="Q5" pad="3"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="ROTATE_CW">
<contactref element="U$1" pad="5"/>
<contactref element="Q4" pad="3"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="ROTATE_DOWN">
<contactref element="U$1" pad="6"/>
<contactref element="Q3" pad="3"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="ROTATE_UP">
<contactref element="U$1" pad="7"/>
<contactref element="Q1" pad="3"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R5" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R8" pad="2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R9" pad="2"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="R10" pad="2"/>
<contactref element="Q5" pad="1"/>
</signal>
<signal name="PD6_RCCW">
<contactref element="R10" pad="1"/>
<contactref element="U1" pad="D6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="PD7_RCW">
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="D7"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="PB0_RDOWN">
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="D8"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="PB1_RUP">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="D9"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="3"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="LCD_E">
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="D11"/>
</signal>
<signal name="LCD_D4">
<contactref element="U2" pad="11"/>
<contactref element="U1" pad="D5"/>
</signal>
<signal name="LCD_D5">
<contactref element="U2" pad="12"/>
<contactref element="U1" pad="D4"/>
</signal>
<signal name="LCD_D6">
<contactref element="U2" pad="13"/>
<contactref element="U1" pad="D3"/>
</signal>
<signal name="LCD_D7">
<contactref element="U2" pad="14"/>
<contactref element="U1" pad="D2"/>
</signal>
<signal name="TURN_CW">
<contactref element="CW" pad="1"/>
<contactref element="U1" pad="A2"/>
</signal>
<signal name="TURN_CCW">
<contactref element="CCW" pad="1"/>
<contactref element="U1" pad="A3"/>
</signal>
<signal name="TURN_UP/A4/SDA">
<contactref element="UP" pad="1"/>
<contactref element="U1" pad="A4"/>
<contactref element="I2C" pad="2"/>
</signal>
<signal name="TURN_DOWN/A5/SCL">
<contactref element="DOWN" pad="1"/>
<contactref element="U1" pad="A5"/>
<contactref element="I2C" pad="1"/>
</signal>
<signal name="AZV">
<contactref element="U$1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="ELV">
<contactref element="U$1" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="PB2_LCDBACKLIGHT">
<contactref element="U1" pad="D10"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="PB5_REMOTEPWR">
<contactref element="U1" pad="D13"/>
<contactref element="REMOTESWITCH" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="2"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R6" pad="2"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R7" pad="2"/>
<contactref element="LED7" pad="A"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="RES"/>
<contactref element="S1" pad="B2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
