<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="20" width="0.0762" layer="20"/>
<wire x1="0" y1="20" x2="95" y2="20" width="0.0762" layer="20"/>
<wire x1="95" y1="20" x2="95" y2="0" width="0.0762" layer="20"/>
<wire x1="95" y1="0" x2="0" y2="0" width="0.0762" layer="20"/>
<hole x="3" y="17" drill="3"/>
<hole x="92" y="17" drill="3"/>
<hole x="5" y="10.375" drill="2.3114"/>
<hole x="18.125" y="10.375" drill="2.3114"/>
<hole x="76.875" y="10.375" drill="2.3114"/>
<hole x="90" y="10.375" drill="2.3114"/>
<text>MIC</text>
<text> v1.1 \ 07.2017</text>
</plain>
<libraries>
<library name="jst_eph">
<description>JST PH series crimp-style 2mm connectors</description>
<packages>
<package name="B8B-PH-K-S">
</package>
<package name="B9B-PH-K-S">
</package>
<package name="B5B-PH-K-S">
</package>
</packages>
</library>
<library name="con-usb-3">
<description>&lt;b&gt;USB Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by Erik Christiansson (erik@alphafish.com)&lt;/author&gt;&lt;p&gt;
Based on the datasheets for the following products.&lt;br&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;Manufacturer&lt;/td&gt;&lt;td&gt;Part No.&lt;/td&gt;&lt;td&gt;Type&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8317-04AFDXX0&lt;/td&gt;&lt;td&gt;Series A Surface Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8317-04AFHSW0&lt;/td&gt;&lt;td&gt;Series A Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C3817-04AFVSW0&lt;/td&gt;&lt;td&gt;Series A Hole Mounted Up-Right&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8317-04BFHSW0&lt;/td&gt;&lt;td&gt;Series B Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8320-05BFDSB0&lt;/td&gt;&lt;td&gt;Series Mini-B Surface Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Hsuan Mao&lt;/td&gt;&lt;td&gt;C8320-05BFRSB0&lt;/td&gt;&lt;td&gt;Series Mini-B Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Amp&lt;/td&gt;&lt;td&gt;787616-*&lt;/td&gt;&lt;td&gt;Series A Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Amp&lt;/td&gt;&lt;td&gt;787780-1&lt;/td&gt;&lt;td&gt;Series B Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;ACON&lt;/td&gt;&lt;td&gt;UAR80-4****0&lt;/td&gt;&lt;td&gt;Series A Hole Mounted Up-Right&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;ACON&lt;/td&gt;&lt;td&gt;MNC20-5K5*1*&lt;/td&gt;&lt;td&gt;Series Mini-B Surface Mounted&lt;/td&gt;&lt;tr&gt;
&lt;tr&gt;&lt;td&gt;Molex&lt;/td&gt;&lt;td&gt;67068-****&lt;/td&gt;&lt;td&gt;Series B Hole Mounted&lt;/td&gt;&lt;tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO-JACK">
<description>&lt;h3&gt;3.5mm Stereo Audio Jack&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Audio-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Audio_Jack&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="custom">
<packages>
<package name="ESATA-G09-7P">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="USB_HDR" library="jst_eph" package="B8B-PH-K-S" value="USB_HDR">
<attribute name="NAME"/>
</element>
<element name="HDA_HDR" library="jst_eph" package="B9B-PH-K-S" value="HDA_HDR">
<attribute name="NAME"/>
</element>
<element name="USB2" library="con-usb-3" package="USB-A-H" value="2">
<attribute name="NAME"/>
</element>
<element name="USB1" library="con-usb-3" package="USB-A-H" value="1">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="AUDIO-JACK" value="SPK">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="AUDIO-JACK" value="MIC">
<attribute name="PROD_ID" value="CONN-08774"/>
<attribute name="SF_ID" value="PRT-08032"/>
</element>
<element name="E-SATA" library="custom" package="ESATA-G09-7P" value="ESATA-G011-7P11">
<attribute name="NAME"/>
</element>
<element name="SATA_HDR" library="jst_eph" package="B5B-PH-K-S" value="5PIN">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="EHC2_VDD">
<contactref element="USB_HDR" pad="4"/>
<contactref element="USB2" pad="1"/>
</signal>
<signal name="PORT1_L">
<contactref element="HDA_HDR" pad="6"/>
<contactref element="J2" pad="TIP"/>
</signal>
<signal name="SENSE_SEND">
<contactref element="HDA_HDR" pad="3"/>
<contactref element="J2" pad="TSH"/>
<contactref element="J3" pad="TSH"/>
</signal>
<signal name="SENSE1_RETURN">
<contactref element="J2" pad="RSH"/>
<contactref element="HDA_HDR" pad="8"/>
</signal>
<signal name="PORT1_R">
<contactref element="J2" pad="RING"/>
<contactref element="HDA_HDR" pad="7"/>
</signal>
<signal name="PORT2_L">
<contactref element="HDA_HDR" pad="2"/>
<contactref element="J3" pad="TIP"/>
</signal>
<signal name="SENSE2_RETURN">
<contactref element="HDA_HDR" pad="4"/>
<contactref element="J3" pad="RSH"/>
</signal>
<signal name="PORT2_R">
<contactref element="HDA_HDR" pad="5"/>
<contactref element="J3" pad="RING"/>
</signal>
<signal name="EHC1_GND">
<contactref element="USB_HDR" pad="5"/>
<contactref element="USB1" pad="4"/>
</signal>
<signal name="SPK/MIC_GND">
<contactref element="HDA_HDR" pad="1"/>
<contactref element="J2" pad="SLEEVE"/>
<contactref element="J3" pad="SLEEVE"/>
</signal>
<signal name="EHC1_VDD">
<contactref element="USB_HDR" pad="8"/>
<contactref element="USB1" pad="1"/>
</signal>
<signal name="EHC2_D+">
<contactref element="USB_HDR" pad="2"/>
<contactref element="USB2" pad="3"/>
</signal>
<signal name="EHC2_D-">
<contactref element="USB_HDR" pad="3"/>
<contactref element="USB2" pad="2"/>
</signal>
<signal name="EHC1_D+">
<contactref element="USB_HDR" pad="6"/>
<contactref element="USB1" pad="3"/>
</signal>
<signal name="EHC1_D-">
<contactref element="USB_HDR" pad="7"/>
<contactref element="USB1" pad="2"/>
</signal>
<signal name="EHC2_GND">
<contactref element="USB_HDR" pad="1"/>
<contactref element="USB2" pad="4"/>
</signal>
<signal name="ATA_A+">
<contactref element="E-SATA" pad="P$2"/>
<contactref element="SATA_HDR" pad="1"/>
</signal>
<signal name="ATA_A-">
<contactref element="E-SATA" pad="P$3"/>
<contactref element="SATA_HDR" pad="2"/>
</signal>
<signal name="ATA_B-">
<contactref element="E-SATA" pad="P$5"/>
<contactref element="SATA_HDR" pad="4"/>
</signal>
<signal name="ATA_B+">
<contactref element="E-SATA" pad="P$6"/>
<contactref element="SATA_HDR" pad="5"/>
</signal>
<signal name="ATA_GND">
<contactref element="E-SATA" pad="P$7"/>
<contactref element="E-SATA" pad="P$1"/>
<contactref element="E-SATA" pad="P$4"/>
<contactref element="SATA_HDR" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
