<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<description>Board for easy access to ATtiny10 pins with pogo pins or soldered wires. Pads on the back enable powering by an SMD coin cell battery (though the unused pads need to be covered with tape before use).</description>
<plain>
<wire x1="0" y1="0" x2="0" y2="6.35" width="0.1524" layer="20"/>
<wire x1="0" y1="6.35" x2="6.35" y2="6.35" width="0.1524" layer="20"/>
<wire x1="6.35" y1="6.35" x2="6.35" y2="0" width="0.1524" layer="20"/>
<wire x1="6.35" y1="0" x2="0" y2="0" width="0.1524" layer="20"/>
<text>GND</text>
<text>VCC</text>
<text>0.25 in</text>
<text>0.25 in</text>
</plain>
<libraries>
<library name="ATTINY10-TSHR">
<packages>
<package name="SOT95P280X145-6N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TINY10" library="ATTINY10-TSHR" package="SOT95P280X145-6N" value="ATTINY10-TSHR">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" AVR microcontroller; SRAM: 32B; Flash: 1kB; SOT23-6; Usup: 1.8÷5.5V "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="ATTINY10-TSHR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-6 Microchip"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="TINY10" pad="5"/>
</signal>
<signal name="GROUND">
<contactref element="TINY10" pad="2"/>
</signal>
<signal name="PB0/MOSI/WAKE">
<contactref element="TINY10" pad="1"/>
</signal>
<signal name="PB1/SCK/PULSE">
<contactref element="TINY10" pad="3"/>
</signal>
<signal name="PB3/RESET">
<contactref element="TINY10" pad="6"/>
</signal>
<signal name="PB2">
<contactref element="TINY10" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
