(kicad_pcb (version 4) (host pcbnew 4.0.1-3.201512221402+6198~38~ubuntu14.04.1-stable)
  (general
    (links 49)
    (no_connects 0)
    (area 97.527699 91.845 178.584285 137.725)
    (thickness 1.6)
    (drawings 21)
    (tracks 140)
    (zones 0)
    (modules 16)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.4)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEDF7D)
    (pcbplotparams
      (layerselection 0x30000_00000000)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /LCD_RS)
  (net 3 /LCD_RW)
  (net 4 /LCD_EN)
  (net 5 /LED1)
  (net 6 /LCD_D4)
  (net 7 /LCD_D5)
  (net 8 /LCD_D6)
  (net 9 /LCD_D7)
  (net 10 /SD_CS)
  (net 11 /MOSI)
  (net 12 /MISO)
  (net 13 +3V3)
  (net 14 /SCLK)
  (net 15 /BUTTON2)
  (net 16 /SDA)
  (net 17 /BUTTON1)
  (net 18 /LIDAR_MONITOR)
  (net 19 +5V)
  (net 20 /LIDAR_TRIGGER)
  (net 21 /LIDAR_EN)
  (net 22 /SCL)
  (net 23 /LED2)
  (net 24 /BUTTON3)
  (net 25 "Net-(LCD1-Pad3)")
  (net 26 "Net-(LED1-Pad2)")
  (net 27 "Net-(LED2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.762)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /BUTTON1)
    (add_net /BUTTON2)
    (add_net /BUTTON3)
    (add_net /LCD_D4)
    (add_net /LCD_D5)
    (add_net /LCD_D6)
    (add_net /LCD_D7)
    (add_net /LCD_EN)
    (add_net /LCD_RS)
    (add_net /LCD_RW)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /LIDAR_EN)
    (add_net /LIDAR_MONITOR)
    (add_net /LIDAR_TRIGGER)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCL)
    (add_net /SCLK)
    (add_net /SDA)
    (add_net /SD_CS)
    (add_net GND)
    (add_net "Net-(LCD1-Pad3)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED2-Pad2)")
  )
  (module Wickerlib:TEENSY-3.2-NOSILK (layer F.Cu) (tedit 57AFBA27)
    (at 158.75 116.205 270)
    (fp_text reference J1 (at -2 0 270) (layer F.Fab))
    (fp_text value TEENSY3.2-72MHz (at -2.54 20.32 270) (layer F.Fab) hide)
    (fp_text user %R (at 2.54 25.4 270) (layer F.SilkS) hide)
    (pad G1 thru_hole circle (at -10.16 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at -10.16 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -10.16 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -10.16 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /LCD_RS))
    (pad 3 thru_hole circle (at -10.16 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /LCD_RW))
    (pad 4 thru_hole circle (at -10.16 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /LCD_EN))
    (pad 5 thru_hole circle (at -10.16 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /LED1))
    (pad 6 thru_hole circle (at -10.16 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /LCD_D4))
    (pad 7 thru_hole circle (at -10.16 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /LCD_D5))
    (pad 8 thru_hole circle (at -10.16 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /LCD_D6))
    (pad 9 thru_hole circle (at -10.16 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /LCD_D7))
    (pad 10 thru_hole circle (at -10.16 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SD_CS))
    (pad 11 thru_hole circle (at -10.16 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /MOSI))
    (pad 12 thru_hole circle (at -10.16 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /MISO))
    (pad VBAT thru_hole circle (at -7.62 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3V1 thru_hole circle (at -5.08 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 +3V3))
    (pad G2 thru_hole circle (at -2.54 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad PGM thru_hole circle (at 0 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad DAC thru_hole circle (at 2.54 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 5.08 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SCLK))
    (pad 16 thru_hole circle (at 5.08 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /BUTTON2))
    (pad 3V2 thru_hole circle (at 5.08 -5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 +3V3))
    (pad 18 thru_hole circle (at 5.08 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SDA))
    (pad 17 thru_hole circle (at 5.08 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /BUTTON1))
    (pad AG thru_hole circle (at 5.08 -7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 22 thru_hole circle (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LIDAR_MONITOR))
    (pad VIN thru_hole circle (at 5.08 -10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 +5V))
    (pad 21 thru_hole circle (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LIDAR_TRIGGER))
    (pad 20 thru_hole circle (at 5.08 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /LIDAR_EN))
    (pad 19 thru_hole circle (at 5.08 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /SCL))
    (pad 23 thru_hole circle (at 5.08 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 5.08 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /LED2))
    (pad 15 thru_hole circle (at 5.08 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /BUTTON3))
  )
  (module Wickerlib:CONN-HEADER-STRAIGHT-P2.54MM-1x06 (layer F.Cu) (tedit 57AFB99F)
    (at 161.798 127.254 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0.17 8.39 360) (layer F.Fab))
    (fp_text value LIDAR-LITE (at -2.63 6.86 360) (layer F.Fab) hide)
    (fp_text user %R (at 0.14 -2.74 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /LIDAR_EN))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LIDAR_MONITOR))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /SCL))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /SDA))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Wickerlib:LCD-1602A locked (layer B.Cu) (tedit 57902DAA)
    (at 169.80154 99.85502 180)
    (descr http://www.kamami.pl/dl/wc1602a0.pdf)
    (tags "LCD 16x2 Alphanumeric 16pin")
    (fp_text reference LCD1 (at 19.05 0 180) (layer B.Fab))
    (fp_text value LCD-16x2 (at 31.99892 -15.49908 180) (layer B.Fab) hide)
    (pad 1 thru_hole oval (at 0 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 19 +5V))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 25 "Net-(LCD1-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 2 /LCD_RS))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 3 /LCD_RW))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 4 /LCD_EN))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 10 thru_hole oval (at 22.86 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS))
    (pad 11 thru_hole oval (at 25.4 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 6 /LCD_D4))
    (pad 12 thru_hole oval (at 27.94 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 7 /LCD_D5))
    (pad 13 thru_hole oval (at 30.48 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 8 /LCD_D6))
    (pad 14 thru_hole oval (at 33.02 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 9 /LCD_D7))
    (pad 15 thru_hole oval (at 35.56 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 19 +5V))
    (pad 16 thru_hole oval (at 38.1 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 0 thru_hole circle (at -5.4991 0 180) (size 3 3) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad 0 thru_hole circle (at -5.4991 -31.0007 180) (size 3 3) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad 0 thru_hole circle (at 69.49948 -31.0007 180) (size 3 3) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
    (pad 0 thru_hole circle (at 69.49948 0 180) (size 3 3) (drill 2.5) (layers *.Cu *.Mask B.SilkS))
  )
  (module Wickerlib:LED-0603-SMD (layer F.Cu) (tedit 57903B26)
    (at 105.977666 124.828528)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference LED1 (at 0.09 0.04) (layer F.Fab))
    (fp_text value AMBER (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.369 1.778) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(LED1-Pad2)"))
  )
  (module Wickerlib:LED-0603-SMD (layer F.Cu) (tedit 57903B26)
    (at 105.918 120.383528)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference LED2 (at 0.09 0.04) (layer F.Fab))
    (fp_text value AMBER (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.07 1.790472) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(LED2-Pad2)"))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 157.722 124.206)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference R1 (at 0.09 0.04) (layer F.Fab))
    (fp_text value 1K (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 2.806 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 /LIDAR_TRIGGER))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 /LIDAR_MONITOR))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 110.652666 124.828528 180)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference R2 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 1K (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.162666 -1.917472 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /LED1))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(LED1-Pad2)"))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 130.429 121.654 270)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference R3 (at 0.09 0.04 270) (layer F.Fab))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.782 -0.127 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 17 /BUTTON1))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 124.206 121.678 270)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference R4 (at 0.09 0.04 270) (layer F.Fab))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.806 0 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 /BUTTON2))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 117.729 121.654 270)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference R5 (at 0.09 0.04 270) (layer F.Fab))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.782 0.127 360) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 24 /BUTTON3))
  )
  (module Wickerlib:RES-TRIMPOT-BOURNS-3362-SQUARE-TH-CENTER (layer F.Cu) (tedit 5790459A)
    (at 122.936 102.235)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference R6 (at 0 0 90) (layer F.Fab))
    (fp_text value 10K (at 0.508 0.254 90) (layer F.Fab) hide)
    (fp_text user %R (at -2.413 4.953) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 -2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(LCD1-Pad3)"))
    (pad 3 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 +5V))
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 110.652666 120.383528 180)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference R7 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 1K (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.07 -1.790472 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 /LED2))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(LED2-Pad2)"))
  )
  (module Wickerlib:SWITCH-OMRON-MOMENTARY-SMD-B3U-1000P (layer F.Cu) (tedit 57904124)
    (at 130.429 125.349 270)
    (descr SW-B3F-10XX)
    (tags "Omron B3F-10xx")
    (fp_text reference S1 (at 1.778 0 270) (layer F.Fab))
    (fp_text value BUTTON1 (at 1.524 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 5.461 -0.127 360) (layer F.SilkS))
    (pad 2 smd rect (at 3.4 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 /BUTTON1))
  )
  (module Wickerlib:SWITCH-OMRON-MOMENTARY-SMD-B3U-1000P (layer F.Cu) (tedit 57904124)
    (at 124.206 125.349 270)
    (descr SW-B3F-10XX)
    (tags "Omron B3F-10xx")
    (fp_text reference S2 (at 1.778 0 270) (layer F.Fab))
    (fp_text value BUTTON2 (at 1.524 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 5.461 0 360) (layer F.SilkS))
    (pad 2 smd rect (at 3.4 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 /BUTTON2))
  )
  (module Wickerlib:SWITCH-OMRON-MOMENTARY-SMD-B3U-1000P (layer F.Cu) (tedit 57904124)
    (at 117.729 125.349 270)
    (descr SW-B3F-10XX)
    (tags "Omron B3F-10xx")
    (fp_text reference S3 (at 1.778 0 270) (layer F.Fab))
    (fp_text value BUTTON3 (at 1.524 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 5.461 0.127 360) (layer F.SilkS))
    (pad 2 smd rect (at 3.4 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 0 270) (size 0.8 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 /BUTTON3))
  )
  (module Wickerlib:CONN-SD-MICRO-MOLEX-0475710001 (layer F.Cu) (tedit 57958DF9)
    (at 114.3535 110.2985 270)
    (fp_text reference J3 (at 0 3.25 270) (layer F.Fab))
    (fp_text value MICRO-SD (at 4 6.25 270) (layer F.Fab) hide)
    (fp_text user %R (at -7.6825 1.0695 540) (layer F.SilkS))
    (pad G5 smd rect (at 4.8514 5.1 270) (size 1.4 0.9) (layers F.Cu F.Paste F.Mask))
    (pad G2 smd rect (at -5.4135 4.9635 270) (size 1.2 1.15) (layers F.Cu F.Paste F.Mask))
    (pad G3 smd rect (at 4.8264 2.8 270) (size 1.45 1.2) (layers F.Cu F.Paste F.Mask))
    (pad G1 smd rect (at -5.4135 2.3635 270) (size 1.2 1.15) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -2.8135 1.3235 270) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /MISO))
    (pad 8 smd rect (at -3.9135 1.3235 270) (size 0.7 1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.7135 1.3235 270) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -0.6135 1.3235 270) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCLK))
    (pad 4 smd rect (at 0.4865 1.3235 270) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 13 +3V3))
    (pad 1 smd rect (at 3.7865 1.3235 270) (size 0.7 1) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 2.6865 1.3235 270) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /SD_CS))
    (pad 3 smd rect (at 1.5865 1.3235 270) (size 0.7 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /MOSI))
    (pad G4 smd rect (at 5.0514 3.95 270) (size 1 0.7) (layers F.Cu F.Paste F.Mask))
  )
  (gr_text "8/13/16 " (at 172.72 136.525) (layer F.Fab))
  (gr_text "LCD-LiDAR-SD Teensy Hat v1.0" (at 158.75 93.345) (layer F.Fab))
  (gr_text 16 (at 128.524 100.076) (layer F.SilkS))
  (gr_text 1 (at 172.212 99.822) (layer F.SilkS))
  (gr_text "LCD-LiDAR-SD Teensy Hat v1.0\n8/13/16 " (at 157.734 113.792) (layer B.SilkS))
  (gr_text "Teensy 3.2" (at 172.212 113.538 90) (layer F.SilkS))
  (gr_text "LiDAR\n" (at 166.878 127.254) (layer F.SilkS))
  (gr_text "GND\n" (at 149.098 130.967238 90) (layer F.SilkS))
  (gr_text SDA (at 151.638 130.846285 90) (layer F.SilkS))
  (gr_text SCL (at 154.178 130.822095 90) (layer F.SilkS))
  (gr_text MON (at 156.718 131.064 90) (layer F.SilkS))
  (gr_text EN (at 159.258 130.410857 90) (layer F.SilkS))
  (gr_text 5V (at 161.798 130.338285 90) (layer F.SilkS))
  (gr_line (start 97.79 133.35) (end 177.8 133.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.79 97.155) (end 97.79 133.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 97.155) (end 97.79 97.155) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.8 133.35) (end 177.8 97.155) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.8 97.282) (xy 177.8 133.35) (xy 97.79 133.35) (xy 97.79 97.028) (xy 177.8 97.028)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.8 97.426882) (xy 177.8 133.494882) (xy 97.79 133.494882) (xy 97.79 97.172882) (xy 177.8 97.172882)
      )
    )
  )
  (zone (net 13) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 129.032 118.11) (xy 119.888 118.11) (xy 119.888 110.49) (xy 129.032 110.49) (xy 129.032 118.11)
      )
    )
  )
)
