(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~86~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 29)
    (tracks 618)
    (zones 0)
    (modules 19)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.5 6.5)
    (pad_drill 3.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 175 95.5)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GNDD)
  (net 2 GND)
  (net 3 Trig+)
  (net 4 Trig-)
  (net 5 +12V)
  (net 6 VGS)
  (net 7 "Net-(U4-Pad4)")
  (net 8 "Net-(U4-Pad3)")
  (net 9 "Net-(U4-Pad2)")
  (net 10 /6V)
  (net 11 /ZVN_Gate)
  (net 12 /Opto_Out)
  (net 13 "Net-(H1-Pad1)")
  (net 14 "Net-(H2-Pad1)")
  (net 15 "Net-(H3-Pad1)")
  (net 16 "Net-(H4-Pad1)")
  (net 17 Gan_Drain)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Opto_Out)
    (add_net /ZVN_Gate)
    (add_net Gan_Drain)
    (add_net "Net-(H1-Pad1)")
    (add_net "Net-(H2-Pad1)")
    (add_net "Net-(H3-Pad1)")
    (add_net "Net-(H4-Pad1)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad4)")
  )
  (net_class 12V_PWR ""
    (clearance 0.2)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
  )
  (net_class 6V_PWR ""
    (clearance 0.2)
    (trace_width 0.8)
    (via_dia 0.5)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /6V)
    (add_net GNDD)
    (add_net Trig+)
    (add_net Trig-)
    (add_net VGS)
  )
  (net_class VGS_Sig ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U4-Pad2)")
  )
  (module HPMI:RP-1206S (layer F.Cu) (tedit 5E4DD2A2)
    (at 68.7 95.85)
    (fp_text reference U1 (at 7.62 -3.81) (layer F.SilkS))
    (fp_text value RP-1206S (at 7.62 -6.35) (layer F.Fab))
    (pad 7 smd rect (at 15.24 0) (size 1.5 4.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /6V))
    (pad 5 smd rect (at 10.16 0) (size 1.5 4.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at 2.54 0) (size 1.5 4.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0) (size 1.5 4.2) (layers F.Cu F.Paste F.Mask)
      (net 5 +12V))
    (model "../../../../../../Users/Michael/Desktop/HPMI/3D Cad Files/RP-1206S.wrl"
      (offset (xyz 0 0 1.193799982070923))
      (scale (xyz 0.393 0.393 0.393))
      (rotate (xyz 0 0 0))
    )
  )
  (module HPMI:LMB_Heeger_M10 locked (layer F.Cu) (tedit 5ED16501)
    (at 81.5 99.9)
    (fp_text reference H0 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Hole3 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -28.4) (size 9.6 9.6) (drill 4.72) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 1 thru_hole circle (at 0 28.2) (size 9.6 9.6) (drill 4.72) (layers *.Cu *.Mask)
      (net 1 GNDD))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 81.2 99.6 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "4.7 uF" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /6V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 81.2 103.1 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value "0.22 uF" (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 VGS))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HPMI:2_54mm_Edge_2x6 (layer F.Cu) (tedit 5E4DBB20)
    (at 58.4 106.35 90)
    (fp_text reference P1 (at 7.62 -3.81 90) (layer F.SilkS) hide)
    (fp_text value CONN_02X06 (at 6.35 -5.08 90) (layer F.Fab))
    (pad 12 smd rect (at 12.7 0 90) (size 1.5 5.9) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 10.16 0 90) (size 1.5 5.9) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 7.62 0 90) (size 1.5 5.9) (layers B.Cu B.Mask)
      (net 3 Trig+))
    (pad 6 smd rect (at 5.08 0 90) (size 1.5 5.9) (layers B.Cu B.Mask)
      (net 4 Trig-))
    (pad 4 smd rect (at 2.54 0 90) (size 1.5 5.9) (layers B.Cu B.Mask)
      (net 5 +12V))
    (pad 2 smd rect (at 0 0 90) (size 1.5 5.9) (layers B.Cu B.Mask)
      (net 5 +12V))
    (pad 11 smd rect (at 12.7 0 90) (size 1.5 5.9) (layers F.Cu F.Mask)
      (net 5 +12V))
    (pad 9 smd rect (at 10.16 0 90) (size 1.5 5.9) (layers F.Cu F.Mask)
      (net 5 +12V))
    (pad 7 smd rect (at 7.62 0 90) (size 1.5 5.9) (layers F.Cu F.Mask)
      (net 4 Trig-))
    (pad 5 smd rect (at 5.08 0 90) (size 1.5 5.9) (layers F.Cu F.Mask)
      (net 3 Trig+))
    (pad 3 smd rect (at 2.54 0 90) (size 1.5 5.9) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 0 90) (size 1.5 5.9) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module Housings_SOIC:SO-5_4.4x3.6mm_Pitch1.27mm (layer F.Cu) (tedit 591B43FE)
    (at 71.4 104.1)
    (descr "5-Lead Plastic Small Outline (SO), see https://docs.broadcom.com/cs/Satellite?blobcol=urldata&blobheader=application%2Fpdf&blobheadername1=Content-Disposition&blobheadername2=Content-Type&blobheadername3=MDT-Type&blobheadervalue1=attachment%3Bfilename%3DIPD-Selection-Guide_AV00-0254EN_030617.pdf&blobheadervalue2=application%2Fx-download&blobheadervalue3=abinary%253B%2Bcharset%253DUTF-8&blobkey=id&blobnocache=true&blobtable=MungoBlobs&blobwhere=1430884105675&ssbinary=true")
    (tags "SO SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0.1 -3.265) (layer F.SilkS))
    (fp_text value APS1551SX (at 0.05 3.385) (layer F.Fab))
    (fp_text user %R (at 0 -0.065) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -1.27) (size 2 0.64) (layers F.Cu F.Paste F.Mask)
      (net 3 Trig+))
    (pad 3 smd rect (at -3.15 1.27) (size 2 0.64) (layers F.Cu F.Paste F.Mask)
      (net 4 Trig-))
    (pad 4 smd rect (at 3.15 1.27) (size 2 0.64) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 5 smd rect (at 3.15 0) (size 2 0.64) (layers F.Cu F.Paste F.Mask)
      (net 12 /Opto_Out))
    (pad 6 smd rect (at 3.15 -1.27) (size 2 0.64) (layers F.Cu F.Paste F.Mask)
      (net 6 VGS))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SO-5_4.4x3.6mm_Pitch1.27mm.wrl
      (offset (xyz 0 0.01500000025472259 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HPMI:M-542CT (layer F.Cu) (tedit 5E4DEBDB)
    (at 85.9 99.6 270)
    (fp_text reference U4 (at 5 -3 270) (layer F.SilkS))
    (fp_text value M-542CT (at 4 -5 270) (layer F.Fab))
    (pad 5 smd rect (at 7.62 -7.75 270) (size 1.7 2.25) (layers F.Cu F.Paste F.Mask)
      (net 6 VGS))
    (pad 6 smd rect (at 5.08 -7.75 270) (size 1.7 2.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U4-Pad4)"))
    (pad 7 smd rect (at 2.54 -7.75 270) (size 1.7 2.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U4-Pad3)"))
    (pad 8 smd rect (at 0 -7.75 270) (size 1.7 2.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U4-Pad2)"))
    (pad 4 smd rect (at 7.62 0 270) (size 1.7 2.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U4-Pad4)"))
    (pad 3 smd rect (at 5.08 0 270) (size 1.7 2.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U4-Pad3)"))
    (pad 2 smd rect (at 2.54 0 270) (size 1.7 2.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U4-Pad2)"))
    (pad 1 smd rect (at 0 0 270) (size 1.7 2.25) (layers F.Cu F.Paste F.Mask)
      (net 10 /6V))
  )
  (module HPMI:M3_Hole (layer F.Cu) (tedit 5ED1797E)
    (at 70 128.2)
    (fp_text reference H1 (at 0 -4) (layer F.SilkS))
    (fp_text value Hole1 (at 0 -6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.5 6.5) (drill 3.3) (layers *.Cu *.Mask)
      (net 13 "Net-(H1-Pad1)"))
  )
  (module HPMI:M3_Hole (layer F.Cu) (tedit 5E503261)
    (at 70 71.5)
    (fp_text reference H2 (at 0 -4) (layer F.SilkS))
    (fp_text value Hole2 (at 0 -6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.5 6.5) (drill 3.3) (layers *.Cu *.Mask)
      (net 14 "Net-(H2-Pad1)"))
  )
  (module HPMI:SOT-223 (layer F.Cu) (tedit 58CE4E7E)
    (at 91.25 112.55 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at 0 -4.5 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDSD (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 6 VGS))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 VGS))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-323_SC-70 (layer F.Cu) (tedit 58CE4E7E)
    (at 91.1 119.55 180)
    (descr "SOT-323, SC-70")
    (tags "SOT-323 SC-70")
    (attr smd)
    (fp_text reference U5 (at -0.05 -1.95 180) (layer F.SilkS))
    (fp_text value BAT54CFILM (at -0.05 2.05 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.65 90) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 2 smd rect (at -1 0.65 90) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 3 smd rect (at 1 0 90) (size 0.45 0.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-323_SC-70.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module HPMI:MC74VHC540DWR2G (layer F.Cu) (tedit 5ECAC58B)
    (at 79.9 115.05)
    (fp_text reference U3 (at 0 0) (layer F.SilkS))
    (fp_text value MC74VHC540DWR2G (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user * (at -3.3655 -6.3246) (layer F.Fab))
    (fp_text user * (at -5.08 -7.3914) (layer F.SilkS))
    (fp_text user 0.063in/1.6mm (at -4.826 8.8138) (layer Dwgs.User))
    (fp_text user 0.38in/9.652mm (at 0 -8.8138) (layer Dwgs.User))
    (fp_text user 0.021in/0.533mm (at 7.874 -5.715) (layer Dwgs.User))
    (fp_text user 0.05in/1.27mm (at -7.874 -5.08) (layer Dwgs.User))
    (fp_text user * (at -3.3655 -6.3246) (layer F.Fab))
    (fp_text user * (at -5.08 -7.3914) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
    (pad 20 smd rect (at 4.826 -5.715) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 6 VGS))
    (pad 19 smd rect (at 4.826 -4.445) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 18 smd rect (at 4.826 -3.175) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (pad 17 smd rect (at 4.826 -1.905) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (pad 16 smd rect (at 4.826 -0.635) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (pad 15 smd rect (at 4.826 0.635) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (pad 14 smd rect (at 4.826 1.905) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (pad 13 smd rect (at 4.826 3.175) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (pad 12 smd rect (at 4.826 4.445) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (pad 11 smd rect (at 4.826 5.715) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 11 /ZVN_Gate))
    (pad 10 smd rect (at -4.826 5.715) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
    (pad 9 smd rect (at -4.826 4.445) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 /Opto_Out))
    (pad 8 smd rect (at -4.826 3.175) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 /Opto_Out))
    (pad 7 smd rect (at -4.826 1.905) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 /Opto_Out))
    (pad 6 smd rect (at -4.826 0.635) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 /Opto_Out))
    (pad 5 smd rect (at -4.826 -0.635) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 /Opto_Out))
    (pad 4 smd rect (at -4.826 -1.905) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 /Opto_Out))
    (pad 3 smd rect (at -4.826 -3.175) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 /Opto_Out))
    (pad 2 smd rect (at -4.826 -4.445) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 12 /Opto_Out))
    (pad 1 smd rect (at -4.826 -5.715) (size 1.6002 0.5334) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
  )
  (module HPMI:M3_Hole (layer F.Cu) (tedit 5E503261)
    (at 140 90)
    (fp_text reference H3 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value Hole3 (at 0 -6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.5 6.5) (drill 3.3) (layers *.Cu *.Mask)
      (net 15 "Net-(H3-Pad1)"))
  )
  (module HPMI:M3_Hole (layer F.Cu) (tedit 5ED1D876)
    (at 140 110)
    (fp_text reference H4 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value Hole4 (at 0 -6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.5 6.5) (drill 3.3) (layers *.Cu *.Mask)
      (net 16 "Net-(H4-Pad1)"))
  )
  (module HPMI:Anderson_PCB_Power_Contact_x1 (layer F.Cu) (tedit 5D4B2CC6)
    (at 141 72.5)
    (fp_text reference H5 (at -0.11 -3.26 180) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at -0.35 -4.64) (layer F.Fab))
    (pad 1 thru_hole oval (at -0.08 -0.01 90) (size 5 9) (drill oval 1.27 5.23) (layers *.Cu *.Mask)
      (net 17 Gan_Drain))
  )
  (module HPMI:Anderson_PCB_Power_Contact_x1 (layer F.Cu) (tedit 5D4B2CC6)
    (at 141 125.5)
    (fp_text reference H6 (at -0.11 -3.26 180) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at -0.35 -4.64) (layer F.Fab))
    (pad 1 thru_hole oval (at -0.08 -0.01 90) (size 5 9) (drill oval 1.27 5.23) (layers *.Cu *.Mask)
      (net 1 GNDD))
  )
  (module HPMI:GAN_GS66504B (layer F.Cu) (tedit 5D3F5D33)
    (at 106.45 99.83)
    (fp_text reference Q2 (at -4.7 0.5) (layer F.SilkS))
    (fp_text value GaNFET (at 0 -3.81) (layer F.Fab))
    (pad 1 smd rect (at 0 -3.91) (size 3.76 2.6) (layers F.Cu F.Paste F.Mask)
      (net 17 Gan_Drain))
    (pad 2 smd rect (at -3.13 1.81) (size 2.6 1) (layers F.Cu F.Paste F.Mask)
      (net 6 VGS))
    (pad 3 smd rect (at 0.55 2.67) (size 3.76 5.07) (layers F.Cu F.Paste F.Mask)
      (net 1 GNDD))
  )
  (module HPMI:Keystone_8199 (layer F.Cu) (tedit 5ED2D162)
    (at 120 90)
    (fp_text reference H7 (at 6 -3) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 5 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 10 0) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 17 Gan_Drain))
    (pad 1 thru_hole circle (at 5 0) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 17 Gan_Drain))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 17 Gan_Drain))
    (pad 1 thru_hole circle (at 0 -7) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 17 Gan_Drain))
    (pad 1 thru_hole circle (at 5 -7) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 17 Gan_Drain))
    (pad 1 thru_hole circle (at 10 -7) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 17 Gan_Drain))
  )
  (module HPMI:Keystone_8199 (layer F.Cu) (tedit 5ED2D162)
    (at 120 117)
    (fp_text reference H8 (at 6 -3) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 5 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 10 -7) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 1 thru_hole circle (at 5 -7) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 1 thru_hole circle (at 0 -7) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 1 thru_hole circle (at 0 0) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 1 thru_hole circle (at 5 0) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 1 GNDD))
    (pad 1 thru_hole circle (at 10 0) (size 4 4) (drill 1.93) (layers *.Cu *.Mask)
      (net 1 GNDD))
  )
  (gr_line (start 103.9 97.7) (end 109 97.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.9 99.5) (end 109 99.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 109 98.6) (end 109 99.5) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 103.9 98.6) (end 103.9 97.7) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148 131.2) (end 148 68.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 145 68.5) (end 148 68.5) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 145 131.2) (end 145 134.2) (angle -90) (layer Edge.Cuts) (width 0.15))
  (dimension 11.6 (width 0.15) (layer Dwgs.User)
    (gr_text "11.600 mm" (at 75.8 57.1) (layer Dwgs.User))
    (feature1 (pts (xy 81.6 71.5) (xy 81.6 57.813579)))
    (feature2 (pts (xy 70 71.5) (xy 70 57.813579)))
    (crossbar (pts (xy 70 58.4) (xy 81.6 58.4)))
    (arrow1a (pts (xy 81.6 58.4) (xy 80.473496 58.986421)))
    (arrow1b (pts (xy 81.6 58.4) (xy 80.473496 57.813579)))
    (arrow2a (pts (xy 70 58.4) (xy 71.126504 58.986421)))
    (arrow2b (pts (xy 70 58.4) (xy 71.126504 57.813579)))
  )
  (dimension 11.6 (width 0.15) (layer Dwgs.User)
    (gr_text "11.600 mm" (at 75.8 145.9) (layer Dwgs.User))
    (feature1 (pts (xy 81.6 128.2) (xy 81.6 145.186421)))
    (feature2 (pts (xy 70 128.2) (xy 70 145.186421)))
    (crossbar (pts (xy 70 144.6) (xy 81.6 144.6)))
    (arrow1a (pts (xy 81.6 144.6) (xy 80.473496 145.186421)))
    (arrow1b (pts (xy 81.6 144.6) (xy 80.473496 144.013579)))
    (arrow2a (pts (xy 70 144.6) (xy 71.126504 145.186421)))
    (arrow2b (pts (xy 70 144.6) (xy 71.126504 144.013579)))
  )
  (gr_line (start 68.5 134.2) (end 145 134.2) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 68.5 131.2) (end 65.5 131.2) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 68.5 65.5) (end 145 65.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 68.5 68.5) (end 68.5 65.5) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65.5 131.2) (end 65.5 107.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65.5 68.5) (end 65.5 92.6) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.35 102.15) (end 70.35 105.85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.75 105.85) (end 72.75 102.15) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 71.55 102.15) (end 70.35 102.15) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 71.55 105.85) (end 72.75 105.85) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 61.65 92.6) (end 65.5 92.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 65.5 107.35) (end 61.65 107.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 55.15 92.6) (end 61.65 92.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 55.15 107.35) (end 55.15 92.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 61.65 107.35) (end 55.15 107.35) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 98.7 139.95) (xy 73.924961 139.5) (xy 74.07504 64) (xy 98.7 64.45)
      )
    )
  )
  (zone (net 1) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.249921 114.800164) (xy 73.25 114.85) (xy 73.2 114.8)
      )
    )
  )
  (zone (net 1) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.075 64.15) (xy 98.7 63.95) (xy 98.7 139.45) (xy 73.925 139.65)
      )
    )
  )
  (zone (net 17) (net_name Gan_Drain) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.204)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.1 97.4) (xy 104.4 97.4) (xy 104.4 55.5) (xy 158.1 55.5)
      )
    )
  )
  (zone (net 1) (net_name GNDD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158 140.5) (xy 105 140.5) (xy 105 99.9) (xy 158 99.9)
      )
    )
  )
  (zone (net 17) (net_name Gan_Drain) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.1 55.5) (xy 104.4 55.5) (xy 104.4 97.4) (xy 158.1 97.4)
      )
    )
  )
  (zone (net 1) (net_name GNDD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158 99.935501) (xy 105 99.935501) (xy 105 140.535501) (xy 158 140.535501)
      )
    )
  )
)
