(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 241)
    (no_connects 0)
    (area 77.560714 60.96 198.35 152.476201)
    (thickness 1.6)
    (drawings 13)
    (tracks 785)
    (zones 0)
    (modules 52)
    (nets 57)
  )
  (page USLetter)
  (title_block
    (title "L-Star Simplified Software-Defined 6502 Computer")
    (date 2016-12-11)
    (rev 5B)
    (company "(C) 2016 Jac Goudsmit")
    (comment 1 "Open Source Hardware (MIT License)")
    (comment 2 https://github.com/JacGoudsmit/L-Star)
    (comment 3 https://hackaday.io/project/3620)
    (comment 4 https://l-star.org)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1524)
    (edge_width 0.0762)
    (via_size 0.635)
    (via_drill 0.508)
    (via_min_size 0.635)
    (via_min_drill 0.3302)
    (uvia_size 0.635)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.635)
    (uvia_min_drill 0.3302)
    (pcb_text_width 0.254)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.254)
    (mod_text_size 0.762 0.762)
    (mod_text_width 0.1524)
    (pad_size 3.5 3.5)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 87.63 66.675)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.152400)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Plot/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /SDA)
  (net 4 /CLK0/SCL)
  (net 5 /A14)
  (net 6 /A12)
  (net 7 /A7)
  (net 8 /A6)
  (net 9 /A5)
  (net 10 /A4)
  (net 11 /A3)
  (net 12 /A2)
  (net 13 /A1)
  (net 14 /A0)
  (net 15 /D0)
  (net 16 /D1)
  (net 17 /D2)
  (net 18 /D3)
  (net 19 /D4)
  (net 20 /D5)
  (net 21 /D6)
  (net 22 /D7)
  (net 23 /A10)
  (net 24 /A11)
  (net 25 /A9)
  (net 26 /A8)
  (net 27 /A13)
  (net 28 /R/~W)
  (net 29 /A15)
  (net 30 /RDY)
  (net 31 /~IRQ)
  (net 32 /~NMI)
  (net 33 /~SO)
  (net 34 /~RES6502)
  (net 35 /~RES)
  (net 36 "Net-(IC4-Pad30)")
  (net 37 "Net-(IC4-Pad31)")
  (net 38 /P25)
  (net 39 /KBDATA)
  (net 40 /P27)
  (net 41 /P30)
  (net 42 /P31)
  (net 43 /KBCLK)
  (net 44 "Net-(D1-PadA)")
  (net 45 /TVOUT)
  (net 46 /~RAMEN)
  (net 47 /~SYNC)
  (net 48 /P26)
  (net 49 /A16)
  (net 50 +3V3)
  (net 51 /VSUPPLY)
  (net 52 /VIN)
  (net 53 "Net-(P3-Pad5)")
  (net 54 "Net-(P3-Pad1)")
  (net 55 "Net-(P6-Pad2)")
  (net 56 /BE)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.635)
    (via_drill 0.508)
    (uvia_dia 0.635)
    (uvia_drill 0.508)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /BE)
    (add_net /CLK0/SCL)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /KBCLK)
    (add_net /KBDATA)
    (add_net /P25)
    (add_net /P26)
    (add_net /P27)
    (add_net /P30)
    (add_net /P31)
    (add_net /R/~W)
    (add_net /RDY)
    (add_net /SDA)
    (add_net /TVOUT)
    (add_net /~IRQ)
    (add_net /~NMI)
    (add_net /~RAMEN)
    (add_net /~RES)
    (add_net /~RES6502)
    (add_net /~SO)
    (add_net /~SYNC)
    (add_net "Net-(D1-PadA)")
    (add_net "Net-(IC4-Pad30)")
    (add_net "Net-(IC4-Pad31)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P3-Pad5)")
    (add_net "Net-(P6-Pad2)")
  )
  (net_class power ""
    (clearance 0.1524)
    (trace_width 0.381)
    (via_dia 1.524)
    (via_drill 0.762)
    (uvia_dia 1.524)
    (uvia_drill 0.762)
    (add_net +3V3)
    (add_net +5V)
    (add_net /VIN)
    (add_net /VSUPPLY)
    (add_net GND)
  )
  (module 00Jac:00JG-DIP-40__600 (layer F.Cu) (tedit 5758F9F9)
    (at 120.65 116.84 270)
    (descr "Module Dil 40 pins, pads ronds, e=600 mils")
    (tags DIL)
    (fp_text reference IC3 (at -12.7 0 270) (layer F.SilkS) hide)
    (fp_text value W65C02S6TPG-14 (at 12.7 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -24.13 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -21.59 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /RDY))
    (pad 3 thru_hole oval (at -19.05 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at -16.51 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /~IRQ))
    (pad 5 thru_hole oval (at -13.97 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at -11.43 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~NMI))
    (pad 7 thru_hole oval (at -8.89 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~SYNC))
    (pad 8 thru_hole oval (at -6.35 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 9 thru_hole oval (at -3.81 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A0))
    (pad 10 thru_hole oval (at -1.27 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A1))
    (pad 11 thru_hole oval (at 1.27 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A2))
    (pad 12 thru_hole oval (at 3.81 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A3))
    (pad 13 thru_hole oval (at 6.35 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A4))
    (pad 14 thru_hole oval (at 8.89 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A5))
    (pad 15 thru_hole oval (at 11.43 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A6))
    (pad 16 thru_hole oval (at 13.97 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A7))
    (pad 17 thru_hole oval (at 16.51 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A8))
    (pad 18 thru_hole oval (at 19.05 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A9))
    (pad 19 thru_hole oval (at 21.59 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A10))
    (pad 20 thru_hole oval (at 24.13 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A11))
    (pad 21 thru_hole oval (at 24.13 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 22 thru_hole oval (at 21.59 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A12))
    (pad 23 thru_hole oval (at 19.05 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A13))
    (pad 24 thru_hole oval (at 16.51 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A14))
    (pad 25 thru_hole oval (at 13.97 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A15))
    (pad 26 thru_hole oval (at 11.43 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /D7))
    (pad 27 thru_hole oval (at 8.89 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D6))
    (pad 28 thru_hole oval (at 6.35 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D5))
    (pad 29 thru_hole oval (at 3.81 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D4))
    (pad 30 thru_hole oval (at 1.27 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D3))
    (pad 31 thru_hole oval (at -1.27 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D2))
    (pad 32 thru_hole oval (at -3.81 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /D1))
    (pad 33 thru_hole oval (at -6.35 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D0))
    (pad 34 thru_hole oval (at -8.89 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /R/~W))
    (pad 35 thru_hole oval (at -11.43 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 36 thru_hole oval (at -13.97 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BE))
    (pad 37 thru_hole oval (at -16.51 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /CLK0/SCL))
    (pad 38 thru_hole oval (at -19.05 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /~SO))
    (pad 39 thru_hole oval (at -21.59 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 40 thru_hole oval (at -24.13 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~RES6502))
    (model Sockets_DIP/DIP-40__600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-RCAsocket (layer F.Cu) (tedit 57C282BC)
    (at 180.34 138.43 270)
    (descr RCJ-01X)
    (tags "RCA socket")
    (fp_text reference P6 (at 0 9.525 270) (layer F.SilkS) hide)
    (fp_text value "VIDEO OUT" (at 0 8.255 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 4.8 4.8) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at 5 4.5 270) (size 4.8 4.8) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -5 4.5 270) (size 4.8 4.8) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2.9 2.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(P6-Pad2)"))
  )
  (module 00Jac:00JG-OSHW-logo_silkscreen-front_7mm (layer F.Cu) (tedit 5350C5AA)
    (at 132.715 138.43 90)
    (fp_text reference U1 (at 0 3.71094 90) (layer F.SilkS) hide)
    (fp_text value "OSHW Logo" (at 0 -3.71094 90) (layer F.SilkS) hide)
  )
  (module 00Jac:00JG-NKK_CS12ANW03 (layer F.Cu) (tedit 57DDE44A)
    (at 95.885 94.615 90)
    (descr cs-6426.pdf)
    (tags "switch, slider switch, spdt")
    (fp_text reference SW3 (at -5.08 0 180) (layer F.SilkS) hide)
    (fp_text value <ON (at -4.445 -6.35 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -4.7 90) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 52 /VIN))
    (pad 2 thru_hole circle (at 0 0 90) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 51 /VSUPPLY))
    (pad 3 thru_hole circle (at 0 4.7 90) (size 3.5 3.5) (drill 1.6) (layers *.Cu *.Mask F.SilkS))
  )
  (module 00Jac:00JG-MountHoleM3 (layer F.Cu) (tedit 57DDE4D4)
    (at 91.44 142.875)
    (descr "Mount Hole")
    (tags Mechanical)
    (fp_text reference U2 (at -2.54 -2.54) (layer F.SilkS) hide)
    (fp_text value "Mount hole" (at 2.54 2.54) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 2.032) (solder_paste_margin -2.032) (clearance 2.032))
  )
  (module 00Jac:00JG-MountHoleM3 (layer F.Cu) (tedit 57DDE4FE)
    (at 167.64 70.485)
    (descr "Mount Hole")
    (tags Mechanical)
    (fp_text reference U4 (at -2.54 -2.54) (layer F.SilkS) hide)
    (fp_text value "Mount hole" (at 2.54 2.54) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 2.032) (solder_paste_margin -2.032) (clearance 2.032))
  )
  (module 00Jac:00JG-MountHoleM3 (layer F.Cu) (tedit 57DE41B9)
    (at 167.64 142.875)
    (descr "Mount Hole")
    (tags Mechanical)
    (fp_text reference U3 (at -2.54 -2.54) (layer F.SilkS) hide)
    (fp_text value "Mount hole" (at 2.54 2.54) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask F.SilkS)
      (solder_mask_margin 2.032) (solder_paste_margin -2.032) (clearance 2.032))
  )
  (module 00Jac:00JG-Pin_Header_Straight_1x08 (layer F.Cu) (tedit 5758D027)
    (at 184.15 81.28)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP5 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value P27 (at 0 19.685) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /KBCLK))
    (pad 2 thru_hole circle (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P27))
    (pad 3 thru_hole circle (at 0 5.08) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P27))
    (pad 4 thru_hole circle (at 0 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P27))
    (pad 5 thru_hole circle (at 0 10.16) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P27))
    (pad 6 thru_hole circle (at 0 12.7) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P27))
    (pad 7 thru_hole circle (at 0 15.24) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P27))
    (pad 8 thru_hole circle (at 0 17.78) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P27))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 00Jac:00JG-Pin_Header_Straight_1x08 (layer F.Cu) (tedit 575A3C53)
    (at 181.61 81.28)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP4 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value RDY/~SO~/~SYNC~/~NMI~/~IRQ~/~RES~/~RAM~/+3.3 (at 4.826 8.89 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole circle (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~RAMEN))
    (pad 3 thru_hole circle (at 0 5.08) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~RES6502))
    (pad 4 thru_hole circle (at 0 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /~IRQ))
    (pad 5 thru_hole circle (at 0 10.16) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~NMI))
    (pad 6 thru_hole circle (at 0 12.7) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~SYNC))
    (pad 7 thru_hole circle (at 0 15.24) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /~SO))
    (pad 8 thru_hole circle (at 0 17.78) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /RDY))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 00Jac:00JG-Pin_Header_Straight_1x08 (layer F.Cu) (tedit 5758D027)
    (at 179.07 81.28)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP3 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value P26 (at 0 19.685) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /KBDATA))
    (pad 2 thru_hole circle (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /P26))
    (pad 3 thru_hole circle (at 0 5.08) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /P26))
    (pad 4 thru_hole circle (at 0 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /P26))
    (pad 5 thru_hole circle (at 0 10.16) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /P26))
    (pad 6 thru_hole circle (at 0 12.7) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /P26))
    (pad 7 thru_hole circle (at 0 15.24) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /P26))
    (pad 8 thru_hole circle (at 0 17.78) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /P26))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 00Jac:00JG-Pin_Header_Straight_1x08 (layer F.Cu) (tedit 575A3C5F)
    (at 176.53 81.28)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value RDY/~SO~/~SYNC~/~NMI~/~IRQ~/~RES~/A16/GND (at -4.572 8.89 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /A16))
    (pad 3 thru_hole circle (at 0 5.08) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~RES6502))
    (pad 4 thru_hole circle (at 0 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /~IRQ))
    (pad 5 thru_hole circle (at 0 10.16) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~NMI))
    (pad 6 thru_hole circle (at 0 12.7) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~SYNC))
    (pad 7 thru_hole circle (at 0 15.24) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /~SO))
    (pad 8 thru_hole circle (at 0 17.78) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /RDY))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 00Jac:00JG-Pin_Header_Straight_1x08 (layer F.Cu) (tedit 5758D027)
    (at 173.99 81.28)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value P25 (at 0 19.685) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TVOUT))
    (pad 2 thru_hole circle (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /P25))
    (pad 3 thru_hole circle (at 0 5.08) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /P25))
    (pad 4 thru_hole circle (at 0 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /P25))
    (pad 5 thru_hole circle (at 0 10.16) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /P25))
    (pad 6 thru_hole circle (at 0 12.7) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /P25))
    (pad 7 thru_hole circle (at 0 15.24) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /P25))
    (pad 8 thru_hole circle (at 0 17.78) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /P25))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module 00Jac:00JG-BARREL_JACK_RAPC722X (layer F.Cu) (tedit 57DDDEEE)
    (at 119.38 64.77 180)
    (descr rapc722x_cd.pdf)
    (fp_text reference P7 (at 0 -19.8 180) (layer F.SilkS) hide)
    (fp_text value "7-15V 1.5A IN" (at -10.795 -3.175 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -13.74 180) (size 5.5 5.5) (drill 3.5) (layers *.Cu *.SilkS *.Mask)
      (net 52 /VIN))
    (pad 2 thru_hole circle (at 0 -7.49 180) (size 5.5 5.5) (drill 3) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 4.8 -10.74 180) (size 5.3 5.3) (drill 3) (layers *.Cu *.SilkS *.Mask))
  )
  (module 00Jac:00JG-DIP-8__300 (layer F.Cu) (tedit 5758F520)
    (at 147.32 74.93 270)
    (descr "8 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference IC1 (at 0 6.35 270) (layer F.SilkS) hide)
    (fp_text value 24LC512 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 3.81 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at -1.27 3.81 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 1.27 3.81 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 4 thru_hole oval (at 3.81 3.81 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 3.81 -3.81 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SDA))
    (pad 6 thru_hole oval (at 1.27 -3.81 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /CLK0/SCL))
    (pad 7 thru_hole oval (at -1.27 -3.81 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 8 thru_hole oval (at -3.81 -3.81 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (model Sockets_DIP/DIP-8__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 153.67 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R9 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~RES))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 161.29 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R6 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /P31))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 128.27 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R5 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 3K3 (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /~SO))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 138.43 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R4 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 3K3 (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~NMI))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 130.81 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R3 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 3K3 (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /~IRQ))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 125.73 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 3K3 (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /RDY))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 57C20EF0)
    (at 133.35 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R15 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(D1-PadA)"))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 175.26 107.95 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R14 (at 6.985 0 90) (layer F.SilkS) hide)
    (fp_text value 270 (at 0 0.127 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(P6-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TVOUT))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 185.42 107.95 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R13 (at 6.985 0 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 0.127 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P3-Pad5)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /KBCLK))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 180.34 107.95 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R12 (at 6.985 0 90) (layer F.SilkS) hide)
    (fp_text value 100 (at 0 0.127 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /KBDATA))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 182.88 107.95 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R11 (at 6.985 0 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 0.127 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P3-Pad5)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 177.8 107.95 90)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R10 (at 6.985 0 90) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 0.127 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 140.97 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 3K3 (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~RES6502))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 158.75 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R7 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SDA))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 156.21 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R8 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /CLK0/SCL))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-DIP-40__600 (layer F.Cu) (tedit 5758F9F9)
    (at 147.32 116.84 270)
    (descr "Module Dil 40 pins, pads ronds, e=600 mils")
    (tags DIL)
    (fp_text reference IC4 (at -12.7 0 270) (layer F.SilkS) hide)
    (fp_text value P8X32A (at 12.7 0 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -24.13 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D0))
    (pad 2 thru_hole oval (at -21.59 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /D1))
    (pad 3 thru_hole oval (at -19.05 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D2))
    (pad 4 thru_hole oval (at -16.51 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D3))
    (pad 5 thru_hole oval (at -13.97 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D4))
    (pad 6 thru_hole oval (at -11.43 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D5))
    (pad 7 thru_hole oval (at -8.89 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D6))
    (pad 8 thru_hole oval (at -6.35 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /D7))
    (pad 9 thru_hole oval (at -3.81 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 10 thru_hole oval (at -1.27 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole oval (at 1.27 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~RES))
    (pad 12 thru_hole oval (at 3.81 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 13 thru_hole oval (at 6.35 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A0))
    (pad 14 thru_hole oval (at 8.89 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A1))
    (pad 15 thru_hole oval (at 11.43 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A2))
    (pad 16 thru_hole oval (at 13.97 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A3))
    (pad 17 thru_hole oval (at 16.51 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A4))
    (pad 18 thru_hole oval (at 19.05 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A5))
    (pad 19 thru_hole oval (at 21.59 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A6))
    (pad 20 thru_hole oval (at 24.13 7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A7))
    (pad 21 thru_hole oval (at 24.13 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A8))
    (pad 22 thru_hole oval (at 21.59 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A9))
    (pad 23 thru_hole oval (at 19.05 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A10))
    (pad 24 thru_hole oval (at 16.51 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A11))
    (pad 25 thru_hole oval (at 13.97 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A12))
    (pad 26 thru_hole oval (at 11.43 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A13))
    (pad 27 thru_hole oval (at 8.89 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A14))
    (pad 28 thru_hole oval (at 6.35 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A15))
    (pad 29 thru_hole oval (at 3.81 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 30 thru_hole oval (at 1.27 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(IC4-Pad30)"))
    (pad 31 thru_hole oval (at -1.27 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(IC4-Pad31)"))
    (pad 32 thru_hole oval (at -3.81 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 33 thru_hole oval (at -6.35 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /R/~W))
    (pad 34 thru_hole oval (at -8.89 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /P25))
    (pad 35 thru_hole oval (at -11.43 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /P26))
    (pad 36 thru_hole oval (at -13.97 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P27))
    (pad 37 thru_hole oval (at -16.51 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 /CLK0/SCL))
    (pad 38 thru_hole oval (at -19.05 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SDA))
    (pad 39 thru_hole oval (at -21.59 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /P30))
    (pad 40 thru_hole oval (at -24.13 -7.62 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /P31))
    (model Sockets_DIP/DIP-40__600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-C1V5 (layer F.Cu) (tedit 57DDE3D2)
    (at 106.045 96.266)
    (fp_text reference C9 (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value 47u/16V (at 3.81 1.27 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret/C1V7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-C1V5 (layer F.Cu) (tedit 57F88CB1)
    (at 99.3775 87.63 270)
    (fp_text reference C8 (at 0 3.175 270) (layer F.SilkS) hide)
    (fp_text value 47u/16V (at 3.175 0.3175 540) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret/C1V7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-C1V5 (layer F.Cu) (tedit 57DDE3C7)
    (at 109.22 92.075)
    (fp_text reference C7 (at 0 3.175) (layer F.SilkS) hide)
    (fp_text value 47u/16V (at 3.175 -3.175) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /VSUPPLY))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret/C1V7.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-Pin_Header_Angled_1x04 (layer F.Cu) (tedit 575A391E)
    (at 173.99 73.66 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -6.35 0 270) (layer F.SilkS) hide)
    (fp_text value "PROP PLUG" (at 0 -11.43 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.27 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~RES))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /P31))
    (pad 4 thru_hole circle (at 3.81 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /P30))
    (model Pin_Headers/Pin_Header_Angled_1x04.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-PUSHBUTTON (layer F.Cu) (tedit 575A3F43)
    (at 147.32 85.09)
    (descr PTS645_13feb14.pdf)
    (tags PUSHBUTTON)
    (fp_text reference SW1 (at 0 4.445) (layer F.SilkS) hide)
    (fp_text value RESET (at 0 4.445) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.25 -2.25) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~RES))
    (pad 1 thru_hole circle (at 3.25 -2.25) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~RES))
    (pad 2 thru_hole circle (at -3.25 2.25) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3.25 2.25) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module 00Jac:00JG-PUSHBUTTON (layer F.Cu) (tedit 575A3F14)
    (at 120.65 85.09 180)
    (descr PTS645_13feb14.pdf)
    (tags PUSHBUTTON)
    (fp_text reference SW2 (at 0 4.445 180) (layer F.SilkS) hide)
    (fp_text value RESET6502 (at 0 -4.445 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -3.25 -2.25 180) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at 3.25 -2.25 180) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -3.25 2.25 180) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~RES6502))
    (pad 2 thru_hole circle (at 3.25 2.25 180) (size 2.032 2.032) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~RES6502))
  )
  (module 00Jac:00JG-LED5MM (layer F.Cu) (tedit 575A3FED)
    (at 133.985 85.09 270)
    (descr "LED 5mm - Lead pitch 100mil (2,54mm)")
    (tags "LED led 5mm 5MM 100mil 2,54mm")
    (fp_text reference D1 (at 0 -4.445 270) (layer F.SilkS) hide)
    (fp_text value POWER (at 4.445 0 360) (layer F.SilkS))
    (pad A thru_hole rect (at -1.27 0 270) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(D1-PadA)"))
    (pad K thru_hole circle (at 1.27 0 270) (size 2.032 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/leds/led5_vertical_verde.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-CapacitorMLCC (layer F.Cu) (tedit 575A45A1)
    (at 172.72 104.14 270)
    (descr C49e.pdf)
    (tags C)
    (fp_text reference C6 (at 3.81 0 270) (layer F.SilkS) hide)
    (fp_text value 470p (at 5.08 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.25 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TVOUT))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret/C1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-CapacitorMLCC (layer F.Cu) (tedit 57DE26A9)
    (at 90.17 134.62 270)
    (descr C49e.pdf)
    (tags C)
    (fp_text reference C5 (at 3.81 0 270) (layer F.SilkS) hide)
    (fp_text value 100n (at -4.445 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.25 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret/C1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-CapacitorMLCC (layer F.Cu) (tedit 57DDF13A)
    (at 110.49 109.22 90)
    (descr C49e.pdf)
    (tags C)
    (fp_text reference C4 (at 3.81 0 90) (layer F.SilkS) hide)
    (fp_text value 100n (at -5.08 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.25 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole circle (at 1.25 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret/C1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-CapacitorMLCC (layer F.Cu) (tedit 57DE182C)
    (at 157.48 114.3 270)
    (descr C49e.pdf)
    (tags C)
    (fp_text reference C3 (at 3.81 0 270) (layer F.SilkS) hide)
    (fp_text value 100n (at -5.08 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.25 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole circle (at 1.25 0 270) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret/C1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-CapacitorMLCC (layer F.Cu) (tedit 57DE1839)
    (at 137.16 119.38 90)
    (descr C49e.pdf)
    (tags C)
    (fp_text reference C2 (at 3.81 0 90) (layer F.SilkS) hide)
    (fp_text value 100n (at 4.445 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.25 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole circle (at 1.25 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret/C1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-CapacitorMLCC (layer F.Cu) (tedit 57DE1814)
    (at 147.32 68.58 180)
    (descr C49e.pdf)
    (tags C)
    (fp_text reference C1 (at 3.81 0 180) (layer F.SilkS) hide)
    (fp_text value 100n (at -4.445 0.635 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.25 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole circle (at 1.25 0 180) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Discret/C1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-Crystal_HC49-U_Vertical (layer F.Cu) (tedit 57DDF17C)
    (at 161.29 116.332 90)
    (descr "Crystal, Quarz, HC49/U, vertical, stehend,")
    (tags "Crystal, Quarz, HC49/U, vertical, stehend,")
    (fp_text reference X1 (at -7.493 0 90) (layer F.SilkS) hide)
    (fp_text value 5MHz (at 8.382 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.44094 0 90) (size 2.032 2.032) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(IC4-Pad30)"))
    (pad 2 thru_hole circle (at 2.44094 0 90) (size 2.032 2.032) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(IC4-Pad31)"))
  )
  (module 00Jac:00JG-Pin_Header_Straight_1x02 (layer F.Cu) (tedit 575A4934)
    (at 113.03 85.09 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP7 (at 3.81 0 270) (layer F.SilkS) hide)
    (fp_text value RESET6502 (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~RES6502))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-Pin_Header_Straight_1x02 (layer F.Cu) (tedit 575A4938)
    (at 154.94 85.09 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP6 (at 3.81 0 270) (layer F.SilkS) hide)
    (fp_text value RESET (at 0 2.54 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~RES))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-DIP-32__600 (layer F.Cu) (tedit 5758FD66)
    (at 100.33 119.38 90)
    (descr "32 pins DIL package, round pads")
    (tags DIL)
    (fp_text reference IC2 (at -10.16 0 90) (layer F.SilkS) hide)
    (fp_text value AS6C1008-55PCN (at 10.16 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at -16.51 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /A16))
    (pad 3 thru_hole oval (at -13.97 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A9))
    (pad 4 thru_hole oval (at -11.43 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A8))
    (pad 5 thru_hole oval (at -8.89 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A7))
    (pad 6 thru_hole oval (at -6.35 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A6))
    (pad 7 thru_hole oval (at -3.81 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A5))
    (pad 8 thru_hole oval (at -1.27 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A4))
    (pad 9 thru_hole oval (at 1.27 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A3))
    (pad 10 thru_hole oval (at 3.81 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A2))
    (pad 11 thru_hole oval (at 6.35 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A1))
    (pad 12 thru_hole oval (at 8.89 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A0))
    (pad 13 thru_hole oval (at 11.43 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D2))
    (pad 14 thru_hole oval (at 13.97 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /D1))
    (pad 15 thru_hole oval (at 16.51 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D0))
    (pad 16 thru_hole oval (at 19.05 7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 17 thru_hole oval (at 19.05 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D3))
    (pad 18 thru_hole oval (at 16.51 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D4))
    (pad 19 thru_hole oval (at 13.97 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D5))
    (pad 20 thru_hole oval (at 11.43 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D6))
    (pad 21 thru_hole oval (at 8.89 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 /D7))
    (pad 22 thru_hole oval (at 6.35 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~RAMEN))
    (pad 23 thru_hole oval (at 3.81 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A14))
    (pad 24 thru_hole oval (at 1.27 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 25 thru_hole oval (at -1.27 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A13))
    (pad 26 thru_hole oval (at -3.81 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A12))
    (pad 27 thru_hole oval (at -6.35 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A10))
    (pad 28 thru_hole oval (at -8.89 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A11))
    (pad 29 thru_hole oval (at -11.43 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 /R/~W))
    (pad 30 thru_hole oval (at -13.97 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 31 thru_hole oval (at -16.51 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A15))
    (pad 32 thru_hole oval (at -19.05 -7.62 90) (size 1.524 2.032) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (model Sockets_DIP/DIP-32__600.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-R400 (layer F.Cu) (tedit 5758F6D7)
    (at 135.89 74.93 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R16 (at 6.985 0 270) (layer F.SilkS) hide)
    (fp_text value 3K3 (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole oval (at -5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 2.032 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BE))
    (model Discret/R3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-MiniDin6 (layer F.Cu) (tedit 57C14179)
    (at 187.96 123.825 270)
    (descr ENG_CD_5749266_O.pdf)
    (tags "MINI DIN")
    (fp_text reference P3 (at 0 15.875 270) (layer F.SilkS) hide)
    (fp_text value "PS/2 KBD" (at 0 15.875 270) (layer F.SilkS))
    (pad 3 thru_hole circle (at 6.76 5.51 270) (size 3.81 3.81) (drill 2.4) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at -6.76 5.51 270) (size 3.81 3.81) (drill 2.4) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at -3.4 8.5 270) (size 1.778 2.032) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at -3.4 11 270) (size 1.778 2.032) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P3-Pad5)"))
    (pad 4 thru_hole oval (at 3.4 8.5 270) (size 1.778 2.032) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole circle (at 0 4.7 270) (size 3.81 3.81) (drill 2.4) (layers *.Cu *.SilkS *.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at 3.4 11 270) (size 1.778 2.032) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at -1.3 8.5 270) (size 1.778 2.032) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 1.3 8.5 270) (size 1.778 2.032) (drill 1.1) (layers *.Cu *.Mask F.SilkS))
  )
  (module 00Jac:00JG-TO-220_Neutral123_Horizontal_LargePads-Heatsink (layer F.Cu) (tedit 57F88CA7)
    (at 105.41 87.63)
    (descr "TO-220, Neutral, Horizontal, Large Pads,")
    (tags "TO-220, Neutral, Horizontal, Large Pads,")
    (fp_text reference IC5 (at 0.24892 -22.84984) (layer F.SilkS) hide)
    (fp_text value LM1086-5.0 (at 0 2.54 180) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V) (clearance 0.635) (zone_connect 1))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 51 /VSUPPLY))
    (pad 2 thru_hole rect (at 0 -16.764 90) (size 16.51 10.668) (drill 3.79984 (offset -4.572 0)) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (model Transistors_TO-220/TO-220_Neutral123_Horizontal_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-TO-220_Neutral123_Horizontal_LargePads-Heatsink (layer F.Cu) (tedit 57F88CBC)
    (at 93.345 87.63)
    (descr "TO-220, Neutral, Horizontal, Large Pads,")
    (tags "TO-220, Neutral, Horizontal, Large Pads,")
    (fp_text reference IC6 (at 0.24892 -22.84984) (layer F.SilkS) hide)
    (fp_text value LM1086-3.3 (at 0 2.54) (layer F.SilkS))
    (pad 2 thru_hole oval (at 0 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3) (clearance 0.635) (zone_connect 1))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 3.50012 1.69926) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole rect (at 0 -16.764 90) (size 16.51 10.668) (drill 3.79984 (offset -4.572 0)) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (model Transistors_TO-220/TO-220_Neutral123_Horizontal_LargePads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module 00Jac:00JG-Pin_Header_Straight_2x25 (layer F.Cu) (tedit 57C29F1E)
    (at 166.37 76.2)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 1.27 -2.54) (layer F.SilkS) hide)
    (fp_text value EXPANSION (at -2.54 2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /A16))
    (pad 2 thru_hole oval (at 2.54 0) (size 2.032 1.778) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /~RES))
    (pad 3 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /~RAMEN))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /KBCLK))
    (pad 5 thru_hole oval (at 0 5.08) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /BE))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /KBDATA))
    (pad 7 thru_hole oval (at 0 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /RDY))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /TVOUT))
    (pad 9 thru_hole oval (at 0 10.16) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 +3V3))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole oval (at 0 12.7) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /~RES6502))
    (pad 13 thru_hole oval (at 0 15.24) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /~NMI))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /~IRQ))
    (pad 15 thru_hole oval (at 0 17.78) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /~SO))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /~SYNC))
    (pad 17 thru_hole oval (at 0 20.32) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /D0))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /P31))
    (pad 19 thru_hole oval (at 0 22.86) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /D1))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /P30))
    (pad 21 thru_hole oval (at 0 25.4) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D2))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /SDA))
    (pad 23 thru_hole oval (at 0 27.94) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D3))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /CLK0/SCL))
    (pad 25 thru_hole oval (at 0 30.48) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D4))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /P27))
    (pad 27 thru_hole oval (at 0 33.02) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D5))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /P26))
    (pad 29 thru_hole oval (at 0 35.56) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D6))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /P25))
    (pad 31 thru_hole oval (at 0 38.1) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /D7))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /R/~W))
    (pad 33 thru_hole oval (at 0 40.64) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /A0))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A15))
    (pad 35 thru_hole oval (at 0 43.18) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /A1))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /A14))
    (pad 37 thru_hole oval (at 0 45.72) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /A2))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /A13))
    (pad 39 thru_hole oval (at 0 48.26) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /A3))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A12))
    (pad 41 thru_hole oval (at 0 50.8) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /A4))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /A11))
    (pad 43 thru_hole oval (at 0 53.34) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A5))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /A10))
    (pad 45 thru_hole oval (at 0 55.88) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A6))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /A9))
    (pad 47 thru_hole oval (at 0 58.42) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A7))
    (pad 48 thru_hole oval (at 2.54 58.42) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /A8))
    (pad 49 thru_hole oval (at 0 60.96) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 50 thru_hole oval (at 2.54 60.96) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x25.wrl
      (at (xyz 0.05 -1.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (dimension 80.01 (width 0.254) (layer Dwgs.User)
    (gr_text "3.1500 in" (at 83.185 106.68 90) (layer Dwgs.User))
    (feature1 (pts (xy 86.995 66.675) (xy 81.915 66.675)))
    (feature2 (pts (xy 86.995 146.685) (xy 81.915 146.685)))
    (crossbar (pts (xy 84.455 146.685) (xy 84.455 66.675)))
    (arrow1a (pts (xy 84.455 66.675) (xy 85.041421 67.801504)))
    (arrow1b (pts (xy 84.455 66.675) (xy 83.868579 67.801504)))
    (arrow2a (pts (xy 84.455 146.685) (xy 85.041421 145.558496)))
    (arrow2b (pts (xy 84.455 146.685) (xy 83.868579 145.558496)))
  )
  (dimension 99.695 (width 0.254) (layer Dwgs.User)
    (gr_text "99.695 mm" (at 137.4775 151.13) (layer Dwgs.User))
    (feature1 (pts (xy 187.325 147.32) (xy 187.325 152.4)))
    (feature2 (pts (xy 87.63 147.32) (xy 87.63 152.4)))
    (crossbar (pts (xy 87.63 149.86) (xy 187.325 149.86)))
    (arrow1a (pts (xy 187.325 149.86) (xy 186.198496 150.446421)))
    (arrow1b (pts (xy 187.325 149.86) (xy 186.198496 149.273579)))
    (arrow2a (pts (xy 87.63 149.86) (xy 88.756504 150.446421)))
    (arrow2b (pts (xy 87.63 149.86) (xy 88.756504 149.273579)))
  )
  (dimension 99.695 (width 0.254) (layer Dwgs.User)
    (gr_text "3.9250 in" (at 137.4775 62.23) (layer Dwgs.User))
    (feature1 (pts (xy 187.325 66.04) (xy 187.325 60.96)))
    (feature2 (pts (xy 87.63 66.04) (xy 87.63 60.96)))
    (crossbar (pts (xy 87.63 63.5) (xy 187.325 63.5)))
    (arrow1a (pts (xy 187.325 63.5) (xy 186.198496 64.086421)))
    (arrow1b (pts (xy 187.325 63.5) (xy 186.198496 62.913579)))
    (arrow2a (pts (xy 87.63 63.5) (xy 88.756504 64.086421)))
    (arrow2b (pts (xy 87.63 63.5) (xy 88.756504 62.913579)))
  )
  (gr_line (start 87.63 146.685) (end 87.63 66.675) (angle 90) (layer Edge.Cuts) (width 0.0762))
  (gr_line (start 187.325 146.685) (end 87.63 146.685) (angle 90) (layer Edge.Cuts) (width 0.0762))
  (gr_line (start 187.325 66.675) (end 187.325 146.685) (angle 90) (layer Edge.Cuts) (width 0.0762))
  (gr_line (start 87.63 66.675) (end 187.325 66.675) (angle 90) (layer Edge.Cuts) (width 0.0762))
  (dimension 80.01 (width 0.3) (layer Dwgs.User)
    (gr_text "80.010 mm" (at 191.85 106.68 90) (layer Dwgs.User))
    (feature1 (pts (xy 187.96 66.675) (xy 193.2 66.675)))
    (feature2 (pts (xy 187.96 146.685) (xy 193.2 146.685)))
    (crossbar (pts (xy 190.5 146.685) (xy 190.5 66.675)))
    (arrow1a (pts (xy 190.5 66.675) (xy 191.086421 67.801504)))
    (arrow1b (pts (xy 190.5 66.675) (xy 189.913579 67.801504)))
    (arrow2a (pts (xy 190.5 146.685) (xy 191.086421 145.558496)))
    (arrow2b (pts (xy 190.5 146.685) (xy 189.913579 145.558496)))
  )
  (gr_text "L-STAR PLUS rev 5\n(C) 2016 Jac Goudsmit\nhttps://www.L-Star.org" (at 132.715 132.08 90) (layer F.SilkS))
  (zone (net 50) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 187.325 146.685) (xy 87.757 146.685) (xy 87.757 85.09) (xy 111.76 85.09) (xy 111.76 66.675)
        (xy 187.325 66.675)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 187.325 146.685) (xy 87.757 146.685) (xy 87.757 85.09) (xy 111.76 85.09) (xy 111.76 66.675)
        (xy 187.325 66.675)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 95.25 140.97) (xy 95.25 144.78) (xy 105.41 144.78) (xy 105.41 140.97)
      )
    )
  )
)
