(kicad_pcb (version 4) (host pcbnew 4.0.2-1.fc23-product)
  (general
    (links 7)
    (no_connects 0)
    (area 101.854 71.882 144.272 104.394)
    (thickness 1.6)
    (drawings 72)
    (tracks 82)
    (zones 0)
    (modules 3)
    (nets 35)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad0)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J1-Pad5)")
  (net 7 "Net-(J1-Pad6)")
  (net 8 "Net-(J1-Pad7)")
  (net 9 "Net-(J1-Pad8)")
  (net 10 "Net-(J1-Pad17A)")
  (net 11 "Net-(J1-Pad3V1)")
  (net 12 "Net-(J1-PadG2)")
  (net 13 "Net-(J1-PadPGM)")
  (net 14 "Net-(J1-PadDAC)")
  (net 15 "Net-(J1-Pad16)")
  (net 16 "Net-(J1-Pad18)")
  (net 17 "Net-(J1-Pad17)")
  (net 18 "Net-(J1-PadG3)")
  (net 19 "Net-(J1-Pad22)")
  (net 20 "Net-(J1-PadVIN)")
  (net 21 "Net-(J1-Pad21)")
  (net 22 "Net-(J1-Pad20)")
  (net 23 "Net-(J1-Pad19)")
  (net 24 "Net-(J1-Pad23)")
  (net 25 "Net-(J1-Pad14)")
  (net 26 "Net-(J1-Pad15)")
  (net 27 "Net-(J2-Pad7)")
  (net 28 /OLED_GND)
  (net 29 /MOSI)
  (net 30 /CLK)
  (net 31 /DC)
  (net 32 /CS)
  (net 33 /OLED_VIN)
  (net 34 /RST)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CLK)
    (add_net /CS)
    (add_net /DC)
    (add_net /MOSI)
    (add_net /OLED_GND)
    (add_net /OLED_VIN)
    (add_net /RST)
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad17)")
    (add_net "Net-(J1-Pad17A)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad3V1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadG2)")
    (add_net "Net-(J1-PadG3)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(J2-Pad7)")
  )
  (module Symbols:Symbol_OSHW-Logo_CopperTop (layer B.Cu) (tedit 573A94FB)
    (at 107.95 93.98 180)
    (descr "Symbol, OSHW-Logo, Copper Top,")
    (tags "Symbol, OSHW-Logo, Copper Top,")
    (fp_text reference "" (at 0.09906 4.38912 180) (layer B.SilkS))
    (fp_text value "" (at 0.30988 -6.56082 180) (layer B.Fab))
  )
  (module TEENSY-LC (layer F.Cu) (tedit 573A94F4)
    (at 115.824 89.916 90)
    (fp_text reference "" (at -2.032 -9.906 90) (layer F.SilkS))
    (fp_text value TEENSY-LC (at -2.54 20.32 270) (layer F.Fab))
    (pad G1 thru_hole circle (at -10.16 -10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /OLED_GND))
    (pad 0 thru_hole circle (at -10.16 -7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /MOSI))
    (pad 10 thru_hole circle (at -10.16 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CLK))
    (pad 11 thru_hole circle (at -10.16 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /DC))
    (pad 12 thru_hole circle (at -10.16 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /CS))
    (pad 17A thru_hole circle (at -7.62 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad17A)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad3V1)"))
    (pad G2 thru_hole circle (at -2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-PadG2)"))
    (pad PGM thru_hole circle (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /RST))
    (pad 16 thru_hole circle (at 5.08 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad16)"))
    (pad 3V2 thru_hole circle (at 5.08 -5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /OLED_VIN))
    (pad 18 thru_hole circle (at 5.08 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 5.08 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad17)"))
    (pad G3 thru_hole circle (at 5.08 -7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-PadG3)"))
    (pad 22 thru_hole circle (at 5.08 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J1-Pad19)"))
    (pad 23 thru_hole circle (at 5.08 -2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at 5.08 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J1-Pad15)"))
  )
  (module Wickerlib:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 0)
    (at 112.776 77.724 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value OLED (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /CS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /RST))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /DC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /CLK))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /MOSI))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /OLED_VIN))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(J2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /OLED_GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text drew@oshpark.com (at 122.428 102.616) (layer F.Mask))
  (gr_text "DREW FUSTINI" (at 120.396 97.282) (layer F.SilkS))
  (gr_text "DREW FUSTINI" (at 120.396 97.282) (layer B.SilkS))
  (gr_text drew@oshpark.com (at 122.428 102.616) (layer F.SilkS))
  (gr_circle (center 110.236 73.66) (end 110.744 74.422) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 133.35 73.66) (end 132.588 73.152) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.108 100.838) (end 102.108 98.806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.664 104.394) (end 102.108 100.838) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.95 104.394) (end 105.664 104.394) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.272 99.06) (end 144.272 90.678) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.938 104.394) (end 144.272 99.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.188 104.394) (end 138.938 104.394) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.108 78.74) (end 102.108 99.314) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108.712 72.136) (end 102.108 78.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.858 72.136) (end 108.712 72.136) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.272 82.55) (end 133.858 72.136) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.272 90.932) (end 144.272 82.55) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.156 101.6) (xy 111.506 101.6) (xy 111.506 104.14) (xy 105.918 104.14) (xy 104.902 103.124)
        (xy 104.902 101.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.604 102.108) (xy 139.446 102.108) (xy 139.446 103.124) (xy 138.938 103.632) (xy 138.684 103.886)
        (xy 133.604 103.886)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.252 93.472) (xy 111.252 98.552) (xy 105.41 98.552) (xy 104.648 98.298) (xy 104.648 92.964)
        (xy 105.156 92.71) (xy 106.68 91.186) (xy 108.966 91.186) (xy 111.252 93.472)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.174 98.298) (xy 128.27 98.298) (xy 128.27 96.012) (xy 122.174 96.012)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 112.776 96.012) (xy 119.126 96.012) (xy 119.126 98.298) (xy 112.776 98.298)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.87 78.74) (xy 105.41 78.74) (xy 105.41 81.534) (xy 102.87 81.534)
      )
    )
  )
)
