(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 520)
    (zones 0)
    (modules 32)
    (nets 58)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.254000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 D2)
  (net 2 LG)
  (net 3 LH)
  (net 4 D5)
  (net 5 LA)
  (net 6 LB)
  (net 7 LC)
  (net 8 LD)
  (net 9 LE)
  (net 10 LF)
  (net 11 GND)
  (net 12 5V)
  (net 13 VCC)
  (net 14 SRCLK)
  (net 15 RCLK)
  (net 16 OE)
  (net 17 SER)
  (net 18 10)
  (net 19 11)
  (net 20 "Net-(J1-Pad10)")
  (net 21 14)
  (net 22 15)
  (net 23 16)
  (net 24 17)
  (net 25 18)
  (net 26 19)
  (net 27 20)
  (net 28 21)
  (net 29 22)
  (net 30 23)
  (net 31 BH)
  (net 32 "Net-(R1-Pad2)")
  (net 33 "Net-(R2-Pad2)")
  (net 34 "Net-(R3-Pad2)")
  (net 35 "Net-(R4-Pad2)")
  (net 36 "Net-(R5-Pad2)")
  (net 37 "Net-(R6-Pad2)")
  (net 38 "Net-(R7-Pad2)")
  (net 39 "Net-(R8-Pad2)")
  (net 40 D4)
  (net 41 BG)
  (net 42 BA)
  (net 43 "Net-(U1-Pad9)")
  (net 44 BF)
  (net 45 BE)
  (net 46 BD)
  (net 47 BC)
  (net 48 BB)
  (net 49 "Net-(U2-Pad9)")
  (net 50 "Net-(U3-Pad1)")
  (net 51 D0)
  (net 52 D1)
  (net 53 D3)
  (net 54 D6)
  (net 55 D7)
  (net 56 "Net-(U3-Pad18)")
  (net 57 "Net-(U3-Pad20)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 10)
    (add_net 11)
    (add_net 14)
    (add_net 15)
    (add_net 16)
    (add_net 17)
    (add_net 18)
    (add_net 19)
    (add_net 20)
    (add_net 21)
    (add_net 22)
    (add_net 23)
    (add_net 5V)
    (add_net BA)
    (add_net BB)
    (add_net BC)
    (add_net BD)
    (add_net BE)
    (add_net BF)
    (add_net BG)
    (add_net BH)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net GND)
    (add_net LA)
    (add_net LB)
    (add_net LC)
    (add_net LD)
    (add_net LE)
    (add_net LF)
    (add_net LG)
    (add_net LH)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad18)")
    (add_net "Net-(U3-Pad20)")
    (add_net OE)
    (add_net RCLK)
    (add_net SER)
    (add_net SRCLK)
    (add_net VCC)
  )
  (module AOR_custom:AOR_LOGO (layer F.Cu) (tedit 5C26ADAA)
    (at 153.924 98.552)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC11819)
    (at 177.546 52.324)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC11819)
    (at 146.812 46.736)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC11819)
    (at 158.496 103.886)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 171.956 46.99)
    (fp_text reference D1 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D2))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 LG))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 171.956 57.658)
    (fp_text reference D2 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 LH))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 D2))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 128.4986 88.6968)
    (fp_text reference D3 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D5))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 LA))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 138.54176 88.6968)
    (fp_text reference D4 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 LB))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D5))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 148.58492 88.6968)
    (fp_text reference D5 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D5))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 LC))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 158.62808 88.6968)
    (fp_text reference D6 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 LD))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D5))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 168.67124 88.6968)
    (fp_text reference D7 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D5))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 LE))
  )
  (module "AOR_custom:WL-SMTW SMD LED" (layer F.Cu) (tedit 5C2849BC)
    (at 178.7144 88.6968)
    (fp_text reference D8 (at 0 -2.3) (layer F.SilkS))
    (fp_text value LED (at 0.1 2.5) (layer F.Fab))
    (pad 2 smd roundrect (at 1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 LF))
    (pad 1 smd roundrect (at -1.425 0) (size 1.6 2.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 D5))
  )
  (module Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical (layer B.Cu) (tedit 59DE0251)
    (at 129.794 82.042)
    (descr "Through hole straight IDC box header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole IDC box header THT 2x10 2.54mm double row")
    (fp_text reference J1 (at 1.27 6.604) (layer B.SilkS))
    (fp_text value Conn_01x20 (at 1.27 -29.464) (layer B.Fab))
    (fp_text user %R (at 1.27 -11.43) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 5V))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 VCC))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 SRCLK))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 RCLK))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 OE))
    (pad 7 thru_hole oval (at 0 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 SER))
    (pad 8 thru_hole oval (at 2.54 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 10))
    (pad 9 thru_hole oval (at 0 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 11))
    (pad 10 thru_hole oval (at 2.54 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 14))
    (pad 12 thru_hole oval (at 2.54 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 15))
    (pad 13 thru_hole oval (at 0 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 16))
    (pad 14 thru_hole oval (at 2.54 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 17))
    (pad 15 thru_hole oval (at 0 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 18))
    (pad 16 thru_hole oval (at 2.54 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 19))
    (pad 17 thru_hole oval (at 0 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 20))
    (pad 18 thru_hole oval (at 2.54 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 21))
    (pad 19 thru_hole oval (at 0 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 22))
    (pad 20 thru_hole oval (at 2.54 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 23))
    (model ${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 128.016 94.488 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value Conn_01x02 (at 0 -4.87 180) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 140.97 58.166 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 0 2.33 270) (layer B.SilkS))
    (fp_text value Conn_01x06 (at 0 -15.03 270) (layer B.Fab))
    (fp_text user %R (at 0 -6.35 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 GND))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 VCC))
    (pad 3 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 16))
    (pad 4 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 17))
    (pad 5 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 BH))
    (pad 6 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 10))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5B391E66)
    (at 137.668 65.024 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -2.032 270) (layer B.SilkS))
    (fp_text value SolderJumper_2_Open (at 0 -1.9 270) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 13 VCC) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 20 "Net-(J1-Pad10)") (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.622 64.262)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -3.302 -0.254) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 LA))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 32 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.622 66.802)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -3.302 -0.254) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 33 "Net-(R2-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 LB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.622 69.342)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -3.302 -0.254) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 LC))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 34 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.622 71.882)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -3.302 -0.254) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 35 "Net-(R4-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 LD))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.622 74.422)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -3.302 -0.254) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 LE))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 36 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.622 76.962)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -3.302 -0.254) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 37 "Net-(R6-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 LF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.622 79.502)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -3.302 -0.254) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 LG))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 38 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.622 82.042)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -3.302 0) (layer F.SilkS))
    (fp_text value 100 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 39 "Net-(R8-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 LH))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 136.398 48.768)
    (fp_text reference SW1 (at -7.112 -4.064) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 18 10) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 LG))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 D4))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 41 BG) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 139.0142 101.981)
    (fp_text reference SW2 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 LG))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 D5))
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 41 BG) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
  )
  (module AOR_custom:Adafruit_10mm_elast_w_LED (layer F.Cu) (tedit 5C282F1B)
    (at 169.0116 101.981)
    (fp_text reference SW3 (at -0.1 -6.35) (layer F.SilkS))
    (fp_text value SW_Push_LED (at 0 7.62) (layer F.SilkS) hide)
    (pad 1 smd custom (at -5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 31 BH) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start 5.08 2.794) (end 5.08 4.191) (width 0.4))
        (gr_line (start 2.413 0) (end 2.7178 1.27) (width 0.4))
        (gr_line (start 2.7178 1.27) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.4168 -1.27) (end 6.3754 -2.286) (width 0.4))
        (gr_line (start 2.9972 3.6068) (end 3.7084 2.3368) (width 0.4))
        (gr_line (start 7.2136 -3.5814) (end 6.3754 -2.2606) (width 0.4))
        (gr_line (start 7.1882 3.6068) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 2.413 0) (end 0 0) (width 0.4))
        (gr_line (start 7.747 0) (end 9.271 0) (width 0.4))
        (gr_line (start 8.6868 2.1082) (end 7.366 1.397) (width 0.4))
        (gr_line (start 8.7122 -2.032) (end 7.3914 -1.27) (width 0.4))
        (gr_line (start 2.9718 -3.556) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 1.4478 -2.1082) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 3.7084 2.3368) (end 5.0546 2.7686) (width 0.4))
        (gr_line (start 5.0546 2.7686) (end 6.4008 2.3622) (width 0.4))
        (gr_line (start 7.3406 1.4224) (end 7.747 0) (width 0.4))
        (gr_line (start 6.3754 -2.286) (end 5.08 -2.667) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 3.7846 -2.286) (width 0.4))
        (gr_line (start 5.08 -2.667) (end 5.08 -4.064) (width 0.4))
        (gr_line (start 1.4478 2.0828) (end 2.7178 1.2954) (width 0.4))
        (gr_line (start 6.4008 2.3622) (end 7.3406 1.4224) (width 0.4))
        (gr_line (start 3.7846 -2.286) (end 2.794 -1.3208) (width 0.4))
        (gr_line (start 2.794 -1.3208) (end 2.3876 -0.0254) (width 0.4))
      ))
    (pad 3 thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 D5))
    (pad 4 thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 LH))
    (pad 2 smd custom (at 5.08 0) (size 0.4 0.4) (layers F.Cu F.Mask)
      (net 19 11) (zone_connect 0)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_line (start -7.5438 -2.4892) (end -8.6868 -3.556) (width 0.4))
        (gr_line (start -5.969 -3.4036) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -4.1656 -3.4544) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -1.6256 0.9652) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -4.1656 3.4544) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -8.4582 -0.8382) (end -10.0076 -1.2954) (width 0.4))
        (gr_line (start -2.6162 2.4638) (end -1.5494 3.5814) (width 0.4))
        (gr_line (start -1.6256 -0.8636) (end -0.2032 -1.2954) (width 0.4))
        (gr_line (start -2.5654 -2.4892) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start 0 0) (end -0.1778 1.3716) (width 0.4))
        (gr_line (start -0.2032 -1.3208) (end 0 0) (width 0.4))
        (gr_line (start -0.1778 1.3716) (end -0.635 2.4638) (width 0.4))
        (gr_line (start -0.635 2.4638) (end -1.524 3.5814) (width 0.4))
        (gr_line (start -1.524 3.5814) (end -2.4892 4.3434) (width 0.4))
        (gr_line (start -3.7338 4.8514) (end -5.08 5.0546) (width 0.4))
        (gr_line (start -2.4892 4.3434) (end -3.7338 4.8514) (width 0.4))
        (gr_line (start -5.08 5.0546) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -7.62 -4.3942) (end -6.4262 -4.8514) (width 0.4))
        (gr_line (start -6.4262 -4.8514) (end -5.08 -5.0292) (width 0.4))
        (gr_line (start -5.08 -5.0292) (end -3.7592 -4.8006) (width 0.4))
        (gr_line (start -3.7592 -4.8006) (end -2.5654 -4.2926) (width 0.4))
        (gr_line (start -1.5494 -3.4798) (end -0.6858 -2.4638) (width 0.4))
        (gr_line (start -2.5654 -4.2926) (end -1.5494 -3.4798) (width 0.4))
        (gr_line (start -0.6858 -2.4638) (end -0.2032 -1.3208) (width 0.4))
        (gr_line (start -6.4008 4.8768) (end -7.5946 4.3688) (width 0.4))
        (gr_line (start -7.5946 4.3688) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -8.6868 3.556) (end -9.4996 2.54) (width 0.4))
        (gr_line (start -9.4996 2.54) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -10.0076 -1.2954) (end -9.4488 -2.5146) (width 0.4))
        (gr_line (start -9.4488 -2.5146) (end -8.7122 -3.5814) (width 0.4))
        (gr_line (start -7.62 2.5146) (end -8.6868 3.556) (width 0.4))
        (gr_line (start -6.0198 3.5052) (end -6.4008 4.8768) (width 0.4))
        (gr_line (start -8.5344 0.9398) (end -10.033 1.3462) (width 0.4))
        (gr_line (start -8.7122 -3.5814) (end -7.62 -4.3942) (width 0.4))
      ))
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 140.97 73.66)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -6) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 VCC))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 BA))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 SER))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 OE))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 RCLK))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 SRCLK))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 VCC))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad9)"))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 BH))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 BG))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 BF))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 BE))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 BD))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 BC))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 BB))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_3.9x9.9mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 158.496 73.66)
    (descr "16-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at 0 -6) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 6) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R2-Pad2)"))
    (pad 2 smd rect (at -2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(R4-Pad2)"))
    (pad 4 smd rect (at -2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(R5-Pad2)"))
    (pad 5 smd rect (at -2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(R6-Pad2)"))
    (pad 6 smd rect (at -2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(R7-Pad2)"))
    (pad 7 smd rect (at -2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(R8-Pad2)"))
    (pad 8 smd rect (at -2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 9 smd rect (at 2.7 4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at 2.7 3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 VCC))
    (pad 11 smd rect (at 2.7 1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 SRCLK))
    (pad 12 smd rect (at 2.7 0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 RCLK))
    (pad 13 smd rect (at 2.7 -0.635) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 OE))
    (pad 14 smd rect (at 2.7 -1.905) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U1-Pad9)"))
    (pad 15 smd rect (at 2.7 -3.175) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R1-Pad2)"))
    (pad 16 smd rect (at 2.7 -4.445) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 VCC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 171.704 72.39 180)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at 0 -7.5 180) (layer F.SilkS))
    (fp_text value TPIC6595 (at 0 7.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 VCC))
    (pad 3 smd rect (at -4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(U2-Pad9)"))
    (pad 4 smd rect (at -4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 D0))
    (pad 5 smd rect (at -4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 D1))
    (pad 6 smd rect (at -4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 D2))
    (pad 7 smd rect (at -4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 D3))
    (pad 8 smd rect (at -4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 VCC))
    (pad 9 smd rect (at -4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 OE))
    (pad 10 smd rect (at -4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 11 smd rect (at 4.7 5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 12 smd rect (at 4.7 4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 RCLK))
    (pad 13 smd rect (at 4.7 3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 SRCLK))
    (pad 14 smd rect (at 4.7 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 D4))
    (pad 15 smd rect (at 4.7 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 D5))
    (pad 16 smd rect (at 4.7 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 D6))
    (pad 17 smd rect (at 4.7 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 D7))
    (pad 18 smd rect (at 4.7 -3.175 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U3-Pad18)"))
    (pad 19 smd rect (at 4.7 -4.445 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 GND))
    (pad 20 smd rect (at 4.7 -5.715 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U3-Pad20)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CC11819)
    (at 129.54 103.886)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module AOR_custom:AOR_LOGO (layer B.Cu) (tedit 5C26ADAA)
    (at 154.686 92.456 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value AOR_LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (gr_text "ACP3-H-PR3-PCB\nREV A, 4-24-2019" (at 154.432 93.98) (layer F.SilkS))
  (gr_text "ACP3-H-PR3-PCB\nREV A, 4-24-2019" (at 154.686 75.946 90) (layer B.SilkS))
  (gr_text GND (at 131.572 94.488) (layer B.SilkS))
  (gr_text 5V (at 130.81 97.282) (layer B.SilkS))
  (gr_text "PIN 12 HIGH" (at 137.668 71.628 90) (layer B.SilkS))
  (gr_line (start 125.984 43.18) (end 125.984 107.442) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.102 43.18) (end 125.984 43.18) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.102 107.442) (end 181.102 43.18) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.984 107.442) (end 181.102 107.442) (layer Edge.Cuts) (width 0.1))
  (zone (net 11) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.984 43.18) (xy 181.102 43.18) (xy 181.102 107.442) (xy 125.984 107.442)
      )
    )
  )
  (zone (net 11) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.984 43.18) (xy 181.102 43.18) (xy 181.102 107.442) (xy 125.984 107.442)
      )
    )
  )
)
