(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 90)
    (no_connects 0)
    (area 144.550001 68.805174 204.016428 149.219001)
    (thickness 1.6)
    (drawings 55)
    (tracks 459)
    (zones 0)
    (modules 35)
    (nets 49)
  )
  (page A4)
  (title_block
    (title "USB AVR Tool")
    (date 2018-06-12)
    (rev B)
    (company Petezah)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.254)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 +3V3)
  (net 5 /MISO)
  (net 6 VCC)
  (net 7 /SCK)
  (net 8 /MOSI)
  (net 9 /ISP_RST)
  (net 10 "Net-(D1-Pad2)")
  (net 11 "Net-(D2-Pad2)")
  (net 12 "Net-(D3-Pad2)")
  (net 13 "Net-(D4-Pad2)")
  (net 14 "Net-(D5-Pad2)")
  (net 15 "Net-(IC1-Pad3)")
  (net 16 "Net-(IC1-Pad4)")
  (net 17 /PD0)
  (net 18 /PD1)
  (net 19 /PD4)
  (net 20 /PD5)
  (net 21 /PD6)
  (net 22 /PD7)
  (net 23 /JTAG_TDI)
  (net 24 /JTAG_TDO)
  (net 25 /JTAG_TMS)
  (net 26 /JTAG_TCK)
  (net 27 /ADC0)
  (net 28 /ADC1)
  (net 29 /SPI_SS)
  (net 30 /LED_STATUS)
  (net 31 /LED_PMODE)
  (net 32 /LED_HEARTBEAT)
  (net 33 /LED_ERR)
  (net 34 /HWB)
  (net 35 /RST)
  (net 36 /TARGET_RST)
  (net 37 "Net-(U1-Pad12)")
  (net 38 "Net-(U1-Pad16)")
  (net 39 "Net-(U1-Pad17)")
  (net 40 "Net-(U1-Pad31)")
  (net 41 /PD2/RX)
  (net 42 /PD3/TX)
  (net 43 "Net-(J8-Pad1)")
  (net 44 "Net-(J8-Pad3)")
  (net 45 /USB_D-)
  (net 46 /USB_D+)
  (net 47 /D+)
  (net 48 /D-)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /ADC0)
    (add_net /ADC1)
    (add_net /D+)
    (add_net /D-)
    (add_net /HWB)
    (add_net /ISP_RST)
    (add_net /JTAG_TCK)
    (add_net /JTAG_TDI)
    (add_net /JTAG_TDO)
    (add_net /JTAG_TMS)
    (add_net /LED_ERR)
    (add_net /LED_HEARTBEAT)
    (add_net /LED_PMODE)
    (add_net /LED_STATUS)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PD0)
    (add_net /PD1)
    (add_net /PD2/RX)
    (add_net /PD3/TX)
    (add_net /PD4)
    (add_net /PD5)
    (add_net /PD6)
    (add_net /PD7)
    (add_net /RST)
    (add_net /SCK)
    (add_net /SPI_SS)
    (add_net /TARGET_RST)
    (add_net /USB_D+)
    (add_net /USB_D-)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad31)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.3048)
    (via_dia 1.3716)
    (via_drill 0.6604)
    (uvia_dia 1.3716)
    (uvia_drill 0.6604)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net VCC)
  )
  (module kicad-libs:ATmega32u4-TQFP44 (layer F.Cu) (tedit 0)
    (at 183.896 107.696 225)
    (tags "TQFP TQFP-44 TQFP44")
    (fp_text reference U1 (at 0 0 225) (layer F.SilkS))
    (fp_text value ATMEGA32U4-AU (at 0 7.95 225) (layer F.Fab))
    (pad 1 smd oval (at -6 -4 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /LED_PMODE))
    (pad 2 smd oval (at -6 -3.2 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd oval (at -6 -2.4 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 48 /D-))
    (pad 4 smd oval (at -6 -1.6 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 47 /D+))
    (pad 5 smd oval (at -6 -0.8 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd oval (at -6 0 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 7 smd oval (at -6 0.8 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 8 smd oval (at -6 1.6 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 29 /SPI_SS))
    (pad 9 smd oval (at -6 2.4 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCK))
    (pad 10 smd oval (at -6 3.2 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 /MOSI))
    (pad 11 smd oval (at -6 4 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 /MISO))
    (pad 12 smd oval (at -4 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U1-Pad12)"))
    (pad 13 smd oval (at -3.2 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 35 /RST))
    (pad 14 smd oval (at -2.4 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 15 smd oval (at -1.6 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd oval (at -0.8 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad16)"))
    (pad 17 smd oval (at 0 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad17)"))
    (pad 18 smd oval (at 0.8 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /PD0))
    (pad 19 smd oval (at 1.6 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /PD1))
    (pad 20 smd oval (at 2.4 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 41 /PD2/RX))
    (pad 21 smd oval (at 3.2 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 42 /PD3/TX))
    (pad 22 smd oval (at 4 6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 /PD5))
    (pad 23 smd oval (at 6 4 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd oval (at 6 3.2 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 25 smd oval (at 6 2.4 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 /PD4))
    (pad 26 smd oval (at 6 1.6 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /PD6))
    (pad 27 smd oval (at 6 0.8 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 22 /PD7))
    (pad 28 smd oval (at 6 0 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 /LED_ERR))
    (pad 29 smd oval (at 6 -0.8 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 32 /LED_HEARTBEAT))
    (pad 30 smd oval (at 6 -1.6 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /TARGET_RST))
    (pad 31 smd oval (at 6 -2.4 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U1-Pad31)"))
    (pad 32 smd oval (at 6 -3.2 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 30 /LED_STATUS))
    (pad 33 smd oval (at 6 -4 315) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 34 /HWB))
    (pad 34 smd oval (at 4 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 35 smd oval (at 3.2 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 36 smd oval (at 2.4 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 23 /JTAG_TDI))
    (pad 37 smd oval (at 1.6 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 24 /JTAG_TDO))
    (pad 38 smd oval (at 0.8 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 25 /JTAG_TMS))
    (pad 39 smd oval (at 0 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 26 /JTAG_TCK))
    (pad 40 smd oval (at -0.8 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 28 /ADC1))
    (pad 41 smd oval (at -1.6 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 27 /ADC0))
    (pad 42 smd oval (at -2.4 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 43 smd oval (at -3.2 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 44 smd oval (at -4 -6 225) (size 0.4 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 179.324 128.524 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -2.54 0.254 450) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 191.516 129.54 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.667 0 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 190.5 101.6 315)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -0.089803 1.526644 315) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 315) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 315) (layer F.Fab))
    (pad 1 smd rect (at -1 0 315) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 315) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 188.976 115.062 45)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 1.796051 45) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 45) (layer F.Fab))
    (pad 1 smd rect (at -1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1 0 45) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 188.976 129.54 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.667 -0.127 270) (layer F.SilkS))
    (fp_text value 10uf (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B0336ED)
    (at 190.5 93.218 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference CON1 (at 5.08 2.54 180) (layer Dwgs.User))
    (fp_text value AVR-ISP-6 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /ISP_RST))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B04844A)
    (at 176.53 117.094 315)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 3.053287 0.179605 315) (layer F.Fab))
    (fp_text value Red (at 2.694077 0.179605 315) (layer Dwgs.User))
    (fp_text user %R (at 0 -1.25 315) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 135) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 135) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B04841B)
    (at 175.514 134.874 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at -2.794 0 180) (layer F.Fab))
    (fp_text value Blue (at 0.127 -1.651 90) (layer Dwgs.User))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B048436)
    (at 176.53 125.984)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 3.048 0) (layer F.Fab))
    (fp_text value Yellow (at 3.81 0) (layer Dwgs.User))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B04842E)
    (at 176.53 121.412)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 3.048 0) (layer F.Fab))
    (fp_text value Green (at 4.318 0) (layer Dwgs.User))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 5B048432)
    (at 176.53 123.698)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 3.048 0) (layer F.Fab))
    (fp_text value Red (at 3.81 0) (layer Dwgs.User))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 5B01D805)
    (at 184.404 126.746)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference IC1 (at 0.762 0) (layer F.SilkS))
    (fp_text value MIC5225-3.3 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 172.212 101.092)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J2 (at 2.54 2.286 270) (layer F.SilkS))
    (fp_text value PORTD (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /PD0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /PD1))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /PD2/RX))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /PD3/TX))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /PD4))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PD5))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /PD6))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /PD7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B047FC6)
    (at 196.088 115.316 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 180) (layer Dwgs.User))
    (fp_text value JTAG (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /JTAG_TDI))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /JTAG_TDO))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /JTAG_TMS))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /JTAG_TCK))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B033600)
    (at 196.088 101.6)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer Dwgs.User))
    (fp_text value ADC (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /ADC0))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /ADC1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B033722)
    (at 186.69 89.408)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33) (layer Dwgs.User))
    (fp_text value SPI (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /MISO))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /MOSI))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SCK))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /SPI_SS))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 179.324 131.064)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.762 1.778) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad3)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 183.388 130.556 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 22 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 /D+))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 /USB_D+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 185.674 130.556 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.651 270) (layer F.SilkS))
    (fp_text value 22 (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 /D-))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /USB_D-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 181.61 117.348 315)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.778 315) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.75 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 315) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /LED_STATUS))
    (pad 2 smd rect (at 0.95 0 315) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 175.514 130.556 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 191.77 112.268 225)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.796051 225) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.75 225) (layer F.Fab))
    (fp_text user %R (at 0 0 225) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 225) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /LED_PMODE))
    (pad 2 smd rect (at 0.95 0 225) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 178.816 114.554 315)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 1.796051 315) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.75 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 315) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 /LED_HEARTBEAT))
    (pad 2 smd rect (at 0.95 0 315) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 176.022 111.76 135)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 -1.796051 135) (layer F.SilkS))
    (fp_text value 2.2K (at 0 1.75 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 135) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /LED_ERR))
    (pad 2 smd rect (at 0.95 0 135) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQQ2 (layer F.Cu) (tedit 5B0335BF)
    (at 177.927 90.678)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE28.pdf")
    (attr smd)
    (fp_text reference SW4 (at 0 0) (layer F.SilkS))
    (fp_text value Reset (at -5.08 0.127) (layer F.SilkS))
    (fp_text user %R (at 0.05 -3.95) (layer F.Fab))
    (pad 1 smd rect (at 3.4 -2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /RST))
    (pad 1 smd rect (at -3.4 -2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /RST))
    (pad 2 smd rect (at -3.4 2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3.4 2) (size 3.2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Buttons_Switches_SMD.3dshapes\SW_SPST_EVQQ2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-libs:Resonator_SMD_muRata_CSTCE_G-3pin_3.0x0.7mm (layer F.Cu) (tedit 5A1DD9EF)
    (at 177.292 100.584 225)
    (fp_text reference Y1 (at 0 -2 225) (layer F.SilkS))
    (fp_text value Resonator (at 0 2 225) (layer F.Fab))
    (pad 1 smd rect (at 1.2 0 225) (size 0.4 2.1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U1-Pad17)"))
    (pad 2 smd rect (at 0 0 225) (size 0.4 2.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.2 0 225) (size 0.4 2.1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U1-Pad16)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B0337B6)
    (at 172.72 96.012 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer Dwgs.User))
    (fp_text value UART (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /PD3/TX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /PD2/RX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B048140)
    (at 172.212 127.762 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 180) (layer Dwgs.User))
    (fp_text value HWB (at 0 -2.032 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /HWB))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B0338B1)
    (at 189.357 120.015 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33 90) (layer Dwgs.User))
    (fp_text value "VCC On/Off" (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 VCC))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J8-Pad3)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B0338AB)
    (at 189.357 123.825 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33 90) (layer Dwgs.User))
    (fp_text value 5V/3V (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J8-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5B0335F4)
    (at 190.5 97.028 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J10 (at 0 8.128 180) (layer Dwgs.User))
    (fp_text value "RST Target/Self" (at 0 7.41 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /RST))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /ISP_RST))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /TARGET_RST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-libs:petezah-logo-xtiny (layer F.Cu) (tedit 5B05A4F9)
    (at 194.818 134.366)
    (fp_text reference G*** (at 5.715 1.143) (layer Dwgs.User) hide)
    (fp_text value LOGO (at 5.969 -1.143) (layer Dwgs.User) hide)
  )
  (module kicad-libs:petezah-logo-tiny (layer B.Cu) (tedit 0)
    (at 190.119 107.315 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module kicad-libs:USB_A_Molex_48037-0001 (layer F.Cu) (tedit 5B2027FB)
    (at 184.15 135.89)
    (fp_text reference J1 (at 0 2.032 180) (layer F.SilkS))
    (fp_text value USB_A (at 0 -3.81) (layer F.Fab))
    (pad "" np_thru_hole circle (at -2.25 0) (size 1.25 1.25) (drill 1.25) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at -5.7 0) (size 3 3) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole circle (at -3.5 -2.1) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at -1 -2.1) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 46 /USB_D+))
    (pad 2 thru_hole circle (at 1 -2.1) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 45 /USB_D-))
    (pad 1 thru_hole circle (at 3.5 -2.1) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 5 thru_hole circle (at 5.7 0) (size 3 3) (drill 2.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 2.25 0) (size 1.25 1.25) (drill 1.25) (layers *.Cu *.Mask))
  )
  (gr_text "USB AVR Tool, Rev B\n(C) 2018 Peter Dunshee" (at 184.277 98.679 45) (layer B.SilkS))
  (gr_text @Petezah (at 185.039 114.554) (layer B.SilkS))
  (gr_text Power (at 173.863 134.874 90) (layer F.SilkS))
  (gr_text Prog (at 180.213 125.984) (layer F.SilkS))
  (gr_text Error (at 180.34 123.825) (layer F.SilkS))
  (gr_text Ready (at 180.721 121.412) (layer F.SilkS))
  (gr_text ! (at 178.181 118.872 315) (layer F.SilkS))
  (gr_text Disable (at 173.99 122.682 270) (layer F.SilkS))
  (gr_text Enable (at 173.99 127.889 270) (layer F.SilkS))
  (gr_text ADC1 (at 194.183 104.14 270) (layer F.SilkS))
  (gr_text ADC0 (at 194.183 101.6 270) (layer F.SilkS))
  (gr_text TDO (at 194.183 112.776 270) (layer F.SilkS))
  (gr_text TMS (at 194.183 107.696 270) (layer F.SilkS))
  (gr_text TMS (at 194.183 110.236 270) (layer F.SilkS))
  (gr_text TDI (at 194.183 115.316 270) (layer F.SilkS))
  (dimension 51.308 (width 0.3) (layer Dwgs.User)
    (gr_text "51.308 mm" (at 156.638 113.03 270) (layer Dwgs.User))
    (feature1 (pts (xy 170.688 138.684) (xy 155.288 138.684)))
    (feature2 (pts (xy 170.688 87.376) (xy 155.288 87.376)))
    (crossbar (pts (xy 157.988 87.376) (xy 157.988 138.684)))
    (arrow1a (pts (xy 157.988 138.684) (xy 157.401579 137.557496)))
    (arrow1b (pts (xy 157.988 138.684) (xy 158.574421 137.557496)))
    (arrow2a (pts (xy 157.988 87.376) (xy 157.401579 88.502504)))
    (arrow2b (pts (xy 157.988 87.376) (xy 158.574421 88.502504)))
  )
  (dimension 27.051 (width 0.3) (layer Dwgs.User)
    (gr_text "27.051 mm" (at 184.2135 75.993) (layer Dwgs.User))
    (feature1 (pts (xy 197.739 87.376) (xy 197.739 74.643)))
    (feature2 (pts (xy 170.688 87.376) (xy 170.688 74.643)))
    (crossbar (pts (xy 170.688 77.343) (xy 197.739 77.343)))
    (arrow1a (pts (xy 197.739 77.343) (xy 196.612496 77.929421)))
    (arrow1b (pts (xy 197.739 77.343) (xy 196.612496 76.756579)))
    (arrow2a (pts (xy 170.688 77.343) (xy 171.814504 77.929421)))
    (arrow2b (pts (xy 170.688 77.343) (xy 171.814504 76.756579)))
  )
  (gr_text < (at 176.53 117.094 315) (layer F.SilkS))
  (gr_text < (at 176.53 121.412) (layer F.SilkS))
  (gr_text < (at 176.53 123.698) (layer F.SilkS))
  (gr_text < (at 176.53 125.984) (layer F.SilkS))
  (gr_text < (at 175.514 134.874 90) (layer F.SilkS))
  (gr_text * (at 189.484 108.077) (layer F.SilkS))
  (gr_text On (at 186.944 120.015 270) (layer F.SilkS))
  (gr_text Off (at 196.85 120.015 270) (layer F.SilkS))
  (gr_text "Target Voltage" (at 191.897 126.365) (layer F.SilkS))
  (gr_text 3V (at 186.944 123.825 270) (layer F.SilkS))
  (gr_text 5V (at 196.85 123.825 270) (layer F.SilkS))
  (gr_text 5V (at 180.34 98.171) (layer F.SilkS))
  (gr_text RX (at 177.8 98.171) (layer F.SilkS))
  (gr_text TX (at 175.26 98.171) (layer F.SilkS))
  (gr_text GND (at 172.72 98.171) (layer F.SilkS))
  (gr_text SS (at 184.15 97.028 270) (layer F.SilkS))
  (gr_text SCK (at 184.15 94.615 270) (layer F.SilkS))
  (gr_text MOSI (at 184.15 91.948 270) (layer F.SilkS))
  (gr_text MISO (at 184.15 89.281 270) (layer F.SilkS))
  (gr_text ISP (at 192.913 88.265) (layer F.SilkS))
  (gr_text RST (at 192.532 99.314 270) (layer F.SilkS))
  (gr_text Target (at 195.326 99.06) (layer F.SilkS))
  (gr_text Self (at 190.119 99.06) (layer F.SilkS))
  (gr_line (start 194.818 87.376) (end 173.482 87.376) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.688 90.17) (end 170.688 127.508) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.688 135.89) (end 170.688 127.508) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 197.612 90.17) (end 197.612 135.89) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.482 90.17) (end 173.482 87.376) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 194.818 90.17) (end 197.612 90.17) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.482 138.684) (end 194.818 138.684) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.482 135.89) (end 170.688 135.89) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 194.818 135.89) (end 197.612 135.89) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 20.066 (width 0.3) (layer Dwgs.User)
    (gr_text "20.066 mm" (at 172.1801 70.155174) (layer Dwgs.User))
    (feature1 (pts (xy 182.2131 80.903174) (xy 182.2131 68.805174)))
    (feature2 (pts (xy 162.1471 80.903174) (xy 162.1471 68.805174)))
    (crossbar (pts (xy 162.1471 71.505174) (xy 182.2131 71.505174)))
    (arrow1a (pts (xy 182.2131 71.505174) (xy 181.086596 72.091595)))
    (arrow1b (pts (xy 182.2131 71.505174) (xy 181.086596 70.918753)))
    (arrow2a (pts (xy 162.1471 71.505174) (xy 163.273604 72.091595)))
    (arrow2b (pts (xy 162.1471 71.505174) (xy 163.273604 70.918753)))
  )
  (dimension 45.212 (width 0.3) (layer Dwgs.User)
    (gr_text "45.212 mm" (at 151.05 110.373153 270) (layer Dwgs.User))
    (feature1 (pts (xy 161.417 132.979153) (xy 149.7 132.979153)))
    (feature2 (pts (xy 161.417 87.767153) (xy 149.7 87.767153)))
    (crossbar (pts (xy 152.4 87.767153) (xy 152.4 132.979153)))
    (arrow1a (pts (xy 152.4 132.979153) (xy 151.813579 131.852649)))
    (arrow1b (pts (xy 152.4 132.979153) (xy 152.986421 131.852649)))
    (arrow2a (pts (xy 152.4 87.767153) (xy 151.813579 88.893657)))
    (arrow2b (pts (xy 152.4 87.767153) (xy 152.986421 88.893657)))
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.688 87.376) (xy 197.739 87.376) (xy 197.739 138.684) (xy 170.688 138.684)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.688 87.376) (xy 197.739 87.376) (xy 197.739 138.684) (xy 170.688 138.684)
      )
    )
  )
)
