(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 3)
    (no_connects 0)
    (area 130.861999 96.190999 147.141001 105.993001)
    (thickness 1.6)
    (drawings 19)
    (tracks 8)
    (zones 0)
    (modules 3)
    (nets 3)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1.5)
    (user_trace_width 1.7)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.5)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net_class Default "Dit is de standaard class."
    (clearance 0.2)
    (trace_width 1.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module Connect:BARREL_JACK (layer F.Cu) (tedit 5936B927)
    (at 139.319 98.679)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at -3.0226 0.1778 270) (layer F.SilkS))
    (fp_text value BARREL_JACK (at -6.2 -5.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole rect (at -6 0) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole rect (at -3 4.7) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5936C1E3)
    (at 143.51 98.679)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at -0.127 5.08) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Symbols:Symbol_Barrel_Polarity (layer F.Cu) (tedit 5765E9A7)
    (at 142.621 104.394)
    (descr "Barrel connector polarity indicator")
    (tags "barrel polarity")
    (fp_text reference REF** (at 0 -2) (layer F.SilkS) hide)
    (fp_text value Symbol_Barrel_Polarity (at 0 2) (layer F.Fab))
  )
  (gr_text ":)" (at 131.699 105.029) (layer B.SilkS))
  (gr_text Trevor's (at 142.621 103.124) (layer B.SilkS))
  (gr_text - (at 139.573 104.394) (layer F.SilkS))
  (gr_text + (at 145.669 104.394) (layer F.SilkS))
  (gr_text "DC Adapter" (at 142.621 104.902) (layer B.SilkS))
  (gr_line (start 130.937 105.918) (end 131.064 105.918) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.937 96.266) (end 131.064 96.266) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.31748 103.37292) (end 137.31748 103.378) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.32104 103.37292) (end 137.31748 103.37292) (angle 90) (layer Edge.Cuts) (width 1))
  (gr_line (start 139.319 97.65284) (end 139.319 99.70516) (angle 90) (layer Edge.Cuts) (width 1))
  (gr_line (start 133.31952 97.65284) (end 133.31952 99.70516) (angle 90) (layer Edge.Cuts) (width 1))
  (gr_line (start 130.937 105.918) (end 130.937 96.266) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.066 105.918) (end 131.064 105.918) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.066 105.664) (end 147.066 105.918) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.066 96.266) (end 147.066 105.664) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145.288 96.266) (end 147.066 96.266) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text - (at 145.796 101.092) (layer F.SilkS))
  (gr_text + (at 145.796 98.679) (layer F.SilkS))
  (gr_line (start 131.064 96.266) (end 145.288 96.266) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.064 96.266) (xy 137.16 96.266) (xy 137.16 100.838) (xy 141.351 100.838) (xy 141.351 99.949)
        (xy 147.066 99.949) (xy 147.066 105.918) (xy 130.937 105.918) (xy 130.937 96.266)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.066 105.918) (xy 130.937 105.918) (xy 130.937 96.266) (xy 147.066 96.266)
      )
    )
  )
)
