<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="23.8" y2="0" width="0" layer="20"/>
<wire x1="23.8" y1="0" x2="23.8" y2="54.6" width="0" layer="20"/>
<wire x1="23.8" y1="54.6" x2="0" y2="54.6" width="0" layer="20"/>
<wire x1="0" y1="54.6" x2="0" y2="0" width="0" layer="20"/>
<text>PWR LED</text>
<text>5V</text>
<text>5V</text>
<text>G</text>
<text>G</text>
<text>RJ45 PINOUT
---------------------
1: RST-
2: RST+
3: PWR+
4: IDE_LED+
5: IDE_LED-
6: PWR-
7: PWR_LED+
8: PWR_LED-</text>
<text>IDE LED</text>
<text>POWER</text>
<text>RESET</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>PiKVM Adapter 
V001
09102020
M.Miller</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X20">
</package>
<package name="RJ45-8">
</package>
<package name="1X04">
</package>
<package name="1X08">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="MyLib2">
<packages>
<package name="SOP-4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP_EVEN" library="SparkFun-Connectors" package="1X20" value="M20"/>
<element name="JP_ODD" library="SparkFun-Connectors" package="1X20" value="M20"/>
<element name="R1" library="SparkFun-Resistors" package="1206" value="390">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="1206" value="390">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="1206" value="390">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="1206" value="390">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="1206" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="1206" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Connectors" package="RJ45-8" value="RJ45-8PTH"/>
<element name="U1" library="MyLib2" package="SOP-4" value="CPC1008">
<attribute name="NAME"/>
</element>
<element name="U2" library="MyLib2" package="SOP-4" value="CPC1008">
<attribute name="NAME"/>
</element>
<element name="U3" library="MyLib2" package="SOP-4" value="CPC1008">
<attribute name="NAME"/>
</element>
<element name="U4" library="MyLib2" package="SOP-4" value="CPC1008">
<attribute name="NAME"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GPIO_14">
<contactref element="JP_EVEN" pad="4"/>
</signal>
<signal name="GPIO_15">
<contactref element="JP_EVEN" pad="5"/>
</signal>
<signal name="GPIO_18">
<contactref element="JP_EVEN" pad="6"/>
</signal>
<signal name="GPIO_23">
<contactref element="JP_EVEN" pad="8"/>
<contactref element="U1" pad="P$1"/>
</signal>
<signal name="GPIO_24">
<contactref element="JP_EVEN" pad="9"/>
<contactref element="U3" pad="P$3"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="GPIO_21">
<contactref element="JP_EVEN" pad="20"/>
</signal>
<signal name="GPIO_20">
<contactref element="JP_EVEN" pad="19"/>
</signal>
<signal name="GPIO_16">
<contactref element="JP_EVEN" pad="18"/>
</signal>
<signal name="GPIO_12">
<contactref element="JP_EVEN" pad="16"/>
</signal>
<signal name="GPIO_25">
<contactref element="JP_EVEN" pad="11"/>
</signal>
<signal name="GPIO_08">
<contactref element="JP_EVEN" pad="12"/>
</signal>
<signal name="GPIO_07">
<contactref element="JP_EVEN" pad="13"/>
</signal>
<signal name="GPIO_01">
<contactref element="JP_EVEN" pad="14"/>
</signal>
<signal name="GPIO_02">
<contactref element="JP_ODD" pad="2"/>
</signal>
<signal name="GPIO_03">
<contactref element="JP_ODD" pad="3"/>
</signal>
<signal name="GPIO_04">
<contactref element="JP_ODD" pad="4"/>
</signal>
<signal name="GPIO_17">
<contactref element="JP_ODD" pad="6"/>
</signal>
<signal name="GPIO_27">
<contactref element="JP_ODD" pad="7"/>
<contactref element="U2" pad="P$1"/>
</signal>
<signal name="GPIO_22">
<contactref element="JP_ODD" pad="8"/>
<contactref element="U4" pad="P$3"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="GPIO_10">
<contactref element="JP_ODD" pad="10"/>
</signal>
<signal name="GPIO_09">
<contactref element="JP_ODD" pad="11"/>
</signal>
<signal name="GPIO_11">
<contactref element="JP_ODD" pad="12"/>
</signal>
<signal name="GPIO_00">
<contactref element="JP_ODD" pad="14"/>
</signal>
<signal name="GPIO_05">
<contactref element="JP_ODD" pad="15"/>
</signal>
<signal name="GPIO_06">
<contactref element="JP_ODD" pad="16"/>
</signal>
<signal name="GPIO_13">
<contactref element="JP_ODD" pad="17"/>
</signal>
<signal name="GPIO_19">
<contactref element="JP_ODD" pad="18"/>
</signal>
<signal name="GPIO_26">
<contactref element="JP_ODD" pad="19"/>
</signal>
<signal name="GND">
<contactref element="JP_EVEN" pad="3"/>
<contactref element="JP_EVEN" pad="7"/>
<contactref element="JP_EVEN" pad="10"/>
<contactref element="JP_EVEN" pad="17"/>
<contactref element="JP_EVEN" pad="15"/>
<contactref element="JP_ODD" pad="5"/>
<contactref element="JP_ODD" pad="13"/>
<contactref element="JP_ODD" pad="20"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP7" pad="4"/>
</signal>
<signal name="3.3V">
<contactref element="JP_ODD" pad="1"/>
<contactref element="JP_ODD" pad="9"/>
<contactref element="U3" pad="P$4"/>
<contactref element="U4" pad="P$4"/>
</signal>
<signal name="5V">
<contactref element="JP_EVEN" pad="1"/>
<contactref element="JP_EVEN" pad="2"/>
<contactref element="JP7" pad="3"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="PWR+">
<contactref element="U1" pad="P$4"/>
<contactref element="U$1" pad="3"/>
<contactref element="JP8" pad="3"/>
</signal>
<signal name="PWR-">
<contactref element="U1" pad="P$3"/>
<contactref element="U$1" pad="6"/>
<contactref element="JP8" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="P$2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="P$2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="RST+">
<contactref element="U2" pad="P$4"/>
<contactref element="U$1" pad="2"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="RST-">
<contactref element="U2" pad="P$3"/>
<contactref element="U$1" pad="1"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U3" pad="P$1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="PWR_LED+">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="JP8" pad="7"/>
</signal>
<signal name="PWR_LED-">
<contactref element="U3" pad="P$2"/>
<contactref element="U$1" pad="8"/>
<contactref element="JP8" pad="8"/>
</signal>
<signal name="N$5">
<contactref element="U4" pad="P$1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="IDE_LED+">
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="IDE_LED-">
<contactref element="U4" pad="P$2"/>
<contactref element="U$1" pad="5"/>
<contactref element="JP8" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
