(kicad_pcb (version 20171130) (host pcbnew "(5.0.2-5)-5")
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 63)
    (zones 0)
    (modules 36)
    (nets 25)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 0.85)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J2-Pad1)")
  (net 3 "Net-(J3-Pad1)")
  (net 4 "Net-(J4-Pad1)")
  (net 5 "Net-(J5-Pad1)")
  (net 6 "Net-(J6-Pad1)")
  (net 7 "Net-(J7-Pad1)")
  (net 8 "Net-(J8-Pad1)")
  (net 9 "Net-(J9-Pad1)")
  (net 10 "Net-(J10-Pad1)")
  (net 11 "Net-(J11-Pad1)")
  (net 12 "Net-(J12-Pad1)")
  (net 13 "Net-(J13-Pad1)")
  (net 14 "Net-(J14-Pad1)")
  (net 15 "Net-(J15-Pad1)")
  (net 16 "Net-(J16-Pad1)")
  (net 17 "Net-(J17-Pad1)")
  (net 18 "Net-(J18-Pad1)")
  (net 19 "Net-(J19-Pad1)")
  (net 20 "Net-(J20-Pad1)")
  (net 21 "Net-(J21-Pad1)")
  (net 22 "Net-(J22-Pad1)")
  (net 23 "Net-(J23-Pad1)")
  (net 24 "Net-(J24-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 1.524)
    (diff_pair_width 1.524)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J11-Pad1)")
    (add_net "Net-(J12-Pad1)")
    (add_net "Net-(J13-Pad1)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J17-Pad1)")
    (add_net "Net-(J18-Pad1)")
    (add_net "Net-(J19-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J20-Pad1)")
    (add_net "Net-(J21-Pad1)")
    (add_net "Net-(J22-Pad1)")
    (add_net "Net-(J23-Pad1)")
    (add_net "Net-(J24-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J7-Pad1)")
    (add_net "Net-(J8-Pad1)")
    (add_net "Net-(J9-Pad1)")
  )
  (net_class trace ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 1.524)
    (diff_pair_width 1.524)
  )
  (module touch:strain30AWG (layer B.Cu) (tedit 5D12D6A3)
    (at 165.1 33.821182)
    (fp_text reference J20 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 20 "Net-(J20-Pad1)"))
  )
  (module touch:strain30AWG (layer B.Cu) (tedit 5D12D6A3)
    (at 165.1 28.821182)
    (fp_text reference J21 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 21 "Net-(J21-Pad1)"))
  )
  (module touch:strain30AWG (layer B.Cu) (tedit 5D12D6A3)
    (at 165.1 23.821182)
    (fp_text reference J22 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 22 "Net-(J22-Pad1)"))
  )
  (module touch:strain30AWG (layer B.Cu) (tedit 5D12D6A3)
    (at 165.1 18.821182)
    (fp_text reference J23 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 23 "Net-(J23-Pad1)"))
  )
  (module touch:strain30AWG (layer B.Cu) (tedit 5D12D6A3)
    (at 165.1 13.821182)
    (fp_text reference J24 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 24 "Net-(J24-Pad1)"))
  )
  (module touch:strain30AWG (layer F.Cu) (tedit 5D12D6A3)
    (at 13.97 38.97)
    (fp_text reference J7 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 7 "Net-(J7-Pad1)"))
  )
  (module touch:strain30AWG (layer F.Cu) (tedit 5D12D6A3)
    (at 13.97 33.97)
    (fp_text reference J6 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 6 "Net-(J6-Pad1)"))
  )
  (module touch:strain30AWG (layer F.Cu) (tedit 5D12D6A3)
    (at 13.97 28.97)
    (fp_text reference J5 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 5 "Net-(J5-Pad1)"))
  )
  (module touch:strain30AWG (layer F.Cu) (tedit 5D12D6A3)
    (at 13.97 23.97)
    (fp_text reference J4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value \ (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 4 "Net-(J4-Pad1)"))
  )
  (module touch:strain30AWG (layer F.Cu) (tedit 5D12D6A3)
    (at 13.97 18.97)
    (fp_text reference J3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 3 "Net-(J3-Pad1)"))
  )
  (module touch:strain30AWG (layer F.Cu) (tedit 5D12D6A3)
    (at 13.97 13.97)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 2 "Net-(J2-Pad1)"))
  )
  (module touch:strain30AWG (layer B.Cu) (tedit 5D12D6A3)
    (at 165.1 38.821182)
    (fp_text reference J19 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu)
      (net 19 "Net-(J19-Pad1)"))
  )
  (module touch:hole30AWG (layer B.Cu) (tedit 5D12D83C)
    (at 161.29 18.821182)
    (fp_text reference J17 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 17 "Net-(J17-Pad1)"))
  )
  (module touch:hole30AWG (layer B.Cu) (tedit 5D12D81F)
    (at 161.29 33.821182)
    (fp_text reference J14 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 14 "Net-(J14-Pad1)"))
  )
  (module touch:hole30AWG (layer B.Cu) (tedit 5D12D847)
    (at 161.29 13.821182)
    (fp_text reference J16 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 16 "Net-(J16-Pad1)"))
  )
  (module touch:hole30AWG (layer B.Cu) (tedit 5D12D827)
    (at 161.29 28.821182)
    (fp_text reference J15 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 15 "Net-(J15-Pad1)"))
  )
  (module touch:hole30AWG (layer B.Cu) (tedit 5D12D832)
    (at 161.29 23.821182)
    (fp_text reference J18 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 18 "Net-(J18-Pad1)"))
  )
  (module touch:hole30AWG (layer B.Cu) (tedit 5D12D805)
    (at 161.29 38.821182)
    (fp_text reference J13 (at 0 -0.5) (layer B.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 0.5) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 13 "Net-(J13-Pad1)"))
  )
  (module touch:hole30AWG (layer F.Cu) (tedit 5D12D7E6)
    (at 17.72412 28.89504)
    (fp_text reference J12 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 12 "Net-(J12-Pad1)"))
  )
  (module touch:hole30AWG (layer F.Cu) (tedit 5D12D7ED)
    (at 17.78 33.97)
    (fp_text reference J11 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 11 "Net-(J11-Pad1)"))
  )
  (module touch:hole30AWG (layer F.Cu) (tedit 5D12D7F3)
    (at 17.90192 38.9382)
    (fp_text reference J10 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 10 "Net-(J10-Pad1)"))
  )
  (module touch:hole30AWG (layer F.Cu) (tedit 5D12D7DE)
    (at 17.78 23.97)
    (fp_text reference J9 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 9 "Net-(J9-Pad1)"))
  )
  (module touch:hole30AWG (layer F.Cu) (tedit 5D12D7D6)
    (at 17.78 18.97)
    (fp_text reference J8 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 8 "Net-(J8-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D085C63)
    (at 34.29 17.78)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D0857CF)
    (at 144.29 35.24)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 13 "Net-(J13-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D0857D9)
    (at 124.29 35.24)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 14 "Net-(J14-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D0857E0)
    (at 104.29 35.24)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 15 "Net-(J15-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D0857A2)
    (at 84.29 35.24)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 12 "Net-(J12-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D08578B)
    (at 64.29 35.24)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP5 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 11 "Net-(J11-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D08579B)
    (at 44.29 35.24)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 10 "Net-(J10-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D0857E8)
    (at 134.29 17.78)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 16 "Net-(J16-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D0857F0)
    (at 114.29 17.78)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 17 "Net-(J17-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D0857FA)
    (at 94.29 17.78)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 18 "Net-(J18-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D085C78)
    (at 74.29 17.78)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 9 "Net-(J9-Pad1)"))
  )
  (module touch:Touch_Pad_10x10mm (layer F.Cu) (tedit 5D08585D)
    (at 54.29 17.78)
    (descr "SMD rectangular pad as test Point, square 4.0mm side length")
    (tags "touch point SMD pad rectangle square")
    (attr virtual)
    (fp_text reference TP2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 3.1) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 10 10) (layers F.Cu F.Mask)
      (net 8 "Net-(J8-Pad1)"))
  )
  (module touch:hole30AWG (layer F.Cu) (tedit 5D12D7CE)
    (at 17.78 13.97)
    (fp_text reference J1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01_Female (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (gr_text "Flex Touch Band\n@helenleigh & @pdp7\n2019-06-26" (at 87.15248 25.97912) (layer B.SilkS))
  (gr_line (start 168.91 10.16) (end 10.16 10.16) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.91 43.18) (end 168.91 10.16) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 10.16 43.18) (end 168.91 43.18) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 10.16 10.16) (end 10.16 43.18) (layer Edge.Cuts) (width 0.1))
)
