(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Eurorack State-Variable Filter")
    (date "2022-11-23")
    (rev "1.2")
    (company "Len Popp")
    (comment 1 "Copyright © 2022 Len Popp CC BY")
    (comment 2 "Board settings comply with requirements of OSH Park https://oshpark.com/")
    (comment 3 "CEM3320 state-variable VCF module - Eurorack 10HP")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/main/")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "-12V")
  (net 4 "Net-(C7-Pad1)")
  (net 5 "Net-(C7-Pad2)")
  (net 6 "/OUT-BP")
  (net 7 "Net-(C12-Pad1)")
  (net 8 "/VEE-U1")
  (net 9 "OUT-HP")
  (net 10 "Net-(C11-Pad1)")
  (net 11 "Net-(C13-Pad1)")
  (net 12 "Net-(C14-Pad1)")
  (net 13 "Net-(C15-Pad2)")
  (net 14 "OUT-LP")
  (net 15 "IN-AUDIO")
  (net 16 "CV-FREQ-1VOCT")
  (net 17 "IN-CV-BUS")
  (net 18 "CV-RES-MOD-N")
  (net 19 "OUT-AUDIO-LP-HP")
  (net 20 "OUT-AUDIO-BP")
  (net 21 "Net-(J9-Pad13)")
  (net 22 "unconnected-(J9-Pad15)")
  (net 23 "unconnected-(J9-Pad16)")
  (net 24 "CV-FREQ-POT")
  (net 25 "CV-FREQ-MOD")
  (net 26 "CV-RES-POT")
  (net 27 "OUT-LP-HP")
  (net 28 "Net-(R1-Pad2)")
  (net 29 "Net-(R8-Pad1)")
  (net 30 "Net-(R10-Pad1)")
  (net 31 "Net-(R13-Pad2)")
  (net 32 "Net-(R11-Pad1)")
  (net 33 "Net-(R10-Pad2)")
  (net 34 "CV-RES-MOD-P")
  (net 35 "Net-(R12-Pad2)")
  (net 36 "Net-(R11-Pad2)")
  (net 37 "Net-(R16-Pad2)")
  (net 38 "Net-(R18-Pad2)")
  (net 39 "Net-(R19-Pad2)")
  (net 40 "Net-(R22-Pad2)")
  (net 41 "Net-(R23-Pad2)")
  (net 42 "Net-(R25-Pad2)")
  (net 43 "unconnected-(U1-Pad5)")
  (net 44 "unconnected-(U1-Pad10)")
  (net 45 "unconnected-(U1-Pad11)")
  (net 46 "unconnected-(U1-Pad18)")
  (net 47 "unconnected-(J9-Pad11)")
  (net 48 "unconnected-(J9-Pad12)")
  (net 49 "Net-(H12-Pad1)")
  (net 50 "Net-(R27-Pad2)")
  (net 51 "Net-(R28-Pad2)")
  (footprint "-lmp-misc:CP_Radial_D4.0mm_P2.50mm" (layer "F.Cu")
    (tedit 612547C9)
    (at 198.247 127.381 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 4mm Electrolytic Capacitor")
    (property "Distributor" "Mouser")
    (property "Distributor2" "Thonk")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/667-ECE-A1VKS100I")
    (property "DistributorPartLink2" "https://www.thonk.co.uk/shop/eurorack-diy-essentials/")
    (property "DistributorPartNum" "667-ECE-A1VKS100I")
    (property "DistributorPartNum2" "Group_Eurorack_DIY_Essential")
    (property "Manufacturer" "Panasonic")
    (property "ManufacturerPartNum" "ECE-A1VKS100I")
    (property "Note" "12 V decoupling")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "Value2" "35 VDC")
    (attr through_hole)
    (fp_text reference "C2" (at 1.25 -3.683 180) (layer "F.SilkS"))
    (fp_text value "10U" (at 1.25 3.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:CP_Radial_D4.0mm_P2.50mm" (layer "F.Cu")
    (tedit 612547C9)
    (at 198.247 132.5558 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 4mm Electrolytic Capacitor")
    (property "Distributor" "Mouser")
    (property "Distributor2" "Thonk")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/667-ECE-A1VKS100I")
    (property "DistributorPartLink2" "https://www.thonk.co.uk/shop/eurorack-diy-essentials/")
    (property "DistributorPartNum" "667-ECE-A1VKS100I")
    (property "DistributorPartNum2" "Group_Eurorack_DIY_Essential")
    (property "Manufacturer" "Panasonic")
    (property "ManufacturerPartNum" "ECE-A1VKS100I")
    (property "Note" "12 V decoupling")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "Value2" "35 VDC")
    (attr through_hole)
    (fp_text reference "C1" (at 1.1752 -3.683) (layer "F.SilkS"))
    (fp_text value "10U" (at 1.25 3.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:Logo_CC_BY" locked (layer "F.Cu")
    (tedit 0)
    (at 206.502 45.72)
    (attr through_hole)
    (fp_text reference "G2" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo_CC_BY" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "-lmp-synth:IDC-Header-Eurorack-16-TH" (layer "F.Cu")
    (tedit 61A6FD03)
    (at 208.28 132.08 180)
    (descr "Through-hole Eurorack 16-pin board power/CV/gate bus connector, shrouded")
    (tags "Through hole vertical IDC box header THT 2x08 2.54mm double row Eurorack")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Wurth-Elektronik/61201621621?qs=ZtY9WdtwX55qFf4n3EFuaA%3D%3D")
    (property "DistributorPartNum" "710-61201621621")
    (property "Manufacturer" "Wurth Elektronik")
    (property "ManufacturerPartNum" "61201621621")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "J9" (at 7.493 17.78) (layer "F.SilkS"))
    (fp_text value "Conn_Eurorack_16" (at 1.27 6.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 -8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 3 "-12V") (pinfunction "-12V") (pintype "power_in"))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "power_in"))
    (pad "3" thru_hole circle locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole circle locked (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "power_in"))
    (pad "5" thru_hole circle locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole circle locked (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "power_in"))
    (pad "7" thru_hole circle locked (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole circle locked (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "power_in"))
    (pad "9" thru_hole circle locked (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "+12V") (pintype "power_in"))
    (pad "10" thru_hole circle locked (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "power_in"))
    (pad "11" thru_hole circle locked (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "unconnected-(J9-Pad11)") (pinfunction "+5V") (pintype "power_in+no_connect"))
    (pad "12" thru_hole circle locked (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "unconnected-(J9-Pad12)") (pintype "power_in+no_connect"))
    (pad "13" thru_hole circle locked (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J9-Pad13)") (pinfunction "CV") (pintype "bidirectional"))
    (pad "14" thru_hole circle locked (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J9-Pad13)") (pintype "bidirectional"))
    (pad "15" thru_hole circle locked (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "unconnected-(J9-Pad15)") (pinfunction "GATE") (pintype "bidirectional+no_connect"))
    (pad "16" thru_hole circle locked (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J9-Pad16)") (pintype "bidirectional+no_connect"))
    (model "${KISYS3DMOD}/Connector_IDC.3dshapes/IDC-Header_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 205.440001 102.87 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Distributor" "Adafruit")
    (property "Distributor2" "Mouser")
    (property "DistributorPartLink" "https://www.adafruit.com/product/392")
    (property "DistributorPartLink2" "https://www.mouser.ca/ProductDetail/649-1012937893601BLF")
    (property "DistributorPartNum" "392")
    (property "DistributorPartNum2" "649-1012937893601BLF")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "JP1" (at 2.921 0.045999 180) (layer "F.SilkS"))
    (fp_text value "CV-BUS" (at 0 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "IN-CV-BUS") (pinfunction "C") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J9-Pad13)") (pinfunction "B") (pintype "passive"))
    (model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:Logo_OSHW" locked (layer "F.Cu")
    (tedit 60F495A1)
    (at 208.534 49.784)
    (descr "Open Source Hardware logo")
    (tags "Open Source Hardware logo")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G4" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo_OSHW" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 189.738 96.012 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "C4" (at -2.794 0) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 191.135 118.11 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "C6" (at 1.25 2.413) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 172.466 88.519 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R19" (at 9.525 0 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R16-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R19-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 191.897 54.229)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/?qs=s%2FCsB4POEK6rPX34eazMCw%3D%3D")
    (property "DistributorPartNum" "594-K180J15C0GF5TL2")
    (property "Manufacturer" "Murata")
    (property "ManufacturerPartNum" "K180J15C0GF5TL2")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "C0G/NP0")
    (attr through_hole)
    (fp_text reference "C11" (at 5.715 0) (layer "F.SilkS"))
    (fp_text value "18P" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "OUT-LP") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-holes:MountingHole_PCB_3.2mm_M3" locked (layer "F.Cu")
    (tedit 622675F6)
    (at 208.488 54.61)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "exclude_from_bom" "")
    (clearance 1.15)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H4" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_M3" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 172.466 96.012 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "C3" (at 5.461 0) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:CP_Radial_D4.0mm_P2.50mm" (layer "F.Cu")
    (tedit 612547C9)
    (at 172.212 67.183 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 4mm Electrolytic Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Panasonic/ECE-A1HKA4R7I?qs=AfGmtpoX2giUuCvV8uNbmg%3D%3D")
    (property "DistributorPartNum" "667-ECE-A1HKA4R7I")
    (property "Manufacturer" "Panasonic")
    (property "ManufacturerPartNum" "ECE-A1HKA4R7I")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C13" (at 5.334 0) (layer "F.SilkS"))
    (fp_text value "4U7" (at 1.25 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 11 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 "/OUT-BP") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 188.722 121.793)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R30" (at 10.414 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(R28-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "OUT-AUDIO-LP-HP") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 199.39 61.468)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-120K?qs=oAGoVhmvjhymMraGPHdD1w%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-120K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-120K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R5" (at -2.413 0) (layer "F.SilkS"))
    (fp_text value "120K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "CV-FREQ-POT") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 177.673 50.419)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R25" (at -0.381 -2.413) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(R25-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-14_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 176.022 88.392)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/?qs=vxEfx8VrU7BHurOY5iQdiA%3D%3D")
    (property "DistributorPartNum" "595-TL074BCN")
    (property "Manufacturer" "Texas Instruments")
    (property "ManufacturerPartNum" "TL074BCN")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 18.034) (layer "F.SilkS"))
    (fp_text value "TL074" (at 3.81 17.57) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R16-Pad2)") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R12-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R1-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)") (pintype "output"))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R11-Pad2)") (pintype "output"))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R11-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R10-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R10-Pad2)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 181.61 46.736)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-680R?qs=oAGoVhmvjhyj6p4bCLlIDg%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-680R")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-680R")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R22" (at 12.954 0) (layer "F.SilkS"))
    (fp_text value "680R" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/VEE-U1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(R22-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-holes:WireHole_D0.8mm_OD1.6mm" (layer "F.Cu")
    (tedit 0)
    (at 172.466 57.531)
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr smd exclude_from_bom)
    (fp_text reference "H13" (at 0 -1.6002 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WireHole_PTH" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 207.01 64.77 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-130K?qs=oAGoVhmvjhwGhRGh%2FUMCLQ%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-130K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-130K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R2" (at 9.906 0) (layer "F.SilkS"))
    (fp_text value "130K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "CV-RES-POT") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R10-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 173.863 125.73 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "C5" (at 1.25 -2.5) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 195.199 85.217 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-39K?qs=oAGoVhmvjhzU8OAJ800nOg%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-39K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-39K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R13" (at 9.398 -0.635 180) (layer "F.SilkS"))
    (fp_text value "39K" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R11-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R13-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 199.39 74.676)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R7" (at -2.286 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "CV-FREQ-MOD") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 188.722 132.588 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R28" (at -2.159 0 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(R28-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 165.227 75.057)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-220K?qs=oAGoVhmvjhzRYglFF6%2Fz8A%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-220K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-220K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R18" (at -2.286 0 90) (layer "F.SilkS"))
    (fp_text value "220K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/OUT-BP") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R18-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-synth:Potentiometer_Bourns_3296WY_Vertical" (layer "F.Cu")
    (tedit 621A5B3C)
    (at 189.738 77.47 90)
    (descr "Potentiometer, vertical, Bourns 3296W or 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W 3296Y")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Bourns/3296W-1-103LF?qs=CL3xLxiry19Id6AEaxYcng%3D%3D")
    (property "DistributorPartNum" "652-3296W-1-103LF")
    (property "Label" "SCALE")
    (property "Manufacturer" "Bourns")
    (property "ManufacturerPartNum" "3296W-1-103LF")
    (property "Note" "3296W or 3296Y type")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV7" (at 3.556 1.397 180) (layer "F.SilkS"))
    (fp_text value "10K" (at -2.54 3.67 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0.005 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R13-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 -1.275 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R13-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R13-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 1.265 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(R13-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 -1.275 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(H12-Pad1)") (pinfunction "3") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(H12-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 173.863 121.92 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R29" (at 10.414 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(R27-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "OUT-AUDIO-BP") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:CP_Radial_D4.0mm_P2.50mm" (layer "F.Cu")
    (tedit 612547C9)
    (at 204.47 82.55 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 4mm Electrolytic Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Panasonic/ECE-A1HKA4R7I?qs=AfGmtpoX2giUuCvV8uNbmg%3D%3D")
    (property "DistributorPartNum" "667-ECE-A1HKA4R7I")
    (property "Manufacturer" "Panasonic")
    (property "ManufacturerPartNum" "ECE-A1HKA4R7I")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C15" (at 5.461 -0.127) (layer "F.SilkS"))
    (fp_text value "4U7" (at 1.25 3.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 27 "OUT-LP-HP") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 13 "Net-(C15-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 189.738 67.31 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C10" (at -3.175 0.889) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/VEE-U1") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 165.227 78.486)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-240K?qs=oAGoVhmvjhw1AcZeqwH5DQ%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-240K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-240K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R17" (at -2.286 0 90) (layer "F.SilkS"))
    (fp_text value "240K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/OUT-BP") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-18_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 176.022 54.102)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Distributor" "Thonk")
    (property "Distributor2" "Electric Druid")
    (property "Distributor3" "SynthCube")
    (property "DistributorPartLink" "https://www.thonk.co.uk/shop/cem3320/")
    (property "DistributorPartLink2" "https://electricdruid.net/product/as3320-vcf/")
    (property "DistributorPartLink3" "https://synthcube.com/cart/synth-diy/parts/ics-and-semiconductors/alfa-rpar-as3320-vcf-ic-cem3320-replacement")
    (property "DistributorPartNum" "EComp_Chip_CURTIS_CEM3320")
    (property "DistributorPartNum2" "AS3320")
    (property "DistributorPartNum3" "ARAS3320MSTR")
    (property "Manufacturer" "Curtis Electromusic")
    (property "ManufacturerPartNum" "3320")
    (property "Note" "or AS3320")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 22.86) (layer "F.SilkS"))
    (fp_text value "CEM3320" (at 3.81 22.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 10.16) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)") (pinfunction "IN") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(R23-Pad2)") (pinfunction "IN") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C12-Pad1)") (pinfunction "CAP") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "unconnected-(U1-Pad5)") (pinfunction "CAP") (pintype "passive+no_connect"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(C13-Pad1)") (pinfunction "OUT") (pintype "output"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "OUT-HP") (pinfunction "OUT") (pintype "output"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(R18-Pad2)") (pinfunction "FB") (pintype "input"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R19-Pad2)") (pinfunction "Q-CTRL") (pintype "input"))
    (pad "10" thru_hole oval (at 7.62 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "unconnected-(U1-Pad10)") (pinfunction "OUT") (pintype "output+no_connect"))
    (pad "11" thru_hole oval (at 7.62 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "unconnected-(U1-Pad11)") (pinfunction "CAP") (pintype "passive+no_connect"))
    (pad "12" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(H12-Pad1)") (pinfunction "FREQ-CTRL") (pintype "input"))
    (pad "13" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "/VEE-U1") (pinfunction "VEE") (pintype "power_in"))
    (pad "14" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "VCC") (pintype "power_in"))
    (pad "15" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "OUT-LP") (pinfunction "OUT") (pintype "output"))
    (pad "16" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C14-Pad1)") (pinfunction "CAP") (pintype "passive"))
    (pad "17" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(R25-Pad2)") (pinfunction "IN") (pintype "input"))
    (pad "18" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "unconnected-(U1-Pad18)") (pinfunction "IN") (pintype "input+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-18_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 197.993 106.553 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-130K?qs=oAGoVhmvjhwGhRGh%2FUMCLQ%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-130K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-130K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R8" (at 9.652 0.127 180) (layer "F.SilkS"))
    (fp_text value "130K" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R11-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 172.847 71.755 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R23" (at 9.906 0 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "OUT-HP") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 194.818 89.408 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R10" (at 3.81 -2.667) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R10-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Rect_L7.2mm_W4.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 172.466 61.722 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/KEMET/PFR5151J63J11L4BULK?qs=RAUrRqLvb8zdG9mspb4b0g%3D%3D")
    (property "DistributorPartNum" "80-PFR5151J63J11L4")
    (property "Manufacturer" "KEMET")
    (property "ManufacturerPartNum" "PFR5151J63J11L4BULK")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C12" (at 8.382 -0.127) (layer "F.SilkS"))
    (fp_text value "150P" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 172.466 110.871 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-91K?qs=oAGoVhmvjhwj2HNQ9kIoow%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-91K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-91K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R14" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "91K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 176.022 81.026)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-25FTE52-2M61?qs=oAGoVhmvjhyTQINNEBI3Mg%3D%3D")
    (property "DistributorPartNum" "603-MFR-25FTE52-2M61")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-25FTE52-2M61")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R21" (at -2.794 0.889 180) (layer "F.SilkS"))
    (fp_text value "2M61" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(R19-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 194.691 103.632 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R11" (at 3.81 2.54) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(R11-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 207.01 68.072 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R4" (at 10.414 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "CV-RES-MOD-N") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 199.39 86.995)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTE52-1M?qs=xZ%2FP%252Ba9zWqaGhNxFhIbSiQ%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTE52-1M")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTE52-1M")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R26" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1M" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C15-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 185.039 125.73 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Texas-Instruments/TL072BCP?qs=p6YqzpSxLIxmo8AyZLsP4g%3D%3D")
    (property "DistributorPartNum" "595-TL072BCP")
    (property "Manufacturer" "Texas Instruments")
    (property "ManufacturerPartNum" "TL072BCP")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "TL072" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "OUT-AUDIO-LP-HP") (pintype "output"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(R28-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C15-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "6" thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(R27-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "OUT-AUDIO-BP") (pintype "output"))
    (pad "8" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Rect_L7.2mm_W4.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 187.198 58.801)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/KEMET/PFR5151J63J11L4BULK?qs=RAUrRqLvb8zdG9mspb4b0g%3D%3D")
    (property "DistributorPartNum" "80-PFR5151J63J11L4")
    (property "Manufacturer" "KEMET")
    (property "ManufacturerPartNum" "PFR5151J63J11L4BULK")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C14" (at 8.001 0) (layer "F.SilkS"))
    (fp_text value "150P" (at 2.5 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 164.846 46.99)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-25FRF52-300K?qs=oAGoVhmvjhxjcdON%252BfMhbw%3D%3D")
    (property "DistributorPartNum" "603-MFR-25FRF52-300K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-25FRF52-300K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R15" (at -2.286 0 90) (layer "F.SilkS"))
    (fp_text value "300K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 172.426 54.102 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/TDK/FG18C0G1H100DNT00?qs=vNwBHymccZ%252BO2Seu5xWjag%3D%3D")
    (property "DistributorPartNum" "810-FG18C0G1H100DNT0")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18C0G1H100DNT00")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "C0G/NP0")
    (attr through_hole)
    (fp_text reference "C8" (at 5.421 0) (layer "F.SilkS"))
    (fp_text value "10P" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "OUT-HP") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:CP_Radial_D4.0mm_P2.50mm" (layer "F.Cu")
    (tedit 612547C9)
    (at 171.069 107.3946 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=4mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 4mm Electrolytic Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Panasonic/ECE-A1HKA4R7I?qs=AfGmtpoX2giUuCvV8uNbmg%3D%3D")
    (property "DistributorPartNum" "667-ECE-A1HKA4R7I")
    (property "Manufacturer" "Panasonic")
    (property "ManufacturerPartNum" "ECE-A1HKA4R7I")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at -0.0474 -3.556 180) (layer "F.SilkS"))
    (fp_text value "4U7" (at 1.25 3.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 4 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 90) (size 1.2 1.2) (drill 0.6) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P1.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 189.357 50.419)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-91K?qs=oAGoVhmvjhwj2HNQ9kIoow%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-91K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-91K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R24" (at 10.414 0) (layer "F.SilkS"))
    (fp_text value "91K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "OUT-LP") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-holes:WireHole_D0.8mm_OD1.6mm" (layer "F.Cu")
    (tedit 0)
    (at 187.198 70.739)
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (attr smd exclude_from_bom)
    (fp_text reference "H12" (at 0 -1.6002 unlocked) (layer "F.SilkS") hide)
    (fp_text value "WireHole_PTH" (at 0 1 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(H12-Pad1)") (pintype "passive"))
  )
  (footprint "-lmp-synth:Potentiometer_Bourns_3296WY_Vertical" (layer "F.Cu")
    (tedit 621A5B3C)
    (at 193.294 109.728)
    (descr "Potentiometer, vertical, Bourns 3296W or 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W 3296Y")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Bourns/3296W-1-253LF?qs=LzhUookPeqx7TmETxQk59w%3D%3D")
    (property "DistributorPartNum" "652-3296W-1-253LF")
    (property "Label" "TUNE")
    (property "Manufacturer" "Bourns")
    (property "ManufacturerPartNum" "3296W-1-253LF")
    (property "Note" "3296W or 3296Y type")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV6" (at -9.398 -1.397) (layer "F.SilkS"))
    (fp_text value "25K" (at -2.54 3.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0.005) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R8-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 -1.275) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R8-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 1.265) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "3") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 -1.275) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "3") (pintype "passive"))
    (model "${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-holes:MountingHole_PCB_3.2mm_M3" locked (layer "F.Cu")
    (tedit 622675F6)
    (at 182.5498 134.112)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm m3")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (property "exclude_from_bom" "")
    (clearance 1.15)
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "H3" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "MountingHole_M3" (at 0 0.009) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 183.642 84.709 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R12" (at 10.414 0) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(R10-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-synth:Potentiometer_Bourns_3296WY_Vertical" (layer "F.Cu")
    (tedit 621A5B3C)
    (at 184.277 41.783)
    (descr "Potentiometer, vertical, Bourns 3296W or 3296Y, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W 3296Y")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/Bourns/3296W-1-202LF?qs=4IMUa6xHmlqkuL3XP8CD4w%3D%3D")
    (property "DistributorPartNum" "652-3296W-1-202LF")
    (property "Label" "DC TRIM")
    (property "Manufacturer" "Bourns")
    (property "ManufacturerPartNum" "3296W-1-202LF")
    (property "Note" "3296W or 3296Y type")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RV8" (at -6.223 3.683) (layer "F.SilkS"))
    (fp_text value "2K" (at -2.54 3.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0.005) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(R22-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 -1.275) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(R22-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 1.265) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 -1.275) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "3") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "-12V") (pinfunction "3") (pintype "passive"))
    (model "${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 207.01 90.678 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-200K?qs=oAGoVhmvjhzyXGTT6oqbfw%3D%3D")
    (property "DistributorPartNum" " 603-MFR-12FTF52-200K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-200K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R1" (at 3.048 -2.667) (layer "F.SilkS"))
    (fp_text value "200K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "IN-AUDIO") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 166.243 118.491)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-68K?qs=oAGoVhmvjhyL5MsnBkXRfA%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-68K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-68K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R27" (at -2.667 0) (layer "F.SilkS"))
    (fp_text value "68K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/OUT-BP") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(R27-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 187.198 63.119)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/810-FG18X7R1H104KNT6")
    (property "DistributorPartNum" "810-FG18X7R1H104KNT6")
    (property "Manufacturer" "TDK")
    (property "ManufacturerPartNum" "FG18X7R1H104KNT06")
    (property "Note" "IC decoupling")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C9" (at 5.334 0) (layer "F.SilkS"))
    (fp_text value "100N" (at 1.25 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 172.466 50.546 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R20" (at 9.906 0.127 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "OUT-HP") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 207.01 71.374 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R3" (at 9.906 -0.127) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "CV-RES-MOD-P") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R10-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 172.466 92.329 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R16" (at 9.525 0 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(R12-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 172.466 101.092 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R9" (at 3.81 -2.37) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "-lmp-misc:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 199.39 77.978)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Distributor" "Mouser")
    (property "DistributorPartLink" "https://www.mouser.ca/ProductDetail/YAGEO/MFR-12FTF52-100K?qs=oAGoVhmvjhxn7uX6J9%2FOug%3D%3D")
    (property "DistributorPartNum" "603-MFR-12FTF52-100K")
    (property "Manufacturer" "YAGEO")
    (property "ManufacturerPartNum" "MFR-12FTF52-100K")
    (property "Sheetfile" "VCF-SV.kicad_sch")
    (property "Sheetname" "")
    (property "Value2" "1%, 1/6 W")
    (attr through_hole)
    (fp_text reference "R6" (at 0 2.54) (layer "F.SilkS"))
    (fp_text value "100K" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "CV-FREQ-1VOCT") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x15_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 210.52 59.69 180)
    (descr "Through hole straight pin header, 1x15, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x15 2.54mm single row")
    (property "Distributor" "Adafruit")
    (property "Distributor2" "Mouser")
    (property "DistributorPartLink" "https://www.adafruit.com/product/392")
    (property "DistributorPartLink2" "https://www.mouser.ca/ProductDetail/649-1012937893601BLF")
    (property "DistributorPartNum" "392")
    (property "DistributorPartNum2" "649-1012937893601BLF")
    (property "Sheetfile" "PanelPower.kicad_sch")
    (property "Sheetname" "PanelPower")
    (attr through_hole)
    (fp_text reference "J11" (at 0.589 -37.973) (layer "B.SilkS"))
    (fp_text value "Conn_Back_Right_Top" (at 0 -37.89) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -17.78 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "CV-FREQ-POT") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "CV-RES-POT") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "CV-RES-MOD-N") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "CV-RES-MOD-P") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "CV-FREQ-MOD") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "CV-FREQ-1VOCT") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "OUT-HP") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "OUT-LP-HP") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "OUT-LP") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "IN-CV-BUS") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 -27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "IN-AUDIO") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "OUT-AUDIO-BP") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 -33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "OUT-AUDIO-LP-HP") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x15_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 161.29 137.414) (end 161.29 38.608) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 161.29 38.608) (end 211.79 38.608) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 211.79 137.414) (end 161.29 137.414) (layer "Edge.Cuts") (width 0.1524))
  (gr_line (start 211.79 38.608) (end 211.79 137.414) (layer "Edge.Cuts") (width 0.1524))
  (gr_text "© 2022 Len Popp" (at 210.947 42.291) (layer "F.SilkS"))
  (gr_text "-12V" (at 198.541996 136.144) (layer "F.SilkS"))
  (gr_text "SV-VCF" (at 162.179 40.767) (layer "F.SilkS"))
  (gr_text "https://len42.github.io/" (at 210.947 40.259) (layer "F.SilkS"))
  (gr_text "CV BUS" (at 211.328 105.918) (layer "F.SilkS"))
  (gr_text "rev. ${REVISION}" (at 166.751 43.18) (layer "F.SilkS"))
  (gr_text "RT1" (at 169.799 57.658) (layer "F.SilkS"))
  (gr_text "SCALE" (at 189.738 86.487) (layer "F.SilkS"))
  (gr_text "RT1" (at 187.198 72.771) (layer "F.SilkS"))
  (gr_text "DC\nTRIM" (at 187.325 41.91) (layer "F.SilkS"))
  (gr_text "Main" (at 162.179 43.18) (layer "F.SilkS"))
  (gr_text "TUNE" (at 182.245 110.617) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.381) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 212.511996 144.145)
        (xy 160.314996 144.145)
        (xy 160.314996 38.227)
        (xy 212.511996 38.227)
      )
    )
  )
)
