(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (comment 4 "AISLER Project ID: FMWPPUGV")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (aux_axis_origin 88.9 47.9044)
    (grid_origin 88.9 69.85)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "Net-(D2-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J4-Pad4)")
  (net 6 "Net-(J4-Pad3)")
  (net 7 "Net-(J4-Pad2)")
  (net 8 "Net-(J4-Pad1)")
  (net 9 "Net-(J3-Pad4)")
  (net 10 "Net-(J3-Pad3)")
  (net 11 "Net-(J3-Pad2)")
  (net 12 "Net-(J3-Pad1)")
  (net 13 "Net-(R1-Pad2)")
  (net 14 "Net-(R2-Pad2)")
  (net 15 "Net-(D1-Pad1)")
  (net 16 "Net-(J1-Pad4)")
  (net 17 "Net-(Q1-Pad1)")
  (net 18 "Net-(J2-Pad4)")
  (net 19 "Net-(J2-Pad3)")
  (net 20 "Net-(J2-Pad2)")
  (net 21 "Net-(J2-Pad1)")
  (footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical" (layer "F.Cu")
    (tedit 5C28146C)
    (at 91.9226 66.7004 90)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (attr through_hole)
    (fp_text reference "J1" (at 3.7592 1.8034) (layer "F.SilkS"))
    (fp_text value "JST XH" (at 3.75 4.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 2.7 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 15 "Net-(D1-Pad1)"))
    (pad "2" thru_hole oval locked (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad "3" thru_hole oval locked (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad "4" thru_hole oval locked (at 7.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad4)"))
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 101.1014 54.2696)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (attr smd)
    (fp_text reference "Q1" (at -2.21412 0.00512 180) (layer "F.SilkS"))
    (fp_text value "BC847/547" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(Q1-Pad1)"))
    (pad "2" smd rect locked (at -1 0.95) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J1-Pad4)"))
    (pad "3" smd rect locked (at 1 0) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(D1-Pad2)"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 100.4984 50.231 180)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (attr smd)
    (fp_text reference "Q2" (at -1.99568 -0.03052 180) (layer "F.SilkS"))
    (fp_text value "BC847/547" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 -0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(Q1-Pad1)"))
    (pad "2" smd rect locked (at -1 0.95 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(J1-Pad4)"))
    (pad "3" smd rect locked (at 1 0 180) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "Net-(D2-Pad2)"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 96.45396 67.52326 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.39268 -0.08128 90) (layer "F.SilkS"))
    (fp_text value "390R" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.9905 0.0635 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad2)"))
    (pad "2" smd roundrect locked (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(R1-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5B301BBD)
    (at 101.81346 56.80964)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (attr smd)
    (fp_text reference "R2" (at 0.90414 -1.10236) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(Q1-Pad1)"))
    (pad "2" smd roundrect locked (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(R2-Pad2)"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 100.08108 63.53048 90)
    (descr "4-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils), Clearance8mm")
    (tags "SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil Clearance8mm")
    (attr smd)
    (fp_text reference "U1" (at 0.23368 0.127 90) (layer "F.SilkS"))
    (fp_text value "TLP521" (at 0 3.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -4.765 -1.27 90) (size 1.5 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "Net-(R1-Pad2)"))
    (pad "2" smd rect locked (at -4.765 1.27 90) (size 1.5 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J1-Pad3)"))
    (pad "3" smd rect locked (at 4.765 1.27 90) (size 1.5 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(R2-Pad2)"))
    (pad "4" smd rect locked (at 4.765 -1.27 90) (size 1.5 1.78) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "Net-(D1-Pad1)"))
    (model "${KISYS3DMOD}/Package_DIP.3dshapes/SMDIP-4_W9.53mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_DPDT_Omron_G5V-2" (layer "F.Cu")
    (tedit 5FCDDFF6)
    (at 104.902 50.292)
    (descr "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v2.pdf")
    (tags "Omron G5V-2 Relay DPDT")
    (attr through_hole)
    (fp_text reference "K1" (at 3.81 9.779) (layer "F.SilkS"))
    (fp_text value "G6A-274P" (at -2.41 9.01 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.94 9.16) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 -0.002) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (pad "4" thru_hole circle locked (at 0 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad3)"))
    (pad "6" thru_hole circle locked (at 0 12.69) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad3)"))
    (pad "8" thru_hole circle locked (at 0 17.78) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (pad "9" thru_hole circle locked (at 7.63 17.79) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad4)"))
    (pad "11" thru_hole circle locked (at 7.63 12.71) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(J4-Pad4)"))
    (pad "13" thru_hole circle locked (at 7.62 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad "16" thru_hole circle locked (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad2)"))
    (model "${KISYS3DMOD}/Relay_THT.3dshapes/Relay_DPDT_Omron_G5V-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical" (layer "F.Cu")
    (tedit 5C28146C)
    (at 141.9352 62.8142 90)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (attr through_hole)
    (fp_text reference "J3" (at 3.7465 2.1209 180) (layer "F.SilkS"))
    (fp_text value "JST XH" (at 3.75 4.6 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 2.7 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 12 "Net-(J3-Pad1)"))
    (pad "2" thru_hole oval locked (at 2.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad2)"))
    (pad "3" thru_hole oval locked (at 5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad3)"))
    (pad "4" thru_hole oval locked (at 7.5 0 90) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad4)"))
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_DPDT_Omron_G5V-2" (layer "F.Cu")
    (tedit 5FCDDFFF)
    (at 129.3876 50.1904)
    (descr "http://omronfs.omron.com/en_US/ecb/products/pdf/en-g5v2.pdf")
    (tags "Omron G5V-2 Relay DPDT")
    (attr through_hole)
    (fp_text reference "K2" (at 4.0005 10.0965) (layer "F.SilkS"))
    (fp_text value "G6A-274P" (at -2.41 9.01 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.94 9.16) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0.0996) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (pad "4" thru_hole circle locked (at 0 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad2)"))
    (pad "6" thru_hole circle locked (at 0 12.69) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)"))
    (pad "8" thru_hole circle locked (at 0 17.78) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(J3-Pad2)"))
    (pad "9" thru_hole circle locked (at 7.63 17.79) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(J3-Pad1)"))
    (pad "11" thru_hole circle locked (at 7.63 12.71) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(J4-Pad1)"))
    (pad "13" thru_hole circle locked (at 7.62 7.62) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad1)"))
    (pad "16" thru_hole circle locked (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(D2-Pad2)"))
    (model "${KISYS3DMOD}/Relay_THT.3dshapes/Relay_DPDT_Omron_G5V-2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical" (layer "F.Cu")
    (tedit 5FCDDFEB)
    (at 124.4854 53.0352 180)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (attr through_hole)
    (fp_text reference "J2" (at 3.7973 2.1844) (layer "F.SilkS"))
    (fp_text value "JST XH" (at 3.75 4.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 2.7) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0.046 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147)
      (net 21 "Net-(J2-Pad1)"))
    (pad "2" thru_hole oval locked (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad2)"))
    (pad "3" thru_hole oval locked (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad3)"))
    (pad "4" thru_hole oval locked (at 7.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical" (layer "F.Cu")
    (tedit 5FCDDFE3)
    (at 124.5616 60.6044 180)
    (descr "JST XH series connector, B4B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (attr through_hole)
    (fp_text reference "J4" (at 3.8735 2.2098) (layer "F.SilkS"))
    (fp_text value "JST XH" (at 3.75 4.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 2.7) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at -0.0048 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask) (roundrect_rratio 0.147)
      (net 8 "Net-(J4-Pad1)"))
    (pad "2" thru_hole oval locked (at 2.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)"))
    (pad "3" thru_hole oval locked (at 5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad3)"))
    (pad "4" thru_hole oval locked (at 7.5 0 180) (size 1.7 1.95) (drill 0.95) (layers *.Cu *.Mask)
      (net 5 "Net-(J4-Pad4)"))
    (model "${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B4B-XH-A_1x04_P2.50mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7)
    (at 133.2229 50.292)
    (descr "SOD-123")
    (tags "SOD-123")
    (attr smd)
    (fp_text reference "D2" (at 0 2 180) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0 -2.1 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 180) (layer "B.Fab"))
    (pad "1" smd rect (at -1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "Net-(D1-Pad1)"))
    (pad "2" smd rect (at 1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "Net-(D2-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "B.Cu")
    (tedit 58645DC7)
    (at 108.8389 50.2666)
    (descr "SOD-123")
    (tags "SOD-123")
    (attr smd)
    (fp_text reference "D1" (at 0 2 180) (layer "B.SilkS"))
    (fp_text value "1N4148" (at 0 -2.1 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2 180) (layer "B.Fab"))
    (pad "1" smd rect (at -1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "Net-(D1-Pad1)"))
    (pad "2" smd rect (at 1.65 0) (size 0.9 1.2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "Net-(D1-Pad2)"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 158.75 44.5135) (end 158.75 44.5135) (layer "Edge.Cuts") (width 0.05))
  (gr_circle (center 95.31096 50.55128) (end 96.91096 50.55128) (layer "Edge.Cuts") (width 0.5) (fill none))
  (gr_line (start 145.796 47.879) (end 88.9 47.879) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 88.9 69.85) (end 145.796 69.85) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 145.796 69.85) (end 145.796 47.879) (layer "Edge.Cuts") (width 0.1))
  (gr_circle (center 125.1966 66.66484) (end 126.7966 66.66484) (layer "Edge.Cuts") (width 0.5) (fill none))
  (gr_line (start 88.9 47.879) (end 88.9 69.85) (layer "Edge.Cuts") (width 0.1))
  (gr_text "1A" (at 144.511223 60.4266) (layer "B.SilkS"))
  (gr_text "1B" (at 144.40408 62.87008) (layer "B.SilkS"))
  (gr_text "2B" (at 144.40408 55.35676) (layer "B.SilkS"))
  (gr_text "2A" (at 144.511223 57.94248) (layer "B.SilkS"))
  (gr_text "GND" (at 95.2754 59.309) (layer "B.SilkS"))
  (gr_text "-2B-" (at 116.98224 56.8198 90) (layer "B.SilkS"))
  (gr_text "-2A-" (at 119.4308 56.819801 90) (layer "B.SilkS"))
  (gr_text "+3.3V" (at 96.0374 64.2239) (layer "B.SilkS"))
  (gr_text "Signal" (at 96.0755 61.6458) (layer "B.SilkS"))
  (gr_text "+5V" (at 95.3008 66.7639) (layer "B.SilkS"))
  (gr_text "-1B-" (at 124.49556 56.8198 90) (layer "B.SilkS"))
  (gr_text "-1A-" (at 121.95048 56.819801 90) (layer "B.SilkS"))
  (gr_text "to Stepper" (at 118.2878 56.388) (layer "F.SilkS"))
  (gr_text "SMuFF\nCtrl" (at 92.6084 54.8767) (layer "F.SilkS"))
  (gr_text "from\nSMuFF" (at 142.40256 50.72888) (layer "F.SilkS"))
  (gr_text "2020-2023 by\nTechnik Gegg" (at 114.30508 67.90944) (layer "F.SilkS"))
  (gr_text "from Printer" (at 118.9228 63.9445) (layer "F.SilkS"))
  (gr_text "Rev:2\n" (at 141.61008 67.47256) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Margin")
    (pts (xy 125.42012 66.83248) (xy 125.42012 69.85508))
    (height -22.6568)
    (gr_text "3.0226 mm" (at 146.92692 68.34378 90) (layer "Margin"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Margin")
    (pts (xy 88.93048 50.57648) (xy 95.33128 50.57648))
    (height -6.27888)
    (gr_text "6.4008 mm" (at 92.13088 43.1476) (layer "Margin"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Margin")
    (pts (xy 95.33128 47.88408) (xy 95.33128 50.5968))
    (height 9.58088)
    (gr_text "2.7127 mm" (at 84.6004 49.24044 90) (layer "Margin"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Margin")
    (pts (xy 145.796 47.879) (xy 145.796 69.85))
    (height -5.715)
    (gr_text "21.9710 mm" (at 150.361 58.8645 90) (layer "Margin"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Margin")
    (pts (xy 125.4252 69.9135) (xy 88.8873 69.85))
    (height -2.451007)
    (gr_text "36.5380 mm" (at 107.153989 71.182755 -0.09957546373) (layer "Margin"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Margin")
    (pts (xy 145.796 69.85) (xy 88.8873 69.85))
    (height -5.4991)
    (gr_text "56.9087 mm" (at 117.34165 74.1991) (layer "Margin"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.12) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.CrtYd")
    (pts (xy 145.796 47.879) (xy 145.796 69.85))
    (height -1.3335)
    (gr_text "21.9710 mm" (at 145.9795 58.8645 90) (layer "F.CrtYd"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.05) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 16) (net_name "Net-(J1-Pad4)") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.91524 47.85868)
        (xy 88.91524 69.81444)
        (xy 145.72488 69.81444)
        (xy 145.72488 47.88408)
        (xy 88.92032 47.86376)
      )
    )
  )
)
