(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 29)
    (zones 0)
    (modules 6)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/rev0/"))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad5)")
  (net 2 GND)
  (net 3 VCC)
  (net 4 "Net-(A1-Pad7)")
  (net 5 "Net-(A1-Pad8)")
  (net 6 "Net-(A1-Pad12)")
  (net 7 "Net-(A1-Pad11)")
  (net 8 "Net-(A1-Pad9)")
  (net 9 "Net-(A1-Pad10)")
  (net 10 "Net-(A1-Pad4)")
  (net 11 SCL)
  (net 12 SDA)
  (net 13 /ADDR)
  (net 14 "Net-(A1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ADDR)
    (add_net GND)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad4)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(J1-Pad5)")
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
  )
  (module MELEXIS_TECHNOLOGIES_NV_MLX90640ESF-BAA-000-TU:MELEXIS_TECHNOLOGIES_NV_MLX90640ESF-BAA-000-TU_0 (layer F.Cu) (tedit 5F08C176)
    (at 26.67 40.64 315)
    (descr "32x24 Thermal Array Sensor 3.3V 120 Degree Total FOV")
    (fp_text reference U1 (at -2.3 -5.5 135) (layer F.SilkS) hide)
    (fp_text value MLX90640 (at 0 0 135) (layer F.Fab))
    (pad 3 thru_hole circle (at -2.698 -1.117 315) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.117 -2.698 315) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 4 thru_hole circle (at 1.117 2.698 315) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 11 SCL))
    (pad 1 thru_hole rect (at 2.698 1.117 315) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 SDA))
  )
  (module Adafruit:Adafruit_MCP2221A_Breakout (layer F.Cu) (tedit 5F3FCACB)
    (at 36.83 27.94)
    (descr "General Purpose USB to GPIO ADC I2C, https://www.adafruit.com/product/4471")
    (tags "MCP2221A GPIO ADC I2C Stemma QT")
    (fp_text reference A1 (at 6.35 -7.35) (layer F.SilkS) hide)
    (fp_text value Adafruit_MCP2221A_Breakout (at 6.35 20.32) (layer F.Fab))
    (fp_text user %R (at 6.35 6.35) (layer F.Fab))
    (pad 7 thru_hole oval (at 12.7 12.7) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad7)"))
    (pad 8 thru_hole oval (at 12.7 10.16) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad8)"))
    (pad 12 thru_hole circle (at 12.7 0) (size 2.1 2.1) (drill 1.02) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad12)"))
    (pad 11 thru_hole oval (at 12.7 2.54) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 7 "Net-(A1-Pad11)"))
    (pad 9 thru_hole oval (at 12.7 7.62) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad9)"))
    (pad 10 thru_hole oval (at 12.7 5.08) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad10)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 3 VCC))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 11 SCL))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.1 1.9) (drill 1.02) (layers *.Cu *.Mask)
      (net 12 SDA))
    (model ${KISYS3DMOD}/Module.3dshapes/Adafruit_HUZZAH_ESP8266_breakout.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745284)
    (at 54.61 45.72)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference INT (at 0 -1.778) (layer F.SilkS))
    (fp_text value SolderJumper_2_Bridged (at 0 1.9) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 4 "Net-(A1-Pad7)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 "Net-(J1-Pad5)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5C745321)
    (at 59.69 45.72)
    (descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference ADDR (at 0 -1.8) (layer F.SilkS))
    (fp_text value SolderJumper_3_Bridged12 (at 0 1.9) (layer F.Fab))
    (pad 1 smd custom (at -1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 2 GND) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)) (width 0))
      ))
    (pad 2 smd rect (at 0 0) (size 1 1.5) (layers F.Cu F.Mask)
      (net 13 /ADDR))
    (pad 3 smd custom (at 1.3 0) (size 1 0.5) (layers F.Cu F.Mask)
      (net 3 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy -0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy -0.55 0.75)) (width 0))
      ))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A430)
    (at 58.42 26.67)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference "ElectronicFans OPT3001" (at -2.54 5.08 90) (layer F.SilkS))
    (fp_text value "ElectronicFans OPT3001" (at 0 15.47) (layer F.Fab))
    (fp_text user %R (at 0 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /ADDR))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 SDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 30.48 36.195 135)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference C1 (at 0 1.27 135) (layer F.SilkS))
    (fp_text value C (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.7875 0 135) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VCC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 31.75 31.75) (end 31.75 33.02) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 60.96 45.72) (end 60.96 48.26) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 22.86 45.72) (end 20.32 45.72) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 22.86 35.56) (end 22.86 33.02) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 60.96 22.86) (end 63.5 22.86) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 35.56 22.86) (end 35.56 20.32) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 60.96 20.32) (end 35.56 20.32) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.5 45.72) (end 63.5 22.86) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 22.86 48.26) (end 60.96 48.26) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 20.32 35.56) (end 20.32 45.72) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 31.75 33.02) (end 22.86 33.02) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 33.02 22.86) (end 33.02 31.75) (layer Edge.Cuts) (width 0.05))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.77 49.53) (xy 19.05 49.53) (xy 19.05 19.05) (xy 64.77 19.05)
      )
    )
  )
  (zone (net 3) (net_name VCC) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.77 49.53) (xy 19.05 49.53) (xy 19.05 19.05) (xy 64.77 19.05)
      )
    )
  )
)
