(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 26)
    (no_connects 0)
    (area 74.422 48.641 253.746001 141.097001)
    (thickness 1.6)
    (drawings 27)
    (tracks 565)
    (zones 0)
    (modules 23)
    (nets 38)
  )
  (page A4)
  (title_block
    (date "lun. 30 mars 2015")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 2.08)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 3.048)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 110.998 126.365)
    (grid_origin 110.998 126.365)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /IOREF)
  (net 2 /Reset)
  (net 3 +5V)
  (net 4 GND)
  (net 5 /Vin)
  (net 6 /A0)
  (net 7 /A1)
  (net 8 /A2)
  (net 9 /A3)
  (net 10 /AREF)
  (net 11 "/A4(SDA)")
  (net 12 "/A5(SCL)")
  (net 13 "/9(**)")
  (net 14 /8)
  (net 15 /7)
  (net 16 "/6(**)")
  (net 17 /4)
  (net 18 "/1(Tx)")
  (net 19 "/0(Rx)")
  (net 20 "/13(SCK)")
  (net 21 "/10(**/SS)")
  (net 22 "Net-(P1-Pad1)")
  (net 23 +3V3)
  (net 24 "/12(MISO)")
  (net 25 "/11(**/MOSI)")
  (net 26 /Red_Source)
  (net 27 /Red_Drain)
  (net 28 /Red_Gate)
  (net 29 /Green_Source)
  (net 30 /Green_Drain)
  (net 31 /Green_Gate)
  (net 32 /Blue_Source)
  (net 33 /Blue_Drain)
  (net 34 /Blue_Gate)
  (net 35 /Red_Gate1)
  (net 36 /Green_Gate1)
  (net 37 /Blue_Gate1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 2.08)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net "/0(Rx)")
    (add_net "/1(Tx)")
    (add_net "/10(**/SS)")
    (add_net "/11(**/MOSI)")
    (add_net "/12(MISO)")
    (add_net "/13(SCK)")
    (add_net /4)
    (add_net "/6(**)")
    (add_net /7)
    (add_net /8)
    (add_net "/9(**)")
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net "/A4(SDA)")
    (add_net "/A5(SCL)")
    (add_net /AREF)
    (add_net /Blue_Drain)
    (add_net /Blue_Gate)
    (add_net /Blue_Gate1)
    (add_net /Blue_Source)
    (add_net /Green_Drain)
    (add_net /Green_Gate)
    (add_net /Green_Gate1)
    (add_net /Green_Source)
    (add_net /IOREF)
    (add_net /Red_Drain)
    (add_net /Red_Gate)
    (add_net /Red_Gate1)
    (add_net /Red_Source)
    (add_net /Reset)
    (add_net /Vin)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 552168D2)
    (at 138.938 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 8.89 -2.54) (layer F.SilkS))
    (fp_text value Power (at 8.89 -4.064) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /IOREF))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Reset))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 +3V3))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /Vin))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x06 locked (layer F.Cu) (tedit 552168D6)
    (at 161.798 123.825)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at 6.604 -2.54) (layer F.SilkS))
    (fp_text value Analog (at 6.604 -4.064) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /A0))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /A1))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /A2))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /A3))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "/A4(SDA)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "/A5(SCL)"))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x06.wrl
      (at (xyz 0.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x10 locked (layer F.Cu) (tedit 552168BF)
    (at 129.794 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P3 (at 11.43 2.794) (layer F.SilkS))
    (fp_text value Digital (at 11.43 4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "/A5(SCL)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "/A4(SDA)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /AREF))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "/13(SCK)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "/12(MISO)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "/11(**/MOSI)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "/10(**/SS)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "/9(**)"))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /8))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x10.wrl
      (at (xyz 0.45 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Socket_Strip_Arduino_1x08 locked (layer F.Cu) (tedit 552168C7)
    (at 156.718 75.565)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P4 (at 8.89 2.794) (layer F.SilkS))
    (fp_text value Digital (at 8.89 4.318) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /7))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "/6(**)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /Green_Source))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /4))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /Blue_Source))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /Red_Source))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "/1(Tx)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "/0(Rx)"))
    (model ${KIPRJMOD}/Socket_Arduino_Uno.3dshapes/Socket_header_Arduino_1x08.wrl
      (at (xyz 0.35 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5BEAF838)
    (at 124.968 123.825)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P5 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5BEAF7FB)
    (at 177.038 118.745)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P6 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5BEAF830)
    (at 126.238 75.565)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P7 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Socket_Arduino_Uno:Arduino_1pin locked (layer F.Cu) (tedit 5BEAF823)
    (at 177.038 90.805)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P8 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 3.048) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
  )
  (module Parts:Mosfet30V60A (layer F.Cu) (tedit 5BD88676)
    (at 134.366 92.329)
    (fp_text reference J1 (at 0.254 2.7305) (layer F.SilkS))
    (fp_text value .1inchHeader (at 0.254 -2.4765) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /Red_Source))
    (pad 2 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /Red_Drain))
    (pad 3 thru_hole circle (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 /Red_Gate))
  )
  (module Parts:Mosfet30V60A (layer F.Cu) (tedit 5BD88676)
    (at 154.686 84.709)
    (fp_text reference J2 (at 0.254 2.7305) (layer F.SilkS))
    (fp_text value .1inchHeader (at 0.254 -2.4765) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 /Green_Source))
    (pad 2 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /Green_Drain))
    (pad 3 thru_hole circle (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /Green_Gate))
  )
  (module Parts:Mosfet30V60A (layer F.Cu) (tedit 5BD88676)
    (at 161.798 104.013)
    (fp_text reference J3 (at 0.254 2.7305) (layer F.SilkS))
    (fp_text value .1inchHeader (at 0.254 -2.4765) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /Blue_Source))
    (pad 2 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /Blue_Drain))
    (pad 3 thru_hole circle (at 2.54 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /Blue_Gate))
  )
  (module Parts:Through-Hole (layer F.Cu) (tedit 5BE480DD)
    (at 134.366 97.917)
    (fp_text reference P9 (at 0 3.81) (layer F.SilkS))
    (fp_text value Pad (at 0.0635 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /Red_Drain))
  )
  (module Parts:Through-Hole (layer F.Cu) (tedit 5BE480DD)
    (at 141.986 99.441)
    (fp_text reference P10 (at 0 3.81) (layer F.SilkS))
    (fp_text value Pad (at 0.0635 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /Red_Gate1))
  )
  (module Parts:Through-Hole (layer F.Cu) (tedit 5BE480DD)
    (at 149.098 89.789)
    (fp_text reference P11 (at 0 3.81) (layer F.SilkS))
    (fp_text value Pad (at 0.0635 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 /Green_Drain))
  )
  (module Parts:Through-Hole (layer F.Cu) (tedit 5BE480DD)
    (at 154.178 96.393)
    (fp_text reference P12 (at 0 3.81) (layer F.SilkS))
    (fp_text value Pad (at 0.0635 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /Green_Gate1))
  )
  (module Parts:Through-Hole (layer F.Cu) (tedit 5BE480DD)
    (at 157.734 112.141)
    (fp_text reference P13 (at 0 3.81) (layer F.SilkS))
    (fp_text value Pad (at 0.0635 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /Blue_Drain))
  )
  (module Parts:Through-Hole (layer F.Cu) (tedit 5BE480DD)
    (at 171.45 107.061)
    (fp_text reference P14 (at 0 3.81) (layer F.SilkS))
    (fp_text value Pad (at 0.0635 -2.794) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 /Blue_Gate1))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5BEB0FD9)
    (at 141.986 92.837 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /Red_Gate1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /Red_Gate))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5BEB1031)
    (at 157.734 89.789 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /Green_Gate1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /Green_Gate))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5BEB1000)
    (at 164.846 112.649 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.524 90) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /Blue_Gate1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /Blue_Gate))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 147.066 99.441 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /Red_Gate1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 149.606 93.345)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7) (layer F.SilkS))
    (fp_text value R (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /Green_Gate1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 167.386 107.061 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 /Blue_Gate))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 138.938 121.285 90) (layer F.SilkS))
  (gr_line (start 177.038 74.549) (end 175.514 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 85.979) (end 177.038 74.549) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 88.519) (end 177.038 85.979) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.578 121.285) (end 179.578 88.519) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 123.825) (end 179.578 121.285) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.038 126.365) (end 177.038 123.825) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.998 126.365) (end 177.038 126.365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.998 73.025) (end 110.998 126.365) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.514 73.025) (end 110.998 73.025) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 102.87 67.437) (xy 185.674 67.437) (xy 185.674 130.429) (xy 101.854 130.429) (xy 101.854 67.437)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 185.674 130.429) (xy 101.854 130.429) (xy 101.854 67.437) (xy 185.674 67.437)
      )
    )
  )
)
