(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 32)
    (no_connects 0)
    (area 119.424999 42.924999 175.575001 108.075001)
    (thickness 1.6)
    (drawings 67)
    (tracks 265)
    (zones 0)
    (modules 2)
    (nets 33)
  )
  (page A4)
  (title_block
    (title "Gameboy Cartridge Breakout")
    (date 2017-03-05)
    (rev 2)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 7)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VDD)
  (net 3 CLK)
  (net 4 WR)
  (net 5 RD)
  (net 6 CS)
  (net 7 A0)
  (net 8 A1)
  (net 9 A2)
  (net 10 A3)
  (net 11 A4)
  (net 12 A5)
  (net 13 A6)
  (net 14 A7)
  (net 15 A8)
  (net 16 A9)
  (net 17 A10)
  (net 18 A11)
  (net 19 A12)
  (net 20 A13)
  (net 21 A14)
  (net 22 A15)
  (net 23 D0)
  (net 24 D1)
  (net 25 D2)
  (net 26 D3)
  (net 27 D4)
  (net 28 D5)
  (net 29 D6)
  (net 30 D7)
  (net 31 RST)
  (net 32 AUDIO)
  (net_class Default "This is the default net class."
    (clearance 0.25)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A10)
    (add_net A11)
    (add_net A12)
    (add_net A13)
    (add_net A14)
    (add_net A15)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net A8)
    (add_net A9)
    (add_net AUDIO)
    (add_net CLK)
    (add_net CS)
    (add_net D0)
    (add_net D1)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net RD)
    (add_net RST)
    (add_net WR)
  )
  (net_class wide-track ""
    (clearance 0.25)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VDD)
  )
  (module Pin_Headers:Pin_Header_Straight_2x16_Pitch2.54mm (layer F.Cu) (tedit 58B71C80)
    (at 128.75 57.75 90)
    (descr "Through hole straight pin header, 2x16, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x16 2.54mm double row")
    (fp_text reference P1 (at 1.27 -2.39 90) (layer F.SilkS))
    (fp_text value CONN_02X16 (at -2.5 19.25 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VDD))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 CLK))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 WR))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 RD))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 CS))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 A0))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 A1))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 A2))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 A3))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 A4))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 A5))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 A6))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 A7))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 A8))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 A9))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 A10))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 A11))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 A12))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 A13))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 A14))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 A15))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 D0))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 D1))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 D2))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 D3))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 D4))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 D5))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 D6))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 D7))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 RST))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 AUDIO))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x16.wrl
      (at (xyz 0.05 -0.75 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module GameBoy:gb-cart-connector (layer F.Cu) (tedit 58B70941)
    (at 146.75 100.75)
    (fp_text reference CART1 (at -1.25 -1) (layer F.SilkS) hide)
    (fp_text value gb-cart (at -0.5 8) (layer F.Fab) hide)
    (fp_text user GND (at 24.25 -2 90) (layer F.SilkS))
    (fp_text user VDD (at -22.75 -2 90) (layer F.SilkS))
    (pad 32 connect rect (at 24.25 3.5) (size 1.5 7) (layers F.Cu F.Mask)
      (net 1 GND) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 1 connect rect (at -22.75 3.5) (size 1.5 7) (layers F.Cu F.Mask)
      (net 2 VDD) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 2 connect rect (at -21 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 3 CLK) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 3 connect rect (at -19.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 4 WR) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 4 connect rect (at -18 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 5 RD) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 5 connect rect (at -16.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 6 CS) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 6 connect rect (at -15 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 7 A0) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 7 connect rect (at -13.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 8 A1) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 8 connect rect (at -12 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 9 A2) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 9 connect rect (at -10.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 10 A3) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 10 connect rect (at -9 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 11 A4) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 11 connect rect (at -7.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 12 A5) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 12 connect rect (at -6 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 13 A6) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 13 connect rect (at -4.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 14 A7) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 14 connect rect (at -3 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 15 A8) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 15 connect rect (at -1.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 16 A9) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 16 connect rect (at 0 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 17 A10) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 17 connect rect (at 1.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 18 A11) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 18 connect rect (at 3 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 19 A12) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 19 connect rect (at 4.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 20 A13) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 20 connect rect (at 6 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 21 A14) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 21 connect rect (at 7.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 22 A15) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 22 connect rect (at 9 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 23 D0) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 23 connect rect (at 10.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 24 D1) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 24 connect rect (at 12 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 25 D2) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 25 connect rect (at 13.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 26 D3) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 26 connect rect (at 15 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 27 D4) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 27 connect rect (at 16.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 28 D5) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 28 connect rect (at 18 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 29 D6) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 29 connect rect (at 19.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 30 D7) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 30 connect rect (at 21 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 31 RST) (solder_mask_margin 0.5) (clearance 0.25))
    (pad 31 connect rect (at 22.5 3.5) (size 1 7) (layers F.Cu F.Mask)
      (net 32 AUDIO) (solder_mask_margin 0.5) (clearance 0.25))
  )
  (gr_text gb-cart-breakout (at 147.75 45.75) (layer F.Mask))
  (gr_text gb-cart-breakout (at 147.75 45.75) (layer F.Cu))
  (gr_text "Nick Palmer\nGameBoy Cart Breakout\n2017\nv2.0" (at 148.25 70.75) (layer B.SilkS))
  (gr_text AUDIO (at 167 62.5 90) (layer F.SilkS))
  (gr_text D7 (at 164.5 61 90) (layer F.SilkS))
  (gr_text D1 (at 156.75 61 90) (layer F.SilkS))
  (gr_text GND (at 167 51.5 90) (layer F.SilkS))
  (gr_text RST (at 164.5 50 90) (layer F.SilkS))
  (gr_text D6 (at 161.75 52 90) (layer F.SilkS))
  (gr_text D0 (at 154.25 52 90) (layer F.SilkS))
  (gr_text A14 (at 151.5 51.5 90) (layer F.SilkS))
  (gr_text A1 (at 136.5 61 90) (layer F.SilkS))
  (gr_text A15 (at 154.25 61.5 90) (layer F.SilkS))
  (gr_text A0 (at 133.75 52 90) (layer F.SilkS))
  (gr_text CS (at 134 61 90) (layer F.SilkS))
  (gr_text WR (at 131.5 61.25 90) (layer F.SilkS))
  (gr_text VDD (at 128.75 61.5 90) (layer F.SilkS))
  (gr_text RD (at 131.25 52 90) (layer F.SilkS))
  (gr_text CLK (at 128.75 51.5 90) (layer F.SilkS))
  (dimension 28.5 (width 0.3) (layer B.Fab)
    (gr_text "28.500 mm" (at 133.25 38.15) (layer B.Fab))
    (feature1 (pts (xy 147.5 43) (xy 147.5 36.8)))
    (feature2 (pts (xy 119 43) (xy 119 36.8)))
    (crossbar (pts (xy 119 39.5) (xy 147.5 39.5)))
    (arrow1a (pts (xy 147.5 39.5) (xy 146.373496 40.086421)))
    (arrow1b (pts (xy 147.5 39.5) (xy 146.373496 38.913579)))
    (arrow2a (pts (xy 119 39.5) (xy 120.126504 40.086421)))
    (arrow2b (pts (xy 119 39.5) (xy 120.126504 38.913579)))
  )
  (gr_line (start 122 58.5) (end 122 69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.5 57.5) (end 121 57.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.5 44) (end 119.5 56.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121 58.5) (end 121 57.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 120.5 56.5) (end 120.5 57.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 120.5 44) (end 119.5 44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.5 43) (end 120.5 43) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.5 45) (end 171.5 44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.5 46) (end 172.5 46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.5 56.5) (end 175.5 47) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174 57.5) (end 174.5 57.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 170.5 44) (end 170.5 43) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.5 45) (end 172.5 46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174.5 47) (end 174.5 46) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174.5 56.5) (end 175.5 56.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 69) (end 173 58.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 174 58.5) (end 173 58.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 69.5) (end 173 69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 69.5) (end 122 69) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.5 72) (end 122 69.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.5 77) (end 119.5 72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 79.5) (end 119.5 77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 85.5) (end 122 79.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.5 88) (end 122 85.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.5 93) (end 119.5 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 95.5) (end 119.5 93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 122 99) (end 122 95.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.5 72) (end 173 69.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.5 77) (end 175.5 72) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 79.5) (end 175.5 77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 85.5) (end 173 79.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.5 88) (end 173 85.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.5 93) (end 175.5 88) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 95.5) (end 175.5 93) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 99) (end 173 95.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 65 (width 0.3) (layer F.Fab)
    (gr_text "65.000 mm" (at 107.65 75.5 270) (layer F.Fab))
    (feature1 (pts (xy 119 108) (xy 106.3 108)))
    (feature2 (pts (xy 119 43) (xy 106.3 43)))
    (crossbar (pts (xy 109 43) (xy 109 108)))
    (arrow1a (pts (xy 109 108) (xy 108.413579 106.873496)))
    (arrow1b (pts (xy 109 108) (xy 109.586421 106.873496)))
    (arrow2a (pts (xy 109 43) (xy 108.413579 44.126504)))
    (arrow2b (pts (xy 109 43) (xy 109.586421 44.126504)))
  )
  (dimension 3 (width 0.3) (layer F.Fab)
    (gr_text "3.000 mm" (at 190.5 44 90) (layer F.Fab))
    (feature1 (pts (xy 176 43) (xy 188.7 43)))
    (feature2 (pts (xy 176 46) (xy 188.7 46)))
    (crossbar (pts (xy 186 46) (xy 186 43)))
    (arrow1a (pts (xy 186 43) (xy 186.586421 44.126504)))
    (arrow1b (pts (xy 186 43) (xy 185.413579 44.126504)))
    (arrow2a (pts (xy 186 46) (xy 186.586421 44.873496)))
    (arrow2b (pts (xy 186 46) (xy 185.413579 44.873496)))
  )
  (dimension 4.5 (width 0.3) (layer F.Fab)
    (gr_text "4.500 mm" (at 175 35) (layer F.Fab))
    (feature1 (pts (xy 171.5 43) (xy 171.5 36.8)))
    (feature2 (pts (xy 176 43) (xy 176 36.8)))
    (crossbar (pts (xy 176 39.5) (xy 171.5 39.5)))
    (arrow1a (pts (xy 171.5 39.5) (xy 172.626504 38.913579)))
    (arrow1b (pts (xy 171.5 39.5) (xy 172.626504 40.086421)))
    (arrow2a (pts (xy 176 39.5) (xy 174.873496 38.913579)))
    (arrow2b (pts (xy 176 39.5) (xy 174.873496 40.086421)))
  )
  (dimension 57 (width 0.3) (layer F.Fab)
    (gr_text "57.000 mm" (at 147.5 27.65) (layer F.Fab))
    (feature1 (pts (xy 119 43) (xy 119 26.3)))
    (feature2 (pts (xy 176 43) (xy 176 26.3)))
    (crossbar (pts (xy 176 29) (xy 119 29)))
    (arrow1a (pts (xy 119 29) (xy 120.126504 28.413579)))
    (arrow1b (pts (xy 119 29) (xy 120.126504 29.586421)))
    (arrow2a (pts (xy 176 29) (xy 174.873496 28.413579)))
    (arrow2b (pts (xy 176 29) (xy 174.873496 29.586421)))
  )
  (gr_arc (start 173 100) (end 172 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 122 100) (end 122 99) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172 108) (end 172 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123 108) (end 123 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123 108) (end 172 108) (angle 90) (layer Edge.Cuts) (width 0.15))
)
