(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 274)
    (zones 0)
    (modules 12)
    (nets 82)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.25)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.8 0.5)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.1)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.30048 0.32)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 21 44)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VCC)
  (net 3 /3V3OUT)
  (net 4 "Net-(D1-Pad1)")
  (net 5 /LED)
  (net 6 "Net-(D2-Pad1)")
  (net 7 /BSL_PCOUTMCUIN)
  (net 8 /BSL_RST)
  (net 9 /BSL_TCK)
  (net 10 /BSL_PCINMCUOUT)
  (net 11 "Net-(U2-Pad6)")
  (net 12 "Net-(U2-Pad8)")
  (net 13 "Net-(U2-Pad9)")
  (net 14 "Net-(U2-Pad10)")
  (net 15 "Net-(U2-Pad11)")
  (net 16 "Net-(U2-Pad12)")
  (net 17 "Net-(U2-Pad13)")
  (net 18 "Net-(U2-Pad14)")
  (net 19 "Net-(U2-Pad19)")
  (net 20 /VBUS)
  (net 21 /RXLED)
  (net 22 /TXLED)
  (net 23 "Net-(U2-Pad24)")
  (net 24 "Net-(U2-Pad27)")
  (net 25 "Net-(U2-Pad28)")
  (net 26 "Net-(J1-Pad4)")
  (net 27 /TCK)
  (net 28 /TMS)
  (net 29 /TDI)
  (net 30 /TDO)
  (net 31 /~RST~)
  (net 32 /TST)
  (net 33 /RXIN)
  (net 34 /TXOUT)
  (net 35 "Net-(U1-Pad2)")
  (net 36 "Net-(U1-Pad3)")
  (net 37 "Net-(U1-Pad4)")
  (net 38 "Net-(U1-Pad5)")
  (net 39 "Net-(U1-Pad6)")
  (net 40 "Net-(U1-Pad7)")
  (net 41 "Net-(U1-Pad8)")
  (net 42 "Net-(U1-Pad9)")
  (net 43 "Net-(U1-Pad10)")
  (net 44 "Net-(U1-Pad11)")
  (net 45 "Net-(U1-Pad14)")
  (net 46 "Net-(U1-Pad15)")
  (net 47 "Net-(U1-Pad16)")
  (net 48 "Net-(U1-Pad17)")
  (net 49 "Net-(U1-Pad18)")
  (net 50 "Net-(U1-Pad19)")
  (net 51 "Net-(U1-Pad20)")
  (net 52 "Net-(U1-Pad21)")
  (net 53 "Net-(U1-Pad23)")
  (net 54 "Net-(U1-Pad24)")
  (net 55 "Net-(U1-Pad25)")
  (net 56 "Net-(U1-Pad27)")
  (net 57 "Net-(U1-Pad28)")
  (net 58 "Net-(U1-Pad29)")
  (net 59 "Net-(U1-Pad30)")
  (net 60 "Net-(U1-Pad31)")
  (net 61 "Net-(U1-Pad37)")
  (net 62 "Net-(U1-Pad38)")
  (net 63 "Net-(U1-Pad39)")
  (net 64 "Net-(U1-Pad40)")
  (net 65 "Net-(U1-Pad41)")
  (net 66 "Net-(U1-Pad42)")
  (net 67 "Net-(U1-Pad43)")
  (net 68 "Net-(U1-Pad48)")
  (net 69 "Net-(U1-Pad49)")
  (net 70 "Net-(U1-Pad50)")
  (net 71 "Net-(U1-Pad51)")
  (net 72 "Net-(U1-Pad52)")
  (net 73 "Net-(U1-Pad53)")
  (net 74 "Net-(U1-Pad54)")
  (net 75 "Net-(U1-Pad55)")
  (net 76 "Net-(U1-Pad56)")
  (net 77 "Net-(U1-Pad59)")
  (net 78 "Net-(U1-Pad60)")
  (net 79 "Net-(U1-Pad61)")
  (net 80 /USBDP)
  (net 81 /USBDM)
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.1)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (diff_pair_width 0.25)
    (diff_pair_gap 0.25)
    (add_net /3V3OUT)
    (add_net /BSL_PCINMCUOUT)
    (add_net /BSL_PCOUTMCUIN)
    (add_net /BSL_RST)
    (add_net /BSL_TCK)
    (add_net /LED)
    (add_net /RXIN)
    (add_net /RXLED)
    (add_net /TCK)
    (add_net /TDI)
    (add_net /TDO)
    (add_net /TMS)
    (add_net /TST)
    (add_net /TXLED)
    (add_net /TXOUT)
    (add_net /USBDM)
    (add_net /USBDP)
    (add_net /VBUS)
    (add_net /VCC)
    (add_net /~RST~)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad41)")
    (add_net "Net-(U1-Pad42)")
    (add_net "Net-(U1-Pad43)")
    (add_net "Net-(U1-Pad48)")
    (add_net "Net-(U1-Pad49)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad50)")
    (add_net "Net-(U1-Pad51)")
    (add_net "Net-(U1-Pad52)")
    (add_net "Net-(U1-Pad53)")
    (add_net "Net-(U1-Pad54)")
    (add_net "Net-(U1-Pad55)")
    (add_net "Net-(U1-Pad56)")
    (add_net "Net-(U1-Pad59)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad60)")
    (add_net "Net-(U1-Pad61)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
  )
  (module USB_MICROB_MOLEX (layer F.Cu) (tedit 5E2EBA7F)
    (at 25.75 39.25 270)
    (descr "MICRO USB B SOCKET (MOLEX)")
    (clearance 0.09906)
    (fp_text reference J1 (at -2 -1.25 270) (layer F.SilkS))
    (fp_text value USB_MICROB (at 0 6 270) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0 0.69088 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 80 /USBDP))
    (pad 2 smd rect (at -0.65024 0.69088 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 81 /USBDM))
    (pad 1 smd rect (at -1.30048 0.69088 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 20 /VBUS))
    (pad 4 smd rect (at 0.65024 0.69088 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.30048 0.69088 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.46126 1.04902 270) (size 1.47574 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.46126 1.04902 270) (size 1.47574 2.10058) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.91338 3.35026 270) (size 2.3749 1.89992) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.91338 3.35026 270) (size 2.3749 1.89992) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -0.8382 3.35026 270) (size 1.17602 1.89992) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0.8382 3.35026 270) (size 1.17602 1.89992) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module microgdfet:PIN_ARRAY_7X2_SIDE (layer B.Cu) (tedit 5E2EB953)
    (at 39.5 34.25 90)
    (fp_text reference P1 (at 10 0 180) (layer B.SilkS) hide)
    (fp_text value CONN_2x7 (at 0 0 90) (layer B.SilkS) hide)
    (pad 7 smd rect (at 0 0 90) (size 1.5 3) (layers B.Cu B.Paste B.Mask)
      (net 27 /TCK))
    (pad 5 smd rect (at -2.54 0 90) (size 1.5 3) (layers B.Cu B.Paste B.Mask)
      (net 28 /TMS))
    (pad 3 smd rect (at -5.08 0 90) (size 1.5 3) (layers B.Cu B.Paste B.Mask)
      (net 29 /TDI))
    (pad 1 smd rect (at -7.62 0 90) (size 1.5 3) (layers B.Cu B.Paste B.Mask)
      (net 30 /TDO))
    (pad 9 smd rect (at 2.54 0 90) (size 1.5 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 5.08 0 90) (size 1.5 3) (layers B.Cu B.Paste B.Mask)
      (net 31 /~RST~))
    (pad 13 smd rect (at 7.62 0 90) (size 1.5 3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -7.62 0 90) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 2 /VCC))
    (pad 4 smd rect (at -5.08 0 90) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 2 /VCC))
    (pad 6 smd rect (at -2.54 0 90) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0 0 90) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 32 /TST))
    (pad 10 smd rect (at 2.54 0 90) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 5.08 0 90) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 33 /RXIN))
    (pad 14 smd rect (at 7.62 0 90) (size 1.5 3) (layers F.Cu F.Paste F.Mask)
      (net 34 /TXOUT))
  )
  (module microgdfet:0805 (layer F.Cu) (tedit 53DFD474)
    (at 28.25 42.25 90)
    (attr smd)
    (fp_text reference C1 (at 2 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 2 /VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microgdfet:0805 (layer F.Cu) (tedit 53DFD474)
    (at 33.5 28.75 270)
    (attr smd)
    (fp_text reference C2 (at 2.25 0) (layer F.SilkS))
    (fp_text value 100n (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3OUT))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microgdfet:0805 (layer F.Cu) (tedit 53DFD474)
    (at 32.25 35.5 90)
    (attr smd)
    (fp_text reference D1 (at 2 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microgdfet:0805 (layer F.Cu) (tedit 53DFD474)
    (at 31 26.75 270)
    (attr smd)
    (fp_text reference D2 (at -2 0) (layer F.SilkS))
    (fp_text value LED (at 0 0.381 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 22 /TXLED))
    (pad 1 smd rect (at -0.9525 0 270) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microgdfet:0805 (layer F.Cu) (tedit 53DFD474)
    (at 31 30.25 90)
    (attr smd)
    (fp_text reference D3 (at -2.25 0 180) (layer F.SilkS))
    (fp_text value LED (at 0 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 21 /RXLED))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microgdfet:0805 (layer F.Cu) (tedit 53DFD474)
    (at 29.5 36 180)
    (attr smd)
    (fp_text reference R1 (at 0 1.25) (layer F.SilkS))
    (fp_text value 330 (at 0 0.381 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 /LED))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microgdfet:0805 (layer F.Cu) (tedit 53DFD474)
    (at 34 25.25 180)
    (attr smd)
    (fp_text reference R2 (at -2.25 0 270) (layer F.SilkS))
    (fp_text value 330 (at 0 0.381 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 1 smd rect (at -0.9525 0 180) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 2 /VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microgdfet:0805 (layer F.Cu) (tedit 5E3D1CD6)
    (at 35.75 28 90)
    (attr smd)
    (fp_text reference R3 (at -2 0 180) (layer F.SilkS))
    (fp_text value 0R (at 0 0.381 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3OUT))
    (pad 2 smd rect (at 0.9525 0 90) (size 0.889 1.397) (layers F.Cu F.Paste F.Mask)
      (net 2 /VCC))
    (model smd/chip_cms.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microgdfet:TQFP64 (layer B.Cu) (tedit 5424268A)
    (at 30 36.25 90)
    (descr "TQFP-64 0.8mm pitch")
    (clearance 0.085)
    (attr smd)
    (fp_text reference U1 (at 5.75 -7.5 90) (layer B.SilkS))
    (fp_text value MSP430F2618_64 (at -0.75 -7.5 90) (layer B.SilkS))
    (pad 1 smd rect (at -3.75 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 /VCC))
    (pad 2 smd rect (at -3.25 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.75 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.25 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -1.75 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -1.25 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -0.75 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -0.25 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 0.25 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(U1-Pad9)"))
    (pad 10 smd rect (at 0.75 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 1.25 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 1.75 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 5 /LED))
    (pad 13 smd rect (at 2.25 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 /BSL_PCINMCUOUT))
    (pad 14 smd rect (at 2.75 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 3.25 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(U1-Pad15)"))
    (pad 16 smd rect (at 3.75 -5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U1-Pad16)"))
    (pad 17 smd rect (at 5.9 -3.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at 5.9 -3.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at 5.9 -2.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 5.9 -2.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 5.9 -1.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 5.9 -1.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 7 /BSL_PCOUTMCUIN))
    (pad 23 smd rect (at 5.9 -0.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(U1-Pad23)"))
    (pad 24 smd rect (at 5.9 -0.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(U1-Pad24)"))
    (pad 25 smd rect (at 5.9 0.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 55 "Net-(U1-Pad25)"))
    (pad 26 smd rect (at 5.9 0.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 31 /~RST~))
    (pad 27 smd rect (at 5.9 1.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(U1-Pad27)"))
    (pad 28 smd rect (at 5.9 1.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(U1-Pad28)"))
    (pad 29 smd rect (at 5.9 2.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(U1-Pad29)"))
    (pad 30 smd rect (at 5.9 2.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(U1-Pad30)"))
    (pad 31 smd rect (at 5.9 3.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(U1-Pad31)"))
    (pad 32 smd rect (at 5.9 3.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 10 /BSL_PCINMCUOUT))
    (pad 33 smd rect (at 3.75 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 /BSL_PCOUTMCUIN))
    (pad 34 smd rect (at 3.25 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 34 /TXOUT))
    (pad 35 smd rect (at 2.75 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 33 /RXIN))
    (pad 36 smd rect (at 2.25 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 32 /TST))
    (pad 37 smd rect (at 1.75 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(U1-Pad37)"))
    (pad 38 smd rect (at 1.25 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(U1-Pad38)"))
    (pad 39 smd rect (at 0.75 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(U1-Pad39)"))
    (pad 40 smd rect (at 0.25 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(U1-Pad40)"))
    (pad 41 smd rect (at -0.25 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(U1-Pad41)"))
    (pad 42 smd rect (at -0.75 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(U1-Pad42)"))
    (pad 43 smd rect (at -1.25 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(U1-Pad43)"))
    (pad 44 smd rect (at -1.75 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 28 /TMS))
    (pad 45 smd rect (at -2.25 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 29 /TDI))
    (pad 46 smd rect (at -2.75 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 30 /TDO))
    (pad 47 smd rect (at -3.25 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 27 /TCK))
    (pad 48 smd rect (at -3.75 5.9 90) (size 0.32 0.8) (layers B.Cu B.Paste B.Mask)
      (net 68 "Net-(U1-Pad48)"))
    (pad 49 smd rect (at -5.9 3.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 69 "Net-(U1-Pad49)"))
    (pad 50 smd rect (at -5.9 3.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 70 "Net-(U1-Pad50)"))
    (pad 51 smd rect (at -5.9 2.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(U1-Pad51)"))
    (pad 52 smd rect (at -5.9 2.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(U1-Pad52)"))
    (pad 53 smd rect (at -5.9 1.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(U1-Pad53)"))
    (pad 54 smd rect (at -5.9 1.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(U1-Pad54)"))
    (pad 55 smd rect (at -5.9 0.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(U1-Pad55)"))
    (pad 56 smd rect (at -5.9 0.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(U1-Pad56)"))
    (pad 57 smd rect (at -5.9 -0.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 9 /BSL_TCK))
    (pad 58 smd rect (at -5.9 -0.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 8 /BSL_RST))
    (pad 59 smd rect (at -5.9 -1.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 77 "Net-(U1-Pad59)"))
    (pad 60 smd rect (at -5.9 -1.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 78 "Net-(U1-Pad60)"))
    (pad 61 smd rect (at -5.9 -2.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 79 "Net-(U1-Pad61)"))
    (pad 62 smd rect (at -5.9 -2.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 63 smd rect (at -5.9 -3.25 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 64 smd rect (at -5.9 -3.75 90) (size 0.8 0.32) (layers B.Cu B.Paste B.Mask)
      (net 2 /VCC))
    (model smd\smd_lqfp\tqfp-64_08.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module microgdfet:TSSOP28 (layer F.Cu) (tedit 54242986)
    (at 26 29.25)
    (descr "TSSOP28: plastic thin shrink small outline package; 28 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot361-1_po.pdf)")
    (tags "SSOP 0.65")
    (clearance 0.125)
    (attr smd)
    (fp_text reference U2 (at -4 -4.75 90) (layer F.SilkS))
    (fp_text value FT232R_SSOP (at -4 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.85 -4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /BSL_PCOUTMCUIN))
    (pad 2 smd rect (at -2.85 -3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /BSL_RST))
    (pad 3 smd rect (at -2.85 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /BSL_TCK))
    (pad 4 smd rect (at -2.85 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /VCC))
    (pad 5 smd rect (at -2.85 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /BSL_PCINMCUOUT))
    (pad 6 smd rect (at -2.85 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -2.85 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -2.85 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U2-Pad8)"))
    (pad 9 smd rect (at -2.85 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad9)"))
    (pad 10 smd rect (at -2.85 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at -2.85 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad11)"))
    (pad 12 smd rect (at -2.85 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad12)"))
    (pad 13 smd rect (at -2.85 3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad13)"))
    (pad 14 smd rect (at -2.85 4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad14)"))
    (pad 15 smd rect (at 2.85 4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 80 /USBDP))
    (pad 16 smd rect (at 2.85 3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 81 /USBDM))
    (pad 17 smd rect (at 2.85 2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3OUT))
    (pad 18 smd rect (at 2.85 2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 19 smd rect (at 2.85 1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 2.85 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 20 /VBUS))
    (pad 21 smd rect (at 2.85 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 2.85 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 21 /RXLED))
    (pad 23 smd rect (at 2.85 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 /TXLED))
    (pad 24 smd rect (at 2.85 -1.625) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U2-Pad24)"))
    (pad 25 smd rect (at 2.85 -2.275) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at 2.85 -2.925) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 27 smd rect (at 2.85 -3.575) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad27)"))
    (pad 28 smd rect (at 2.85 -4.225) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad28)"))
    (model Housings_SSOP/TSSOP-28_4.5x9.95mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "GOODFET42-MICRO\nTravis Goodspeed\n    F4GRX 2020" (at 29 39.5) (layer F.SilkS))
  (gr_line (start 41 44) (end 21 44) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 41 24) (end 21 24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (dimension 20 (width 0.3) (layer Dwgs.User)
    (gr_text "20,000 mm" (at 31 46.35) (layer Dwgs.User))
    (feature1 (pts (xy 41 45) (xy 41 47.7)))
    (feature2 (pts (xy 21 45) (xy 21 47.7)))
    (crossbar (pts (xy 21 45) (xy 41 45)))
    (arrow1a (pts (xy 41 45) (xy 39.873496 45.586421)))
    (arrow1b (pts (xy 41 45) (xy 39.873496 44.413579)))
    (arrow2a (pts (xy 21 45) (xy 22.126504 45.586421)))
    (arrow2b (pts (xy 21 45) (xy 22.126504 44.413579)))
  )
  (dimension 20 (width 0.3) (layer Dwgs.User)
    (gr_text "20,000 mm" (at 44.35 34 90) (layer Dwgs.User))
    (feature1 (pts (xy 43 24) (xy 45.7 24)))
    (feature2 (pts (xy 43 44) (xy 45.7 44)))
    (crossbar (pts (xy 43 44) (xy 43 24)))
    (arrow1a (pts (xy 43 24) (xy 43.586421 25.126504)))
    (arrow1b (pts (xy 43 24) (xy 42.413579 25.126504)))
    (arrow2a (pts (xy 43 44) (xy 43.586421 42.873496)))
    (arrow2b (pts (xy 43 44) (xy 42.413579 42.873496)))
  )
  (gr_line (start 41 24) (end 41 44) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 21 44) (end 21 24) (angle 90) (layer Edge.Cuts) (width 0.1))
)
