(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 35)
    (tracks 69)
    (zones 0)
    (modules 13)
    (nets 16)
  )
  (page A4)
  (title_block
    (date "30 Jan 2020")
    (rev "Vers 1.0")
    (comment 1 "Started 30 Jan 2020... last day UK in EU.")
    (comment 2 "PCB277- Carrier for dual optocoupler. My second.")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(LEDS1-Pad1)")
  (net 2 "Net-(LEDS1-Pad2)")
  (net 3 "Net-(LEDS2-Pad2)")
  (net 4 "Net-(LEDS2-Pad1)")
  (net 5 "Net-(P1-Pad1)")
  (net 6 "Net-(P1-Pad4)")
  (net 7 "Net-(P2-Pad1)")
  (net 8 "Net-(P2-Pad2)")
  (net 9 "Net-(P2-Pad3)")
  (net 10 "Net-(P2-Pad4)")
  (net 11 "Net-(P2-Pad5)")
  (net 12 "Net-(RLC1-Pad1)")
  (net 13 "Net-(RLC2-Pad1)")
  (net 14 "Net-(RPC1-Pad2)")
  (net 15 "Net-(RPC2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(LEDS1-Pad1)")
    (add_net "Net-(LEDS1-Pad2)")
    (add_net "Net-(LEDS2-Pad1)")
    (add_net "Net-(LEDS2-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P2-Pad3)")
    (add_net "Net-(P2-Pad4)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(RLC1-Pad1)")
    (add_net "Net-(RLC2-Pad1)")
    (add_net "Net-(RPC1-Pad2)")
    (add_net "Net-(RPC2-Pad2)")
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 222.25 128.27)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LEDS1 (at 1.27 2.794) (layer F.SilkS))
    (fp_text value ~ (at 1.27 2.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(LEDS1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(LEDS1-Pad2)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_THT:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 222.25 139.446)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference LEDS2 (at 1.27 -2.794) (layer F.SilkS))
    (fp_text value ~ (at 1.27 2.96) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(LEDS2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(LEDS2-Pad1)"))
    (model ${KISYS3DMOD}/LED_THT.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:Frm_Camden_CTB3051-but-1x04_P3.50mm" (layer F.Cu) (tedit 5E32D7AC)
    (at 214.122 139.446 90)
    (descr "Molex 734 Male header (for PCBs); Straight solder pin 1 x 1 mm, 734-134 , 4 Pins (http://www.farnell.com/datasheets/2157639.pdf), generated with kicad-footprint-generator")
    (tags "connector Wago  side entry")
    (fp_text reference "P1(pin1)" (at 12.6365 0 180) (layer F.SilkS))
    (fp_text value Conn_01x04_Female (at -1.778 -17.399 90) (layer F.Fab))
    (fp_text user %R (at -13.716 -2.286 180) (layer F.Fab))
    (fp_text user "Wires out this side" (at 5.334 -2.54 270) (layer F.SilkS))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 5 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 3.5 0 90) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 "Net-(LEDS1-Pad1)"))
    (pad 3 thru_hole oval (at 7 0 90) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 4 "Net-(LEDS2-Pad1)"))
    (pad 4 thru_hole oval (at 10.5 0 90) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad4)"))
    (model ${KISYS3DMOD}/Connector_Wago.3dshapes/Wago_734-134_1x04_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "aaTKB frm Jan2020:Frm_Camden_CTB3051-but-1x05_P3.50mm" (layer F.Cu) (tedit 5E32AF5B)
    (at 246.126 127.254 270)
    (descr "Molex 734 Male header (for PCBs); Straight solder pin 1 x 1 mm, 734-134 , 4 Pins (http://www.farnell.com/datasheets/2157639.pdf), generated with kicad-footprint-generator")
    (tags "connector Wago  side entry")
    (fp_text reference "P2(pin1)" (at -1.9685 -0.3175 180) (layer F.SilkS))
    (fp_text value Conn_01x05_Female (at 7.62 -17.018 90) (layer F.Fab))
    (fp_text user %R (at -14.478 0 180) (layer F.Fab))
    (fp_text user "Wires out this side" (at 6.9 -2.85 270) (layer F.SilkS))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask) (roundrect_rratio 0.125)
      (net 7 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 3.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad2)"))
    (pad 3 thru_hole oval (at 7 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 10.5 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad4)"))
    (pad 5 thru_hole oval (at 14 0 270) (size 2 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad5)"))
    (model ${KISYS3DMOD}/Connector_Wago.3dshapes/Wago_734-134_1x04_P3.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 219.71 132.08 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLC1 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value ~ (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 20.32 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(RLC1-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(LEDS1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 219.71 135.636 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLC2 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value ~ (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 22.606 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(LEDS2-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(RLC2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 228.854 127.508)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLS1 (at 2.54 0) (layer F.SilkS))
    (fp_text value ~ (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.54 -15.24) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(LEDS1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 228.854 140.716)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RLS2 (at 2.54 0) (layer F.SilkS))
    (fp_text value ~ (at 2.54 1.92) (layer F.Fab))
    (fp_text user %R (at 2.286 14.986) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(LEDS2-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 240.284 132.08 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RPC1 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value ~ (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 20.066 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 "Net-(P2-Pad2)"))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(RPC1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 240.284 136.906 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RPC2 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value ~ (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 24.384 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(RPC2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 237.744 132.08 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RPU1 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 10k (at 23.368 -0.762 90) (layer F.Fab))
    (fp_text user %R (at 20.066 -0.508 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(RPC1-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 237.744 136.906 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference RPU2 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 10k (at 27.686 0 90) (layer F.Fab))
    (fp_text user %R (at 24.13 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 5.08 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(RPC2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 227.584 130.302)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 1.27) (layer F.SilkS))
    (fp_text value OptoCoup-Dual-Inturned (at 6.096 28.194) (layer F.Fab))
    (fp_text user %R (at 4.064 6.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(P1-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(RPC2-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(RLC1-Pad1)"))
    (pad 6 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(RLC2-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad4)"))
    (pad 8 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(RPC1-Pad2)"))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "<- instance" (at 222.8088 142.5448) (layer F.SilkS))
  (gr_text Ch2Out (at 244.6655 140.462) (layer B.SilkS))
  (gr_text "GndCh2\n" (at 244.6655 138.7475) (layer B.SilkS))
  (gr_text "GndCh1\n" (at 244.348 134.239) (layer B.SilkS))
  (gr_text Ch1Out (at 244.475 130.302) (layer B.SilkS))
  (gr_text Vpu (at 244.4115 127.381) (layer B.SilkS))
  (gr_text "NOTE: WEIRD... but \"mess with\" at your peril... LOTS of things \"fit\"\nif you ignore this tiny detail...\nThe terminals in P1 seem to be 4,3,2,1(top\nto bottom, pp footprint. In all other\nways, the TOP pin is pin 1." (at 180.5305 129.286) (layer F.SilkS))
  (gr_text Ch.2 (at 216.8525 137.4775 90) (layer B.SilkS))
  (gr_text Ch.1 (at 216.8525 130.7465 90) (layer B.SilkS))
  (gr_text - (at 211.328 139.319) (layer B.SilkS))
  (gr_text - (at 211.1375 132.3975) (layer B.SilkS))
  (gr_text + (at 211.1375 135.9535) (layer B.SilkS))
  (gr_text + (at 211.074 128.8415) (layer B.SilkS))
  (gr_text "Started\n  30 Jan 2020" (at 229.997 129.286 90) (layer B.SilkS))
  (gr_text PCB277-dual-opto-coupler.htm (at 223.647 142.621) (layer B.SilkS))
  (gr_text http://bit.ly/PCB277opto (at 209.8675 125.349) (layer F.SilkS))
  (gr_text http://sheepdogguides.com/elec/pcb/.... (at 231.14 125.2855) (layer B.SilkS))
  (gr_text 1.0 (at 221.742 134.62) (layer F.SilkS))
  (gr_text Vers (at 221.488 133.096) (layer F.SilkS))
  (gr_line (start 209.55 143.51) (end 209.55 124.46) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 250.698 143.51) (end 209.55 143.51) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 250.698 124.46) (end 250.698 143.51) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 209.55 124.46) (end 250.698 124.46) (layer Edge.Cuts) (width 0.05))
)
