(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 44)
    (no_connects 0)
    (area 146.674999 107.924999 172.575001 118.075001)
    (thickness 1.6)
    (drawings 30)
    (tracks 181)
    (zones 0)
    (modules 16)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.3048)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (trace_clearance 0.2032)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f8_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /VDD18)
  (net 3 "Net-(C3-Pad1)")
  (net 4 /VDD)
  (net 5 /SCL)
  (net 6 /SDA)
  (net 7 /SCL18)
  (net 8 /SDA18)
  (net 9 "Net-(C1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net /SCL)
    (add_net /SCL18)
    (add_net /SDA)
    (add_net /SDA18)
    (add_net /VDD)
    (add_net /VDD18)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 166.25 114.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.25 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B04D74A)
    (at 158.08 109.21)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VDD18))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDA18))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SCL18))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5B04D733)
    (at 170.78 109.21)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /VDD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SCL))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5AA49CD7)
    (at 153 109.21)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /VDD18))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /SDA18))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SCL18))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module ICP-10100 (layer F.Cu) (tedit 5A9B8F62)
    (at 149.25 114.5)
    (fp_text reference U1 (at 0 2.25 180) (layer F.SilkS))
    (fp_text value ICP-10100 (at 0 -2) (layer F.Fab))
    (fp_text user REF** (at 0 2.25) (layer F.Fab))
    (pad 1 smd rect (at -0.775 -0.25 90) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.775 0.25 90) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL18))
    (pad 3 smd rect (at -0.5 0.775) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 0.775) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDA18))
    (pad 5 smd rect (at 0.5 0.775) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 6 smd rect (at 0.775 0.25 90) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at 0.775 -0.25 90) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 0.5 -0.775 180) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 0 -0.775) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at -0.5 -0.775) (size 0.28 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 148.5 111.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.5 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 161.25 110.25 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /VDD18))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 167 110.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.25) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6 (layer F.Cu) (tedit 5B04E20E)
    (at 163.75 115 90)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference Q1 (at -2.15 0 180) (layer F.SilkS))
    (fp_text value UM6K34NTCN (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 -0.65 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDA18))
    (pad 3 smd rect (at -0.95 0.65 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL))
    (pad 5 smd rect (at 0.95 0 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /VDD18))
    (pad 2 smd rect (at -0.95 0 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /VDD18))
    (pad 4 smd rect (at 0.95 0.65 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL18))
    (pad 6 smd rect (at 0.95 -0.65 90) (size 0.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDA))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 161.25 113.25 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.5 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /VDD18))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDA18))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 161.25 116 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /VDD18))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL18))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 167 112 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -2 0 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 167.75 114.5 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.25 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 163.75 111.25)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 0 -2.25) (layer F.SilkS))
    (fp_text value AP7313R (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /VDD18))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 150 111.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 2.4 0 270) (layer F.SilkS))
    (fp_text value Ferrite (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /VDD18))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:Bites (layer F.Cu) (tedit 5A9767B0)
    (at 155.5 113 270)
    (fp_text reference J4 (at 3.25 0 270) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 -1.25 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.5 0 270) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 /VDD18))
    (pad 2 thru_hole circle (at -0.5 0 270) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 /SDA18))
    (pad 3 thru_hole circle (at 0.5 0 270) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 /SCL18))
    (pad 4 thru_hole circle (at 1.5 0 270) (size 0.75 0.75) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (dimension 12.7 (width 0.3) (layer Dwgs.User)
    (gr_text "0.5000 in" (at 164.465 126.572) (layer Dwgs.User))
    (feature1 (pts (xy 170.815 123.19) (xy 170.815 127.922)))
    (feature2 (pts (xy 158.115 123.19) (xy 158.115 127.922)))
    (crossbar (pts (xy 158.115 125.222) (xy 170.815 125.222)))
    (arrow1a (pts (xy 170.815 125.222) (xy 169.688496 125.808421)))
    (arrow1b (pts (xy 170.815 125.222) (xy 169.688496 124.635579)))
    (arrow2a (pts (xy 158.115 125.222) (xy 159.241504 125.808421)))
    (arrow2b (pts (xy 158.115 125.222) (xy 159.241504 124.635579)))
  )
  (dimension 16.25 (width 0.3) (layer Dwgs.User)
    (gr_text "16.250 mm" (at 164.375 121.6) (layer Dwgs.User))
    (feature1 (pts (xy 172.5 118.5) (xy 172.5 122.95)))
    (feature2 (pts (xy 156.25 118.5) (xy 156.25 122.95)))
    (crossbar (pts (xy 156.25 120.25) (xy 172.5 120.25)))
    (arrow1a (pts (xy 172.5 120.25) (xy 171.373496 120.836421)))
    (arrow1b (pts (xy 172.5 120.25) (xy 171.373496 119.663579)))
    (arrow2a (pts (xy 156.25 120.25) (xy 157.376504 120.836421)))
    (arrow2b (pts (xy 156.25 120.25) (xy 157.376504 119.663579)))
  )
  (dimension 8 (width 0.2) (layer Dwgs.User)
    (gr_text "8.000 mm" (at 150.75 121.6) (layer Dwgs.User))
    (feature1 (pts (xy 154.75 118.5) (xy 154.75 122.95)))
    (feature2 (pts (xy 146.75 118.5) (xy 146.75 122.95)))
    (crossbar (pts (xy 146.75 120.25) (xy 154.75 120.25)))
    (arrow1a (pts (xy 154.75 120.25) (xy 153.623496 120.836421)))
    (arrow1b (pts (xy 154.75 120.25) (xy 153.623496 119.663579)))
    (arrow2a (pts (xy 146.75 120.25) (xy 147.876504 120.836421)))
    (arrow2b (pts (xy 146.75 120.25) (xy 147.876504 119.663579)))
  )
  (dimension 25.75 (width 0.3) (layer Dwgs.User)
    (gr_text "25.750 mm" (at 159.625 104.4) (layer Dwgs.User))
    (feature1 (pts (xy 172.5 107.5) (xy 172.5 103.05)))
    (feature2 (pts (xy 146.75 107.5) (xy 146.75 103.05)))
    (crossbar (pts (xy 146.75 105.75) (xy 172.5 105.75)))
    (arrow1a (pts (xy 172.5 105.75) (xy 171.373496 106.336421)))
    (arrow1b (pts (xy 172.5 105.75) (xy 171.373496 105.163579)))
    (arrow2a (pts (xy 146.75 105.75) (xy 147.876504 106.336421)))
    (arrow2b (pts (xy 146.75 105.75) (xy 147.876504 105.163579)))
  )
  (dimension 10 (width 0.25) (layer Dwgs.User)
    (gr_text "10.00 mm" (at 143.4 113 270) (layer Dwgs.User))
    (feature1 (pts (xy 146 118) (xy 142.05 118)))
    (feature2 (pts (xy 146 108) (xy 142.05 108)))
    (crossbar (pts (xy 144.75 108) (xy 144.75 118)))
    (arrow1a (pts (xy 144.75 118) (xy 144.163579 116.873496)))
    (arrow1b (pts (xy 144.75 118) (xy 145.336421 116.873496)))
    (arrow2a (pts (xy 144.75 108) (xy 144.163579 109.126504)))
    (arrow2b (pts (xy 144.75 108) (xy 145.336421 109.126504)))
  )
  (gr_text G (at 151.3 116.9) (layer B.SilkS))
  (gr_text C (at 151.3 114.3) (layer B.SilkS))
  (gr_text D (at 151.3 111.7) (layer B.SilkS))
  (gr_text V (at 151.3 109.25) (layer B.SilkS))
  (gr_text G (at 159.75 117) (layer B.SilkS))
  (gr_text C (at 159.8 114.4) (layer B.SilkS))
  (gr_text D (at 159.75 111.75) (layer B.SilkS))
  (gr_text V (at 159.75 109.25) (layer B.SilkS))
  (gr_line (start 156.25 108) (end 172.5 108) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.75 118) (end 146.75 118) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.75 108) (end 146.75 108) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.75 110) (end 154.75 108) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.25 110) (end 156.25 108) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155.5 110) (end 156.25 110) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155.5 116) (end 154.75 116) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.25 118) (end 156.25 116) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.75 116) (end 154.75 118) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 146.75 118) (end 146.75 108) (layer Edge.Cuts) (width 0.15))
  (gr_text ICP-10100 (at 148.9 113 90) (layer B.SilkS))
  (gr_text GND (at 169.75 116.75) (layer B.SilkS))
  (gr_text SCL (at 169.75 114.25) (layer B.SilkS))
  (gr_text SDA (at 169.75 111.75) (layer B.SilkS))
  (gr_text 2.8-5V (at 169.75 109.25) (layer B.SilkS))
  (gr_line (start 172.5 118) (end 156.25 118) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172.5 108) (end 172.5 118) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 147.25 108.5) (xy 152.25 108.5) (xy 152.25 113.5) (xy 158.75 113.5) (xy 158.75 108.5)
        (xy 170 108.5) (xy 170 115.25) (xy 171.75 115.25) (xy 171.75 117.5) (xy 156.75 117.5)
        (xy 156.75 115.75) (xy 156 115) (xy 155 115) (xy 154.25 115.75) (xy 154.25 117.5)
        (xy 147.25 117.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.2032)
    (fill yes (arc_segments 16) (thermal_gap 0.2032) (thermal_bridge_width 0.254))
    (polygon
      (pts
        (xy 147.25 108.5) (xy 152.25 108.5) (xy 152.25 113.5) (xy 158.75 113.5) (xy 158.75 108.5)
        (xy 170 108.5) (xy 170 115.25) (xy 171.75 115.25) (xy 171.75 117.5) (xy 156.75 117.5)
        (xy 156.75 115.75) (xy 156 115) (xy 155 115) (xy 154.25 115.75) (xy 154.25 117.5)
        (xy 147.25 117.5)
      )
    )
  )
)
