(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 23)
    (no_connects 0)
    (area 146.325 91.364999 203.275001 118.185001)
    (thickness 1.6)
    (drawings 5)
    (tracks 24)
    (zones 0)
    (modules 7)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(Q1-Pad1)")
  (net 2 "Net-(P1-Pad3)")
  (net 3 "Net-(Q2-Pad1)")
  (net 4 "Net-(P1-Pad2)")
  (net 5 "Net-(Q3-Pad1)")
  (net 6 "Net-(P1-Pad1)")
  (net 7 "Net-(U1-Pad1)")
  (net 8 +5V)
  (net 9 "Net-(U1-Pad3)")
  (net 10 "Net-(U1-Pad5)")
  (net 11 "Net-(U1-Pad7)")
  (net 12 "Net-(U1-Pad8)")
  (net 13 "Net-(U1-Pad10)")
  (net 14 "Net-(U1-Pad11)")
  (net 15 "Net-(U1-Pad12)")
  (net 16 "Net-(U1-Pad13)")
  (net 17 "Net-(U1-Pad15)")
  (net 18 "Net-(U1-Pad16)")
  (net 19 "Net-(U1-Pad17)")
  (net 20 "Net-(U1-Pad18)")
  (net 21 "Net-(U1-Pad19)")
  (net 22 "Net-(U1-Pad21)")
  (net 23 "Net-(U1-Pad22)")
  (net 24 "Net-(U1-Pad23)")
  (net 25 "Net-(U1-Pad24)")
  (net 26 "Net-(U1-Pad26)")
  (net 27 "Net-(U1-Pad27)")
  (net 28 "Net-(U1-Pad28)")
  (net 29 "Net-(U1-Pad29)")
  (net 30 "Net-(U1-Pad31)")
  (net 31 GND)
  (net 32 "Net-(U1-Pad36)")
  (net 33 "Net-(U1-Pad37)")
  (net 34 "Net-(U1-Pad38)")
  (net 35 "Net-(U1-Pad40)")
  (net 36 +12V)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 5987B2A1)
    (at 170.18 104.14 90)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference Q2 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value IRLB8721PBF (at 0 -3.81 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(Q2-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 31 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module libraries:CUI-PJ-102A_dc-barrel-jack (layer F.Cu) (tedit 0)
    (at 179.07 104.14)
    (fp_text reference CON1 (at 0 5.08) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 0) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 3) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 36 +12V))
    (pad 2 thru_hole circle (at 0 -3) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 31 GND))
    (pad 2 thru_hole circle (at -4.7 0) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask F.SilkS)
      (net 31 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_2x20 (layer F.Cu) (tedit 5987B287)
    (at 200.66 113.03 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference U1 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value Raspberry_Pi_2_3 (at 6.35 5.08 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 +5V))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "Net-(U1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "Net-(U1-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "Net-(U1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "Net-(U1-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "Net-(U1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "Net-(U1-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(U1-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 21 thru_hole oval (at 0 25.4 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(U1-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(U1-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(U1-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(U1-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 26 thru_hole oval (at 2.54 30.48 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(U1-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 31 thru_hole oval (at 0 38.1 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "Net-(Q2-Pad1)"))
    (pad 33 thru_hole oval (at 0 40.64 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad1)"))
    (pad 34 thru_hole oval (at 2.54 40.64 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 35 thru_hole oval (at 0 43.18 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 "Net-(Q3-Pad1)"))
    (pad 36 thru_hole oval (at 2.54 43.18 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 40 thru_hole oval (at 2.54 48.26 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 "Net-(U1-Pad40)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04 (layer F.Cu) (tedit 5987B28E)
    (at 160.02 96.52)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 3.81 -2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 +12V))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 0)
    (at 193.04 104.14)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference U2 (at 0 -5.08) (layer F.SilkS))
    (fp_text value LM7805CT (at 0 3.81) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 31 GND))
    (pad 1 thru_hole oval (at -2.54 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 36 +12V))
    (pad 3 thru_hole oval (at 2.54 0 90) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 8 +5V))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 5987B29F)
    (at 163.83 104.14 90)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference Q1 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value IRLB8721PBF (at 0 -3.81 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(P1-Pad2)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 "Net-(Q1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 31 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 5987B2A4)
    (at 157.48 104.14 90)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference Q3 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value IRLB8721PBF (at 0 -3.81 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad1)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(Q3-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 31 GND))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 203.2 118.11) (end 203.2 116.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 118.11) (end 203.2 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.86 91.44) (end 149.86 118.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 91.44) (end 149.86 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 116.84) (end 203.2 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 36) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.2 118.11) (xy 149.86 118.11) (xy 149.86 91.44) (xy 203.2 91.44)
      )
    )
  )
  (zone (net 31) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 203.2 118.11) (xy 149.86 118.11) (xy 149.86 91.44) (xy 203.2 91.44)
      )
    )
  )
)
