(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.69672)
    (drawings 28)
    (tracks 252)
    (zones 0)
    (modules 35)
    (nets 64)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu power hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3048)
    (user_trace_width 0.889)
    (user_trace_width 2.032)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 40.64 15.24)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 12V)
  (net 3 5V)
  (net 4 3.3V)
  (net 5 12V-RAW)
  (net 6 DATA+)
  (net 7 DATA-)
  (net 8 CLK-)
  (net 9 CLK+)
  (net 10 PT_P)
  (net 11 ROT_P)
  (net 12 WAT_P)
  (net 13 PD_P)
  (net 14 HB_P)
  (net 15 FR_SIG)
  (net 16 24V)
  (net 17 RPM_SIG)
  (net 18 D-)
  (net 19 D+)
  (net 20 CC1)
  (net 21 CC2)
  (net 22 SBU1)
  (net 23 SBU2)
  (net 24 "Net-(PS1-Pad2)")
  (net 25 "Net-(PS1-Pad7)")
  (net 26 "Net-(PS1-Pad8)")
  (net 27 "Net-(U1-Pad3)")
  (net 28 "Net-(U1-Pad4)")
  (net 29 "Net-(U1-Pad11)")
  (net 30 "Net-(U1-Pad12)")
  (net 31 "Net-(U1-Pad16)")
  (net 32 "Net-(U1-Pad17)")
  (net 33 "Net-(U1-Pad24)")
  (net 34 "Net-(U1-Pad25)")
  (net 35 "Net-(U2-Pad19)")
  (net 36 "Net-(U2-Pad20)")
  (net 37 "Net-(U2-Pad22)")
  (net 38 "Net-(U2-Pad23)")
  (net 39 "Net-(U2-Pad24)")
  (net 40 "Net-(U2-Pad25)")
  (net 41 "Net-(U2-Pad26)")
  (net 42 "Net-(U2-Pad27)")
  (net 43 /PS1_VCC)
  (net 44 /USB_GND)
  (net 45 /VBUS)
  (net 46 /HP_DI)
  (net 47 /HP_RO)
  (net 48 /PT_P_DIV)
  (net 49 /ROT_P_DIV)
  (net 50 /WAT_P_DIV)
  (net 51 /PD_P_DIV)
  (net 52 /HB_P_DIV)
  (net 53 /RPM_SIG_DIV)
  (net 54 "Net-(U2-Pad28)")
  (net 55 "Net-(U2-Pad16)")
  (net 56 "Net-(U2-Pad14)")
  (net 57 "Net-(U2-Pad5)")
  (net 58 "Net-(U2-Pad3)")
  (net 59 "Net-(U2-Pad18)")
  (net 60 "Net-(U2-Pad17)")
  (net 61 "Net-(U2-Pad1)")
  (net 62 "Net-(U2-Pad2)")
  (net 63 "Net-(R15-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /HB_P_DIV)
    (add_net /HP_DI)
    (add_net /HP_RO)
    (add_net /PD_P_DIV)
    (add_net /PT_P_DIV)
    (add_net /ROT_P_DIV)
    (add_net /RPM_SIG_DIV)
    (add_net /USB_GND)
    (add_net /VBUS)
    (add_net /WAT_P_DIV)
    (add_net CC1)
    (add_net CC2)
    (add_net CLK+)
    (add_net CLK-)
    (add_net D+)
    (add_net D-)
    (add_net DATA+)
    (add_net DATA-)
    (add_net FR_SIG)
    (add_net GND)
    (add_net HB_P)
    (add_net "Net-(PS1-Pad2)")
    (add_net "Net-(PS1-Pad7)")
    (add_net "Net-(PS1-Pad8)")
    (add_net "Net-(R15-Pad2)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad14)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad5)")
    (add_net PD_P)
    (add_net PT_P)
    (add_net ROT_P)
    (add_net RPM_SIG)
    (add_net SBU1)
    (add_net SBU2)
    (add_net WAT_P)
  )
  (net_class 12V ""
    (clearance 0.4572)
    (trace_width 0.635)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 12V)
  )
  (net_class 12V_RAW ""
    (clearance 0.4572)
    (trace_width 0.635)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 12V-RAW)
  )
  (net_class 24V ""
    (clearance 0.3048)
    (trace_width 0.381)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PS1_VCC)
    (add_net 24V)
  )
  (net_class 3V3 ""
    (clearance 0.3048)
    (trace_width 0.3048)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3.3V)
  )
  (net_class 5V ""
    (clearance 0.3048)
    (trace_width 0.3048)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V)
  )
  (module Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown (layer B.Cu) (tedit 5AC8BA0D)
    (at 208.384 67.056 90)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference IC3 (at 2.54 20.58 -90) (layer B.SilkS))
    (fp_text value MIC29500-3.3WT (at 2.54 -2 -90) (layer B.Fab))
    (fp_text user %R (at 2.54 20.58 -90) (layer B.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 3.3V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad "" np_thru_hole oval (at 2.54 16.66 90) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Drill_Monitor_PCB:BRK-USB-CPV2.0 (layer F.Cu) (tedit 615B6FDF)
    (at 199.898 76.962 90)
    (fp_text reference U1 (at -5.842 -5.334 90) (layer F.SilkS))
    (fp_text value BRK-USB-CP (at -5.842 -2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 44 /USB_GND))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 27 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 28 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 45 /VBUS))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 22 SBU1))
    (pad 7 thru_hole circle (at 0 15.24 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 D-))
    (pad 8 thru_hole circle (at 0 17.78 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 D+))
    (pad 9 thru_hole circle (at 0 20.32 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 20 CC1))
    (pad 10 thru_hole circle (at 0 22.86 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 45 /VBUS))
    (pad 11 thru_hole circle (at 0 25.4 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 29 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 0 27.94 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 30 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at 0 30.48 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 44 /USB_GND))
    (pad 14 thru_hole circle (at -12.192 0 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at -12.192 2.54 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 44 /USB_GND))
    (pad 16 thru_hole circle (at -12.192 5.08 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad16)"))
    (pad 17 thru_hole circle (at -12.192 7.62 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at -12.192 10.16 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 45 /VBUS))
    (pad 19 thru_hole circle (at -12.192 12.7 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 21 CC2))
    (pad 20 thru_hole circle (at -12.192 15.24 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 19 D+))
    (pad 21 thru_hole circle (at -12.192 17.78 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 18 D-))
    (pad 22 thru_hole circle (at -12.192 20.32 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 23 SBU2))
    (pad 23 thru_hole circle (at -12.192 22.86 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 45 /VBUS))
    (pad 24 thru_hole circle (at -12.192 25.4 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 33 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at -12.192 27.94 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 34 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at -12.192 30.48 90) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 44 /USB_GND))
    (pad "" np_thru_hole circle (at 6.604 0 90) (size 4.064 4.064) (drill 3.4544) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -18.796 0 90) (size 4.064 4.064) (drill 3.4544) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -6.096 29.972 90) (size 4.064 4.064) (drill 3.4544) (layers *.Cu *.Mask))
  )
  (module Drill_Monitor_PCB:STMF405_Feather (layer F.Cu) (tedit 615B6E1B)
    (at 177.7492 93.218 270)
    (fp_text reference U2 (at -11.0744 17.3228 90) (layer F.SilkS))
    (fp_text value STM32F405_Feather (at -10.414 11.3792 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at -19.05 41.91 270) (size 3.175 3.175) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 41.91 270) (size 3.175 3.175) (drill 2.54) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -19.05 -3.81 270) (size 3.175 3.175) (drill 2.54) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 0 0 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 55 "Net-(U2-Pad16)"))
    (pad 15 thru_hole circle (at 0 2.54 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 3.3V))
    (pad 14 thru_hole circle (at 0 5.08 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 56 "Net-(U2-Pad14)"))
    (pad 13 thru_hole circle (at 0 7.62 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at 0 10.16 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 48 /PT_P_DIV))
    (pad 11 thru_hole circle (at 0 12.7 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 51 /PD_P_DIV))
    (pad 10 thru_hole circle (at 0 15.24 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 50 /WAT_P_DIV))
    (pad 9 thru_hole circle (at 0 17.78 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 49 /ROT_P_DIV))
    (pad 8 thru_hole circle (at 0 20.32 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 52 /HB_P_DIV))
    (pad 7 thru_hole circle (at 0 22.86 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 15 FR_SIG))
    (pad 6 thru_hole circle (at 0 25.4 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 46 /HP_DI))
    (pad 5 thru_hole circle (at 0 27.94 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 57 "Net-(U2-Pad5)"))
    (pad 4 thru_hole circle (at 0 30.48 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 63 "Net-(R15-Pad2)"))
    (pad 3 thru_hole circle (at 0 33.02 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 58 "Net-(U2-Pad3)"))
    (pad 28 thru_hole circle (at -20.32 10.16 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 54 "Net-(U2-Pad28)"))
    (pad 27 thru_hole circle (at -20.32 12.7 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 42 "Net-(U2-Pad27)"))
    (pad 26 thru_hole circle (at -20.32 15.24 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 41 "Net-(U2-Pad26)"))
    (pad 25 thru_hole circle (at -20.32 17.78 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 40 "Net-(U2-Pad25)"))
    (pad 24 thru_hole circle (at -20.32 20.32 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 39 "Net-(U2-Pad24)"))
    (pad 23 thru_hole circle (at -20.32 22.86 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 38 "Net-(U2-Pad23)"))
    (pad 22 thru_hole circle (at -20.32 25.4 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 37 "Net-(U2-Pad22)"))
    (pad 21 thru_hole circle (at -20.32 27.94 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 53 /RPM_SIG_DIV))
    (pad 20 thru_hole circle (at -20.32 30.48 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-Pad20)"))
    (pad 19 thru_hole circle (at -20.32 33.02 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 35 "Net-(U2-Pad19)"))
    (pad 18 thru_hole circle (at -20.32 35.56 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 59 "Net-(U2-Pad18)"))
    (pad 17 thru_hole circle (at -20.32 38.1 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 60 "Net-(U2-Pad17)"))
    (pad 1 thru_hole circle (at 0 38.1 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 61 "Net-(U2-Pad1)"))
    (pad 2 thru_hole circle (at 0 35.56 270) (size 1.62 1.62) (drill 1.02) (layers *.Cu *.Mask)
      (net 62 "Net-(U2-Pad2)"))
    (pad "" np_thru_hole circle (at -1.27 -3.81 270) (size 3.175 3.175) (drill 2.54) (layers *.Cu *.Mask))
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 129.2606 94.5642 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R16 (at -2.6924 -0.0254 90) (layer F.SilkS))
    (fp_text value 3320 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R15-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5A02E8C5)
    (at 120.65 84.963 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference IC2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MAX490EEPA+ (at 3.81 9.95) (layer F.Fab))
    (fp_text user %R (at 3.81 3.81) (layer F.Fab))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 DATA+))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 DATA-))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /HP_DI))
    (pad 6 thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 CLK-))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /HP_RO))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 CLK+))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 5V))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 203.962 61.976 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C8 (at 1.016 -2.286 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 3.3V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Drill_Monitor_PCB:DT1348PABCDR015 (layer F.Cu) (tedit 0)
    (at 102.136 53.328 270)
    (descr DT13-48PABCD-R015-1)
    (tags Connector)
    (fp_text reference J1 (at 41.16 16.3475 90) (layer F.SilkS))
    (fp_text value DT13-48PABCD-R015 (at 41.16 23.904 90) (layer F.SilkS) hide)
    (fp_text user %R (at 41.16 22.275 90) (layer F.Fab))
    (pad A1 thru_hole circle (at 0 0 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 17 RPM_SIG))
    (pad A2 thru_hole circle (at 0 4.45 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 15 FR_SIG))
    (pad A3 thru_hole circle (at 0 8.9 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 3 5V))
    (pad A4 thru_hole circle (at 0 13.35 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A5 thru_hole circle (at 0 17.8 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A6 thru_hole circle (at 0 22.25 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad A7 thru_hole circle (at -9.12 22.25 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A8 thru_hole circle (at -9.12 17.8 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A9 thru_hole circle (at -9.12 13.35 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A10 thru_hole circle (at -9.12 8.9 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 5 12V-RAW))
    (pad A11 thru_hole circle (at -9.12 4.45 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A12 thru_hole circle (at -9.12 0 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 16 24V))
    (pad B1 thru_hole circle (at 26.16 0 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 14 HB_P))
    (pad B2 thru_hole circle (at 26.16 4.45 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B3 thru_hole circle (at 26.16 8.9 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B4 thru_hole circle (at 26.16 13.35 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B5 thru_hole circle (at 26.16 17.8 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B6 thru_hole circle (at 26.16 22.25 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad B7 thru_hole circle (at 17.04 22.25 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad B8 thru_hole circle (at 17.04 17.8 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad B9 thru_hole circle (at 17.04 13.35 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 6 DATA+))
    (pad B10 thru_hole circle (at 17.04 8.9 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 7 DATA-))
    (pad B11 thru_hole circle (at 17.04 4.45 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 8 CLK-))
    (pad B12 thru_hole circle (at 17.04 0 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 9 CLK+))
    (pad C1 thru_hole circle (at 65.28 0 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 10 PT_P))
    (pad C2 thru_hole circle (at 65.28 4.45 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 13 PD_P))
    (pad C3 thru_hole circle (at 65.28 8.9 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 12 WAT_P))
    (pad C4 thru_hole circle (at 65.28 13.35 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 11 ROT_P))
    (pad C5 thru_hole circle (at 65.28 17.8 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C6 thru_hole circle (at 65.28 22.25 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad C7 thru_hole circle (at 56.16 22.25 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad C8 thru_hole circle (at 56.16 17.8 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad C9 thru_hole circle (at 56.16 13.35 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad C10 thru_hole circle (at 56.16 8.9 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C11 thru_hole circle (at 56.16 4.45 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C12 thru_hole circle (at 56.16 0 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D1 thru_hole circle (at 91.44 0 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 45 /VBUS))
    (pad D2 thru_hole circle (at 91.44 4.45 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 23 SBU2))
    (pad D3 thru_hole circle (at 91.44 8.9 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 20 CC1))
    (pad D4 thru_hole circle (at 91.44 13.35 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 18 D-))
    (pad D5 thru_hole circle (at 91.44 17.8 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D6 thru_hole circle (at 91.44 22.25 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D7 thru_hole circle (at 82.32 22.25 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D8 thru_hole circle (at 82.32 17.8 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad D9 thru_hole circle (at 82.32 13.35 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 19 D+))
    (pad D10 thru_hole circle (at 82.32 8.9 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 21 CC2))
    (pad D11 thru_hole circle (at 82.32 4.45 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 22 SBU1))
    (pad D12 thru_hole circle (at 82.32 0 270) (size 2.739 2.739) (drill 1.826) (layers *.Cu *.Mask)
      (net 44 /USB_GND))
    (pad MH1 thru_hole circle (at -17.895 21.11 270) (size 5.25 5.25) (drill 3.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad MH2 thru_hole circle (at 100.215 21.11 270) (size 5.25 5.25) (drill 3.5) (layers *.Cu *.Mask)
      (net 1 GND))
    (model DT13-48PABCD-R015.stp
      (offset (xyz 41.15999922925132 -56.36999808529242 13.74999979349584))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 167.894 50.546 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 5.08 -2.47 90) (layer F.SilkS))
    (fp_text value 1N5818 (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.SilkS))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user %R (at 5.47 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 12V-RAW))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 12V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Varistor:RV_Disc_D15.5mm_W3.9mm_P7.5mm (layer F.Cu) (tedit 5A0F68DF)
    (at 161.29 60.706 90)
    (descr "Varistor, diameter 15.5mm, width 3.9mm, pitch 7.5mm")
    (tags "varistor SIOV")
    (fp_text reference RV1 (at 3.75 3.65 90) (layer F.SilkS))
    (fp_text value V22ZA3P (at 3.75 -2.25 90) (layer F.Fab))
    (fp_text user %R (at 3.75 0.7 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 7.5 1.4 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 12V-RAW))
    (model ${KISYS3DMOD}/Varistor.3dshapes/RV_Disc_D15.5mm_W3.9mm_P7.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 125.9078 86.9442 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R15 (at 10.2616 0.0762 90) (layer F.SilkS))
    (fp_text value 1820 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(R15-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /HP_RO))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 123.952 79.121)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R14 (at 3.81 -2.286) (layer F.SilkS))
    (fp_text value 1820 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 3.3V))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /HP_DI))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 147.6502 101.1936 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R13 (at 10.414 -3.556 90) (layer F.SilkS))
    (fp_text value 3320 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /HB_P_DIV))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 151.2062 108.8136 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R12 (at -2.794 -3.81 90) (layer F.SilkS))
    (fp_text value 1820 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 /HB_P_DIV))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 HB_P))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 155.5242 101.1936 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R11 (at 10.414 -3.556 90) (layer F.SilkS))
    (fp_text value 3320 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /ROT_P_DIV))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 159.0802 108.8136 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at -2.794 -3.556 90) (layer F.SilkS))
    (fp_text value 1820 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /ROT_P_DIV))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 ROT_P))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 119.253 73.279)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 9.906 0) (layer F.SilkS))
    (fp_text value 165 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 FR_SIG))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 120.904 62.103 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at -2.286 -3.683) (layer F.SilkS))
    (fp_text value 3320 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /RPM_SIG_DIV))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 113.284 65.659)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 9.906 -3.683) (layer F.SilkS))
    (fp_text value 1820 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 /RPM_SIG_DIV))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 RPM_SIG))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 163.3982 101.1936 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 10.16 -3.556 90) (layer F.SilkS))
    (fp_text value 3320 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /WAT_P_DIV))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 166.9542 108.8136 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at -2.54 -3.556 90) (layer F.SilkS))
    (fp_text value 1820 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 /WAT_P_DIV))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 WAT_P))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 171.2722 101.1936 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 10.16 -3.556 90) (layer F.SilkS))
    (fp_text value 3320 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /PD_P_DIV))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 174.8282 108.8136 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at -2.54 -3.556 90) (layer F.SilkS))
    (fp_text value 1820 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 /PD_P_DIV))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 PD_P))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 179.1462 101.1936 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 9.906 -3.556 90) (layer F.SilkS))
    (fp_text value 3320 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /PT_P_DIV))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 182.7022 108.8136 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at -2.286 -3.556 90) (layer F.SilkS))
    (fp_text value 1820 (at 3.81 2.37 90) (layer F.Fab))
    (fp_text user %R (at 3.81 0 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /PT_P_DIV))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 PT_P))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Drill_Monitor_PCB:TIM351215 (layer F.Cu) (tedit 0)
    (at 135.128 44.196 90)
    (descr "TIM 3.5-1215-1")
    (tags "Power Supply")
    (fp_text reference PS1 (at -2.032 -23.114 90) (layer F.SilkS))
    (fp_text value TIM_3.5-1215 (at -4.41 -8.89 90) (layer F.SilkS) hide)
    (fp_text user %R (at -4.41 -8.89 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(PS1-Pad2)"))
    (pad 7 thru_hole circle (at 0 -15.24 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(PS1-Pad7)"))
    (pad 8 thru_hole circle (at 0 -17.78 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(PS1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 -17.78 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 24V))
    (pad 10 thru_hole circle (at -10.16 -15.24 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole circle (at -10.16 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 /PS1_VCC))
    (model TIM_3.5-1215.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_THT:L_Axial_L20.0mm_D8.0mm_P25.40mm_Horizontal (layer F.Cu) (tedit 5AE59B05)
    (at 141.732 44.196)
    (descr "Inductor, Axial series, Axial, Horizontal, pin pitch=25.4mm, , length*diameter=20*8mm^2")
    (tags "Inductor Axial series Axial Horizontal pin pitch 25.4mm  length 20mm diameter 8mm")
    (fp_text reference L1 (at 12.7 -5.12) (layer F.SilkS))
    (fp_text value 10uH (at 12.7 5.12) (layer F.Fab))
    (fp_text user %R (at 12.7 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 25.4 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad 1 thru_hole circle (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 43 /PS1_VCC))
    (model ${KISYS3DMOD}/Inductor_THT.3dshapes/L_Axial_L20.0mm_D8.0mm_P25.40mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown (layer B.Cu) (tedit 5AC8BA0D)
    (at 205.74 50.5206 90)
    (descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Horizontal RM 2.54mm")
    (fp_text reference IC1 (at 2.54 20.58 270) (layer B.SilkS))
    (fp_text value LM2940T-5.0_NOPB (at 2.54 -2 270) (layer B.Fab))
    (fp_text user %R (at 2.54 20.58 270) (layer B.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 12V))
    (pad "" np_thru_hole oval (at 2.54 16.66 90) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 181.61 64.77 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 5.08 -2.47 90) (layer F.SilkS))
    (fp_text value 1N5919BG (at 5.08 2.47 90) (layer F.Fab))
    (fp_text user K (at 0 -2.1 90) (layer F.SilkS))
    (fp_text user K (at 0 -2.1 90) (layer F.Fab))
    (fp_text user %R (at 5.47 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 5V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 120.65 93.773 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C7 (at 2.587 -2.286 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 5V))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 191.77 55.372 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C6 (at 7.874 0 90) (layer F.SilkS))
    (fp_text value 47uF (at 2.5 5.25 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 198.374 55.452 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C5 (at 1.698 -2.2 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D8.0mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 181.61 44.45 270)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (fp_text reference C4 (at 2.5 -5.25 90) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 5.25 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 189.738 44.45 270)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C3 (at 2.5 -2.2 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 172.72 46.736 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C2 (at 3.556 -2.032 90) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 2.2 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 12V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm (layer F.Cu) (tedit 5AE50EF0)
    (at 141.605 54.356)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (fp_text reference C1 (at 2.5 -2.2) (layer F.SilkS))
    (fp_text value 10uF (at 2.5 2.2) (layer F.Fab))
    (fp_text user %R (at 2.5 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /PS1_VCC))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 24V (at 102.108 40.64 90) (layer F.SilkS))
  (gr_text 12V_RAW (at 93.218 38.862 90) (layer F.SilkS))
  (gr_text RPM_SIG (at 102.108 58.928 90) (layer F.SilkS))
  (gr_text FR_SIG (at 97.536 58.166 90) (layer F.SilkS))
  (gr_text CLK+ (at 102.108 66.294 90) (layer F.SilkS))
  (gr_text CLK- (at 97.536 66.294 90) (layer F.SilkS))
  (gr_text DATA- (at 93.218 66.04 90) (layer F.SilkS))
  (gr_text DATA+ (at 88.646 66.04 90) (layer F.SilkS))
  (gr_text HB_P (at 102.108 83.566 90) (layer F.SilkS))
  (gr_text PT_P (at 102.108 122.174 90) (layer F.SilkS))
  (gr_text PD_P (at 97.79 122.428 90) (layer F.SilkS))
  (gr_text WAT_P (at 93.218 122.936 90) (layer F.SilkS))
  (gr_text ROT_P (at 88.646 122.936 90) (layer F.SilkS))
  (gr_text USB_GND (at 102.235 130.302 90) (layer F.SilkS))
  (gr_text SBU1 (at 97.79 131.699 90) (layer F.SilkS))
  (gr_text VCONN (at 93.345 131.191 90) (layer F.SilkS))
  (gr_text D+ (at 88.773 132.588 90) (layer F.SilkS))
  (gr_text VBUS (at 102.108 148.463 90) (layer F.SilkS))
  (gr_text SBU2 (at 97.663 148.59 90) (layer F.SilkS))
  (gr_text CC (at 93.218 147.955 90) (layer F.SilkS))
  (gr_text D- (at 88.773 147.828 90) (layer F.SilkS))
  (gr_text "Hy-Tech Drilling\nht-dm-01001\nRev 2.0" (at 208.534 134.62) (layer F.SilkS))
  (gr_line (start 236.728 30.988) (end 75.438 30.988) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 236.728 157.988) (end 75.438 157.988) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 240.538 34.798) (end 240.538 154.178) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 236.728 30.988) (end 240.538 34.798) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 236.728 157.988) (end 240.538 154.178) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 75.438 30.988) (end 75.438 157.988) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.998 157.988) (xy 110.998 150.368) (xy 235.458 150.368) (xy 235.458 157.988)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 240.538 157.988) (xy 235.458 157.988) (xy 235.458 95.504) (xy 224.536 95.504) (xy 224.536 93.472)
        (xy 235.458 93.472) (xy 235.458 38.608) (xy 110.998 38.608) (xy 110.998 30.988) (xy 240.538 30.988)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635) (smoothing chamfer) (radius 0.762))
    (polygon
      (pts
        (xy 110.998 38.608) (xy 235.458 38.608) (xy 235.458 150.368) (xy 110.998 150.368) (xy 110.998 157.988)
        (xy 75.438 157.988) (xy 75.438 30.988) (xy 110.998 30.988)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 227.838 69.596) (xy 214.376 69.596) (xy 214.376 59.436) (xy 227.838 59.436)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 225.298 53.086) (xy 211.836 53.086) (xy 211.836 42.926) (xy 225.298 42.926)
      )
    )
  )
)
