<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="24.13" y2="0" width="0" layer="20"/>
<wire x1="24.13" y1="0" x2="25.4" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="25.4" y1="1.27" x2="25.4" y2="24.13" width="0" layer="20"/>
<wire x1="25.4" y1="24.13" x2="24.13" y2="25.4" width="0" layer="20" curve="90"/>
<wire x1="24.13" y1="25.4" x2="1.27" y2="25.4" width="0" layer="20"/>
<wire x1="1.27" y1="25.4" x2="0" y2="24.13" width="0" layer="20" curve="90"/>
<wire x1="0" y1="24.13" x2="0" y2="1.27" width="0" layer="20"/>
</plain>
<libraries>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x5 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="atmel" package="DIL08" value="TINY13-20PU">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13-20PU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="9171550"/>
<attribute name="OC_NEWARK" value="96K6521"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X5-SHROUDED" value="AVR_SPI_PROG_5X2PTH2">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08671"/>
<attribute name="SF_ID" value="PRT-08506"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="8"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="4"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="8"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="5"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="6"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="7"/>
<contactref element="J1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
