(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 18)
    (no_connects 0)
    (area 147.954999 107.886499 172.085001 141.443501)
    (thickness 1.6002)
    (drawings 9)
    (tracks 81)
    (zones 0)
    (modules 6)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Anode)
  (net 4 /Din)
  (net 5 "Net-(J1-Pad3)")
  (net 6 /HV6)
  (net 7 /HV5)
  (net 8 /HV10)
  (net 9 /HV4)
  (net 10 /HV9)
  (net 11 /HV3)
  (net 12 /HV8)
  (net 13 /HV2)
  (net 14 /HV7)
  (net 15 /HV1)
  (net 16 "Net-(J1-Pad5)")
  (net 17 "Net-(N1-PadA)")
  (net 18 "Net-(J1-Pad15)")
  (net 19 "Net-(LED1-Pad2-DO)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(LED1-Pad2-DO)")
    (add_net "Net-(N1-PadA)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module adafruit:adafruit-WS2812B (layer F.Cu) (tedit 5A39BE5B)
    (at 160.02 119.38 90)
    (attr smd)
    (fp_text reference LED1 (at 0.0635 3.2385 90) (layer F.SilkS))
    (fp_text value WS2812B5050 (at 0 0 90) (layer F.SilkS) hide)
    (pad 1-VD smd rect (at 2.44856 1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2-DO smd rect (at 2.44856 -1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED1-Pad2-DO)"))
    (pad 3-GN smd rect (at -2.44856 -1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4-DI smd rect (at -2.44856 1.64846 270) (size 1.4986 0.89916) (layers F.Cu F.Paste F.Mask)
      (net 4 /Din))
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer F.Cu) (tedit 5A6FF4A0)
    (at 170.18 136.84 270)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at -2.26 9.96 360) (layer F.SilkS) hide)
    (fp_text value Nixie (at 1.27 22.65 270) (layer F.Fab))
    (fp_text user %R (at 1.27 10.16 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV6))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV5))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV10))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV4))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV9))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV3))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV8))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV2))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV7))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /HV1))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A39C51B)
    (at 160.02 114.38 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 180) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 164.0205 118.9355 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module mynixies:mynixies-6844A-D-SUB (layer F.Cu) (tedit 5A6FF482)
    (at 160.00984 119.39016)
    (descr "THIS FOOTPRINT USES FEMALE D-SUB PINS AS 'SOCKETS'.")
    (tags "THIS FOOTPRINT USES FEMALE D-SUB PINS AS 'SOCKETS'.")
    (attr virtual)
    (fp_text reference N1 (at 0.07366 -10.42416) (layer F.SilkS))
    (fp_text value 6844AD-SUB (at 0.635 0) (layer F.SilkS) hide)
    (fp_text user Bot (at -0.18034 5.76834) (layer F.SilkS))
    (fp_text user Top (at 0.01016 -3.69316) (layer F.SilkS))
    (pad 0 thru_hole circle (at 6.51256 5.1943) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 8 /HV10))
    (pad 1 thru_hole circle (at -6.51256 5.19176) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 15 /HV1))
    (pad 2 thru_hole circle (at -8.12038 1.85166) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 13 /HV2))
    (pad 3 thru_hole circle (at -8.12038 -1.8542) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 11 /HV3))
    (pad 4 thru_hole circle (at -6.51256 -5.1943) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 9 /HV4))
    (pad 5 thru_hole circle (at -3.61442 -7.5057) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 7 /HV5))
    (pad 6 thru_hole circle (at 3.61442 -7.5057) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 6 /HV6))
    (pad 7 thru_hole circle (at 6.51256 -5.19176) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 14 /HV7))
    (pad 8 thru_hole circle (at 8.12038 -1.85166) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 12 /HV8))
    (pad 9 thru_hole circle (at 8.12038 1.85166) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 10 /HV9))
    (pad A thru_hole circle (at 3.61442 7.5057) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask)
      (net 17 "Net-(N1-PadA)"))
    (pad N/C thru_hole circle (at 0 8.3312) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask))
    (pad N/C2 thru_hole circle (at 0 -8.3312) (size 2.4003 2.4003) (drill 1.6002) (layers *.Cu *.Paste *.Mask))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 169.02 128.28 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.0735 1.8245 270) (layer F.SilkS))
    (fp_text value 18k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(N1-PadA)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /Anode))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 148.0185 134.62) (end 148.59 134.62) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 171.45 134.62) (end 172.0215 134.62) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 160.02 119.38) (end 148.59 119.38) (angle 180) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.59 119.38) (end 148.59 134.62) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 171.45 119.38) (end 171.45 134.62) (layer Edge.Cuts) (width 0.127))
  (gr_text "nixies.us\nB-13-B" (at 160.5915 120.9675 90) (layer B.Mask))
  (gr_line (start 148.02 141.38) (end 148.0185 134.62) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 172.02 141.38) (end 172.0215 134.62) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 148.02 141.38) (end 172.02 141.38) (layer Edge.Cuts) (width 0.127))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer) (radius 1))
    (polygon
      (pts
        (xy 163.2585 109.22) (xy 167.005 111.1885) (xy 169.545 114.4905) (xy 170.688 118.999) (xy 170.688 135.128)
        (xy 171.577 135.1915) (xy 171.45 140.7795) (xy 148.463 140.7795) (xy 148.5265 135.3185) (xy 149.098 135.3185)
        (xy 149.225 118.364) (xy 150.114 115.1255) (xy 151.8285 112.014) (xy 155.5115 109.2835) (xy 160.0835 108.585)
      )
    )
  )
)
