(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 21)
    (no_connects 0)
    (area 142.684499 46.164499 198.183501 68.643501)
    (thickness 1.6)
    (drawings 55)
    (tracks 25)
    (zones 0)
    (modules 8)
    (nets 8)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 1.2)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.9)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x011fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 /ANT1)
  (net 2 /ANT2)
  (net 3 /MEGA-PIN15)
  (net 4 /MEGA-PIN16)
  (net 5 /MEGA-PIN19)
  (net 6 "/MEGA-PIN14(TX)")
  (net 7 /GND)
  (net_class Default "Dit is de standaard class."
    (clearance 0.3)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /GND)
    (add_net "/MEGA-PIN14(TX)")
    (add_net /MEGA-PIN15)
    (add_net /MEGA-PIN16)
    (add_net /MEGA-PIN19)
  )
  (net_class "RF 433" ""
    (clearance 0.7)
    (trace_width 0.9)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /ANT1)
    (add_net /ANT2)
  )
  (module BRICE:Arduino_Mega_RFLINK_433 (layer Top) (tedit 59E66B2C)
    (at 99.06 99.06)
    (fp_text reference AR1 (at 10.414 -64.897) (layer F.SilkS) hide)
    (fp_text value ARDUNIO_MEGA_RFLINK_SIMPLE (at 10.414 -66.802) (layer F.Fab))
    (fp_text user "Arduino Mega Rev 3" (at 72.39 -11.43) (layer B.SilkS) hide)
    (fp_text user 2017 (at 89.662 -50.8) (layer B.SilkS))
    (pad 7 thru_hole circle (at 45.72 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 55.88 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 53.34 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 50.8 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at 48.26 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 35 thru_hole circle (at 96.52 -33.02) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 34 thru_hole circle (at 93.98 -33.02) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad GND thru_hole circle (at 45.72 -45.72) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 16 thru_hole circle (at 73.66 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /MEGA-PIN16))
    (pad 17 thru_hole circle (at 76.2 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at 83.82 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 71.12 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /MEGA-PIN15))
    (pad 14 thru_hole circle (at 68.58 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "/MEGA-PIN14(TX)"))
    (pad 18 thru_hole circle (at 78.74 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 19 thru_hole circle (at 81.28 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /MEGA-PIN19))
    (pad 21 thru_hole circle (at 86.36 -50.8) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
  )
  (module BRICE:SYN115 (layer Top) (tedit 59E6547C)
    (at 169.164 60.452)
    (fp_text reference U2 (at -5.715 1.27 90) (layer F.SilkS) hide)
    (fp_text value SYN115 (at -3.81 -6.985 180) (layer F.Fab))
    (fp_text user SYN115 (at 5.715 -3.556 90) (layer F.SilkS))
    (fp_text user Ant (at 3.175 -1.905) (layer F.SilkS))
    (fp_text user GND (at 0 -1.905) (layer F.SilkS))
    (fp_text user DAT (at -2.54 -1.905) (layer F.SilkS))
    (fp_text user VCC (at -5.08 -1.905) (layer F.SilkS))
    (pad 4 thru_hole circle (at 3.175 -3.7465 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 /ANT1))
    (pad 3 thru_hole circle (at 0 -3.7465 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 2 thru_hole circle (at -2.54 -3.7465 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "/MEGA-PIN14(TX)"))
    (pad 1 thru_hole rect (at -5.08 -3.7465 270) (size 1.5 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /MEGA-PIN15))
  )
  (module Connectors:SMB_Straight (layer Top) (tedit 59E50B7C)
    (at 183.896 61.468)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference AE1 (at 0 -4.85) (layer F.SilkS))
    (fp_text value Antenne_Shield (at 0 5.05) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 /ANT1))
    (model Connectors.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:SMB_Straight (layer Top) (tedit 59E50B64)
    (at 150.368 61.468)
    (descr "SMB pcb mounting jack")
    (tags "SMB Jack  Striaght")
    (fp_text reference AE2 (at 0 -4.826 180) (layer F.SilkS))
    (fp_text value Antenne_Shield (at 0 5.05) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 /ANT2))
    (model Connectors.3dshapes/SMB_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BRICE:RF_RXB6 (layer Top) (tedit 59E512DE)
    (at 168.148 51.816)
    (fp_text reference RE1 (at 0 -0.635) (layer F.SilkS) hide)
    (fp_text value RXB6 (at 0 -5.08) (layer F.Fab))
    (fp_text user Data (at 17.653 1.397 180) (layer F.SilkS))
    (fp_text user Vcc (at 12.7 1.397) (layer F.SilkS))
    (fp_text user Gnd (at 20.32 1.397 180) (layer F.SilkS))
    (fp_text user Gnd (at -15.24 1.397 180) (layer F.SilkS))
    (fp_text user Gnd (at -17.78 1.397 180) (layer F.SilkS))
    (fp_text user Ant (at -20.32 1.397 180) (layer F.SilkS))
    (pad 8 thru_hole circle (at -20.32 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 /ANT2))
    (pad 7 thru_hole circle (at -17.78 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 6 thru_hole circle (at -15.24 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /GND))
    (pad 5 thru_hole circle (at -12.7 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 4 thru_hole rect (at 12.7 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 /MEGA-PIN16))
    (pad 3 thru_hole circle (at 15.24 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 17.78 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /MEGA-PIN19))
    (pad 1 thru_hole circle (at 20.32 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /GND))
  )
  (module BRICE:FS1000A (layer Top) (tedit 59E51410)
    (at 167.64 66.04)
    (fp_text reference U1 (at -7.874 0.508) (layer F.SilkS) hide)
    (fp_text value FS1000A (at 0 2.54) (layer F.Fab))
    (fp_text user FS1000A (at 6.604 0) (layer F.SilkS))
    (fp_text user gnd (at 2.54 -2.54) (layer F.SilkS))
    (fp_text user vcc (at 0 -2.54) (layer F.SilkS))
    (fp_text user Dat (at -2.54 -2.54) (layer F.SilkS))
    (pad 1 thru_hole circle (at -2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "/MEGA-PIN14(TX)"))
    (pad 2 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /MEGA-PIN15))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 /GND))
  )
  (module Symbols:OSHW-Symbol_8.9x8mm_SilkScreen (layer Bottom) (tedit 0)
    (at 157.988 55.88 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Symbol_8.9x8mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Symbols:WEEE-Logo_4.2x6mm_SilkScreen (layer Bottom) (tedit 0)
    (at 176.53 54.356 180)
    (descr "Waste Electrical and Electronic Equipment Directive")
    (tags "Logo WEEE")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value WEEE-Logo_4.2x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_line (start 142.748 67.564) (end 142.748 47.244) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 143.764 67.564) (end 143.764 68.58) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 144.78 46.228) (end 143.764 46.228) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 145.288 68.58) (end 143.764 68.58) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 146.304 46.228) (end 144.78 46.228) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_text GND (at 144.78 51.308) (layer F.SilkS))
  (gr_text "RFLINK A - V1 - 433Mhz" (at 164.084 53.34) (layer F.SilkS))
  (gr_text 2017 (at 188.976 48.26) (layer F.SilkS))
  (gr_line (start 155.956 46.228) (end 146.304 46.228) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 156.972 48.768) (end 156.972 47.244) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 164.592 49.784) (end 157.988 49.784) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.608 47.244) (end 165.608 48.768) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 197.104 68.58) (end 145.288 68.58) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 198.12 64.516) (end 198.12 67.564) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 191.008 62.484) (end 191.008 47.244) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 197.104 63.5) (end 192.024 63.5) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 192.024 62.484) (end 192.024 63.5) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 189.992 46.228) (end 166.624 46.228) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 166.624 47.244) (end 165.608 47.244) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 164.592 48.768) (end 165.608 48.768) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 157.988 48.768) (end 157.988 49.784) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 155.956 47.244) (end 155.956 46.228) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 143.764 47.244) (end 142.748 47.244) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 197.104 67.564) (end 198.12 67.564) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 197.104 64.516) (end 197.104 63.5) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 189.992 47.244) (end 189.992 46.228) (angle 90) (layer Edge.Cuts) (width 0.127))
  (gr_text "NB: \nFS1000A ou SYN115" (at 167.64 61.468) (layer F.SilkS))
  (gr_text RXB6 (at 176.53 52.07) (layer F.SilkS))
  (gr_text "DESIGN IN FRENCH\nZIONIII - RFLINK A V1\nhttps://easydomoticz.com/" (at 166.37 62.484) (layer B.SilkS))
  (zone (net 7) (net_name /GND) (layer Bottom) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.972 49.784) (xy 165.608 49.784) (xy 165.608 46.228) (xy 191.008 46.228) (xy 191.008 63.5)
        (xy 198.12 63.5) (xy 198.12 68.58) (xy 142.748 68.58) (xy 142.748 46.228) (xy 156.972 46.228)
      )
    )
  )
  (zone (net 7) (net_name /GND) (layer Top) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.972 49.784) (xy 165.608 49.784) (xy 165.608 46.228) (xy 191.008 46.228) (xy 191.008 63.5)
        (xy 198.12 63.5) (xy 198.12 68.58) (xy 142.748 68.58) (xy 142.748 46.228) (xy 156.972 46.228)
      )
    )
    (polygon
      (pts        (xy 182.626 60.452) (xy 182.626 62.484) (xy 176.784 62.738) (xy 171.958 57.912) (xy 173.736 56.134)
        (xy 177.8 60.452) (xy 178.054 60.452)
      )
    )
    (polygon
      (pts        (xy 146.812 52.324) (xy 148.717 51.054) (xy 151.511 55.0545) (xy 151.511 60.452) (xy 151.511 61.468)
        (xy 149.225 61.468) (xy 149.225 55.753)
      )
    )
  )
)
