(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 19)
    (no_connects 0)
    (area 116.02 71.612879 146.12 108.3)
    (thickness 1.6)
    (drawings 8)
    (tracks 68)
    (zones 0)
    (modules 11)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.13)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.6 0.4)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f8_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbs/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +BATT)
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(R1-Pad2)")
  (net 8 "Net-(R1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59C2C029)
    (at 132.79 100.11 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -1.77 1.96 360) (layer F.SilkS))
    (fp_text value 47uF (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59C2BEB8)
    (at 122.8 90.48 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -1.55 1.85 180) (layer F.SilkS))
    (fp_text value 10nF (at 0 2.1 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59C2BF47)
    (at 122.76 95.48 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -1.47 -2 360) (layer F.SilkS))
    (fp_text value 15K (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59C2C02F)
    (at 127.95 99.62)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference TH1 (at 1.06 1.84) (layer F.SilkS))
    (fp_text value TH_PTH (at 0 2.1) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module idlehands_footprints:Button_CKN9112CT-ND (layer F.Cu) (tedit 59C2D063)
    (at 131.2 87.29 180)
    (fp_text reference SW1 (at 22.85 -4.72 180) (layer F.SilkS) hide)
    (fp_text value SPST (at -18.52 -1.59 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 4.75 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
    (pad 2 smd rect (at 4.75 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -4.75 -2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad1)"))
    (pad 1 smd rect (at -4.75 2.25 180) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +BATT))
  )
  (module LEDs:LED-0805 (layer F.Cu) (tedit 59C2C039)
    (at 138.28 92.08 90)
    (descr "LED 0805 smd package")
    (tags "LED 0805 SMD")
    (attr smd)
    (fp_text reference D2 (at 0.68 -2.18 180) (layer F.SilkS))
    (fp_text value LED (at 0 1.75 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.04902 0 270) (size 1.19888 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED-0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59C2C064)
    (at 138.28 96.63 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 1.77 2.11 360) (layer F.SilkS))
    (fp_text value 1K (at 0 2.1 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module idlehands_footprints:CoinCellHolder_SM locked (layer B.Cu) (tedit 5912910E)
    (at 131.04 93.06 180)
    (fp_text reference BT1 (at -0.1 7.4 180) (layer B.SilkS))
    (fp_text value Battery (at 0 -6.2 180) (layer B.Fab))
    (pad 2 smd rect (at -10.98 0 180) (size 2.79 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
    (pad 1 smd circle (at 0 0 180) (size 17.72 17.72) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 10.98 0 180) (size 2.79 5.08) (layers B.Cu B.Paste B.Mask)
      (net 2 +BATT))
  )
  (module smd_challenge:smdc1_cu (layer F.Cu) (tedit 0)
    (at 123.2 90.72)
    (fp_text reference LogoCu (at 0 0) (layer F.SilkS) hide)
    (fp_text value CU (at 0.75 0) (layer F.SilkS) hide)
  )
  (module smd_challenge:smdc1_mask (layer F.Cu) (tedit 0)
    (at 123.2 90.71)
    (fp_text reference LogoMask (at 0 0) (layer F.SilkS) hide)
    (fp_text value MASK (at 0.75 0) (layer F.SilkS) hide)
  )
  (module idlehands_footprints:LMC555CMX (layer F.Cu) (tedit 59C52399)
    (at 130.91 93.68 180)
    (fp_text reference U1 (at -0.07 -1.52 180) (layer F.SilkS))
    (fp_text value LMC555 (at -0.07 -3.33 360) (layer F.SilkS))
    (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0 180) (layer Cmts.User))
    (pad 1 smd rect (at -2.4638 -1.905 180) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.4638 -0.635 180) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -2.4638 0.635 180) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (pad 4 smd rect (at -2.4638 1.905 180) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad1)"))
    (pad 5 smd rect (at 2.4638 1.905 180) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 6 smd rect (at 2.4638 0.635 180) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at 2.4638 -0.635 180) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R1-Pad2)"))
    (pad 8 smd rect (at 2.4638 -1.905 180) (size 1.9812 0.5588) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R1-Pad1)"))
  )
  (gr_text "patreon.com/seanhodgins\nyoutube.com/seanhodginsfilms\n" (at 131.15 81.8) (layer B.SilkS))
  (gr_circle (center 131.07 74.66288) (end 132.57 74.66288) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 126.07 77.001915) (end 126.658235 78.913453) (angle -72.895365) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.07 77.001915) (end 128.07 74.66288) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 131.07 74.66288) (end 134.07 74.66288) (angle -180.000005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.07 74.66288) (end 134.07 77.001915) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 136.07 77.001915) (end 134.07 77.001915) (angle -72.895361) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 131.07 93.25) (end 126.658236 78.913462) (angle -325.790731) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.13))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 99.86 106.75) (xy 104.31 73.03) (xy 131.37 64.23) (xy 163.3 86.35) (xy 147.96 113.41)
        (xy 96.43 116.17)
      )
    )
  )
)
