<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="2.54" y2="0" width="0.254" layer="20"/>
<wire x1="2.54" y1="0" x2="199.39" y2="0" width="0.254" layer="20"/>
<wire x1="199.39" y1="0" x2="201.93" y2="1.27" width="0.254" layer="20"/>
<wire x1="201.93" y1="1.27" x2="201.93" y2="22.86" width="0.254" layer="20"/>
<wire x1="201.93" y1="22.86" x2="199.39" y2="24.13" width="0.254" layer="20"/>
<wire x1="199.39" y1="24.13" x2="2.54" y2="24.13" width="0.254" layer="20"/>
<wire x1="2.54" y1="24.13" x2="0" y2="22.86" width="0.254" layer="20"/>
<wire x1="0" y1="22.86" x2="0" y2="1.27" width="0.254" layer="20"/>
<text>+5VDC</text>
<text>GND</text>
<text>   RV-Project.Com Cylon Eye LED Board Ver3.3A</text>
<text>   RV-Project.Com Cylon Eye LED Board</text>
<text>   RV-Project.Com Cylon Eye LED Board Ver3.3A</text>
<text>DATA  5V  GND</text>
<text>GND  5V DATA</text>
<text> Bezel
Outline</text>
<text>3/13/2019</text>
<text>Order 2 Oz Copper!</text>
<text>http://www.rv-project.com/projects/cyloneye.php</text>
<text>Shell: https://amzn.to/2VZ0d85
LED: Adafruit 2760
TVS: SMF8.0A
Capacitor: 0.01uF Ceramic 1206
R1: 470 1206
R2-3: 1K 1206
Connector: Tayda A777</text>
</plain>
<libraries>
<library name="alsstuff">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="1206-CAP">
</package>
<package name="5050NEOPIXELRGB">
</package>
<package name="1206-RES">
</package>
</packages>
</library>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="1206-RES">
</package>
<package name="WAFER3PINVERTICAL">
</package>
<package name="CREATIVECOMMONS">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="USA">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="alsstuff" package="1206-CAP" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="alsstuff" package="1206-CAP" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="alsstuff" package="1206-CAP" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="alsstuff" package="5050NEOPIXELRGB" value="RGB_NEOPIXELS5050">
<attribute name="NAME"/>
</element>
<element name="LED2" library="alsstuff" package="5050NEOPIXELRGB" value="RGB_NEOPIXELS5050">
<attribute name="NAME"/>
</element>
<element name="LED1" library="alsstuff" package="5050NEOPIXELRGB" value="RGB_NEOPIXELS5050">
<attribute name="NAME"/>
</element>
<element name="R1" library="alsstuff" package="1206-RES" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="alsstuff" package="5050NEOPIXELRGB" value="RGB_NEOPIXELS5050">
<attribute name="NAME"/>
</element>
<element name="LED5" library="alsstuff" package="5050NEOPIXELRGB" value="RGB_NEOPIXELS5050">
<attribute name="NAME"/>
</element>
<element name="LED6" library="alsstuff" package="5050NEOPIXELRGB" value="RGB_NEOPIXELS5050">
<attribute name="NAME"/>
</element>
<element name="LED7" library="alsstuff" package="5050NEOPIXELRGB" value="RGB_NEOPIXELS5050">
<attribute name="NAME"/>
</element>
<element name="LED8" library="alsstuff" package="5050NEOPIXELRGB" value="RGB_NEOPIXELS5050">
<attribute name="NAME"/>
</element>
<element name="LED9" library="alsstuff" package="5050NEOPIXELRGB" value="RGB_NEOPIXELS5050">
<attribute name="NAME"/>
</element>
<element name="C4" library="alsstuff" package="1206-CAP" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="alsstuff" package="1206-CAP" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="alsstuff" package="1206-CAP" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="alsstuff" package="1206-CAP" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="alsstuff" package="1206-CAP" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="alsstuff" package="1206-CAP" value="0.1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TVS1" library="a-lib" package="1206-RES" value="8v">
<attribute name="NAME"/>
</element>
<element name="TVS2" library="a-lib" package="1206-RES" value="8v">
<attribute name="NAME"/>
</element>
<element name="J1" library="a-lib" package="WAFER3PINVERTICAL" value="WAFER3PVERTICAL">
<attribute name="NAME"/>
</element>
<element name="U$1" library="a-lib" package="CREATIVECOMMONS" value=""/>
<element name="R2" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TVS3" library="a-lib" package="1206-RES" value="8v">
<attribute name="NAME"/>
</element>
<element name="TVS4" library="a-lib" package="1206-RES" value="8v">
<attribute name="NAME"/>
</element>
<element name="R3" library="a-lib" package="1206-RES" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="a-lib_Asthetics" package="USA" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED1" pad="1"/>
<contactref element="LED2" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="1"/>
<contactref element="LED3" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="LED1" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="LED3" pad="2"/>
<contactref element="LED2" pad="2"/>
<contactref element="LED1" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="LED4" pad="2"/>
<contactref element="LED5" pad="2"/>
<contactref element="LED6" pad="2"/>
<contactref element="LED7" pad="2"/>
<contactref element="LED8" pad="2"/>
<contactref element="LED9" pad="2"/>
<contactref element="TVS2" pad="2"/>
<contactref element="J1" pad="P$2"/>
<contactref element="TVS4" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="1"/>
<contactref element="TVS1" pad="2"/>
<contactref element="J1" pad="P$1"/>
</signal>
<signal name="N$9">
</signal>
<signal name="N$4">
<contactref element="LED3" pad="1"/>
<contactref element="LED4" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="LED4" pad="1"/>
<contactref element="LED5" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="LED5" pad="1"/>
<contactref element="LED6" pad="4"/>
</signal>
<signal name="N$12">
<contactref element="LED6" pad="1"/>
<contactref element="LED7" pad="4"/>
</signal>
<signal name="N$13">
<contactref element="LED7" pad="1"/>
<contactref element="LED8" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="LED8" pad="1"/>
<contactref element="LED9" pad="4"/>
</signal>
<signal name="GND">
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="LED3" pad="3"/>
<contactref element="LED2" pad="3"/>
<contactref element="LED1" pad="3"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="LED4" pad="3"/>
<contactref element="LED5" pad="3"/>
<contactref element="LED6" pad="3"/>
<contactref element="LED7" pad="3"/>
<contactref element="LED8" pad="3"/>
<contactref element="LED9" pad="3"/>
<contactref element="TVS2" pad="1"/>
<contactref element="TVS1" pad="1"/>
<contactref element="J1" pad="P$3"/>
<contactref element="R2" pad="1"/>
<contactref element="TVS3" pad="1"/>
<contactref element="TVS4" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R2" pad="2"/>
<contactref element="LED9" pad="1"/>
<contactref element="TVS3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
