(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 202)
    (zones 0)
    (modules 18)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(Disp1-Pad12)")
  (net 4 "Net-(Disp1-Pad11)")
  (net 5 "Net-(Disp1-Pad10)")
  (net 6 "Net-(Disp1-Pad9)")
  (net 7 "Net-(Disp1-Pad8)")
  (net 8 "Net-(Disp1-Pad7)")
  (net 9 "Net-(Disp1-Pad6)")
  (net 10 "Net-(Disp1-Pad5)")
  (net 11 "Net-(Disp1-Pad4)")
  (net 12 "Net-(Disp1-Pad3)")
  (net 13 "Net-(Disp1-Pad2)")
  (net 14 "Net-(Disp1-Pad1)")
  (net 15 "Net-(J1-Pad4)")
  (net 16 "Net-(J1-Pad3)")
  (net 17 "Net-(J1-Pad2)")
  (net 18 "Net-(J2-Pad4)")
  (net 19 "Net-(J2-Pad2)")
  (net 20 "Net-(J2-Pad1)")
  (net 21 "Net-(J3-Pad5)")
  (net 22 "Net-(J3-Pad1)")
  (net 23 "Net-(R3-Pad2)")
  (net 24 "Net-(R4-Pad2)")
  (net 25 "Net-(R5-Pad2)")
  (net 26 "Net-(R6-Pad2)")
  (net 27 "Net-(R7-Pad2)")
  (net 28 "Net-(R8-Pad2)")
  (net 29 "Net-(R9-Pad2)")
  (net 30 "Net-(R10-Pad2)")
  (net 31 "Net-(U1-Pad3)")
  (net 32 "Net-(U1-Pad2)")
  (net 33 "Net-(U2-Pad9)")
  (net 34 "Net-(U3-Pad9)")
  (net 35 "Net-(U3-Pad15)")
  (net 36 "Net-(U3-Pad4)")
  (net 37 "Net-(U3-Pad3)")
  (net 38 "Net-(U3-Pad2)")
  (net 39 "Net-(U3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(Disp1-Pad1)")
    (add_net "Net-(Disp1-Pad10)")
    (add_net "Net-(Disp1-Pad11)")
    (add_net "Net-(Disp1-Pad12)")
    (add_net "Net-(Disp1-Pad2)")
    (add_net "Net-(Disp1-Pad3)")
    (add_net "Net-(Disp1-Pad4)")
    (add_net "Net-(Disp1-Pad5)")
    (add_net "Net-(Disp1-Pad6)")
    (add_net "Net-(Disp1-Pad7)")
    (add_net "Net-(Disp1-Pad8)")
    (add_net "Net-(Disp1-Pad9)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad15)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad9)")
  )
  (module digikey-footprints:DIP-16_W7.62mm (layer F.Cu) (tedit 59C51584)
    (at 136.271 84.455 270)
    (fp_text reference U3 (at 3.94 8.763 180) (layer F.SilkS))
    (fp_text value SN74HC595N (at 3.8 20 90) (layer F.Fab))
    (fp_text user REF** (at 3.84 7.97 90) (layer F.Fab))
    (pad 9 thru_hole circle (at 7.62 17.78 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(U3-Pad9)"))
    (pad 8 thru_hole circle (at 0 17.78 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole circle (at 7.62 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole circle (at 7.62 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(U3-Pad15)"))
    (pad 14 thru_hole circle (at 7.62 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad9)"))
    (pad 13 thru_hole circle (at 7.62 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at 7.62 10.16 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad1)"))
    (pad 11 thru_hole circle (at 7.62 12.7 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad2)"))
    (pad 10 thru_hole circle (at 7.62 15.24 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 7 thru_hole circle (at 0 15.24 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(Disp1-Pad8)"))
    (pad 6 thru_hole circle (at 0 12.7 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(Disp1-Pad9)"))
    (pad 5 thru_hole circle (at 0 10.16 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(Disp1-Pad12)"))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(U3-Pad4)"))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(U3-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(U3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(U3-Pad1)"))
  )
  (module digikey-footprints:DIP-16_W7.62mm (layer F.Cu) (tedit 59C51584)
    (at 165.1 84.455 270)
    (fp_text reference U2 (at 3.937 8.89 180) (layer F.SilkS))
    (fp_text value SN74HC595N (at 3.8 20 90) (layer F.Fab))
    (fp_text user REF** (at 3.84 7.97 90) (layer F.Fab))
    (pad 9 thru_hole circle (at 7.62 17.78 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad9)"))
    (pad 8 thru_hole circle (at 0 17.78 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole circle (at 7.62 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 15 thru_hole circle (at 7.62 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(R6-Pad2)"))
    (pad 14 thru_hole circle (at 7.62 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad3)"))
    (pad 13 thru_hole circle (at 7.62 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at 7.62 10.16 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad1)"))
    (pad 11 thru_hole circle (at 7.62 12.7 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad2)"))
    (pad 10 thru_hole circle (at 7.62 15.24 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 7 thru_hole circle (at 0 15.24 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 6 thru_hole circle (at 0 12.7 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(R4-Pad2)"))
    (pad 5 thru_hole circle (at 0 10.16 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(R5-Pad2)"))
    (pad 4 thru_hole circle (at 0 7.62 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(R7-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(R8-Pad2)"))
    (pad 2 thru_hole circle (at 0 2.54 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(R9-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(R10-Pad2)"))
  )
  (module digikey-footprints:DIP-8_W7.62mm (layer B.Cu) (tedit 5B86B3A2)
    (at 142.748 76.962 90)
    (descr http://media.digikey.com/pdf/Data%20Sheets/Lite-On%20PDFs/6N137%20Series.pdf)
    (fp_text reference U1 (at 4.064 -3.81) (layer B.SilkS))
    (fp_text value ATTINY85-20PU (at 3.94 -10.33 -90) (layer B.Fab))
    (fp_text user REF** (at 3.94 -3.49 -90) (layer B.Fab))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 7 thru_hole circle (at 7.62 -2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 6 thru_hole circle (at 7.62 -5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad1)"))
    (pad 5 thru_hole circle (at 7.62 -7.62 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad2)"))
    (pad 4 thru_hole circle (at 0 -7.62 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 -5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(U1-Pad3)"))
    (pad 2 thru_hole circle (at 0 -2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(U1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad5)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.336 68.58)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 3.81 0) (layer F.SilkS))
    (fp_text value 120 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(Disp1-Pad10)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 158.496 74.676)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R9 (at 3.81 0) (layer F.SilkS))
    (fp_text value 120 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(R9-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Disp1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.336 71.628)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R4 (at 3.81 0) (layer F.SilkS))
    (fp_text value 120 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(Disp1-Pad11)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal locked (layer F.Cu) (tedit 5AE5139B)
    (at 158.496 77.724)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R10 (at 3.81 0) (layer F.SilkS))
    (fp_text value 120 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(R10-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(Disp1-Pad5)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.336 74.676)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R5 (at 3.81 0) (layer F.SilkS))
    (fp_text value 120 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(Disp1-Pad7)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 148.336 77.724)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R6 (at 3.81 0) (layer F.SilkS))
    (fp_text value 120 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(R6-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(Disp1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 158.496 68.58)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R7 (at 3.81 0) (layer F.SilkS))
    (fp_text value 120 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(R7-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Disp1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 158.496 71.628)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R8 (at 3.81 0) (layer F.SilkS))
    (fp_text value 120 (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(R8-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(Disp1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 120.904 74.676)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 120.904 71.628)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10K (at 3.81 2.37) (layer F.Fab))
    (fp_text user %R (at 3.81 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad2)"))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 143.51 90.932 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J3 (at 1.27 7.366) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 155.575 95.25 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0.762 -2.921 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 131.572 78.105)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J1 (at 0 -13.081) (layer B.SilkS))
    (fp_text value Screw_Terminal_01x05 (at 0 -12.49) (layer B.Fab))
    (fp_text user %R (at 0 -5.08 -90) (layer B.Fab))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Display_7Segment:CA56-12SYKWA (layer F.Cu) (tedit 5A02FE84)
    (at 135.89 80.8736 90)
    (descr "4 digit 7 segment green LED, http://www.kingbright.com/attachments/file/psearch/000/00/00/CA56-12SYKWA(Ver.6A).pdf")
    (tags "4 digit 7 segment green LED")
    (fp_text reference Disp1 (at -0.6604 -16.256 180) (layer F.SilkS))
    (fp_text value LN5643R-11 (at 3.8 32.8 90) (layer F.Fab))
    (fp_text user %R (at 8.128 6.604 90) (layer F.Fab))
    (pad 12 thru_hole circle (at 15.24 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(Disp1-Pad12)"))
    (pad 11 thru_hole circle (at 15.24 2.54 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(Disp1-Pad11)"))
    (pad 10 thru_hole circle (at 15.24 5.08 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(Disp1-Pad10)"))
    (pad 9 thru_hole circle (at 15.24 7.62 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(Disp1-Pad9)"))
    (pad 8 thru_hole circle (at 15.24 10.16 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(Disp1-Pad8)"))
    (pad 7 thru_hole circle (at 15.24 12.7 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(Disp1-Pad7)"))
    (pad 6 thru_hole circle (at 0 12.7 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(Disp1-Pad6)"))
    (pad 5 thru_hole circle (at 0 10.16 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(Disp1-Pad5)"))
    (pad 4 thru_hole circle (at 0 7.62 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Disp1-Pad4)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(Disp1-Pad3)"))
    (pad 2 thru_hole circle (at 0 2.54 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(Disp1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(Disp1-Pad1)"))
    (model ${KISYS3DMOD}/Display_7Segment.3dshapes/CA56-12SYKWA.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 145.796 72.136 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C1 (at -2.286 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 2.5 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Sam Pearce" (at 122.174 89.662) (layer B.SilkS))
  (gr_text "I2C Temp v1" (at 161.798 65.532) (layer B.SilkS))
  (gr_line (start 116.84 93.599) (end 116.84 93.218) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 117.221 93.599) (end 116.84 93.599) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.84 93.218) (end 116.84 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.987 93.599) (end 117.221 93.599) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 153.67 97.282) (end 149.987 93.599) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.64 97.282) (end 153.67 97.282) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.64 63.5) (end 116.84 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.64 97.282) (end 167.64 63.5) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 167.64 97.282) (xy 153.67 97.282) (xy 149.987 93.599) (xy 116.713 93.599) (xy 116.84 63.5)
        (xy 167.64 63.5)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 167.64 97.282) (xy 153.67 97.282) (xy 149.987 93.599) (xy 116.713 93.599) (xy 116.84 63.5)
        (xy 167.64 63.5)
      )
    )
  )
)
