(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.646)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(material "Liquid Photo")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0254)
				(material "SMOBC")
				(epsilon_r 3.3)
				(loss_tangent 0)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.524)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0356)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0254)
				(material "SMOBC")
				(epsilon_r 3.3)
				(loss_tangent 0)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(material "Liquid Photo")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints yes)
		(tenting front back)
		(aux_axis_origin 127.20111 115.16359)
		(grid_origin 127.20111 115.16359)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+3.3V")
	(net 3 "/Power Subsystem/STAT")
	(net 4 "/Power Subsystem/*PG")
	(net 5 "VBUS")
	(net 6 "/Power Subsystem/VDD")
	(net 7 "/Power Subsystem/*INT")
	(net 8 "/Power Subsystem/TS")
	(net 9 "/Power Subsystem/TS_BIAS")
	(net 10 "/Power Subsystem/ILIM")
	(net 11 "Net-(U309-SW)")
	(net 12 "+BATT")
	(net 13 "Net-(U309-REGN)")
	(net 14 "Net-(U309-BTST)")
	(net 15 "Net-(U309-PMID)")
	(net 16 "Net-(D303-A)")
	(net 17 "Net-(D304-A)")
	(net 18 "Net-(U312-L1_1)")
	(net 19 "Net-(U312-FB)")
	(net 20 "Net-(U312-L2_1)")
	(net 21 "Net-(U312-EN)")
	(net 22 "Net-(C423-Pad1)")
	(net 23 "/Power Subsystem/SDA")
	(net 24 "/Power Subsystem/SCL")
	(net 25 "unconnected-(X309-Pad8)")
	(net 26 "/Power Subsystem/BMS_out")
	(net 27 "unconnected-(X309-Pad5)")
	(net 28 "Net-(Q305-D)")
	(net 29 "Net-(Q305-G)")
	(net 30 "Net-(U308-BIN)")
	(net 31 "Net-(U312-VOUT_1)")
	(net 32 "Net-(U312-PG)")
	(net 33 "Net-(J307-CC2)")
	(net 34 "Net-(J307-CC1)")
	(net 35 "/Power Subsystem/D-")
	(net 36 "/Power Subsystem/D+")
	(net 37 "Net-(J305-Pad2)")
	(net 38 "Net-(D308-A)")
	(net 39 "unconnected-(J307-SBU1-Pad10)")
	(net 40 "unconnected-(J307-SBU2-Pad4)")
	(net 41 "unconnected-(U309-*QON-Pad7)")
	(net 42 "unconnected-(X309-Pad4)")
	(net 43 "Net-(U301-VBUS)")
	(net 44 "Net-(U301-RSTb)")
	(net 45 "Net-(U301-SUSPENDb)")
	(net 46 "unconnected-(U301-GPIO.6-Pad20)")
	(net 47 "unconnected-(U301-DSR-Pad27)")
	(net 48 "unconnected-(U301-CTS-Pad23)")
	(net 49 "unconnected-(U301-RI{slash}CLK-Pad2)")
	(net 50 "unconnected-(U301-GPIO.0{slash}TXT-Pad19)")
	(net 51 "/Power Subsystem/TXD")
	(net 52 "unconnected-(U301-CHREN-Pad13)")
	(net 53 "/Power Subsystem/RXD")
	(net 54 "unconnected-(U301-CHR1-Pad14)")
	(net 55 "unconnected-(U301-SUSPEND-Pad12)")
	(net 56 "unconnected-(U301-NC-Pad10)")
	(net 57 "unconnected-(U301-GPIO.5-Pad21)")
	(net 58 "unconnected-(U301-GPIO.3{slash}WAKEUP-Pad16)")
	(net 59 "unconnected-(U301-GPIO.2{slash}RS485-Pad17)")
	(net 60 "unconnected-(U301-DCD-Pad1)")
	(net 61 "unconnected-(U301-GPIO.1{slash}RXT-Pad18)")
	(net 62 "unconnected-(U301-GPIO.4-Pad22)")
	(net 63 "unconnected-(U301-CHR0-Pad15)")
	(net 64 "Net-(D301-A)")
	(net 65 "unconnected-(J301-Pin_2-Pad2)")
	(net 66 "unconnected-(U301-DTR-Pad28)")
	(net 67 "unconnected-(U301-RTS-Pad24)")
	(net 68 "unconnected-(X309-Pad6)")
	(net 69 "/Power Subsystem/~{BAT_INT}")
	(net 70 "Net-(U309-VBUS)")
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 141.100018 78.95)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP323"
			(at 2.85 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 31 "Net-(U312-VOUT_1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:1N5819HW-7-F_DIO"
		(layer "F.Cu")
		(at 162.503206 85.3125)
		(tags "1N5819HW-7-F ")
		(property "Reference" "D301"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148WT"
			(at 0 -1.8 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/ds30396.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "75V 0.15A Fast switching Diode, SOD-523"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?523*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.65321 -0.8125 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.65321 -0.8125 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.1684 0 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.1684 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7218 0)
			(size 1.1176 0.6604)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "VBUS")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7218 0)
			(size 1.1176 0.6604)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "Net-(D301-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/Parts/1N5819HW_7_F/1N5819HW-7-F.STEP"
			(offset
				(xyz 0 0 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 167.600022 103.95)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP338"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 8 "/Power Subsystem/TS")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 160.700014 93.05 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R305"
			(at 0 -1.35 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Net-(U309-VBUS)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 155.250022 102.95)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP334"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 12 "+BATT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 157.700014 89.9)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP327"
			(at 1.499986 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 5 "VBUS")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 146.95 91.2 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R344"
			(at 2.05 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Power Subsystem/*INT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 131.200022 85.95)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP324"
			(at -1.45 0.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 2 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 165.950022 96)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP337"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 10 "/Power Subsystem/ILIM")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 159.750022 104.45)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP335"
			(at 2.249978 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 9 "/Power Subsystem/TS_BIAS")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 157.700014 93.45)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP326"
			(at 1.499986 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 70 "Net-(U309-VBUS)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 150.329138 102 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C400"
			(at -0.053725 1.201156 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uf"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:JST_B2B-XH-A"
		(layer "B.Cu")
		(at 140.911638 110.05 180)
		(property "Reference" "J305"
			(at 5.7825 -2.55 0)
			(layer "B.SilkS")
		)
		(property "Value" "B2B-XH-A"
			(at 3.67 -4.76 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "N/A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "7 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "JST Sales America Inc."
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 1.25 -0.525 180)
			(size 1.575 1.575)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -1.25 -0.525 180)
			(size 1.575 1.575)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J305-Pad2)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/Parts/B2B_XH_A/B2B-XH-A.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 160.404124 102.2125 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R345"
			(at 0 1.249999 90)
			(layer "B.SilkS")
		)
		(property "Value" "R"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/Power Subsystem/TS_BIAS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/Power Subsystem/TS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 157.244276 93.843544)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C403"
			(at 0 1.2053 0)
			(layer "B.SilkS")
		)
		(property "Value" "47nF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U309-SW)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U309-BTST)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 140.443052 89.91318 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R339"
			(at 2.464336 -0.060189 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Subsystem/SCL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 139.279138 73.9 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C427"
			(at 2.35 -0.05 135)
			(layer "B.SilkS")
		)
		(property "Value" "22u"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U312-VOUT_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 162.044012 99.30766 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R335"
			(at -0.055991 -1.263955 0)
			(layer "B.SilkS")
		)
		(property "Value" "TBD"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/Power Subsystem/ILIM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 158.729138 77 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R303"
			(at 0.051156 -1.146275 90)
			(layer "B.SilkS")
		)
		(property "Value" "22.1K"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(U301-VBUS)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 148.904138 92.8)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C407"
			(at 2.524996 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "20uF"
			(at -0.141421 -1.272792 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/Power Subsystem/BMS_out")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "B.Cu")
		(at 146.529138 103.2 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q305"
			(at -2.448844 -0.496275 0)
			(layer "B.SilkS")
		)
		(property "Value" "2N7002"
			(at 0 -2.4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NDS7002A-D.PDF"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.115A Id, 60V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q305-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(Q305-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 166.71691 93.887609 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R342"
			(at 0.034047 0.938765 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D303-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "B.Cu")
		(at 133.032863 76.698844 180)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H305"
			(at 0 3.7 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MountHole"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 144.129138 87.4)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R320"
			(at 0 -1 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(U312-PG)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "Net-(D308-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 143.229971 84.341735 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C418"
			(at 0.007109 1.147108 90)
			(layer "B.SilkS")
		)
		(property "Value" "100n"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U312-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "B.Cu")
		(at 165.029138 108.8 180)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H307"
			(at 0 3.7 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MountHole"
			(at 0 -3.7 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:CONN12_016JA1R1500_JAE"
		(layer "B.Cu")
		(at 162.529138 82.3499 -90)
		(tags "DX07S016JA1R1500 ")
		(property "Reference" "J307"
			(at 3.1 -2.908 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "DX07S016JA1R1500"
			(at 3.1 -2.908 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "1"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "JAE Industry Ltd."
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.31 mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(clearance 0.1682)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 3.1 -2.908 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0.1 -1.054 270)
			(size 0.6096 0.6096)
			(drill 0.6096)
			(layers)
		)
		(pad "1" smd rect
			(at 0 0 270)
			(size 0.5588 1.0922)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at 0.749999 0 270)
			(size 0.5588 1.0922)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 64 "Net-(D301-A)")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 1.350001 0 270)
			(size 0.3048 1.0414)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 34 "Net-(J307-CC1)")
			(pinfunction "CC1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.85 0 270)
			(size 0.3048 1.0414)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 40 "unconnected-(J307-SBU2-Pad4)")
			(pinfunction "SBU2")
			(pintype "no_connect")
		)
		(pad "5" smd rect
			(at 2.349999 0 270)
			(size 0.3048 1.0414)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Power Subsystem/D-")
			(pinfunction "D-")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.85 0 270)
			(size 0.3048 1.0414)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "/Power Subsystem/D+")
			(pinfunction "D+")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 3.349999 0 270)
			(size 0.3048 1.0414)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "/Power Subsystem/D+")
			(pinfunction "D+__1")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 3.850001 0 270)
			(size 0.3048 1.0414)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Power Subsystem/D-")
			(pinfunction "D-__1")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 4.35 0 270)
			(size 0.3048 1.0414)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "Net-(J307-CC2)")
			(pinfunction "CC2")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 4.849999 0 270)
			(size 0.3048 1.0414)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 39 "unconnected-(J307-SBU1-Pad10)")
			(pinfunction "SBU1")
			(pintype "no_connect")
		)
		(pad "11" smd rect
			(at 5.45 0 270)
			(size 0.5588 1.0922)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 64 "Net-(D301-A)")
			(pinfunction "VBUS__1")
			(pintype "power_in")
		)
		(pad "12" smd rect
			(at 6.199999 0 270)
			(size 0.5588 1.0922)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND__1")
			(pintype "power_in")
		)
		(pad "13" thru_hole oval
			(at -1.220002 -0.670999 180)
			(size 2.158 1.158)
			(drill oval 1.65 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "14" thru_hole oval
			(at 7.419601 -0.670999 180)
			(size 2.158 1.158)
			(drill oval 1.65 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole oval
			(at -1.220002 -4.496 180)
			(size 2.458 1.158)
			(drill oval 1.95 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "16" thru_hole oval
			(at 7.420001 -4.496 180)
			(size 2.458 1.158)
			(drill oval 1.95 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "17" thru_hole oval
			(at 6.099999 -1.054001 270)
			(size 1.0532 0.8032)
			(drill oval 0.85 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "18" smd rect
			(at 1.7 -4.496 180)
			(size 2.0066 0.9906)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "19" smd rect
			(at 4.499999 -4.496 180)
			(size 2.0066 0.9906)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/Parts/DX07S016JA1R1500/DX07S016JA1R1500.STEP"
			(offset
				(xyz 3.1 -3.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "capstone-project:WQFN-HR18__RYK_TEX"
		(layer "B.Cu")
		(at 155.579138 98.3 180)
		(tags "BQ25620RYKR ")
		(property "Reference" "U309"
			(at -0.106066 -2.298844 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "BQ25622RYKR"
			(at -0.085132 3.160579 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/bq25620"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "WQFN-HR18__RYK_TEX")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(fp_text user "*"
			(at -2.25 1.45 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -2.25 1.45 0)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -0.762 0.635 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.762 0.635 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.024992 0.850001 180)
			(size 0.127 0.127)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "Net-(U309-BTST)")
			(pinfunction "BTST")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.388 0.392999 180)
			(size 0.624992 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "Net-(U309-REGN)")
			(pinfunction "REGN")
			(pintype "power_out")
		)
		(pad "3" smd rect
			(at -1.388 -0.007 180)
			(size 0.624992 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "/Power Subsystem/*PG")
			(pinfunction "*PG")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -1.388 -0.406999 180)
			(size 0.624992 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "/Power Subsystem/ILIM")
			(pinfunction "ILIM")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -1.024992 -0.850001 180)
			(size 0.127 0.127)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "/Power Subsystem/TS_BIAS")
			(pinfunction "TS_BIAS")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -0.624999 -1.15 90)
			(size 0.599999 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "/Power Subsystem/TS")
			(pinfunction "TS")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -0.225 -1.15 90)
			(size 0.599999 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 41 "unconnected-(U309-*QON-Pad7)")
			(pinfunction "*QON")
			(pintype "input+no_connect")
		)
		(pad "8" smd rect
			(at 0.175 -0.95 180)
			(size 0.2 0.999998)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "+BATT")
			(pinfunction "BAT")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 0.574999 -0.95 180)
			(size 0.2 0.999998)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "/Power Subsystem/BMS_out")
			(pinfunction "SYS")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at 0.974999 -0.850001 180)
			(size 0.127 0.127)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "/Power Subsystem/STAT")
			(pinfunction "STAT")
			(pintype "output")
		)
		(pad "11" smd rect
			(at 1.4 -0.406999 180)
			(size 0.599999 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "/Power Subsystem/*INT")
			(pinfunction "*INT")
			(pintype "output")
		)
		(pad "12" smd rect
			(at 1.4 -0.007 180)
			(size 0.599999 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "/Power Subsystem/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 1.4 0.392999 180)
			(size 0.599999 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "/Power Subsystem/SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "14" smd rect
			(at 0.974999 0.850001 180)
			(size 0.127 0.127)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "*CE")
			(pintype "input")
		)
		(pad "15" smd rect
			(at 0.574999 0.95 180)
			(size 0.2 0.999998)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "16" smd rect
			(at 0.175 0.95 180)
			(size 0.2 0.999998)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "Net-(U309-SW)")
			(pinfunction "SW")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -0.225 0.949999 180)
			(size 0.2 0.999998)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "Net-(U309-PMID)")
			(pinfunction "PMID")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -0.624999 1.141 90)
			(size 0.618998 0.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 70 "Net-(U309-VBUS)")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/BQ25622ERYKR/BQ25622ERYKR.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 153.344276 93.093544 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C404"
			(at -2.6947 0.011413 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0.036764 1.521688 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U309-PMID)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 142.429138 80)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C423"
			(at 0.003725 0.998844 0)
			(layer "B.SilkS")
		)
		(property "Value" "C"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(C423-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U312-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 160.729138 77 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R302"
			(at 0.001156 1.103725 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Net-(U301-SUSPENDb)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:TPS63020DSJR"
		(layer "B.Cu")
		(at 146.929138 79.4 90)
		(descr "DSJ (R-PVSON-N14)")
		(tags "Integrated Circuit")
		(property "Reference" "U312"
			(at -2.9 -0.100004 0)
			(layer "B.SilkS")
		)
		(property "Value" "TPS63020QDSJRQ1"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.arrow.com/en/products/tps63020qdsjrq1/texas-instruments?region=nac"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Switching Voltage Regulators Single Inductor Buck Boost Converter"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "1"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "595-TPS63020QDSJRQ1"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TPS63020QDSJRQ1?qs=VymPLiRQZISDN5SwwPCkkQ%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TPS63020QDSJRQ1"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd oval
			(at -1.5 -1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "Net-(U312-EN)")
			(pinfunction "VINA")
			(pintype "passive")
		)
		(pad "2" smd oval
			(at -1 -1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd oval
			(at -0.5 -1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "Net-(U312-FB)")
			(pinfunction "FB")
			(pintype "passive")
		)
		(pad "4" smd oval
			(at 0 -1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "Net-(U312-VOUT_1)")
			(pinfunction "VOUT_1")
			(pintype "passive")
		)
		(pad "5" smd oval
			(at 0.5 -1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "Net-(U312-VOUT_1)")
			(pinfunction "VOUT_2")
			(pintype "passive")
		)
		(pad "6" smd oval
			(at 1 -1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "Net-(U312-L2_1)")
			(pinfunction "L2_1")
			(pintype "passive")
		)
		(pad "7" smd oval
			(at 1.5 -1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "Net-(U312-L2_1)")
			(pinfunction "L2_2")
			(pintype "passive")
		)
		(pad "8" smd oval
			(at 1.5 1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 18 "Net-(U312-L1_1)")
			(pinfunction "L1_1")
			(pintype "passive")
		)
		(pad "9" smd oval
			(at 1 1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 18 "Net-(U312-L1_1)")
			(pinfunction "L1_2")
			(pintype "passive")
		)
		(pad "10" smd oval
			(at 0.5 1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "/Power Subsystem/BMS_out")
			(pinfunction "VIN_1")
			(pintype "passive")
		)
		(pad "11" smd oval
			(at 0 1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "/Power Subsystem/BMS_out")
			(pinfunction "VIN_2")
			(pintype "passive")
		)
		(pad "12" smd oval
			(at -0.5 1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "Net-(U312-EN)")
			(pinfunction "EN")
			(pintype "passive")
		)
		(pad "13" smd oval
			(at -1 1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "Net-(U312-EN)")
			(pinfunction "PS/SYNC")
			(pintype "passive")
		)
		(pad "14" smd oval
			(at -1.5 1.4 90)
			(size 0.24 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "Net-(U312-PG)")
			(pinfunction "PG")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 0 0)
			(size 1.58 2.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "PGND_1")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -1.813 0.69)
			(size 0.2 0.775)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -1.813 0.23)
			(size 0.2 0.775)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -1.813 -0.23)
			(size 0.2 0.775)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -1.813 -0.69)
			(size 0.2 0.775)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 1.813 -0.69)
			(size 0.2 0.775)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 1.813 -0.23)
			(size 0.2 0.775)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 1.813 0.23)
			(size 0.2 0.775)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 1.813 0.69)
			(size 0.2 0.775)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/Parts/TPS63020DSJR/TPS63020DSJR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
		(model "C:/Users/zackp/OneDrive/Desktop/TPS63020DSJR/TPS63020DSJR.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 159.571169 93.099133 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C406"
			(at -0.000289 -1.061694 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Net-(U309-VBUS)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 164.925006 101.7425 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "TH301"
			(at 0.906344 -1.507857 90)
			(layer "B.SilkS")
		)
		(property "Value" "Thermistor_NTC"
			(at -0.395259 -1.760171 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Temperature dependent resistor, negative temperature coefficient"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*NTC* *Thermistor* PIN?ARRAY* bornier* *Terminal?Block* R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Power Subsystem/TS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 160.329138 81 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R348"
			(at 0 -1.2 90)
			(layer "B.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "Net-(J307-CC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 148.929138 94.4)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C445"
			(at 2.449996 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/Power Subsystem/BMS_out")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "B.Cu")
		(at 165.029138 76.75 180)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H306"
			(at 0 3.7 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MountHole"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 144.282863 99.848844)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R321"
			(at 0 -1.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "1.8M"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U308-BIN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/Power Subsystem/VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:TVS-SP05_LTF"
		(layer "B.Cu")
		(at 157.329138 90)
		(tags "SP0503BAHTG ")
		(property "Reference" "CR301"
			(at 0 -2.35 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "SP0503BAHTG"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "SP0503BAHTG"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TVS-SP05_LTF TVS-SP05_LTF-M TVS-SP05_LTF-L")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.44145 2.667 0)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -1.44145 2.667 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.3175 1.4478 0)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -0.3175 1.4478 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.18745 0.9652)
			(size 0.9779 0.5588)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -1.18745 -0.9652)
			(size 0.9779 0.5588)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Power Subsystem/D-")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 1.18745 -0.9652)
			(size 0.9779 0.5588)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "/Power Subsystem/D+")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 1.18745 0.9652)
			(size 0.9779 0.5588)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 64 "Net-(D301-A)")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/Parts/SP0503BAHTG/SP0503BAHTG.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "B.Cu")
		(at 147.054138 74.3625 180)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L341"
			(at -0.028725 1.113656 0)
			(layer "B.SilkS")
		)
		(property "Value" "L"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U312-L1_1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U312-L2_1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 143.729138 91.8 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R324"
			(at -2.501156 0.046275 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/Power Subsystem/~{BAT_INT}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 144.282863 101.448844 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R323"
			(at 2.65 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(Q305-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U308-BIN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "B.Cu")
		(at 133.029138 108.8 180)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H308"
			(at 0 3.7 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MountHole"
			(at 0 -3.7 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 139.279138 75.45 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C429"
			(at 2.35 0 135)
			(layer "B.SilkS")
		)
		(property "Value" "22u"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U312-VOUT_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 150.902216 104.073521)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R325"
			(at -0.067551 1.193409 0)
			(layer "B.SilkS")
		)
		(property "Value" "tbd"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(Q305-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:QFN28_5X5_SIL"
		(layer "B.Cu")
		(at 155.129138 83 -45)
		(tags "CP2102N-A02-GQFN28 ")
		(property "Reference" "U301"
			(at -3.783024 -0.106063 45)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "CP2102N-A02-GQFN28"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "CP2102N-A02-GQFN28"
			(at 0 0 135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN28_5X5_SIL QFN28_5X5_SIL-M QFN28_5X5_SIL-L")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(clearance 0.15)
		(attr smd)
		(fp_text user "*"
			(at -3.181983 2.545587 135)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at -1.8415 1.75 135)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at -1.8415 1.75 135)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.3241 1.5 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "unconnected-(U301-DCD-Pad1)")
			(pinfunction "DCD")
			(pintype "input+no_connect")
		)
		(pad "2" smd rect
			(at -2.324099 1.000001 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "unconnected-(U301-RI{slash}CLK-Pad2)")
			(pinfunction "RI/CLK")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd rect
			(at -2.3241 0.499999 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "4" smd rect
			(at -2.3241 0 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "/Power Subsystem/D+")
			(pinfunction "D+")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.3241 -0.499999 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Power Subsystem/D-")
			(pinfunction "D-")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -2.324099 -1.000001 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at -2.3241 -1.5 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "+3.3V")
			(pinfunction "VREGIN")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at -1.5 -2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "Net-(U301-VBUS)")
			(pinfunction "VBUS")
			(pintype "input")
		)
		(pad "9" smd rect
			(at -1.000001 -2.324099 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 44 "Net-(U301-RSTb)")
			(pinfunction "RSTb")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at -0.499999 -2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 56 "unconnected-(U301-NC-Pad10)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "11" smd rect
			(at 0 -2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 45 "Net-(U301-SUSPENDb)")
			(pinfunction "SUSPENDb")
			(pintype "output")
		)
		(pad "12" smd rect
			(at 0.499999 -2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 55 "unconnected-(U301-SUSPEND-Pad12)")
			(pinfunction "SUSPEND")
			(pintype "output+no_connect")
		)
		(pad "13" smd rect
			(at 1.000001 -2.324099 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 52 "unconnected-(U301-CHREN-Pad13)")
			(pinfunction "CHREN")
			(pintype "output+no_connect")
		)
		(pad "14" smd rect
			(at 1.5 -2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 54 "unconnected-(U301-CHR1-Pad14)")
			(pinfunction "CHR1")
			(pintype "output+no_connect")
		)
		(pad "15" smd rect
			(at 2.3241 -1.5 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 63 "unconnected-(U301-CHR0-Pad15)")
			(pinfunction "CHR0")
			(pintype "output+no_connect")
		)
		(pad "16" smd rect
			(at 2.324099 -1.000001 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 58 "unconnected-(U301-GPIO.3{slash}WAKEUP-Pad16)")
			(pinfunction "GPIO.3/WAKEUP")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" smd rect
			(at 2.3241 -0.499999 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 59 "unconnected-(U301-GPIO.2{slash}RS485-Pad17)")
			(pinfunction "GPIO.2/RS485")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" smd rect
			(at 2.3241 0 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "unconnected-(U301-GPIO.1{slash}RXT-Pad18)")
			(pinfunction "GPIO.1/RXT")
			(pintype "bidirectional+no_connect")
		)
		(pad "19" smd rect
			(at 2.3241 0.499999 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "unconnected-(U301-GPIO.0{slash}TXT-Pad19)")
			(pinfunction "GPIO.0/TXT")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" smd rect
			(at 2.324099 1.000001 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 46 "unconnected-(U301-GPIO.6-Pad20)")
			(pinfunction "GPIO.6")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" smd rect
			(at 2.3241 1.5 225)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 57 "unconnected-(U301-GPIO.5-Pad21)")
			(pinfunction "GPIO.5")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" smd rect
			(at 1.5 2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 62 "unconnected-(U301-GPIO.4-Pad22)")
			(pinfunction "GPIO.4")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" smd rect
			(at 1.000001 2.324099 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 48 "unconnected-(U301-CTS-Pad23)")
			(pinfunction "CTS")
			(pintype "input+no_connect")
		)
		(pad "24" smd rect
			(at 0.499999 2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 67 "unconnected-(U301-RTS-Pad24)")
			(pinfunction "RTS")
			(pintype "output+no_connect")
		)
		(pad "25" smd rect
			(at 0 2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 53 "/Power Subsystem/RXD")
			(pinfunction "RXD")
			(pintype "input")
		)
		(pad "26" smd rect
			(at -0.499999 2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 51 "/Power Subsystem/TXD")
			(pinfunction "TXD")
			(pintype "output")
		)
		(pad "27" smd rect
			(at -1.000001 2.324099 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 47 "unconnected-(U301-DSR-Pad27)")
			(pinfunction "DSR")
			(pintype "input+no_connect")
		)
		(pad "28" smd rect
			(at -1.5 2.3241 315)
			(size 0.254 0.9652)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 66 "unconnected-(U301-DTR-Pad28)")
			(pinfunction "DTR")
			(pintype "output+no_connect")
		)
		(pad "29" smd rect
			(at 0 0 315)
			(size 3.3528 3.3528)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/Parts/CP2102N_A02_GQFN28/CP2102N-A02-GQFN28.step"
			(offset
				(xyz 0 0 0.3)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 140.079138 79.45 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R362"
			(at -0.098844 -1.196275 90)
			(layer "B.SilkS")
		)
		(property "Value" "R"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(U312-PG)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U312-VOUT_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 142.075546 90.802608 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R337"
			(at 2.503764 0.007317 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/Power Subsystem/SDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:DSBGA9-YZF_TEX"
		(layer "B.Cu")
		(at 145.329138 96.099874 -90)
		(tags "BQ27427YZFR ")
		(property "Reference" "U308"
			(at 0 3.302 90)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "BQ27427YZFR"
			(at -0.136225 -4.064 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/bq27427"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSBGA9-YZF_TEX DSBGA9-YZF_TEX-M DSBGA9-YZF_TEX-L")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(clearance 0.14)
		(attr smd)
		(fp_text user "A"
			(at -1.4351 0.500126 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -0.500126 1.4605 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at 0.500126 1.4605 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "C"
			(at -1.4351 -0.500126 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -0.549874 1.479142 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "A"
			(at -1.449874 0.479142 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "C"
			(at -1.449874 -0.520858 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "3"
			(at 0.500126 1.479142 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "3"
			(at 0.500126 1.4605 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "C"
			(at -1.4351 -0.500126 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "1"
			(at -0.500126 1.4605 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "A"
			(at -1.4351 0.500126 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "A1" smd circle
			(at -0.500126 0.500126 270)
			(size 0.2794 0.2794)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 69 "/Power Subsystem/~{BAT_INT}")
			(pinfunction "GPOUT")
			(pintype "output")
		)
		(pad "A2" smd circle
			(at 0 0.500126 270)
			(size 0.2794 0.2794)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "/Power Subsystem/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "A3" smd circle
			(at 0.500126 0.500126 270)
			(size 0.2794 0.2794)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "/Power Subsystem/SCL")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "B1" smd circle
			(at -0.500126 0 270)
			(size 0.2794 0.2794)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "Net-(U308-BIN)")
			(pinfunction "BIN")
			(pintype "input")
		)
		(pad "B2" smd circle
			(at 0 0 270)
			(size 0.2794 0.2794)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_out")
		)
		(pad "B3" smd circle
			(at 0.500126 0 270)
			(size 0.2794 0.2794)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "/Power Subsystem/VDD")
			(pinfunction "VDD")
			(pintype "output")
		)
		(pad "C1" smd circle
			(at -0.500126 -0.500126 270)
			(size 0.2794 0.2794)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_out")
		)
		(pad "C2" smd circle
			(at 0 -0.500126 270)
			(size 0.2794 0.2794)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "/Power Subsystem/BMS_out")
			(pinfunction "SRX")
			(pintype "input")
		)
		(pad "C3" smd circle
			(at 0.500126 -0.500126 270)
			(size 0.2794 0.2794)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "+BATT")
			(pinfunction "BAT")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/BQ27427YZFR/BQ27427YZFR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "B.Cu")
		(at 132.729138 101 90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J301"
			(at 0.101156 3.803725 90)
			(layer "B.SilkS")
		)
		(property "Value" "Stemma QT"
			(at 0 -3.98 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4208/4208_Kaweei_C13396_diagram.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic shielded connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1SH*")
		(sheetname "/")
		(sheetfile "system-testbed.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 2 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 2 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "unconnected-(J301-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd roundrect
			(at 0.5 2 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/Power Subsystem/SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 2 90)
			(size 0.6 1.55)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/Power Subsystem/SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 -1.875 90)
			(size 1.2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.8 -1.875 90)
			(size 1.2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Users/zackp/OneDrive/Desktop/Hardware(1.3)/Hardware(1.2)/Hardware(1.1)/Hardware(1.1)/Hardware/Hardware/KiCAD/system-testbed/capstone-project.pretty/3dmodels/5394 1.9in TFT Display.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Users/zackp/OneDrive/Desktop/Hardware(1.3)/Hardware(1.2)/Hardware(1.1)/Hardware(1.1)/Hardware/Hardware/KiCAD/system-testbed/capstone-project.pretty/3dmodels/217177-0001.stp"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Users/zackp/OneDrive/Desktop/Hardware(1.3)/Hardware(1.2)/Hardware(1.1)/Hardware(1.1)/Hardware/Hardware/KiCAD/system-testbed/capstone-project.pretty/3dmodels/SM04B-SRSS-TB.step"
			(offset
				(xyz 0 1.5 -0.5)
			)
			(scale
				(xyz 1 1 1.1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 143.229138 77.65 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R355"
			(at 2.75 0.05 90)
			(layer "B.SilkS")
		)
		(property "Value" "R"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U312-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U312-VOUT_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 147.37042 100.223798)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C394"
			(at 0 -1.245949 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/Power Subsystem/VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "B.Cu")
		(at 131.929138 87.8 90)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X309"
			(at -0.3125 -0.475 90)
			(layer "B.SilkS")
		)
		(property "Value" "EYESPI"
			(at 0.1 -4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "system-testbed.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -4.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -3.75 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.75 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 42 "unconnected-(X309-Pad4)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -2.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "unconnected-(X309-Pad5)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -1.75 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 68 "unconnected-(X309-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -1.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -0.75 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "unconnected-(X309-Pad8)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -0.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 69 "/Power Subsystem/~{BAT_INT}")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 0.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 0.75 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 1.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at 1.75 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "/Power Subsystem/SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at 2.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "/Power Subsystem/SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at 2.75 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "/Power Subsystem/*INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at 3.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at 3.75 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 51 "/Power Subsystem/TXD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at 4.25 3.35 90)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 53 "/Power Subsystem/RXD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z1" smd rect
			(at -6.05 0.6 90)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z2" smd rect
			(at 6.05 0.6 90)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 0.5 0.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded"
		(layer "B.Cu")
		(at 139.432863 103.848844 90)
		(descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
		(tags "test point wire loop bead")
		(property "Reference" "TP329"
			(at -1.5 -2.2 135)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 2.8 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 3 3)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 159.929138 74.2 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R304"
			(at 0 1.101156 0)
			(layer "B.SilkS")
		)
		(property "Value" "47.5K"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(U301-VBUS)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 142.479138 82)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R356"
			(at -2.6 0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "R"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U312-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 139.304138 77 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C430"
			(at 2.421275 0.301156 135)
			(layer "B.SilkS")
		)
		(property "Value" "22u"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U312-VOUT_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "B.Cu")
		(at 167.305139 96.21603 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D303"
			(at 0 1.223999 90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/Power Subsystem/STAT")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D303-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 153.244001 103.330454 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C395"
			(at 0.08161 1.188862 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "+BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "B.Cu")
		(at 164.149238 94.576556 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D304"
			(at -0.277712 1.166375 90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.787501 0 270)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/Power Subsystem/*PG")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.787501 0 270)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D304-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 161.936016 103.267536 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R346"
			(at -0.106066 -1.378858 90)
			(layer "B.SilkS")
		)
		(property "Value" "R"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/Power Subsystem/TS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 141.679138 77.65 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R358"
			(at 2.75 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "R"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(C423-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U312-VOUT_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:LTST-C190KRKT"
		(layer "B.Cu")
		(at 146.729138 88.2 90)
		(descr "LTST-C190KRKT")
		(tags "LED")
		(property "Reference" "D308"
			(at -2.2 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.8 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.8 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "Net-(D308-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "LTST-C190KRKT.stp"
			(offset
				(xyz -0.02999999888 0 0.279999997)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -180 -180 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 147.929138 85.2 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C415"
			(at 2.496275 -0.048844 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/Power Subsystem/BMS_out")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 166.399589 91.90058)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C408"
			(at 1.883274 -0.051736 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7u"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:SW_100SP1T1B4M2QE"
		(layer "B.Cu")
		(at 153.729138 109.35 -90)
		(property "Reference" "S301"
			(at -0.001156 -7.103725 90)
			(layer "B.SilkS")
		)
		(property "Value" "100SP1T1B4M2QE"
			(at 7.295 -7.635 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "E"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "29.68 mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "E-Switch"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 4.7 270)
			(size 2.775 2.775)
			(drill 1.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J305-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0 0 270)
			(size 2.775 2.775)
			(drill 1.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J305-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 0 -4.7 270)
			(size 2.775 2.775)
			(drill 1.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+BATT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/Parts/100SP1T1B4M2QE/100SP1T1B4M2QE.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
		(model "C:/Users/zackp/OneDrive/Desktop/100SP1T1B4M2QE/SW_100SP1T1B4M2QE.kicad_mod"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Users/zackp/OneDrive/Desktop/100SP1T1B4M2QE/100SP1T1B4M2QE.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1.1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 137.529138 80.4 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R322"
			(at 0.001156 -1.146275 90)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U312-VOUT_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 154.240073 75.844344 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C301"
			(at -1.8955 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(U301-VBUS)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 161.329138 97 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C401"
			(at -0.051156 -1.103725 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(U309-REGN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 154.944276 93.093544 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C405"
			(at -2.6947 0.061413 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U309-PMID)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 140.069518 97.138892 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 147.929138 83.59 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C413"
			(at 2.496275 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10u"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/Regulators/")
		(sheetfile "Other Blocks.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/Power Subsystem/BMS_out")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 164.729138 97)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R343"
			(at 0 1.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D304-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 151.929138 76.6)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C302"
			(at 0 -1.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 161.913032 93.096439 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R334"
			(at -1.896439 -0.016106 0)
			(layer "B.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(J307-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 156.329138 75 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R301"
			(at 1.951156 0.003725 0)
			(layer "B.SilkS")
		)
		(property "Value" "1K"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(U301-RSTb)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "B.Cu")
		(at 150.529138 96.2 180)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L339"
			(at 0 -1.4125 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uH"
			(at 0.58 -7.625 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Subsystem/")
		(sheetfile "power-subsystem.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U309-SW)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/Power Subsystem/BMS_out")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 133.05705 72.037937)
		(end 165.0572 72.037947)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 128.55721 76.537945)
		(mid 129.875112 73.355958)
		(end 133.05705 72.037937)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 133.030516 113.780566)
		(mid 129.865767 112.453087)
		(end 128.557179 109.28048)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 169.557169 109.305215)
		(mid 168.230424 112.471244)
		(end 165.057149 113.780566)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.557169 92.897915)
		(end 128.557159 76.537945)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.057149 113.780566)
		(end 133.030516 113.780566)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 165.0572 72.037947)
		(mid 168.242511 73.359313)
		(end 169.557159 76.547403)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.557169 92.897952)
		(end 169.557169 109.305215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 128.557179 109.28048)
		(end 128.557169 92.897915)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.557159 76.547403)
		(end 169.557159 92.897952)
		(layer "Edge.Cuts")
	)
	(gr_text "V_Bus (current TP's)"
		(at 156.5 96 90)
		(layer "F.SilkS")
	)
	(gr_text "+BATT (Voltage TP)"
		(at 154 106.55 90)
		(layer "F.SilkS")
	)
	(gr_text "ILIM"
		(at 165.1 97.85 0)
		(layer "F.SilkS")
	)
	(gr_text "TS"
		(at 167.15 102.75 0)
		(layer "F.SilkS")
	)
	(gr_text "Vout (current TP's)"
		(at 133.2 85.5 40)
		(layer "F.SilkS")
	)
	(gr_text "TS_Bias"
		(at 158.25 106.2 0)
		(layer "F.SilkS")
	)
	(gr_text "Vout_TP\n(should be 3.3V)"
		(at 129.55 88.7 0)
		(layer "F.SilkS")
	)
	(gr_text "Batt Input"
		(at 143.129134 106.85 -0)
		(layer "B.SilkS")
	)
	(gr_text "BMS"
		(at 156.129134 96.35 -0)
		(layer "B.SilkS")
	)
	(gr_text "BMS-out ->"
		(at 149.429134 91.25 -90)
		(layer "B.SilkS")
	)
	(gr_text "^USB->UART"
		(at 154.379134 87.95 -45)
		(layer "B.SilkS")
	)
	(gr_text "Buck/Boost"
		(at 149.579134 76.7 -0)
		(layer "B.SilkS")
	)
	(gr_text "MOSFET"
		(at 144.779134 102.35 -270)
		(layer "B.SilkS")
	)
	(gr_text "Feul Gauge"
		(at 146.629134 98.3 -90)
		(layer "B.SilkS")
	)
	(gr_text "USB"
		(at 160.629134 86.2 -90)
		(layer "B.SilkS")
	)
	(gr_text "EYESPI"
		(at 132.429146 87.45 -90)
		(layer "B.Fab")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(arc
					(start 128.60048 109.305294)
					(mid 129.909068 112.477901)
					(end 133.073817 113.80538)
				)
				(arc
					(start 165.10045 113.80538)
					(mid 168.273725 112.496058)
					(end 169.60047 109.330029)
				)
				(xy 169.60047 92.922766)
				(arc
					(start 169.60046 76.572217)
					(mid 168.285812 73.384127)
					(end 165.100501 72.062761)
				)
				(arc
					(start 133.100351 72.062751)
					(mid 129.918413 73.380772)
					(end 128.600511 76.562759)
				)
				(xy 128.60047 92.922729)
			)
		)
	)
	(embedded_fonts no)
)
