(kicad_pcb (version 4) (host pcbnew 4.0.1-3.201512221402+6198~38~ubuntu14.04.1-stable)
  (general
    (links 90)
    (no_connects 9)
    (area 104.572999 64.756001 178.510001 126.00138)
    (thickness 1.6)
    (drawings 84)
    (tracks 463)
    (zones 0)
    (modules 121)
    (nets 71)
  )
  (page A4)
  (title_block
    (title "Protoboard DIP for C.H.I.P. Computer")
    (date 2016-05-07)
    (rev v1.0)
    (company "This design uses a KiCad DIP template created by Jenner for Wickerlib")
    (comment 1 "Released under the CERN Open Hardware License v1.2")
    (comment 2 "wickerboxen@gmail.com - http://wickerbox.net/ ")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3302)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.27)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.254)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 0.6858 0.3302)
    (user_via 0.762 0.4064)
    (user_via 0.8636 0.508)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 120.65 121.92)
    (grid_origin 115.57 121.92)
    (visible_elements FFFEDF7D)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3.3V)
  (net 4 VCHG)
  (net 5 /TS)
  (net 6 +1.8V)
  (net 7 VBAT)
  (net 8 /TWI1-SDA)
  (net 9 /PWRON)
  (net 10 /TWI1-SCK)
  (net 11 /X1)
  (net 12 /X2)
  (net 13 /Y1)
  (net 14 /Y2)
  (net 15 /LCD-D2)
  (net 16 /PWM0)
  (net 17 /LCD-D4)
  (net 18 /LCD-D3)
  (net 19 /LCD-D6)
  (net 20 /LCD-D5)
  (net 21 /LCD-D10)
  (net 22 /LCD-D7)
  (net 23 /LCD-D12)
  (net 24 /LCD-D11)
  (net 25 /LCD-D14)
  (net 26 /LCD-D13)
  (net 27 /LCD-D18)
  (net 28 /LCD-D15)
  (net 29 /LCD-D20)
  (net 30 /LCD-D19)
  (net 31 /LCD-D22)
  (net 32 /LCD-D21)
  (net 33 /LCD-CLK)
  (net 34 /LCD-D23)
  (net 35 /LCD-VSYNC)
  (net 36 /LCD-HSYNC)
  (net 37 /LCD-DE)
  (net 38 /UART1-TX)
  (net 39 /HPL)
  (net 40 /UART1-RX)
  (net 41 /HPCOM)
  (net 42 /FEL)
  (net 43 /HPR)
  (net 44 /MICM)
  (net 45 /LRADC)
  (net 46 /MICIN1)
  (net 47 /XIO-P0)
  (net 48 /XIO-P1)
  (net 49 /XIO-P2)
  (net 50 /XIO-P3)
  (net 51 /XIO-P4)
  (net 52 /XIO-P5)
  (net 53 /XIO-P6)
  (net 54 /XIO-P7)
  (net 55 /AP-EINT1)
  (net 56 /AP-EINT3)
  (net 57 /TWI2-SDA)
  (net 58 /TWI2-SCK)
  (net 59 /CSIPCK)
  (net 60 /CSICK)
  (net 61 /CSIHSYNC)
  (net 62 /CSIVSYNC)
  (net 63 /CSID0)
  (net 64 /CSID1)
  (net 65 /CSID2)
  (net 66 /CSID3)
  (net 67 /CSID4)
  (net 68 /CSID5)
  (net 69 /CSID6)
  (net 70 /CSID7)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +1.8V)
    (add_net +3.3V)
    (add_net +5V)
    (add_net /AP-EINT1)
    (add_net /AP-EINT3)
    (add_net /CSICK)
    (add_net /CSID0)
    (add_net /CSID1)
    (add_net /CSID2)
    (add_net /CSID3)
    (add_net /CSID4)
    (add_net /CSID5)
    (add_net /CSID6)
    (add_net /CSID7)
    (add_net /CSIHSYNC)
    (add_net /CSIPCK)
    (add_net /CSIVSYNC)
    (add_net /FEL)
    (add_net /HPCOM)
    (add_net /HPL)
    (add_net /HPR)
    (add_net /LCD-CLK)
    (add_net /LCD-D10)
    (add_net /LCD-D11)
    (add_net /LCD-D12)
    (add_net /LCD-D13)
    (add_net /LCD-D14)
    (add_net /LCD-D15)
    (add_net /LCD-D18)
    (add_net /LCD-D19)
    (add_net /LCD-D2)
    (add_net /LCD-D20)
    (add_net /LCD-D21)
    (add_net /LCD-D22)
    (add_net /LCD-D23)
    (add_net /LCD-D3)
    (add_net /LCD-D4)
    (add_net /LCD-D5)
    (add_net /LCD-D6)
    (add_net /LCD-D7)
    (add_net /LCD-DE)
    (add_net /LCD-HSYNC)
    (add_net /LCD-VSYNC)
    (add_net /LRADC)
    (add_net /MICIN1)
    (add_net /MICM)
    (add_net /PWM0)
    (add_net /PWRON)
    (add_net /TS)
    (add_net /TWI1-SCK)
    (add_net /TWI1-SDA)
    (add_net /TWI2-SCK)
    (add_net /TWI2-SDA)
    (add_net /UART1-RX)
    (add_net /UART1-TX)
    (add_net /X1)
    (add_net /X2)
    (add_net /XIO-P0)
    (add_net /XIO-P1)
    (add_net /XIO-P2)
    (add_net /XIO-P3)
    (add_net /XIO-P4)
    (add_net /XIO-P5)
    (add_net /XIO-P6)
    (add_net /XIO-P7)
    (add_net /Y1)
    (add_net /Y2)
    (add_net GND)
    (add_net VBAT)
    (add_net VCHG)
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 81.28)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V65 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 78.74)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V64 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 83.82)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V66 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 91.44)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V69 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 93.98)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V610 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 99.06)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V612 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 96.52)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V611 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 86.36)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V67 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 88.9)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V68 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 111.76)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V617 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 109.22)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V616 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 101.6)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V613 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 104.14)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V614 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 114.3)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V618 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 116.84)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V619 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 144.018 106.68)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V615 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 116.84)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V519 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 114.3)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V518 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 116.84)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V619 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 114.3)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V618 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 116.84)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V819 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 116.84)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V719 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 116.84)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V419 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 116.84)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V319 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 114.3)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V818 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 114.3)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V718 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 114.3)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V418 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 114.3)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V318 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 111.76)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V817 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 111.76)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V717 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 111.76)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V617 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 111.76)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V517 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 111.76)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V417 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 111.76)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V317 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 109.22)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V816 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 109.22)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V716 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 109.22)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V616 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 109.22)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V516 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 109.22)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V416 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 109.22)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V316 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 106.68)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V815 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 106.68)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V715 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 106.68)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V615 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 106.68)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V515 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 106.68)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V415 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 106.68)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V315 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 104.14)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V814 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 104.14)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V714 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 104.14)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V614 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 104.14)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V514 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 104.14)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V414 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 104.14)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V314 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 101.6)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V813 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 101.6)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V713 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 101.6)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V613 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 101.6)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V513 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 101.6)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V413 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 101.6)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V313 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 99.06)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V812 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 99.06)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V712 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 99.06)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V612 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 99.06)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V512 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 99.06)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V412 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 99.06)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V312 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 96.52)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V811 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 96.52)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V711 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 96.52)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V611 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 96.52)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V511 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 96.52)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V411 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 96.52)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V311 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 93.98)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V810 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 93.98)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V710 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 93.98)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V610 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 93.98)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V510 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 93.98)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V410 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 93.98)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V310 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 91.44)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V89 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 91.44)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V79 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 91.44)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V69 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 91.44)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V59 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 91.44)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V49 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 91.44)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V39 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 88.9)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V88 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 88.9)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V78 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 88.9)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V68 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 88.9)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V58 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 88.9)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V48 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 88.9)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V38 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 86.36)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V87 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 86.36)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V77 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 86.36)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V67 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 86.36)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V57 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 86.36)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V47 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 86.36)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V37 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 83.82)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V86 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 83.82)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V76 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 83.82)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V66 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 83.82)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V56 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 83.82)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V46 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 83.82)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V36 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 81.28)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V85 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 81.28)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V75 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 81.28)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V65 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 81.28)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V55 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 81.28)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V45 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 81.28)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V35 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 78.74)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V84 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 149.098 78.74)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V74 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 146.558 78.74)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V64 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 141.478 78.74)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V54 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 138.938 78.74)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V44 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 78.74)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V34 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 151.638 76.2)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V83 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:PINHOLE-40MIL (layer F.Cu) (tedit 572EAAC3)
    (at 136.398 76.2)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference V33 (at 0.508 -2.54) (layer F.SilkS) hide)
    (fp_text value PINHOLE-40MIL (at -2.1 2.88 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:DIP_Header_2x20 (layer F.Cu) (tedit 572EB04C)
    (at 124.968 71.12)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference J13 (at 0.508 -2.54) (layer B.SilkS) hide)
    (fp_text value DIP-HEADER-2x20 (at -3.048 5.588 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCHG))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3.3V))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /TS))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 +1.8V))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 VBAT))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /TWI1-SDA))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /PWRON))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /TWI1-SCK))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /X1))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /X2))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /Y1))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /Y2))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /LCD-D2))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /PWM0))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /LCD-D4))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LCD-D3))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /LCD-D6))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LCD-D5))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /LCD-D10))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LCD-D7))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /LCD-D12))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /LCD-D11))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /LCD-D14))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /LCD-D13))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /LCD-D18))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /LCD-D15))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /LCD-D20))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /LCD-D19))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /LCD-D22))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /LCD-D21))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /LCD-CLK))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /LCD-D23))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /LCD-VSYNC))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /LCD-HSYNC))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /LCD-DE))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:DIP_Header_2x20 (layer F.Cu) (tedit 572EB04F)
    (at 160.528 71.12)
    (descr "Standard 2x20 DIP header based on KiCad Pin Header 2x20")
    (tags "pin header")
    (fp_text reference J14 (at 2.032 -2.54) (layer B.SilkS) hide)
    (fp_text value DIP-HEADER-2x20 (at -3.048 5.588 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /UART1-TX))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /HPL))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /UART1-RX))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /HPCOM))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /FEL))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /HPR))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3.3V))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /MICM))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /LRADC))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /MICIN1))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /XIO-P0))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /XIO-P1))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /XIO-P2))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /XIO-P3))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /XIO-P4))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /XIO-P5))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /XIO-P6))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /XIO-P7))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /AP-EINT1))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /AP-EINT3))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 /TWI2-SDA))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 /TWI2-SCK))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /CSIPCK))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /CSICK))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /CSIHSYNC))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /CSIVSYNC))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /CSID0))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 /CSID1))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 /CSID2))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 /CSID3))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /CSID4))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /CSID5))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 /CSID6))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 /CSID7))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:Symbol_OSHW-Logo_SilkScreen (layer B.Cu) (tedit 572EAEC9)
    (at 144.018 73.66 180)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference REF** (at 0.09906 4.38912 180) (layer B.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 -6.56082 180) (layer B.Fab) hide)
  )
  (module CHIP-DIPs:Protoboard_Holes_1x20 (layer F.Cu) (tedit 5736BA2B)
    (at 155.448 71.12)
    (descr "Strip of protoboard holes")
    (tags "pin header")
    (fp_text reference DNP3 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value HOLES (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /UART1-TX))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /UART1-RX))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /FEL))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3.3V))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 /LRADC))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 /XIO-P0))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 /XIO-P2))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 /XIO-P4))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 /XIO-P6))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 /AP-EINT1))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 /TWI2-SDA))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 /CSIPCK))
    (pad 15 thru_hole circle (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 /CSIHSYNC))
    (pad 16 thru_hole circle (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 /CSID0))
    (pad 17 thru_hole circle (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 /CSID2))
    (pad 18 thru_hole circle (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 /CSID4))
    (pad 19 thru_hole circle (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 /CSID6))
    (pad 20 thru_hole circle (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x20.wrl
      (at (xyz 0 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:Protoboard_Holes_1x20 (layer F.Cu) (tedit 5736B366)
    (at 157.988 71.12)
    (descr "Strip of protoboard holes")
    (tags "pin header")
    (fp_text reference DNP4 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value HOLES (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /HPL))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /HPCOM))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 /HPR))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 /MICM))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 /MICIN1))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 /XIO-P1))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 /XIO-P3))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 /XIO-P5))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 /XIO-P7))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 /AP-EINT3))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 /TWI2-SCK))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 /CSICK))
    (pad 15 thru_hole circle (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 /CSIVSYNC))
    (pad 16 thru_hole circle (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 /CSID1))
    (pad 17 thru_hole circle (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 /CSID3))
    (pad 18 thru_hole circle (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 /CSID5))
    (pad 19 thru_hole circle (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 /CSID7))
    (pad 20 thru_hole circle (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x20.wrl
      (at (xyz 0 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:Protoboard_Holes_1x20 (layer F.Cu) (tedit 5736B366)
    (at 132.715 71.035001)
    (descr "Strip of protoboard holes")
    (tags "pin header")
    (fp_text reference DNP2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value HOLES (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 VCHG))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 /TS))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 VBAT))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /PWRON))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /X2))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 /Y2))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 /PWM0))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /LCD-D3))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /LCD-D5))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /LCD-D7))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /LCD-D11))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /LCD-D13))
    (pad 15 thru_hole circle (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 /LCD-D15))
    (pad 16 thru_hole circle (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 /LCD-D19))
    (pad 17 thru_hole circle (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 /LCD-D21))
    (pad 18 thru_hole circle (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 /LCD-D23))
    (pad 19 thru_hole circle (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 /LCD-HSYNC))
    (pad 20 thru_hole circle (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /LCD-DE))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x20.wrl
      (at (xyz 0 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module CHIP-DIPs:Protoboard_Holes_1x20 (layer F.Cu) (tedit 5736BA24)
    (at 130.175 71.035001)
    (descr "Strip of protoboard holes")
    (tags "pin header")
    (fp_text reference DNP1 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value HOLES (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 3 thru_hole circle (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3.3V))
    (pad 4 thru_hole circle (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 +1.8V))
    (pad 5 thru_hole circle (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /TWI1-SDA))
    (pad 6 thru_hole circle (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /TWI1-SCK))
    (pad 7 thru_hole circle (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /X1))
    (pad 8 thru_hole circle (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 /Y1))
    (pad 9 thru_hole circle (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 /LCD-D2))
    (pad 10 thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /LCD-D4))
    (pad 11 thru_hole circle (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /LCD-D6))
    (pad 12 thru_hole circle (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /LCD-D10))
    (pad 13 thru_hole circle (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /LCD-D12))
    (pad 14 thru_hole circle (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /LCD-D14))
    (pad 15 thru_hole circle (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /LCD-D18))
    (pad 16 thru_hole circle (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 /LCD-D20))
    (pad 17 thru_hole circle (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 /LCD-D22))
    (pad 18 thru_hole circle (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 /LCD-CLK))
    (pad 19 thru_hole circle (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 /LCD-VSYNC))
    (pad 20 thru_hole circle (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x20.wrl
      (at (xyz 0 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "Protoboard DIP\nfor C.H.I.P" (at 143.764 70.612) (layer F.SilkS))
  (gr_text "with love from OSH Park!" (at 144.018 67.564) (layer B.SilkS))
  (gr_line (start 123.698 65.405) (end 164.338 65.405) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.338 65.405) (end 164.338 120.65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.048 120.65) (end 164.338 120.65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.698 120.65) (end 130.048 120.65) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 123.698 65.405) (end 123.698 120.65) (layer Edge.Cuts) (width 0.15))
)
