(kicad_pcb (version 20171130) (host pcbnew "(5.1.7)-1")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 163)
    (zones 0)
    (modules 28)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 89.408 67.056)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND1)
  (net 2 "Net-(C1-Pad1)")
  (net 3 +3V3)
  (net 4 +5V)
  (net 5 /RXLED)
  (net 6 /TXLED)
  (net 7 "Net-(J1-Pad4)")
  (net 8 /TXD)
  (net 9 /RXD)
  (net 10 /D+)
  (net 11 /D-)
  (net 12 "Net-(D1-Pad2)")
  (net 13 "Net-(D2-Pad2)")
  (net 14 /VCCIO)
  (net 15 /Reset)
  (net 16 "Net-(TP8-Pad1)")
  (net 17 "Net-(TP9-Pad1)")
  (net 18 "Net-(TP10-Pad1)")
  (net 19 "Net-(TP11-Pad1)")
  (net 20 "Net-(D3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /D+)
    (add_net /D-)
    (add_net /RXD)
    (add_net /RXLED)
    (add_net /Reset)
    (add_net /TXD)
    (add_net /TXLED)
    (add_net /VCCIO)
    (add_net GND1)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(TP10-Pad1)")
    (add_net "Net-(TP11-Pad1)")
    (add_net "Net-(TP8-Pad1)")
    (add_net "Net-(TP9-Pad1)")
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 96.774 65.405)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP2 (at 0 2.921) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND1))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 105.918 50.165)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP12 (at 0 -3.556) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND1))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 96.774 50.165)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP11 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(TP11-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 99.822 50.165)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP10 (at 0 -3.683) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(TP10-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 108.966 65.405)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP9 (at 0 2.921) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(TP9-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 102.87 65.405)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP8 (at 0 2.921) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(TP8-Pad1)"))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 112.014 50.165)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP7 (at 0 -3.683) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 105.918 65.405)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 2.921) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 9 /RXD))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 99.822 65.405)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 2.921) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 8 /TXD))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 112.014 65.405)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 2.921) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 14 /VCCIO))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 108.966 50.165)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 15 /Reset))
  )
  (module TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 102.87 50.165)
    (descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
    (tags "test point THT pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 -2.413) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 2.05) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(D3-Pad1)"))
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 100.203 52.832 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0.635 -2.921) (layer F.SilkS))
    (fp_text value DIODESCH (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 106.553 52.578)
    (descr "SMT capacitor, 0402")
    (fp_text reference R5 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value R_US (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0.254 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 /Reset))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 113.03 59.055 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference R4 (at 0 0.889 90) (layer F.SilkS))
    (fp_text value R_US (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 113.03 56.896 90)
    (descr "SMT capacitor, 0402")
    (fp_text reference R3 (at 0 -0.9144 90) (layer F.SilkS))
    (fp_text value R_US (at 0 0.8128 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0 90) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at -0.55 0 90) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 107.696 53.721 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C4 (at 0 -1.016) (layer F.SilkS))
    (fp_text value C (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_USB:conn_usb_B_micro_smd (layer F.Cu) (tedit 5ECED1D6)
    (at 91.059 57.785 270)
    (descr "USB B micro SMD connector, Molex P/N 47346-0001")
    (fp_text reference J1 (at 0 2.60096 90) (layer F.SilkS) hide)
    (fp_text value USB_micro-B (at 0 -4.0005 90) (layer F.SilkS) hide)
    (pad 5 smd rect (at 1.30048 -2.65938 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 4 smd rect (at 0.65024 -2.65938 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 -2.65938 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 10 /D+))
    (pad 2 smd rect (at -0.65024 -2.65938 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 11 /D-))
    (pad 1 smd rect (at -1.30048 -2.65938 270) (size 0.44958 1.37922) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad "" smd rect (at -2.46126 -2.2987 270) (size 1.4732 2.10058) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 2.46126 -2.2987 270) (size 1.4732 2.10058) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.91338 0 270) (size 2.3749 1.89738) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 6 smd rect (at 2.91338 0 270) (size 2.3749 1.89738) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 6 smd rect (at 0.8382 0 270) (size 1.17348 1.89738) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 6 smd rect (at -0.8382 0 270) (size 1.17348 1.89738) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (model ${T_LIBS}/3d/t_USB/10118192-002lfc.stp
      (offset (xyz -98 3 -0.4))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Package_SO:SSOP-16_3.9x4.9mm_P0.635mm (layer F.Cu) (tedit 5A02F25C)
    (at 103.505 57.785 90)
    (descr "SSOP16: plastic shrink small outline package; 16 leads; body width 3.9 mm; lead pitch 0.635; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot519-1_po.pdf)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U1 (at -1.524 -3.81 180) (layer F.SilkS))
    (fp_text value FT230XS (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd rect (at 2.6 -2.2225 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(TP11-Pad1)"))
    (pad 15 smd rect (at 2.6 -1.5875 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(TP10-Pad1)"))
    (pad 14 smd rect (at 2.6 -0.9525 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /RXLED))
    (pad 13 smd rect (at 2.6 -0.3175 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 12 smd rect (at 2.6 0.3175 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 11 smd rect (at 2.6 0.9525 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 /Reset))
    (pad 10 smd rect (at 2.6 1.5875 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 9 smd rect (at 2.6 2.2225 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /D-))
    (pad 8 smd rect (at -2.6 2.2225 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /D+))
    (pad 7 smd rect (at -2.6 1.5875 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /TXLED))
    (pad 6 smd rect (at -2.6 0.9525 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(TP9-Pad1)"))
    (pad 5 smd rect (at -2.6 0.3175 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 4 smd rect (at -2.6 -0.3175 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /RXD))
    (pad 3 smd rect (at -2.6 -0.9525 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 /VCCIO))
    (pad 2 smd rect (at -2.6 -1.5875 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(TP8-Pad1)"))
    (pad 1 smd rect (at -2.6 -2.2225 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /TXD))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SSOP-16_3.9x4.9mm_P0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_ferrite_beads:fb_0603 (layer F.Cu) (tedit 0)
    (at 107.188 57.912 270)
    (descr "ferrite beads, 0603")
    (fp_text reference FB2 (at 0 -0.635 90) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 0.635 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at 0.75184 0 270) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 14 /VCCIO))
    (model ${T_LIBS}/3d/t_ferrite_beads/fb_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.54 2.54 2.54))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 96.012 55.245 180)
    (descr "SMT capacitor, 0402")
    (fp_text reference C1 (at 0 -1.016) (layer F.SilkS))
    (fp_text value C (at 0 0.8636) (layer F.SilkS) hide)
    (fp_text user %R (at 0.127 0) (layer F.Fab) hide)
    (pad 2 smd rect (at -0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 1 smd rect (at 0.55 0 180) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 105.283 63.5)
    (descr "SMT capacitor, 0402")
    (fp_text reference R2 (at 0 -0.9144) (layer F.SilkS))
    (fp_text value R_US (at 0 0.762) (layer F.SilkS) hide)
    (fp_text user %R (at 0.1905 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /VCCIO))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /RXD))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_LED:r_1206 (layer F.Cu) (tedit 0)
    (at 111.633 61.087 180)
    (descr "SMT resistor, 1206")
    (fp_text reference D2 (at 0 -1.397) (layer F.SilkS))
    (fp_text value LED (at 1.397 -1.397) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 6 /TXLED))
    (model ${LIBKICAD}/3d/smd_resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_LED:r_1206 (layer F.Cu) (tedit 0)
    (at 111.633 54.737 180)
    (descr "SMT resistor, 1206")
    (fp_text reference D1 (at 0.0254 1.27) (layer F.SilkS))
    (fp_text value LED (at 0 1.27) (layer F.SilkS) hide)
    (pad 2 smd rect (at -1.397 0 180) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at 1.397 0 180) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 5 /RXLED))
    (model ${LIBKICAD}/3d/smd_resistors/r_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 105.029 52.578 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C5 (at 1.397 0 180) (layer F.SilkS))
    (fp_text value C (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0.0635 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_ferrite_beads:fb_0603 (layer F.Cu) (tedit 0)
    (at 96.266 52.705)
    (descr "ferrite beads, 0603")
    (fp_text reference FB1 (at 0 -0.635) (layer F.SilkS))
    (fp_text value Ferrite_Bead (at 0 0.635) (layer F.SilkS) hide)
    (pad 2 smd rect (at -0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at 0.75184 0) (size 0.89916 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ${T_LIBS}/3d/t_ferrite_beads/fb_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 2.54 2.54 2.54))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:cap_0402 (layer F.Cu) (tedit 5BB76BB0)
    (at 103.886 52.578 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C6 (at 0 0.762 90) (layer F.SilkS))
    (fp_text value C (at 0 0.8636 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at -0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND1))
    (pad 1 smd rect (at 0.55 0 270) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (model ${T_LIBS}/3d/t_passive_smd/cap_0402.stp
      (offset (xyz 0 0 0.04999999924907534))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module t_passive_smd:res_0402 (layer F.Cu) (tedit 5BB76B2F)
    (at 101.981 62.738)
    (descr "SMT capacitor, 0402")
    (fp_text reference R1 (at 0.381 -0.889) (layer F.SilkS))
    (fp_text value R_US (at 0 0.8128) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at 0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /VCCIO))
    (pad 2 smd rect (at -0.55 0) (size 0.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /TXD))
    (model ${T_LIBS}/3d/t_passive_smd/res_0402.stp
      (offset (xyz 0 0 0.02999999954944519))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 89.408 67.056) (end 89.408 48.514) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.808 67.056) (end 89.408 67.056) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.808 48.514) (end 114.808 67.056) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.408 48.514) (end 114.808 48.514) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.173 66.421) (xy 90.043 66.421) (xy 90.043 49.149) (xy 114.173 49.149)
      )
    )
  )
  (zone (net 1) (net_name GND1) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.173 66.421) (xy 90.043 66.421) (xy 90.043 49.149) (xy 114.173 49.149)
      )
    )
  )
)
