(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 1028)
    (zones 0)
    (modules 62)
    (nets 63)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.7)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VIN)
  (net 3 3.3V)
  (net 4 USB_OUT+)
  (net 5 USB_OUT-)
  (net 6 5V_BOOST)
  (net 7 SDA)
  (net 8 SCL)
  (net 9 CS)
  (net 10 MISO)
  (net 11 MOSI)
  (net 12 SCLK)
  (net 13 "Net-(C6-Pad1)")
  (net 14 "Net-(C7-Pad2)")
  (net 15 "Net-(C7-Pad1)")
  (net 16 "/Power Subsystems/SYS")
  (net 17 "/USB Interfaces/DTR")
  (net 18 USB_RX)
  (net 19 USB_TX)
  (net 20 "/USB Interfaces/RTS")
  (net 21 VBAT)
  (net 22 "/USB Interfaces/TX")
  (net 23 "/USB Interfaces/RX")
  (net 24 ~RESET)
  (net 25 NET_POW)
  (net 26 "Net-(C19-Pad1)")
  (net 27 "Net-(C20-Pad1)")
  (net 28 AREF)
  (net 29 A1)
  (net 30 A0)
  (net 31 ETH_RX-)
  (net 32 ETH_RX+)
  (net 33 ETH_TX-)
  (net 34 ETH_TX+)
  (net 35 GPIO15)
  (net 36 GPIO38)
  (net 37 GPIO18)
  (net 38 GPIO19)
  (net 39 GPIO17)
  (net 40 GPIO16)
  (net 41 FEATHER_TX)
  (net 42 FEATHER_RX)
  (net 43 GPIO3)
  (net 44 GPIO2)
  (net 45 GPIO1)
  (net 46 GPIO0)
  (net 47 "Net-(J4-Pad3)")
  (net 48 "Net-(J4-Pad2)")
  (net 49 GPIO11)
  (net 50 "/Power Subsystems/DSEL")
  (net 51 "/Power Subsystems/~QON")
  (net 52 "/Power Subsystems/TS")
  (net 53 "/Power Subsystems/ILIM")
  (net 54 "/Power Subsystems/~CE")
  (net 55 "/Power Subsystems/OTG")
  (net 56 "/Power Subsystems/INT")
  (net 57 "/Power Subsystems/STAT")
  (net 58 "/Power Subsystems/ID")
  (net 59 USB_IN+)
  (net 60 USB_IN-)
  (net 61 "Net-(R7-Pad1)")
  (net 62 "Net-(R8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "/Power Subsystems/DSEL")
    (add_net "/Power Subsystems/ID")
    (add_net "/Power Subsystems/ILIM")
    (add_net "/Power Subsystems/INT")
    (add_net "/Power Subsystems/OTG")
    (add_net "/Power Subsystems/STAT")
    (add_net "/Power Subsystems/SYS")
    (add_net "/Power Subsystems/TS")
    (add_net "/Power Subsystems/~CE")
    (add_net "/Power Subsystems/~QON")
    (add_net "/USB Interfaces/DTR")
    (add_net "/USB Interfaces/RTS")
    (add_net "/USB Interfaces/RX")
    (add_net "/USB Interfaces/TX")
    (add_net 3.3V)
    (add_net 5V_BOOST)
    (add_net A0)
    (add_net A1)
    (add_net AREF)
    (add_net CS)
    (add_net ETH_RX+)
    (add_net ETH_RX-)
    (add_net ETH_TX+)
    (add_net ETH_TX-)
    (add_net FEATHER_RX)
    (add_net FEATHER_TX)
    (add_net GND)
    (add_net GPIO0)
    (add_net GPIO1)
    (add_net GPIO11)
    (add_net GPIO15)
    (add_net GPIO16)
    (add_net GPIO17)
    (add_net GPIO18)
    (add_net GPIO19)
    (add_net GPIO2)
    (add_net GPIO3)
    (add_net GPIO38)
    (add_net MISO)
    (add_net MOSI)
    (add_net NET_POW)
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net SCL)
    (add_net SCLK)
    (add_net SDA)
    (add_net USB_IN+)
    (add_net USB_IN-)
    (add_net USB_OUT+)
    (add_net USB_OUT-)
    (add_net USB_RX)
    (add_net USB_TX)
    (add_net VBAT)
    (add_net VIN)
    (add_net ~RESET)
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 135.255 103.505 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 131.38 70.35)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 1.648) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 20 "/USB Interfaces/RTS"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 125.07 66.09)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 1.648) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 17 "/USB Interfaces/DTR"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 154.425 105.2)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at -0.325 -1.925) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 22 "/USB Interfaces/TX"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 157.1 105.2)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 -1.875) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0.025 -1.9) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "/USB Interfaces/RX"))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5C745284)
    (at 157.125 108.725 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at -0.025 -2.675 180) (layer B.SilkS))
    (fp_text value Jumper_NC_Small (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 23 "/USB Interfaces/RX") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 18 USB_RX) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm (layer B.Cu) (tedit 5C745284)
    (at 154.55 108.725 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at -0.025 2.55 180) (layer B.SilkS))
    (fp_text value Jumper_NC_Small (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 22 "/USB Interfaces/TX") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy 0.5 0.75) (xy 0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers B.Cu B.Mask)
      (net 19 USB_TX) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_poly (pts
           (xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)) (width 0))
      ))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.6 77.45 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 0.55 2.3 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.9 78.35 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at 0.5 -1.45) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_Coilcraft_XAL5030 (layer F.Cu) (tedit 5990349C)
    (at 147.18 71.58 270)
    (descr L_Coilcraft_XAL5030)
    (tags "L Coilcraft XAL5030")
    (attr smd)
    (fp_text reference L1 (at -3.63 -1.69 180) (layer F.SilkS))
    (fp_text value 2.2u (at 0 4.572 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.655 0 270) (size 1.2 4.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "/Power Subsystems/SYS"))
    (pad 1 smd rect (at -1.655 0 270) (size 1.2 4.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_Wuerth_MAPI-4030.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1.25 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 142.9 65.4)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 3.3 0) (layer F.SilkS))
    (fp_text value D_Schottky (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 3.3 0) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C7-Pad1)"))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 5V_BOOST))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 141.4 77.7)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at -3.2 -0.2 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 VBAT))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 145.2 76.4)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0.6 -1.4 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "/Power Subsystems/SYS"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 152.24 79.47)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at -0.04 1.53 180) (layer F.SilkS))
    (fp_text value 47u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 5V_BOOST))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 141.4 79.7)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at -3.1 -0.1) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 VBAT))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 143.135 72.52 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 2.48 -0.365 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "/Power Subsystems/SYS"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 138.6 64.9)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at -3.09 0.2) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 5V_BOOST))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.13 66.65)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -2.475 -0.15) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 5V_BOOST))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.13 68.25)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -2.4 -0.17 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 5V_BOOST))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 142.685 68.17 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -2.535 0.26 180) (layer F.SilkS))
    (fp_text value 47n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C7-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 139.8 68.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.3 -0.2 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 129.94 80.18)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 0.26 -1.48) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 133.45 70.94 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -2.3 -0.025 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 135.52 70.9 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.35 0.075 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_S-PWQFN-N24_EP2.7x2.7mm_ThermalVias (layer F.Cu) (tedit 5C5DC2E8)
    (at 139.31 73.445)
    (descr "QFN, 24 Pin (http://www.ti.com/lit/ds/symlink/bq25601.pdf#page=54), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (attr smd)
    (fp_text reference U4 (at -1.5 -3.215) (layer F.SilkS))
    (fp_text value BQ25895RTW (at 0 3.32) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 24 smd roundrect (at -1.25 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "/Power Subsystems/DSEL"))
    (pad 23 smd roundrect (at -0.75 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 5V_BOOST))
    (pad 22 smd roundrect (at -0.25 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(C6-Pad1)"))
    (pad 21 smd roundrect (at 0.25 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(C7-Pad2)"))
    (pad 20 smd roundrect (at 0.75 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C7-Pad1)"))
    (pad 19 smd roundrect (at 1.25 -1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(C7-Pad1)"))
    (pad 18 smd roundrect (at 1.9625 -1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 17 smd roundrect (at 1.9625 -0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 16 smd roundrect (at 1.9625 -0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "/Power Subsystems/SYS"))
    (pad 15 smd roundrect (at 1.9625 0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "/Power Subsystems/SYS"))
    (pad 14 smd roundrect (at 1.9625 0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 VBAT))
    (pad 13 smd roundrect (at 1.9625 1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 VBAT))
    (pad 12 smd roundrect (at 1.25 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "/Power Subsystems/~QON"))
    (pad 11 smd roundrect (at 0.75 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "/Power Subsystems/TS"))
    (pad 10 smd roundrect (at 0.25 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "/Power Subsystems/ILIM"))
    (pad 9 smd roundrect (at -0.25 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 "/Power Subsystems/~CE"))
    (pad 8 smd roundrect (at -0.75 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "/Power Subsystems/OTG"))
    (pad 7 smd roundrect (at -1.25 1.9625) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "/Power Subsystems/INT"))
    (pad 6 smd roundrect (at -1.9625 1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 SDA))
    (pad 5 smd roundrect (at -1.9625 0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 SCL))
    (pad 4 smd roundrect (at -1.9625 0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "/Power Subsystems/STAT"))
    (pad 3 smd roundrect (at -1.9625 -0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 USB_IN-))
    (pad 2 smd roundrect (at -1.9625 -0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 USB_IN+))
    (pad 1 smd roundrect (at -1.9625 -1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VIN))
    (pad "" smd roundrect (at 0.675 0.675) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at 0.675 -0.675) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.675 0.675) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad "" smd roundrect (at -0.675 -0.675) (size 1.13 1.13) (layers F.Paste) (roundrect_rratio 0.221239))
    (pad 25 smd roundrect (at 0 0) (size 2.7 2.7) (layers B.Cu) (roundrect_rratio 0.09259299999999999)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.1 1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.1 1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.1 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.1 0) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 1.1 -1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at 0 -1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 thru_hole circle (at -1.1 -1.1) (size 0.5 0.5) (drill 0.2) (layers *.Cu)
      (net 1 GND))
    (pad 25 smd roundrect (at 0 0) (size 2.7 2.7) (layers F.Cu F.Mask) (roundrect_rratio 0.09259299999999999)
      (net 1 GND))
    (model ${KIPRJMOD}/3dmodels/BQ25895RTWR.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5A02FF57)
    (at 148.29 98.758 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 1.555 4.49 180) (layer F.SilkS))
    (fp_text value AP1117-33 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 157.9 95.5 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.14 0.15 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 3.3V))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 159.6 95.5 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.15 -0.16 180) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0.02 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 3.3V))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_SM06B-SRSS-TB_1x06-1MP_P1.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 164.2745 103.5685 90)
    (descr "JST SH series connector, SM06B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J2 (at 3.3685 -4.3745 180) (layer F.SilkS))
    (fp_text value CON_HEADER_PRG_AVR_ICSP-PTH (at 0 3.98 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad MP smd roundrect (at 3.8 1.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at -3.8 1.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad 6 smd roundrect (at 2.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 1.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 CS))
    (pad 4 smd roundrect (at 0.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 MOSI))
    (pad 3 smd roundrect (at -0.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 SCLK))
    (pad 2 smd roundrect (at -1.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 3.3V))
    (pad 1 smd roundrect (at -2.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 MISO))
    (model ${KIPRJMOD}/3dmodels/SM06B-SRSS-TB.STEP
      (offset (xyz 0 1.5 -0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-SM4-TB_1x02-1MP_P2.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 127.1905 65.913 180)
    (descr "JST PH series connector, S2B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (attr smd)
    (fp_text reference J3 (at -5.4895 1.843) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 5.8) (layer F.Fab))
    (fp_text user %R (at 0 1.5) (layer F.Fab))
    (pad MP smd roundrect (at 3.35 2.9 180) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad MP smd roundrect (at -3.35 2.9 180) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.166667))
    (pad 2 smd roundrect (at 1 -2.85 180) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 VBAT))
    (pad 1 smd roundrect (at -1 -2.85 180) (size 1 3.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/3dmodels/S2B-PH-SM4-TB.stp
      (offset (xyz 0 -4.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Connector_USB:USB_Micro-AB_Molex_47590-0001 (layer F.Cu) (tedit 5DAEB89E)
    (at 118.3005 72.39 270)
    (descr "Micro USB AB receptable, right-angle inverted (https://www.molex.com/pdm_docs/sd/475900001_sd.pdf)")
    (tags "Micro AB USB SMD")
    (attr smd)
    (fp_text reference USB1 (at -5.715 -1.7145) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 3.5 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 1.45 90) (layer Dwgs.User))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (fp_line (start -3.75 1.45) (end -2.8 1.45) (layer Edge.Cuts) (width 0.1))
    (fp_line (start -2.8 -0.125) (end -2.8 1.45) (layer Edge.Cuts) (width 0.1))
    (fp_line (start -1.95 -0.125) (end -1.95 1.45) (layer Edge.Cuts) (width 0.1))
    (fp_line (start -1.95 1.45) (end 1.95 1.45) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.95 -0.125) (end 1.95 1.45) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.8 -0.125) (end 2.8 1.45) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 2.8 1.45) (end 3.75 1.45) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start -2.375 -0.125) (end -2.8 -0.125) (angle 180) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 2.375 -0.125) (end 1.95 -0.125) (angle 180) (layer Edge.Cuts) (width 0.1))
    (pad "" smd rect (at -3.5 0 270) (size 0.3 0.85) (layers F.Paste))
    (pad "" smd rect (at 3.5 0 270) (size 0.3 0.85) (layers F.Paste))
    (pad 6 smd rect (at -3.7375 0 270) (size 0.875 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 3.7375 0 270) (size 0.875 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 0 0 270) (size 2.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 60 USB_IN-))
    (pad 6 thru_hole oval (at 4.175 0 270) (size 1 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -4.175 0 270) (size 1 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.225 -3 270) (size 1.05 1.25) (drill oval 0.65 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 3 smd rect (at 0 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 59 USB_IN+))
    (pad 4 smd rect (at -0.65 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 58 "/Power Subsystems/ID"))
    (pad 5 smd rect (at -1.3 -2.675 270) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -2.225 -3 270) (size 1.05 1.25) (drill oval 0.65 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/3dmodels/47589-0001.stp
      (offset (xyz 0 11.5 2))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (module footprints:67643-0910 (layer F.Cu) (tedit 0)
    (at 170.18 79.629 90)
    (descr 67643-0910)
    (tags Connector)
    (fp_text reference J4 (at -1.146 -7.53 180) (layer F.SilkS))
    (fp_text value USB_A (at 7.2345 -11.976 90) (layer F.SilkS) hide)
    (fp_text user %R (at 7.2345 -11.976 90) (layer F.Fab))
    (pad 6 thru_hole circle (at 13.77 -10.28 90) (size 3.58 3.58) (drill 2.38) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0.63 -10.28 90) (size 3.58 3.58) (drill 2.38) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 10.7 -12.99 90) (size 1.58 1.58) (drill 1.03) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 8.2 -12.99 90) (size 1.58 1.58) (drill 1.03) (layers *.Cu *.Mask)
      (net 47 "Net-(J4-Pad3)"))
    (pad 2 thru_hole circle (at 6.2 -12.99 90) (size 1.58 1.58) (drill 1.03) (layers *.Cu *.Mask)
      (net 48 "Net-(J4-Pad2)"))
    (pad 1 thru_hole circle (at 3.7 -12.99 90) (size 1.58 1.58) (drill 1.03) (layers *.Cu *.Mask)
      (net 6 5V_BOOST))
    (model ${KIPRJMOD}/3dmodels/67643-0910.stp
      (offset (xyz 7 15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm (layer F.Cu) (tedit 5C1FD453)
    (at 128.3 74.75)
    (descr "QFN, 24 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=278), generated with kicad-footprint-generator ipc_dfn_qfn_generator.py")
    (tags "QFN DFN_QFN")
    (attr smd)
    (fp_text reference U3 (at -2.5 -2.775) (layer F.SilkS))
    (fp_text value CP2102N-A01-GQFN24 (at 0 3.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 24 smd roundrect (at -1.25 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 23 smd roundrect (at -0.75 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "/USB Interfaces/DTR"))
    (pad 22 smd roundrect (at -0.25 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 21 smd roundrect (at 0.25 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "/USB Interfaces/RX"))
    (pad 20 smd roundrect (at 0.75 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 "/USB Interfaces/TX"))
    (pad 19 smd roundrect (at 1.25 -1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "/USB Interfaces/RTS"))
    (pad 18 smd roundrect (at 1.9375 -1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 17 smd roundrect (at 1.9375 -0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 16 smd roundrect (at 1.9375 -0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 15 smd roundrect (at 1.9375 0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 14 smd roundrect (at 1.9375 0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at 1.9375 1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at 1.25 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 0.75 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 0.25 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at -0.25 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -0.75 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VIN))
    (pad 7 smd roundrect (at -1.25 1.9375) (size 0.25 0.825) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VIN))
    (pad 6 smd roundrect (at -1.9375 1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 3.3V))
    (pad 5 smd roundrect (at -1.9375 0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 3.3V))
    (pad 4 smd roundrect (at -1.9375 0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 60 USB_IN-))
    (pad 3 smd roundrect (at -1.9375 -0.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 USB_IN+))
    (pad 2 smd roundrect (at -1.9375 -0.75) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.9375 -1.25) (size 0.825 0.25) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.65 0.65) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 -0.65) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 0.65) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 -0.65) (size 1.05 1.05) (layers F.Paste) (roundrect_rratio 0.238095))
    (pad 25 smd roundrect (at 0 0) (size 2.6 2.6) (layers F.Cu F.Mask) (roundrect_rratio 0.096154)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 146.878 104.524)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.029 1.736) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 150.585 104.524 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10u (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VIN))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal (layer F.Cu) (tedit 5B78AD87)
    (at 164.2745 93.472 90)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J5 (at 3.072 -2.7745 180) (layer F.SilkS))
    (fp_text value M04PTH (at 0 3.98 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad MP smd roundrect (at 2.8 1.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at -2.8 1.875 90) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad 4 smd roundrect (at 1.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 SCL))
    (pad 3 smd roundrect (at 0.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 SDA))
    (pad 2 smd roundrect (at -0.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 3.3V))
    (pad 1 smd roundrect (at -1.5 -2 90) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/3dmodels/SM04B-SRSS-TB.STEP
      (offset (xyz 0 1.5 -0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module footprints:HANRUN_HR911105A (layer F.Cu) (tedit 5E634A7E)
    (at 115.57 99.06 90)
    (fp_text reference J1 (at 10.554 8.939 180) (layer F.SilkS))
    (fp_text value HR911105A (at 8.02765 12.354385 90) (layer F.Fab))
    (pad None np_thru_hole circle (at 5.715 0 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad None np_thru_hole circle (at -5.715 0 90) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -7.745 3.05 90) (size 2.445 2.445) (drill 1.63) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole circle (at 7.745 3.05 90) (size 2.445 2.445) (drill 1.63) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 11 thru_hole circle (at -4.085 -4.9 90) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 12 thru_hole circle (at -6.625 -4.9 90) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 10 thru_hole circle (at 4.085 -4.9 90) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 9 thru_hole circle (at 6.625 -4.9 90) (size 1.53 1.53) (drill 1.02) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at -4.44 8.89 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.17 6.35 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -1.9 8.89 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 31 ETH_RX-))
    (pad 5 thru_hole circle (at -0.63 6.35 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 25 NET_POW))
    (pad 4 thru_hole circle (at 0.64 8.89 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 25 NET_POW))
    (pad 3 thru_hole circle (at 1.91 6.35 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 32 ETH_RX+))
    (pad 2 thru_hole circle (at 3.18 8.89 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 33 ETH_TX-))
    (pad 1 thru_hole rect (at 4.45 6.35 90) (size 1.398 1.398) (drill 0.89) (layers *.Cu *.Mask)
      (net 34 ETH_TX+))
    (model ${KIPRJMOD}/3dmodels/RJ45_Hanrun_HR911105A.wrl
      (offset (xyz 4.5 -6.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Module:Onion_Omega2+ locked (layer F.Cu) (tedit 5C6359D3)
    (at 165.1 87.63 270)
    (descr https://onion.io/omega2/)
    (tags "Omega Onion module")
    (fp_text reference U1 (at -1.927 -1.348 180) (layer F.SilkS))
    (fp_text value ONION-OMEGA2 (at 12.2 36.6 90) (layer F.Fab))
    (fp_text user "SD CARD" (at 11.6 42.3 90) (layer Cmts.User))
    (fp_text user %R (at -1.93 -1.4 180) (layer F.Fab))
    (pad 32 thru_hole circle (at 24.4 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole circle (at 24.4 2 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 3.3V))
    (pad 30 thru_hole circle (at 24.4 4 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 USB_OUT+))
    (pad 29 thru_hole circle (at 24.4 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 USB_OUT-))
    (pad 28 thru_hole circle (at 24.4 8 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 USB_RX))
    (pad 27 thru_hole circle (at 24.4 10 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 USB_TX))
    (pad 26 thru_hole circle (at 24.4 12 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 36 GPIO38))
    (pad 25 thru_hole circle (at 24.4 14 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 NET_POW))
    (pad 24 thru_hole circle (at 24.4 16 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 33 ETH_TX-))
    (pad 23 thru_hole circle (at 24.4 18 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 ETH_TX+))
    (pad 22 thru_hole circle (at 24.4 20 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 ETH_RX-))
    (pad 21 thru_hole circle (at 24.4 22 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 32 ETH_RX+))
    (pad 20 thru_hole circle (at 24.4 24 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 GPIO18))
    (pad 19 thru_hole circle (at 24.4 26 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 38 GPIO19))
    (pad 18 thru_hole circle (at 24.4 28 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 SCL))
    (pad 17 thru_hole circle (at 24.4 30 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 SDA))
    (pad 16 thru_hole circle (at 0 30 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 ~RESET))
    (pad 15 thru_hole circle (at 0 28 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 46 GPIO0))
    (pad 14 thru_hole circle (at 0 26 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 45 GPIO1))
    (pad 13 thru_hole circle (at 0 24 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 CS))
    (pad 12 thru_hole circle (at 0 22 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 SCLK))
    (pad 11 thru_hole circle (at 0 20 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 11 MOSI))
    (pad 10 thru_hole circle (at 0 18 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 MISO))
    (pad 9 thru_hole circle (at 0 16 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 FEATHER_TX))
    (pad 8 thru_hole circle (at 0 14 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 FEATHER_RX))
    (pad 7 thru_hole circle (at 0 12 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 35 GPIO15))
    (pad 6 thru_hole circle (at 0 10 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 40 GPIO16))
    (pad 5 thru_hole circle (at 0 8 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 39 GPIO17))
    (pad 4 thru_hole circle (at 0 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 GPIO2))
    (pad 3 thru_hole circle (at 0 4 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 GPIO3))
    (pad 2 thru_hole circle (at 0 2 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 49 GPIO11))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Module.3dshapes/Onion_Omega2+.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:adafruit_featherwing (layer F.Cu) (tedit 59467C6D)
    (at 116.84 83.82)
    (attr virtual)
    (fp_text reference MS1 (at 2.51 1.38) (layer F.SilkS) hide)
    (fp_text value ADAFRUIT_FEATHERWING (at 26.4795 -17.272) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 48.26 -2.54) (size 2.49936 2.49936) (drill 2.49936) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 48.26 -20.32) (size 2.49936 2.49936) (drill 2.49936) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 2.54 -2.54) (size 3.81 3.81) (drill 2.49936) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad "" thru_hole circle (at 2.54 -20.32) (size 3.81 3.81) (drill 2.49936) (layers *.Cu *.Mask)
      (zone_connect 0))
    (pad 28 thru_hole circle (at 16.51 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 21 VBAT))
    (pad 27 thru_hole circle (at 19.05 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 35 GPIO15))
    (pad 26 thru_hole circle (at 21.59 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 2 VIN))
    (pad 25 thru_hole circle (at 24.13 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 36 GPIO38))
    (pad 24 thru_hole circle (at 26.67 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 37 GPIO18))
    (pad 23 thru_hole circle (at 29.21 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 38 GPIO19))
    (pad 22 thru_hole circle (at 31.75 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 9 CS))
    (pad 21 thru_hole circle (at 34.29 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 39 GPIO17))
    (pad 20 thru_hole circle (at 36.83 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 40 GPIO16))
    (pad 19 thru_hole circle (at 39.37 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 49 GPIO11))
    (pad 18 thru_hole circle (at 41.91 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 8 SCL))
    (pad 17 thru_hole circle (at 44.45 -21.59) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 7 SDA))
    (pad 16 thru_hole circle (at 44.45 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask))
    (pad 15 thru_hole circle (at 41.91 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 41 FEATHER_TX))
    (pad 14 thru_hole circle (at 39.37 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 42 FEATHER_RX))
    (pad 13 thru_hole circle (at 36.83 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 10 MISO))
    (pad 12 thru_hole circle (at 34.29 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 11 MOSI))
    (pad 11 thru_hole circle (at 31.75 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 12 SCLK))
    (pad 10 thru_hole circle (at 29.21 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 29 A1))
    (pad 9 thru_hole circle (at 26.67 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 30 A0))
    (pad 8 thru_hole circle (at 24.13 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 43 GPIO3))
    (pad 7 thru_hole circle (at 21.59 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 44 GPIO2))
    (pad 6 thru_hole circle (at 19.05 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 45 GPIO1))
    (pad 5 thru_hole circle (at 16.51 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 46 GPIO0))
    (pad 4 thru_hole circle (at 13.97 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 11.43 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 28 AREF))
    (pad 2 thru_hole circle (at 8.89 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 3 3.3V))
    (pad 1 thru_hole circle (at 6.35 -1.27) (size 1.778 1.778) (drill 0.99822) (layers *.Cu *.Mask)
      (net 24 ~RESET))
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 151 108.6 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C18 (at -0.8 -2.3 180) (layer F.SilkS))
    (fp_text value 1u (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 NET_POW))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 134.9 101.6 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C19 (at 2.2 0.8 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 135.1 106.6 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C20 (at -2.46 -0.7 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(C20-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 141.052 92.905 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C21 (at 2.095 -0.548 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOP65P490X110-8N (layer F.Cu) (tedit 5B226F0B)
    (at 136.6 93.8)
    (attr smd)
    (fp_text reference IC1 (at -1.6 -2.3) (layer F.SilkS))
    (fp_text value MAX11646EUA+T (at -0.226147 2.1966) (layer B.Adhes) hide)
    (pad 8 smd rect (at 2.805 -0.975 180) (size 1.2 0.49) (layers F.Cu F.Paste F.Mask)
      (net 3 3.3V))
    (pad 7 smd rect (at 2.805 -0.325 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.805 0.325 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 SDA))
    (pad 5 smd rect (at 2.805 0.975 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
    (pad 4 smd rect (at -2.9 0.975 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 AREF))
    (pad 3 smd rect (at -2.9 0.325 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.9 -0.325 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 29 A1))
    (pad 1 smd rect (at -2.9 -0.975 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 A0))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP2.54x2.8mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.9 101.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 2 -0.1 180) (layer F.SilkS))
    (fp_text value 49.9R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 ETH_TX+))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C19-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133 101.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 2 0.1 180) (layer F.SilkS))
    (fp_text value 49.9R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 "Net-(C19-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 ETH_TX-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 133 106.6 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -2.46 -0.1 180) (layer F.SilkS))
    (fp_text value 49.9R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 ETH_RX-))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(C20-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 130.9 106.6 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.46 0.09 180) (layer F.SilkS))
    (fp_text value 49.9R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 "Net-(C20-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 ETH_RX+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-143 (layer F.Cu) (tedit 5A02FF57)
    (at 133.8 75.873 270)
    (descr SOT-143)
    (tags SOT-143)
    (attr smd)
    (fp_text reference D5 (at 2.727 0.5 180) (layer F.SilkS))
    (fp_text value SP0503BAHT (at -0.28 2.48 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.77 180) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.1 0.95 180) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 59 USB_IN+))
    (pad 3 smd rect (at 1.1 0.95 180) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 60 USB_IN-))
    (pad 4 smd rect (at 1.1 -0.95 180) (size 1 1.4) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-143.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 151.76 71.89)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at 2.14 0.11 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(R7-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(J4-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 151.8 73.63)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 2.1 0.05 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(J4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT95P275X110-6N (layer F.Cu) (tedit 0)
    (at 151.43 76.43 180)
    (descr "TSOP-6 CASE318G-02")
    (tags "Integrated Circuit")
    (attr smd)
    (fp_text reference U5 (at 3.03 0.93 180) (layer F.SilkS))
    (fp_text value STF202-22T1G (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.25 -0.95 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 5V_BOOST))
    (pad 2 smd rect (at -1.25 0 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 USB_OUT-))
    (pad 3 smd rect (at -1.25 0.95 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 USB_OUT+))
    (pad 4 smd rect (at 1.25 0.95 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(R7-Pad1)"))
    (pad 5 smd rect (at 1.25 0 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(R8-Pad1)"))
    (pad 6 smd rect (at 1.25 -0.95 270) (size 0.6 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/TSOT-23-6.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.5mm locked (layer B.Cu) (tedit 5A0F774F)
    (at 137.66 79.84 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0.06 1.74 180) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 55 "/Power Subsystems/OTG"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm locked (layer B.Cu) (tedit 5A0F774F)
    (at 140.37 79.81 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at -0.13 1.71 180) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 54 "/Power Subsystems/~CE"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm locked (layer B.Cu) (tedit 5A0F774F)
    (at 148.27 79.83 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP7 (at -1.93 1.13) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 51 "/Power Subsystems/~QON"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm locked (layer B.Cu) (tedit 5A0F774F)
    (at 142.97 79.84 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP8 (at -0.33 1.84 180) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 53 "/Power Subsystems/ILIM"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm locked (layer B.Cu) (tedit 5A0F774F)
    (at 134.5 76.9 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP9 (at 2.5 0.1) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 57 "/Power Subsystems/STAT"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm locked (layer B.Cu) (tedit 5A0F774F)
    (at 134.83 79.77 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP10 (at 2.93 -0.03) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 56 "/Power Subsystems/INT"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm locked (layer B.Cu) (tedit 5A0F774F)
    (at 137.4 69 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP11 (at 0 1.648) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 50 "/Power Subsystems/DSEL"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm locked (layer B.Cu) (tedit 5A0F774F)
    (at 145.56 79.85 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP12 (at -1.04 1.85 180) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 52 "/Power Subsystems/TS"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm locked (layer B.Cu) (tedit 5A0F774F)
    (at 123.8 70 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP13 (at -1.4 -1.8) (layer B.SilkS))
    (fp_text value TestPoint (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 58 "/Power Subsystems/ID"))
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 145.7 79.4 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at -2.3 1.8) (layer F.SilkS))
    (fp_text value MBR130T3G (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 VIN))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 VBAT))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Onion-Omega to Feather Adapter\nv0.0.1 20/04/2020\nby Tisham (whatnick) Dhar\nOSHW TAPR" (at 149.86 95.25) (layer B.SilkS))
  (gr_line (start 116.84 63.5) (end 116.8505 68.64) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 110.49 111.76) (end 110.49 110.49) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 110.49 86.36) (end 110.49 85.09) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 110.49 86.36) (end 110.49 83.82) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 110.49 111.76) (end 107.95 111.76) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 165.1 111.76) (end 165.1 114.3) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 165.1 63.5) (end 167.64 63.5) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 119.38 63.5) (end 119.38 60.96) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.49 114.3) (end 116.84 114.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107.95 86.36) (end 107.95 111.76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.84 83.82) (end 110.49 83.82) (layer Edge.Cuts) (width 0.05))
  (dimension 50.8 (width 0.15) (layer Dwgs.User)
    (gr_text "50.800 mm" (at 142.24 52.04) (layer Dwgs.User))
    (feature1 (pts (xy 116.84 60.96) (xy 116.84 52.753579)))
    (feature2 (pts (xy 167.64 60.96) (xy 167.64 52.753579)))
    (crossbar (pts (xy 167.64 53.34) (xy 116.84 53.34)))
    (arrow1a (pts (xy 116.84 53.34) (xy 117.966504 52.753579)))
    (arrow1b (pts (xy 116.84 53.34) (xy 117.966504 53.926421)))
    (arrow2a (pts (xy 167.64 53.34) (xy 166.513496 52.753579)))
    (arrow2b (pts (xy 167.64 53.34) (xy 166.513496 53.926421)))
  )
  (dimension 53.34 (width 0.15) (layer Dwgs.User)
    (gr_text "53.340 mm" (at 179.1 87.63 270) (layer Dwgs.User))
    (feature1 (pts (xy 167.64 114.3) (xy 178.386421 114.3)))
    (feature2 (pts (xy 167.64 60.96) (xy 178.386421 60.96)))
    (crossbar (pts (xy 177.8 60.96) (xy 177.8 114.3)))
    (arrow1a (pts (xy 177.8 114.3) (xy 177.213579 113.173496)))
    (arrow1b (pts (xy 177.8 114.3) (xy 178.386421 113.173496)))
    (arrow2a (pts (xy 177.8 60.96) (xy 177.213579 62.086504)))
    (arrow2b (pts (xy 177.8 60.96) (xy 178.386421 62.086504)))
  )
  (gr_line (start 165.1 60.96) (end 119.38 60.96) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.64 111.76) (end 167.64 63.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.84 114.3) (end 165.1 114.3) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.8505 76.14) (end 116.84 83.82) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169 116) (xy 107 116) (xy 107 60) (xy 169 60)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169 116) (xy 107 116) (xy 107 60) (xy 169 60)
      )
    )
  )
  (zone (net 15) (net_name "Net-(C7-Pad1)") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.8 67) (xy 149.8 71) (xy 149.4 71.4) (xy 144.7 71.4) (xy 144.1 70.8)
        (xy 142.4 70.8) (xy 142.1 71.1) (xy 142.1 71.6) (xy 141.9 71.8) (xy 140 71.8)
        (xy 140 71.1) (xy 141.2 71.1) (xy 142.7 69.6) (xy 142.7 66.9) (xy 143 66.6)
        (xy 149.4 66.6)
      )
    )
  )
  (zone (net 16) (net_name "/Power Subsystems/SYS") (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 149.7 73) (xy 149.7 74.5) (xy 149 75.2) (xy 142.4 75.2) (xy 142.2 75)
        (xy 142.2 74.1) (xy 141.9 73.8) (xy 140.9 73.8) (xy 140.9 73.1) (xy 142.2 73.1)
        (xy 142.5 72.8) (xy 149.5 72.8)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169 116) (xy 107 116) (xy 107 60) (xy 169 60)
      )
    )
  )
  (zone (net 3) (net_name 3.3V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169 116) (xy 107 116) (xy 107 60) (xy 169 60)
      )
    )
  )
)
